#!/bin/sh -e
PATH=$PATH:/home/qi/cae-tools/cameo
PATH=$PATH:/home/moko/svn.openmoko.org/developers/werner/cncmap/gp2rml

NAME=atben
X0=8.6mm
Y0=7.1mm
X=0
Y=0

cameo <<EOF
mm

gerber 35mil ../$NAME-PCB_Edges.gbr
align 1 $X0 $Y0		# align relative to board corner
translate 4mm 4mm	# move to PCB zone assigned to project
#translate 40mm 0mm	# skip over previous boards
array +19mm +2.5mm $X $Y

z 0 -58.9mm		# board surface (tool fully retracted)
z 1.5mm			# slack for extending the tool
z -0.8mm		# board thickness
z -0.5mm		# tool extra depth
clear

# ---- 1st board ----

excellon ../$NAME.drl
drill 7mil 15mil	# 12.5-13.5 mil drill
optimize
write drill.gp

remainder
mill 20mil 0.01mm	# 35 mil endmill; pretend it is a little smaller,
			# to compensate for tool/board deflections
write mill.gp

remainder
empty

gerber 20mil ../$NAME-PCB_Edges.gbr	# 35 mil endmill, 15 mil deflection
offset
append mill.gp

clear

# ---- 2nd board ----

reset

gerber 35mil ../$NAME-PCB_Edges.gbr
rotate 180

align 1 $X0 $Y0		# align relative to board corner
translate 4mm 4mm	# move to PCB zone assigned to project
#translate 40mm 0mm	# skip over previous boards
translate 15mm 0mm
array +19mm +2.5mm $X $Y

clear

excellon ../$NAME.drl
drill 7mil 15mil	# 12.5-13.5 mil drill
optimize
append drill.gp

remainder
mill 20mil 0.01mm	# 35 mil endmill; pretend it is a little smaller,
			# to compensate for tool/board deflections
append mill.gp

remainder
empty

gerber 20mil ../$NAME-PCB_Edges.gbr	# 35 mil endmill, 15 mil deflection
offset
append mill.gp
EOF


gp2rml 2 0.5 0.5 mill.gp >mill.rml
gp2rml 2 0.1 0.5 drill.gp >drill.rml


cat <<EOF >Makefile.mkmk
SPOOL=/home/moko/svn.openmoko.org/developers/werner/cncmap/spool/spool
CNGT=/home/qi/cae-tools/cngt/cngt

.PHONY:		mill drill cng plot dplot

mill:
		PORT=/dev/ttyUSB0 \$(SPOOL) mill.rml

drill:
		PORT=/dev/ttyUSB0 \$(SPOOL) drill.rml

cng:
		\$(CNGT) -57.4 20 mill.gp

plot:
		echo 'plot "drill.gp" with points, "mill.gp" with lines' | \\
		  gnuplot -persist

dplot:
		echo 'plot "< sed /^\$\$/d drill.gp" with linespoints' | \\
		  gnuplot -persist

clean::
		rm -f mill.gp mill.rml drill.gp drill.rml
EOF
