#
# Tags:
#
# F	Footprint name (must be first)
# N	Data sheet identifier (N tag of BOOKSHELF; can be omitted if equal to F)
#

# TI meandered inverted F antenna
F: meander
N: AN043

# Common 4-pin crystal SMT package (pins 1 and 4 are on a short side, pin
# numbering is counter-clockwise)
F: xtal-4
N: nx3225sa

# 0805 package with six pads
F: 0805-6

#
# MMCX board-edge (SMT) female jack
#
# Design based on Molex 73415-0961, This is also compatible with:
#
# Tyco 1408152-1
# Emerson 135-3711-801
# Molex 73415-1261
# Amphenol 262107
#
# Note: footprint changes with PCB thickness !
#
# Known bugs:
# - keepout area marker should be on comment layer
# - pin 2 should be off-center and extend such that proper trace can be
#   connected directly
#
F: mmcx-f-edge
N: 73415-0961

# U.FL/Micro Coax/... receptacle
F: u-fl-receptacle
N: u.fl-receptacle
