ERC control (4/10/2009-04:49:17)

***** Sheet / (Root) 

***** Sheet /LCD_USB/
ERC: Warning Pin input Unconnected (X= 3.950 inches, Y= 2.250 inches
ERC: Warning Pin input Unconnected (X= 3.950 inches, Y= 2.150 inches
ERC: Warning Pin input Unconnected (X= 3.950 inches, Y= 2.100 inches
ERC: Warning Pin input Unconnected (X= 3.950 inches, Y= 2.200 inches

***** Sheet /POWER_TREE/

***** Sheet /FUNCTION_BLOCK/

***** Sheet /MEMORY/
ERC: Warning Pin 3state Unconnected (X= 3.650 inches, Y= 2.950 inches

***** Sheet /AUDIO/

***** Sheet /KEY_MATRIX/

 >> Errors ERC: 5
