NET clk   LOC = "P38";
NET reset LOC = "P71";
NET led   LOC = "P44";

#ADDRESS BUS
#NET "addr<12>" LOC = "P90";
#NET "addr<11>" LOC = "P91";
#NET "addr<10>" LOC = "P85";
#NET "addr<9>" LOC = "P92";
#NET "addr<8>" LOC = "P94";
#NET "addr<7>" LOC = "P95";
#NET "addr<6>" LOC = "P98";
#NET "addr<5>" LOC = "P3";
#NET "addr<4>" LOC = "P2";
#NET "addr<3>" LOC = "P78";
#NET "addr<2>" LOC = "P79";
#NET "addr<1>" LOC = "P83";
#NET "addr<0>" LOC = "P84";

#DATA BUS
#NET "sram_data<7>"  LOC = "P4";
#NET "sram_data<6>"  LOC = "P5";
#NET "sram_data<5>"  LOC = "P9";
#NET "sram_data<4>"  LOC = "P10";
#NET "sram_data<3>"  LOC = "P11";
#NET "sram_data<2>"  LOC = "P12";
#NET "sram_data<1>"  LOC = "P15";
#NET "sram_data<0>"  LOC = "P16";

#CONTROL BUS
#NET "nwe"   LOC = "P88";
#NET "noe"   LOC = "P86";
#NET "ncs"   LOC = "P69";

#ADC
#NET "ADC_EOC"    LOC = "P17";
#NET "ADC_SCLK"   LOC = "P18";
#NET "ADC_SDIN"   LOC = "P22";
#NET "ADC_SDOUT"  LOC = "P23";
#NET "ADC_CS"     LOC = "P24";
#NET "ADC_CSTART" LOC = "P26";


