#
# $Id: ep2c8 897 2007-12-29 13:02:32Z arniml $
#
# This program is free software; you can redistribute it and/or
# modify it under the terms of the GNU General Public License
# as published by the Free Software Foundation; either version 2
# of the License, or (at your option) any later version.
#
# This program is distributed in the hope that it will be useful,
# but WITHOUT ANY WARRANTY; without even the implied warranty of
# MERCHANTABILITY or FITNESS FOR A PARTICULAR PURPOSE.  See the
# GNU General Public License for more details.
#
# You should have received a copy of the GNU General Public License
# along with this program; if not, write to the Free Software
# Foundation, Inc., 59 Temple Place - Suite 330, Boston, MA
# 02111-1307, USA.
#
# Written by H Hartley Sweeten <hsweeten@visionengravers.com>
#
# Note:
#   The signals defined in this file are generic for any EP2C8/EP2C8A.
#   Signalnames according to Altera's package tables are set in the
#   package specific scripts.
#
#                  **Testing Differential Pin Pairs**
#   Refer to the note in the original bsd-files for issues related to
#   testing differential pin pairs!
#
#   Pins T144-1/Q208-1/F256-C3 (BSC198) and T144-2/Q208-2/F256-F4 (BSC197)
#   are dedicated output pins (ASDO and nCSO respectively) when the MSEL
#   pins are connected to set the device in Active Serial programming mode.
#   This configuration file assumes that that mode is not used. Therefore,
#   they are specified as I/O pins.
#
#         | Version (4 bits) | Part number (16 bits) | Manufacturer Id (11 bits) | LSB (1 bit) |
# IDCODE: |         0000     |  0010 0000 1011 0010  |       000 0110 1110       |      1      |
#
# Documentation:
# [1] Altera Corporation, "Cyclone II Device Handbook", CII5V1-3.2
# [2] Altera Corporation, "Pin Information for the Cyclone(r) II EP2C8 & EP2C8A Devices", Version 1.8
# [3] Altera Corporation, "EP2C8F256.BSD", Revision 1.03, 11/10/2006
# [4] Altera Corporation, "EP2C8Q208.BSD", Revision 1.03, 11/10/2006
# [5] Altera Corporation, "EP2C8T144.BSD", Revision 1.03, 11/10/2006

register	BYPASS		1
register	BSR		597
register	IOCSR		5640
register	DEVICE_ID	32
register	USERCODE	32

instruction length 10
instruction	BYPASS		1111111111	BYPASS
instruction	IDCODE		0000000110	DEVICE_ID
instruction	USERCODE	0000000111	USERCODE
instruction	CLAMP		0000001010	BYPASS
instruction	SAMPLE/PRELOAD	0000000101	BSR
instruction	EXTEST		0000001111	BSR
instruction	CONFIG_IO	0000001101	IOCSR
instruction	HIGHZ		0000001011	BYPASS


			# Bank  VREFB Group  Pin Name  Optional Function(s)  Configuration Function  T144  Q208  F256
			# ----  -----------  --------  --------------------  ----------------------  ----  ----  ----
signal BSC198		#  B1    VREFB1N0    IO        ASDO                  ASDO                    1     1     C3
signal BSC197		#  B1    VREFB1N0    IO        nCSO                  nCSO                    2     2     F4
signal BSC196		#  B1    VREFB1N0    IO        LVDS15p               CRC_ERROR               3     3     C1
signal BSC195		#  B1    VREFB1N0    IO        LVDS15n               CLKUSR                  4     4     C2
signal BSC194		#  B1    VREFB1N0    IO        LVDS14p                                             5     D5
signal BSC193		#  B1    VREFB1N0    IO        LVDS14n                                             6     E5
			#  B1    VREFB1N0    VCCIO1                                                  5     7
signal BSC192		#  B1    VREFB1N0    IO        LVDS13p                                             8     F5
			#  B1    VREFB1N0    GND                                                     6     9
signal BSC191		#  B1    VREFB1N0    IO        LVDS13n                                             10
signal BSC190		#  B1    VREFB1N0    IO        LVDS12p                                             11    D3
signal BSC189		#  B1    VREFB1N0    IO        LVDS12n                                             12    D4
			#  B1    VREFB1N0    VCCIO1
signal BSC188		#  B1    VREFB1N0    IO        VREFB1N0                                      7     13    F3
signal BSC187		#  B1    VREFB1N0    IO        LVDS11p                                                   D2
signal BSC186		#  B1    VREFB1N0    IO        LVDS11n                                                   D1
signal BSC185		#  B1    VREFB1N0    IO        LVDS10p                                                   E3
signal BSC184		#  B1    VREFB1N0    IO        LVDS10n                                                   E4
                        #  B1    VREFB1N0    GND
signal BSC183		#  B1    VREFB1N0    IO                                                                  G4
signal BSC182		#  B1    VREFB1N0    IO        LVDS9p                                                    J6
signal BSC181		#  B1    VREFB1N0    IO        LVDS9n                                                    H6
signal BSC180		#  B1    VREFB1N0    IO        LVDS8p                                        8     14    E1
signal BSC179		#  B1    VREFB1N0    IO        LVDS8n                                        9     15    E2
			#  B1    VREFB1N0    VCCIO1
signal TDO		#  B1    VREFB1N0    TDO                             TDO                     10    16    G2
signal TMS		#  B1    VREFB1N0    TMS                             TMS                     11    17    G1
signal TCK		#  B1    VREFB1N0    TCK                             TCK                     12    18    F2
signal TDI		#  B1    VREFB1N0    TDI                             TDI                     13    19    F5
signal BSC178		#  B1    VREFB1N0    DATA0     DATA0                 DATA0                   14    20    F1
signal BSC177		#  B1    VREFB1N0    DCLK      DCLK                  DCLK                    15    21    H4
signal BSC176		#  B1    VREFB1N0    nCE                             nCE                     16    22    G5
signal BSC175		#  B1    VREFB1N0    CLK0      LVDSCLK0p/input(3)                            17    23    H2
signal BSC174		#  B1    VREFB1N0    CLK1      LVDSCLK0n/input(3)                            18    24    H1
                        #  B1    VREFB1N0    GND                                                     19    25
signal BSC173		#  B1    VREFB1N0    nCONFIG                         nCONFIG                 20    26    J5
signal BSC172		#  B1    VREFB1N1    CLK2      LVDSCLK1p/input(3)                            21    27    J2
signal BSC171		#  B1    VREFB1N1    CLK3      LVDSCLK1n/input(3)                            22    28    J1
			#  B1    VREFB1N1    VCCIO1                                                  23    29
signal BSC170		#  B1    VREFB1N1    IO        LVDS7p                                        24    30    K2
signal BSC169		#  B1    VREFB1N1    IO        LVDS7n                                        25    31    K1
signal BSC168		#  B1    VREFB1N1    IO        LVDS6p                                                    K4
			#  B1    VREFB1N1    VCCINT                                                  26    32
signal BSC167		#  B1    VREFB1N1    IO        LVDS6n                                              33    K5
signal BSC166		#  B1    VREFB1N1    IO                                                            34
signal BSC165		#  B1    VREFB1N1    IO        LVDS5p                                              35    L1
			#  B1    VREFB1N1    GND                                                     27    36
signal BSC164		#  B1    VREFB1N1    IO        LVDS5n                                                    L2
			#  B1    VREFB1N1    GND
signal BSC163		#  B1    VREFB1N1    IO        VREFB1N1                                      28    37    J4
			#  B1    VREFB1N1    VCCIO1
signal BSC162		#  B1    VREFB1N1    IO        LVDS4p                                                    M1
signal BSC161		#  B1    VREFB1N1    IO        LVDS4n                                                    M2
signal BSC160		#  B1    VREFB1N1    IO        LVDS3p                                                    M3
			#  B1    VREFB1N1    GND                                                           38
signal BSC159		#  B1    VREFB1N1    IO        LVDS3n                                              39    L3
signal BSC158		#  B1    VREFB1N1    IO        LVDS2p                                              40    N1
signal BSC157		#  B1    VREFB1N1    IO        LVDS2n                                              41    N2
signal BSC156		#  B1    VREFB1N1    IO        LVDS1p                                                    P1
signal BSC155		#  B1    VREFB1N1    IO        LVDS1n                                                    P2
			#  B1    VREFB1N1    VCCIO1                                                  29    42
signal BSC154		#  B1    VREFB1N1    IO                                                            43
signal BSC153		#  B1    VREFB1N1    IO        LVDS0p                                              44    N3
signal BSC152		#  B1    VREFB1N1    IO        LVDS0n                                              45    N4
signal BSC151		#  B1    VREFB1N1    IO                                                      30    46    P3
signal BSC150		#  B1    VREFB1N1    IO        PLL1_OUTp                                     31    47    L4
signal BSC149		#  B1    VREFB1N1    IO        PLL1_OUTn                                     32    48    M4
			#  B1    VREFB1N1    GND                                                     33    49
			#  B1    VREFB1N1    GND_PLL1                                                34    50    L5
			#  B1    VREFB1N1    VCCD_PLL1                                               35    51    L6
			#  B1    VREFB1N1    GND_PLL1                                                36    52    N5
			#  B4    VREFB4N1    VCCA_PLL1                                               37    53    M5
			#  B4    VREFB4N1    GNDA_PLL1                                               38    54    M6
			#  B4    VREFB4N1    GND                                                     39    55
signal BSC148		#  B4    VREFB4N1    IO        LVDS77n               DEV_OE                  40    56    R3
signal BSC147		#  B4    VREFB4N1    IO        LVDS77p                                       41    57    T3
signal BSC146		#  B4    VREFB4N1    IO        LVDS76p                                       42    58    P5
signal BSC145		#  B4    VREFB4N1    IO        LVDS76n                                       43    59    P4
signal BSC144		#  B4    VREFB4N1    IO        LVDS75p                                       44    60    T4
signal BSC143		#  B4    VREFB4N1    IO        LVDS75n                                       45    61    R4
			#  B4    VREFB4N1    VCCIO4                                                  46    62
signal BSC142		#  B4    VREFB4N1    IO        LVDS74p                                       47    63    T5
			#  B4    VREFB4N1    GND
signal BSC141		#  B4    VREFB4N1    IO        LVDS74n                                       48    64    R5
signal BSC140		#  B4    VREFB4N1    IO                                                                  N7
signal BSC139		#  B4    VREFB4N1    IO        LVDS73p                                                   K7
signal BSC138		#  B4    VREFB4N1    IO        LVDS73n                                                   K6
			#  B4    VREFB4N1    VCCIO4
			#  B4    VREFB4N1    GND
signal BSC137		#  B4    VREFB4N1    IO        LVDS72p                                                   T6
			#  B4    VREFB4N1    GND                                                     49    65
signal BSC136		#  B4    VREFB4N1    IO        LVDS72n                                                   R6
signal BSC135		#  B4    VREFB4N1    IO        LVDS71p                                                   P6
signal BSC134		#  B4    VREFB4N1    IO        LVDS71n                                                   N6
			#  B4    VREFB4N1    VCCINT                                                  50    66
signal BSC133		#  B4    VREFB4N1    IO        VREFB4N1                                      51    67    N8
			#  B4    VREFB4N1    VCCIO4
			#  B4    VREFB4N1    GND
signal BSC132		#  B4    VREFB4N1    IO        LVDS70p                                       52    68    T7
signal BSC131		#  B4    VREFB4N1    IO        LVDS70n                                             69    R7
signal BSC130		#  B4    VREFB4N1    IO        LVDS69p                                                   L7
signal BSC129		#  B4    VREFB4N1    IO        LVDS69n                                                   L8
signal BSC128		#  B4    VREFB4N1    IO        LVDS68p                                       53    70    T8
			#  B4    VREFB4N1    VCCIO4                                                  54    71
signal BSC127		#  B4    VREFB4N1    IO        LVDS68n                                       55    72    R8
			#  B4    VREFB4N1    GND                                                     56    73
signal BSC126		#  B4    VREFB4N1    IO        LVDS67p                                       57    74    T9
signal BSC125		#  B4    VREFB4N1    IO        LVDS67n                                       58    75    R9
signal BSC124		#  B4    VREFB4N0    IO        LVDS66p                                       59    76    N9
signal BSC123		#  B4    VREFB4N0    IO        LVDS66n                                       60    77    N10
			#  B4    VREFB4N1    GND                                                     61    78
signal BSC122		#  B4    VREFB4N0    IO        LVDS65p                                                   T11
			#  B4    VREFB4N1    VCCINT                                                  62    79
signal BSC121		#  B4    VREFB4N0    IO        LVDS65n                                                   R11
			#  B4    VREFB4N1    VCCIO4
signal BSC120		#  B4    VREFB4N0    IO                                                            80    P11
			#  B4    VREFB4N0    GND
signal BSC119		#  B4    VREFB4N0    IO        LVDS64p                                             81    L9
signal BSC118		#  B4    VREFB4N0    IO        LVDS64n                                             82    L10
			#  B4    VREFB4N0    VCCIO4                                                        83
signal BSC117		#  B4    VREFB4N0    IO        LVDS63p                                             84    R10
			#  B4    VREFB4N0    GND                                                           85
signal BSC116		#  B4    VREFB4N0    IO        LVDS63n                                             86    T10
signal BSC115		#  B4    VREFB4N0    IO        LVDS62p                                             87    K11
signal BSC114		#  B4    VREFB4N0    IO        LVDS62n                                             88    K10
signal BSC113		#  B4    VREFB4N0    IO        VREFB4N0                                      63    89    N11
signal BSC112		#  B4    VREFB4N0    IO        LVDS61p                                             90    P12
			#  B4    VREFB4N0    VCCIO4                                                        91
signal BSC111		#  B4    VREFB4N0    IO        LVDS61n                                             92    P13
			#  B4    VREFB4N0    GND                                                           93
signal BSC110		#  B4    VREFB4N0    IO        LVDS60p                                       64    94    T12
signal BSC109		#  B4    VREFB4N0    IO        LVDS60n                                       65    95    R12
signal BSC108		#  B4    VREFB4N0    IO                                                            96
signal BSC107		#  B4    VREFB4N0    IO        LVDS59p                                             97    T13
			#  B4    VREFB4N0    VCCIO4                                                  66    98
signal BSC106		#  B4    VREFB4N0    IO        LVDS59n                                       67    99    R13
			#  B4    VREFB4N0    GND                                                     68    100
signal BSC105		#  B4    VREFB4N0    IO        LVDS58p                                       69    101   T14
signal BSC104		#  B4    VREFB4N0    IO        LVDS58n                                       70    102   R14
signal BSC103		#  B4    VREFB4N0    IO        LVDS57p                                       71    103   M11
signal BSC102		#  B4    VREFB4N0    IO        LVDS57n                                       72    104   L11
signal BSC101		#  B3    VREFB3N1    IO        LVDS56n                                       73    105   N12
signal BSC100		#  B3    VREFB3N1    IO        LVDS56p                                       74    106   M12
signal BSC099		#  B3    VREFB3N1    IO        LVDS55n                                                   L12
signal BSC098		#  B3    VREFB3N1    IO        LVDS55p                                                   K13
signal BSC097		#  B3    VREFB3N1    IO        LVDS54n               INIT_DONE               75    107   N13
signal BSC096		#  B3    VREFB3N1    IO        LVDS54p               nCEO                    76    108   N14
			#  B3    VREFB3N1    VCCIO3                                                  77    109
signal BSC095		#  B3    VREFB3N1    IO        LVDS53n                                             110   P15
			#  B3    VREFB3N1    GND                                                     78    111
signal BSC094		#  B3    VREFB3N1    IO        LVDS53p                                             112   P16
signal BSC093		#  B3    VREFB3N1    IO        LVDS52n                                             113   N15
signal BSC092		#  B3    VREFB3N1    IO        LVDS52p                                             114   N16
signal BSC091		#  B3    VREFB3N1    IO                                                                  P14
signal BSC090		#  B3    VREFB3N1    IO        LVDS51n                                             115
signal BSC089		#  B3    VREFB3N1    IO        LVDS51p                                             116
signal BSC088		#  B3    VREFB3N1    IO        VREFB3N1                                      79    117   M14
signal BSC087		#  B3    VREFB3N1    IO        LVDS50n                                                   M15
			#  B3    VREFB3N1    VCCIO3
signal BSC086		#  B3    VREFB3N1    IO        LVDS50p                                                   M16
			#  B3    VREFB3N1    GND
signal BSC085		#  B3    VREFB3N1    IO                                                            118
			#  B3    VREFB3N1    GND                                                     80    119
signal BSC084		#  B3    VREFB3N1    IO                                                                  L14
signal BSC083		#  B3    VREFB3N1    IO        LVDS49n                                                   L15
signal BSC082		#  B3    VREFB3N1    IO        LVDS49p                                                   L16
			#  B3    VREFB3N1    VCCINT                                                  81    120
signal BSC081		#  B3    VREFB3N1    nSTATUS                         nSTATUS                 82    121   M13
			#  B3    VREFB3N1    VCCIO3                                                        122
signal BSC080		#  B3    VREFB3N1    CONF_DONE                       CONF_DONE               83    123   L13
			#  B3    VREFB3N1    GND                                                           124
signal BSC079		#  B3    VREFB3N1    MSEL1                           MSEL1                   84    125   K12
signal BSC078		#  B3    VREFB3N1    MSEL0                           MSEL0                   85    126   J13
signal BSC077		#  B3    VREFB3N1    IO        LVDS48n                                       86    127   K16
signal BSC076		#  B3    VREFB3N1    IO        LVDS48p                                       87    128   K15
signal BSC075		#  B3    VREFB3N1    CLK7      LVDSCLK3n/input(3)                            88    129   J16
signal BSC074		#  B3    VREFB3N1    CLK6      LVDSCLK3p/input(3)                            89    130   J15
signal BSC073		#  B3    VREFB3N0    CLK5      LVDSCLK2n/input(3)                            90    131   H15
signal BSC072		#  B3    VREFB3N0    CLK4      LVDSCLK2p/input(3)                            91    132   H16
signal BSC071		#  B3    VREFB3N0    IO        LVDS47n                                       92    133   H12
signal BSC070		#  B3    VREFB3N0    IO        LVDS47p                                       93    134   J12
signal BSC069		#  B3    VREFB3N0    IO        LVDS46n                                       94    135   G16
			#  B3    VREFB3N0    VCCIO3                                                  95    136
signal BSC068		#  B3    VREFB3N0    IO        LVDS46p                                       96    137   G15
signal BSC067		#  B3    VREFB3N0    IO        LVDS46n                                       97    138   F15
signal BSC066		#  B3    VREFB3N0    IO        LVDS45p                                             139   F16
			#  B3    VREFB3N0    GND                                                     98    140
signal BSC065		#  B3    VREFB3N0    IO        LVDS44n                                             141   J11
signal BSC064		#  B3    VREFB3N0    IO        LVDS44p                                             142   H11
signal BSC063		#  B3    VREFB3N0    IO        LVDS43n                                                   G12
signal BSC062		#  B3    VREFB3N0    IO        LVDS43p                                                   G13
signal BSC061		#  B3    VREFB3N0    IO        LVDS32n                                             143   E13
signal BSC060		#  B3    VREFB3N0    IO        LVDS42p                                             144   F13
signal BSC059		#  B3    VREFB3N0    IO        VREFB3N0                                      99    145   H13
			#  B3    VREFB3N0    VCCIO3
signal BSC058		#  B3    VREFB3N0    IO        LVDS41n                                                   D15
signal BSC057		#  B3    VREFB3N0    IO        LVDS41p                                                   D16
signal BSC056		#  B3    VREFB3N0    IO        LVDS40n                                                   E15
			#  B3    VREFB3N0    GND
signal BSC055		#  B3    VREFB3N0    IO        LVDS40p                                                   E16
signal BSC054		#  B3    VREFB3N0    IO                                                                  F14
signal BSC053		#  B3    VREFB3N0    IO        LVDS39n                                       100   146   C15
signal BSC052		#  B3    VREFB3N0    IO        LVDS39p                                       101   147   C16
			#  B3    VREFB3N0    VCCIO3                                                  102   148
signal BSC051		#  B3    VREFB3N0    IO        LVDS38n                                             149   C14
signal BSC050		#  B3    VREFB3N0    IO        LVDS38p                                             150   D13
signal BSC049		#  B3    VREFB3N0    IO        PLL2_OUTp                                     103   151   E14
signal BSC048		#  B3    VREFB3N0    IO        PLL2_OUTn                                     104   152   D14
			#  B3    VREFB3N0    GND                                                     105   153
			#  B3    VREFB3N0    GND_PLL2                                                106   154   F12
			#  B3    VREFB3N0    VCCD_PLL2                                               107   155   F11
			#  B3    VREFB3N0    GND_PLL2                                                108   156   D12
			#  B2    VREFB2N0    VCCA_PLL2                                               109   157   E12
			#  B2    VREFB2N0    GNDA_PLL2                                               110   158   E11
			#  B2    VREFB2N0    GND                                                     111   159
signal BSC047		#  B2    VREFB2N0    IO        LVDS37n                                       112   160   B14
signal BSC046		#  B2    VREFB2N0    IO        LVDS37p                                       113   161   A14
signal BSC045		#  B2    VREFB2N0    IO        LVDS36n                                       114   162   C13
signal BSC044		#  B2    VREFB2N0    IO        LVDS36p                                       115   163   C12
signal BSC043		#  B2    VREFB2N0    IO        LVDS35n                                             164   B13
signal BSC042		#  B2    VREFB2N0    IO        LVDS35p                                             165   A13
			#  B2    VREFB2N0    VCCIO2                                                  116   166
			#  B2    VREFB2N0    GND                                                     117   167
signal BSC041		#  B2    VREFB2N0    IO        LVDS34n                                       118   168   B12
signal BSC040		#  B2    VREFB2N0    IO        LVDS34p                                       119   169   A12
signal BSC039		#  B2    VREFB2N0    IO        VREFB2N0                                      120   170   C11
signal BSC038		#  B2    VREFB2N0    IO        LVDS33n                                       121   171   B11
			#  B2    VREFB2N0    VCCIO2                                                        172
signal BSC037		#  B2    VREFB2N0    IO        LVDS33p                                       122   173   A11
			#  B2    VREFB2N0    GND                                                           174
signal BSC036		#  B2    VREFB2N0    IO        LVDS32n                                                   G10
signal BSC035		#  B2    VREFB2N0    IO        LVDS32p                                                   G11
signal BSC034		#  B2    VREFB2N0    IO        LVDS31n                                             175   B10
			#  B2    VREFB2N0    VCCIO2
signal BSC033		#  B2    VREFB2N0    IO        LVDS21p                                             176   A10
			#  B2    VREFB2N0    GND
signal BSC032		#  B2    VREFB2N0    IO        LVDS30n                                                   F10
signal BSC031		#  B2    VREFB2N0    IO        LVDS30p                                                   F9
signal BSC030		#  B2    VREFB2N0    IO                                                                  D9
			#  B2    VREFB2N0    GND                                                     123   177
			#  B2    VREFB2N0    VCCINT                                                  124   178
signal BSC029		#  B2    VREFB2N0    IO        LVDS29n                                       125   179   D11
			#  B2    VREFB2N0    VCCIO2
signal BSC028		#  B2    VREFB2N0    IO        LVDS29p                                       126   180   D10
			#  B2    VREFB2N0    GND
signal BSC027		#  B2    VREFB2N0    IO        LVDS28n                                             181   A9
signal BSC026		#  B2    VREFB2N0    IO        LVDS28p                                             182   B9
signal BSC025		#  B2    VREFB2N1    IO        LVDS27n                                                   A8
signal BSC024		#  B2    VREFB2N1    IO        LVDS27p                                                   B8
			#  B2    VREFB2N1    VCCIO2                                                  127   183
signal BSC023		#  B2    VREFB2N1    IO        LVDS26n                                                   A7
			#  B2    VREFB2N1    GND                                                     128   184
signal BSC022		#  B2    VREFB2N1    IO        LVDS26p                                       129   185   B7
			#  B2    VREFB2N1    GND                                                     130   186
signal BSC021		#  B2    VREFB2N1    IO        LVDS25n                                             187   F7
signal BSC020		#  B2    VREFB2N1    IO        LVDS25p                                             188   F8
signal BSC019		#  B2    VREFB2N1    IO        LVDS24n                                             189
			#  B2    VREFB2N1    VCCINT                                                  131   190
signal BSC018		#  B2    VREFB2N1    IO        LVDS24p                                             191
signal BSC017		#  B2    VREFB2N1    IO        VREFB2N1                                      132   192   D8
signal BSC016		#  B2    VREFB2N1    IO        LVDS23n                                       133   193   B6
			#  B2    VREFB2N1    VCCIO2                                                        194
signal BSC015		#  B2    VREFB2N1    IO        LVDS23p                                       134   195   A6
			#  B2    VREFB2N1    GND                                                           196
signal BSC014		#  B2    VREFB2N1    IO        LVDS22n                                                   G6
signal BSC013		#  B2    VREFB2N1    IO        LVDS22p                                                   G7
signal BSC012		#  B2    VREFB2N1    IO                                                                  D7
signal BSC011		#  B2    VREFB2N1    IO        LVDS21n                                             197   D6
			#  B2    VREFB2N1    VCCIO2
signal BSC010		#  B2    VREFB2N1    IO        LVDS21p                                             198   C6
			#  B2    VREFB2N1    GND
signal BSC009		#  B2    VREFB2N1    IO        LVDS20n                                                   C5
signal BSC008		#  B2    VREFB2N1    IO        LVDS20p                                                   C4
signal BSC007		#  B2    VREFB2N1    IO        LVDS19n                                       135   199   B5
signal BSC006		#  B2    VREFB2N1    IO        LVDS19p                                       136   200   A5
signal BSC005		#  B2    VREFB2N1    IO        LVDS18n                                       137   201   B4
			#  B2    VREFB2N1    VCCIO2                                                  138   202
signal BSC004		#  B2    VREFB2N1    IO        LVDS18p                                       139   203   A4
			#  B2    VREFB2N1    GND                                                     140   204
signal BSC003		#  B2    VREFB2N1    IO        LVDS17p                                       141   205   A3
signal BSC002		#  B2    VREFB2N1    IO        LVDS17n               DEV_CLRn                142   206   B3
signal BSC001		#  B2    VREFB2N1    IO        LVDS16p                                       143   207   E6
signal BSC000		#  B2    VREFB2N1    IO        LVDS16n                                       144   208   F6
			#                    VCCINT                                                              G9
			#                    VCCINT                                                              H7
			#                    VCCINT                                                              H10
			#                    VCCINT                                                              J7
			#                    VCCINT                                                              J10
			#                    VCCINT                                                              K8
			#                    VCCIO1                                                              B1
			#                    VCCIO1                                                              G3
			#                    VCCIO1                                                              K3
			#                    VCCIO1                                                              R1
			#                    VCCIO4                                                              M7
			#                    VCCIO4                                                              M10
			#                    VCCIO4                                                              P7
			#                    VCCIO4                                                              P10
			#                    VCCIO4                                                              T2
			#                    VCCIO4                                                              T15
			#                    VCCIO3                                                              B16
			#                    VCCIO3                                                              G14
			#                    VCCIO3                                                              K14
			#                    VCCIO3                                                              R16
			#                    VCCIO2                                                              A2
			#                    VCCIO2                                                              A15
			#                    VCCIO2                                                              C7
			#                    VCCIO2                                                              C10
			#                    VCCIO2                                                              E7
			#                    VCCIO2                                                              E10
			#                    GND                                                                 G8
			#                    GND                                                                 H8
			#                    GND                                                                 H9
			#                    GND                                                                 J8
			#                    GND                                                                 J9
			#                    GND                                                                 K9
			#                    GND                                                                 A1
			#                    GND                                                                 A16
			#                    GND                                                                 B2
			#                    GND                                                                 B15
			#                    GND                                                                 C8
			#                    GND                                                                 C9
			#                    GND                                                                 E8
			#                    GND                                                                 E9
			#                    GND                                                                 H3
			#                    GND                                                                 H14
			#                    GND                                                                 J3
			#                    GND                                                                 J14
			#                    GND                                                                 M8
			#                    GND                                                                 M9
			#                    GND                                                                 P8
			#                    GND                                                                 P9
			#                    GND                                                                 R2
			#                    GND                                                                 R15
			#                    GND                                                                 T1
			#                    GND                                                                 T16

#
# BSC group 198
#   T144 - I/O pin 1 (dedicated output pin in AS mode)
#   Q208 - I/O pin 1 (dedicated output pin in AS mode)
#   F256 - I/O pin C3 (dedicated output pin in AS mode)
#
bit 596 O 1 BSC198 595 1 Z
bit 595 C 1 *
bit 594 I 1 BSC198
#
# BSC group 197
#   T144 - I/O pin 2 (dedicated output pin in AS mode)
#   Q208 - I/O pin 2 (dedicated output pin in AS mode)
#   F256 - I/O pin F4 (dedicated output pin in AS mode)
#
bit 593 O 1 BSC197 592 1 Z
bit 592 C 1 *
bit 591 I 1 BSC197
#
# BSC group 196
#   T144 - I/O pin 3
#   Q208 - I/O pin 3
#   F256 - I/O pin C1
#
bit 590 O 1 BSC196 589 1 Z
bit 589 C 1 *
bit 588 I 1 BSC196
#
# BSC group 195
#   T144 - I/O pin 4
#   Q208 - I/O pin 4
#   F256 - I/O pin C2
#
bit 587 O 1 BSC195 586 1 Z
bit 586 C 1 *
bit 585 I 1 BSC195
#
# BSC group 194 for
#   T144 - unused pad
#   Q208 - I/O pin 5
#   F256 - I/O pin D5
#
bit 584 O 1 BSC194 583 1 Z
bit 583 C 1 *
bit 582 I 1 BSC194
#
# BSC group 193 for
#   T144 - unused pad
#   Q208 - I/O pin 6
#   F256 - I/O pin E5
#
bit 581 O 1 BSC193 580 1 Z
bit 580 C 1 *
bit 579 I 1 BSC193
#
# BSC group 192
#   T144 - unused pad
#   Q208 - I/O pin 8
#   F256 - I/O pin F5
#
bit 578 O 1 BSC192 577 1 Z
bit 577 C 1 *
bit 576 I 1 BSC192
#
# BSC group 191
#   T144 - unused pad
#   Q208 - I/O pin 10
#   F256 - unused pad
#
bit 575 O 1 BSC191 574 1 Z
bit 574 C 1 *
bit 573 I 1 BSC191
#
# BSC group 190
#   T144 - unused pad
#   Q208 - I/O pin 11
#   F256 - I/O pin D3
#
bit 572 O 1 BSC190 571 1 Z
bit 571 C 1 *
bit 570 I 1 BSC190
#
# BSC group 189
#   T144 - unused pad
#   Q208 - I/O pin 12
#   F256 - I/O pin D4
#
bit 569 O 1 BSC189 568 1 Z
bit 568 C 1 *
bit 567 I 1 BSC189
#
# BSC group 188
#   T144 - I/O pin 7
#   Q208 - I/O pin 13
#   F256 - I/O pin F3
#
bit 566 O 1 BSC188 565 1 Z
bit 565 C 1 *
bit 564 I 1 BSC188
#
# BSC group 187
#   T144 - unused pad
#   Q208 - unused pad
#   F256 - I/O pin D2
#
bit 563 O 1 BSC187 562 1 Z
bit 562 C 1 *
bit 561 I 1 BSC187
#
# BSC group 186
#   T144 - unused pad
#   Q208 - unused pad
#   F256 - I/O pin D1
#
bit 560 O 1 BSC186 559 1 Z
bit 559 C 1 *
bit 558 I 1 BSC186
#
# BSC group 185
#   T144 - unused pad
#   Q208 - unused pad
#   F256 - I/O pin E3
#
bit 557 O 1 BSC185 556 1 Z
bit 556 C 1 *
bit 555 I 1 BSC185
#
# BSC group 184
#   T144 - unused pad
#   Q208 - unused pad
#   F256 - I/O pin E4
#
bit 554 O 1 BSC184 553 1 Z
bit 553 C 1 *
bit 552 I 1 BSC184
#
# BSC group 183
#   T144 - unused pad
#   Q208 - unused pad
#   F256 - I/O pin G4
#
bit 551 O 1 BSC183 550 1 Z
bit 550 C 1 *
bit 549 I 1 BSC183
#
# BSC group 182
#   T144 - unused pad
#   Q208 - unused pad
#   F256 - I/O pin J6
#
bit 548 O 1 BSC182 547 1 Z
bit 547 C 1 *
bit 546 I 1 BSC182
#
# BSC group 181
#   T144 - unused pad
#   Q208 - unused pad
#   F256 - I/O pin H6
#
bit 545 O 1 BSC181 544 1 Z
bit 544 C 1 *
bit 543 I 1 BSC181
#
# BSC group 180
#   T144 - I/O pin 8
#   Q208 - I/O pin 14
#   F256 - I/O pin E1
#
bit 542 O 1 BSC180 541 1 Z
bit 541 C 1 *
bit 540 I 1 BSC180
#
# BSC group 179
#   T144 - I/O pin 9
#   Q208 - I/O pin 15
#   F256 - I/O pin E2
#
bit 539 O 1 BSC179 538 1 Z
bit 538 C 1 *
bit 537 I 1 BSC179
#
# BSC group 178 (DATA0)
#   T144 - Family-specific input pin 14
#   Q208 - Family-specific input pin 20
#   F256 - Family-specific input pin F1
#
bit 536 O 1 *
bit 535 O 1 *
bit 534 I 1 BSC178
#
# BSC group 177 (DCLK)
#   T144 - Family-specific input pin 15
#   Q208 - Family-specific input pin 21
#   F256 - Family-specific input pin H4
#
bit 533 O 1 BSC177 532 1 Z
bit 532 C 1 *
bit 531 I 1 BSC177
#
# BSC group 176 (nCE)
#   T144 - untestable Family-specific pin 16
#   Q208 - untestable Family-specific pin 22
#   F256 - untestable Family-specific pin G5
#
bit 530 O 1 *
bit 529 O 1 *
bit 528 O 1 *
#
# BSC group 175 (CLK0)
#   T144 - Family-specific input pin 17
#   Q208 - Family-specific input pin 23
#   F256 - Family-specific input pin H2
#
bit 527 O 1 *
bit 526 O 1 *
bit 525 I 1 BSC175
#
# BSC group 174 (CLK1)
#   T144 - Family-specific input pin 18
#   Q208 - Family-specific input pin 24
#   F256 - Family-specific input pin H1
#
bit 524 O 1 *
bit 523 O 1 *
bit 522 I 1 BSC174
#
# BSC group 173 (nCONFIG)
#   T144 - untestable Family-specific pin 20
#   Q208 - untestable Family-specific pin 26
#   F256 - untestable Family-specific pin J5
#
bit 521 O 1 *
bit 520 O 1 *
bit 519 O 1 *
#
# BSC group 172 (CLK2)
#   T144 - Family-specific input pin 21
#   Q208 - Family-specific input pin 27
#   F256 - Family-specific input pin J2
#
bit 518 O 1 *
bit 517 O 1 *
bit 516 I 1 BSC172
#
# BSC group 171 (CLK3)
#   T144 - Family-specific input pin 22
#   Q208 - Family-specific input pin 28
#   F256 - Family-specific input pin J1
#
bit 515 O 1 *
bit 514 O 1 *
bit 513 I 1 BSC171
#
# BSC group 170
#   T144 - I/O pin 24
#   Q208 - I/O pin 30
#   F256 - I/O pin K2
#
bit 512 O 1 BSC170 511 1 Z
bit 511 C 1 *
bit 510 I 1 BSC170
#
# BSC group 169
#   T144 - I/O pin 25
#   Q208 - I/O pin 31
#   F256 - I/O pin K1
#
bit 509 O 1 BSC169 508 1 Z
bit 508 C 1 *
bit 507 I 1 BSC169
#
# BSC group 168
#   T144 - unused pad
#   Q208 - unused pad
#   F256 - I/O pin K4
#
bit 506 O 1 BSC168 505 1 Z
bit 505 C 1 *
bit 504 I 1 BSC168
#
# BSC group 167
#   T144 - unused pad
#   Q208 - I/O pin 33
#   F256 - I/O pin K5
#
bit 503 O 1 BSC167 502 1 Z
bit 502 C 1 *
bit 501 I 1 BSC167
#
# BSC group 166
#   T144 - unused pad
#   Q208 - I/O pin 34
#   F256 - unused pad
#
bit 500 O 1 BSC166 499 1 Z
bit 499 C 1 *
bit 498 I 1 BSC166
#
# BSC group 165
#   T144 - unused pad
#   Q208 - I/O pin 35
#   F256 - I/O pin L1
#
bit 497 O 1 BSC165 496 1 Z
bit 496 C 1 *
bit 495 I 1 BSC165
#
# BSC group 164
#   T144 - unused pad
#   Q208 - unused pad
#   F256 - I/O pin L2
#
bit 494 O 1 BSC164 493 1 Z
bit 493 C 1 *
bit 492 I 1 BSC164
#
# BSC group 163
#   T144 - I/O pin 28
#   Q208 - I/O pin 37
#   F256 - I/O pin J4
#
bit 491 O 1 BSC163 490 1 Z
bit 490 C 1 *
bit 489 I 1 BSC163
#
# BSC group 162
#   T144 - unused pad
#   Q208 - unused pad
#   F256 - I/O pin M1
#
bit 488 O 1 BSC162 487 1 Z
bit 487 C 1 *
bit 486 I 1 BSC162
#
# BSC group 161
#   T144 - unused pad
#   Q208 - unused pad
#   F256 - I/O pin M2
#
bit 485 O 1 BSC161 484 1 Z
bit 484 C 1 *
bit 483 I 1 BSC161
#
# BSC group 160
#   T144 - unused pad
#   Q208 - unused pad
#   F256 - I/O pin M3
#
bit 482 O 1 BSC160 481 1 Z
bit 481 C 1 *
bit 480 I 1 BSC160
#
# BSC group 159
#   T144 - unused pad
#   Q208 - I/O pin 39
#   F256 - I/O pin L3
#
bit 479 O 1 BSC159 478 1 Z
bit 478 C 1 *
bit 477 I 1 BSC159
#
# BSC group 158
#   T144 - unused pad
#   Q208 - I/O pin 40
#   F256 - I/O pin N1
#
bit 476 O 1 BSC158 475 1 Z
bit 475 C 1 *
bit 474 I 1 BSC158
#
# BSC group 157
#   T144 - unused pad
#   Q208 - I/O pin 41
#   F256 - I/O pin N2
#
bit 473 O 1 BSC157 472 1 Z
bit 472 C 1 *
bit 471 I 1 BSC157
#
# BSC group 156
#   T144 - unused pad
#   Q208 - unused pad
#   F256 - I/O pin P1
#
bit 470 O 1 BSC156 469 1 Z
bit 469 C 1 *
bit 468 I 1 BSC156
#
# BSC group 155
#   T144 - unused pad
#   Q208 - unused pad
#   F256 - I/O pin P2
#
bit 467 O 1 BSC155 466 1 Z
bit 466 C 1 *
bit 465 I 1 BSC155
#
# BSC group 154
#   T144 - unused pad
#   Q208 - I/O pin 43
#   F256 - unused pad
#
bit 464 O 1 BSC154 463 1 Z
bit 463 C 1 *
bit 462 I 1 BSC154
#
# BSC group 153
#   T144 - unused pad
#   Q208 - I/O pin 44
#   F256 - I/O pin N3
#
bit 461 O 1 BSC153 460 1 Z
bit 460 C 1 *
bit 459 I 1 BSC153
#
# BSC group 152
#   T144 - unused pad
#   Q208 - I/O pin 45
#   F256 - I/O pin N4
#
bit 458 O 1 BSC152 457 1 Z
bit 457 C 1 *
bit 456 I 1 BSC152
#
# BSC group 151
#   T144 - I/O pin 30
#   Q208 - I/O pin 46
#   F256 - I/O pin P3
#
bit 455 O 1 BSC151 454 1 Z
bit 454 C 1 *
bit 453 I 1 BSC151
#
# BSC group 150
#   T144 - I/O pin 31
#   Q208 - I/O pin 47
#   F256 - I/O pin L4
#
bit 452 O 1 BSC150 451 1 Z
bit 451 C 1 *
bit 450 I 1 BSC150
#
# BSC group 149
#   T144 - I/O pin 32
#   Q208 - I/O pin 48
#   F256 - I/O pin M4
#
bit 449 O 1 BSC149 448 1 Z
bit 448 C 1 *
bit 447 I 1 BSC149
#
# BSC group 148
#   T144 - I/O pin 40
#   Q208 - I/O pin 56
#   F256 - I/O pin R3
#
bit 446 O 1 BSC148 445 1 Z
bit 445 C 1 *
bit 444 I 1 BSC148
#
# BSC group 147
#   T144 - I/O pin 41
#   Q208 - I/O pin 57
#   F256 - I/O pin T3
#
bit 443 O 1 BSC147 442 1 Z
bit 442 C 1 *
bit 441 I 1 BSC147
#
# BSC group 146
#   T144 - I/O pin 42
#   Q208 - I/O pin 58
#   F256 - I/O pin P5
#
bit 440 O 1 BSC146 439 1 Z
bit 439 C 1 *
bit 438 I 1 BSC146
#
# BSC group 145
#   T144 - I/O pin 43
#   Q208 - I/O pin 59
#   F256 - I/O pin P4
#
bit 437 O 1 BSC145 436 1 Z
bit 436 C 1 *
bit 435 I 1 BSC145
#
# BSC group 144
#   T144 - I/O pin 44
#   Q208 - I/O pin 60
#   F256 - I/O pin T4
#
bit 434 O 1 BSC144 433 1 Z
bit 433 C 1 *
bit 432 I 1 BSC144
#
# BSC group 143
#   T144 - I/O pin 45
#   Q208 - I/O pin 61
#   F256 - I/O pin R4
#
bit 431 O 1 BSC143 430 1 Z
bit 430 C 1 *
bit 429 I 1 BSC143
#
# BSC group 142
#   T144 - I/O pin 47
#   Q208 - I/O pin 63
#   F256 - I/O pin T5
#
bit 428 O 1 BSC142 427 1 Z
bit 427 C 1 *
bit 426 I 1 BSC142
#
# BSC group 141
#   T144 - I/O pin 48
#   Q208 - I/O pin 64
#   F256 - I/O pin R5
#
bit 425 O 1 BSC141 424 1 Z
bit 424 C 1 *
bit 423 I 1 BSC141
#
# BSC group 140
#   T144 - unused pad
#   Q208 - unused pad
#   F256 - I/O pin N7
#
bit 422 O 1 BSC140 421 1 Z
bit 421 C 1 *
bit 420 I 1 BSC140
#
# BSC group 139
#   T144 - unused pad
#   Q208 - unused pad
#   F256 - I/O pin K7
#
bit 419 O 1 BSC139 418 1 Z
bit 418 C 1 *
bit 417 I 1 BSC139
#
# BSC group 138
#   T144 - unused pad
#   Q208 - unused pad
#   F256 - I/O pin K6
#
bit 416 O 1 BSC138 415 1 Z
bit 415 C 1 *
bit 414 I 1 BSC138
#
# BSC group 137
#   T144 - unused pad
#   Q208 - unused pad
#   F256 - I/O pin T6
#
bit 413 O 1 BSC137 412 1 Z
bit 412 C 1 *
bit 411 I 1 BSC137
#
# BSC group 136
#   T144 - unused pad
#   Q208 - unused pad
#   F256 - I/O pin R6
#
bit 410 O 1 BSC136 409 1 Z
bit 409 C 1 *
bit 408 I 1 BSC136
#
# BSC group 135
#   T144 - unused pad
#   Q208 - unused pad
#   F256 - I/O pin P6
#
bit 407 O 1 BSC135 406 1 Z
bit 406 C 1 *
bit 405 I 1 BSC135
#
# BSC group 134
#   T144 - unused pad
#   Q208 - unused pad
#   F256 - I/O pin N6
#
bit 404 O 1 BSC134 403 1 Z
bit 403 C 1 *
bit 402 I 1 BSC134
#
# BSC group 133
#   T144 - I/O pin 51
#   Q208 - I/O pin 67
#   F256 - I/O pin N8
#
bit 401 O 1 BSC133 400 1 Z
bit 400 C 1 *
bit 399 I 1 BSC133
#
# BSC group 132
#   T144 - I/O pin 52
#   Q208 - I/O pin 68
#   F256 - I/O pin T7
#
bit 398 O 1 BSC132 397 1 Z
bit 397 C 1 *
bit 396 I 1 BSC132
#
# BSC group 131
#   T144 - unused pad
#   Q208 - I/O pin 69
#   F256 - I/O pin R7
#
bit 395 O 1 BSC131 394 1 Z
bit 394 C 1 *
bit 393 I 1 BSC131
#
# BSC group 130
#   T144 - unused pad
#   Q208 - unused pad
#   F256 - I/O pin L7
#
bit 392 O 1 BSC130 391 1 Z
bit 391 C 1 *
bit 390 I 1 BSC130
#
# BSC group 129
#   T144 - unused pad
#   Q208 - unused pad
#   F256 - I/O pin L8
#
bit 389 O 1 BSC129 388 1 Z
bit 388 C 1 *
bit 387 I 1 BSC129
#
# BSC group 128
#   T144 - I/O pin 53
#   Q208 - I/O pin 70
#   F256 - I/O pin T8
#
bit 386 O 1 BSC128 385 1 Z
bit 385 C 1 *
bit 384 I 1 BSC128
#
# BSC group 127
#   T144 - I/O pin 55
#   Q208 - I/O pin 72
#   F256 - I/O pin R8
#
bit 383 O 1 BSC127 382 1 Z
bit 382 C 1 *
bit 381 I 1 BSC127
#
# BSC group 126
#   T144 - I/O pin 57
#   Q208 - I/O pin 74
#   F256 - I/O pin T9
#
bit 380 O 1 BSC126 379 1 Z
bit 379 C 1 *
bit 378 I 1 BSC126
#
# BSC group 125
#   T144 - I/O pin 58
#   Q208 - I/O pin 75
#   F256 - I/O pin R9
#
bit 377 O 1 BSC125 376 1 Z
bit 376 C 1 *
bit 375 I 1 BSC125
#
# BSC group 124
#   T144 - I/O pin 59
#   Q208 - I/O pin 76
#   F256 - I/O pin N9
#
bit 374 O 1 BSC124 373 1 Z
bit 373 C 1 *
bit 372 I 1 BSC124
#
# BSC group 123
#   T144 - I/O pin 60
#   Q208 - I/O pin 77
#   F256 - I/O pin N10
#
bit 371 O 1 BSC123 370 1 Z
bit 370 C 1 *
bit 369 I 1 BSC123
#
# BSC group 122
#   T144 - unused pad
#   Q208 - unused pad
#   F256 - I/O pin T11
#
bit 368 O 1 BSC122 367 1 Z
bit 367 C 1 *
bit 366 I 1 BSC122
#
# BSC group 121
#   T144 - unused pad
#   Q208 - unused pad
#   F256 - I/O pin R11
#
bit 365 O 1 BSC121 364 1 Z
bit 364 C 1 *
bit 363 I 1 BSC121
#
# BSC group 120
#   T144 - unused pad
#   Q208 - I/O pin 80
#   F256 - I/O pin P11
#
bit 362 O 1 BSC120 361 1 Z
bit 361 C 1 *
bit 360 I 1 BSC120
#
# BSC group 119
#   T144 - unused pad
#   Q208 - I/O pin 81
#   F256 - I/O pin L9
#
bit 359 O 1 BSC119 358 1 Z
bit 358 C 1 *
bit 357 I 1 BSC119
#
# BSC group 118
#   T144 - unused pad
#   Q208 - I/O pin 82
#   F256 - I/O pin L10
#
bit 356 O 1 BSC118 355 1 Z
bit 355 C 1 *
bit 354 I 1 BSC118
#
# BSC group 117
#   T144 - unused pad
#   Q208 - I/O pin 84
#   F256 - I/O pin R10
#
bit 353 O 1 BSC117 352 1 Z
bit 352 C 1 *
bit 351 I 1 BSC117
#
# BSC group 116
#   T144 - unused pad
#   Q208 - I/O pin 86
#   F256 - I/O pin T10
#
bit 350 O 1 BSC116 349 1 Z
bit 349 C 1 *
bit 348 I 1 BSC116
#
# BSC group 115
#   T144 - unused pad
#   Q208 - I/O pin 87
#   F256 - I/O pin K11
#
bit 347 O 1 BSC115 346 1 Z
bit 346 C 1 *
bit 345 I 1 BSC115
#
# BSC group 114
#   T144 - unused pad
#   Q208 - I/O pin 88
#   F256 - I/O pin K10
#
bit 344 O 1 BSC114 343 1 Z
bit 343 C 1 *
bit 342 I 1 BSC114
#
# BSC group 113
#   T144 - I/O pin 63
#   Q208 - I/O pin 89
#   F256 - I/O pin N11
#
bit 341 O 1 BSC113 340 1 Z
bit 340 C 1 *
bit 339 I 1 BSC113
#
# BSC group 112
#   T144 - unused pad
#   Q208 - I/O pin 90
#   F256 - I/O pin P12
#
bit 338 O 1 BSC112 337 1 Z
bit 337 C 1 *
bit 336 I 1 BSC112
#
# BSC group 111
#   T144 - unused pad
#   Q208 - I/O pin 92
#   F256 - I/O pin P13
#
bit 335 O 1 BSC111 334 1 Z
bit 334 C 1 *
bit 333 I 1 BSC111
#
# BSC group 110
#   T144 - I/O pin 64
#   Q208 - I/O pin 94
#   F256 - I/O pin T12
#
bit 332 O 1 BSC110 331 1 Z
bit 331 C 1 *
bit 330 I 1 BSC110
#
# BSC group 109
#   T144 - I/O pin 65
#   Q208 - I/O pin 95
#   F256 - I/O pin R12
#
bit 329 O 1 BSC109 328 1 Z
bit 328 C 1 *
bit 327 I 1 BSC109
#
# BSC group 108
#   T144 - unused pad
#   Q208 - I/O pin 96
#   F256 - unused pad
#
bit 326 O 1 BSC108 325 1 Z
bit 325 C 1 *
bit 324 I 1 BSC108
#
# BSC group 107
#   T144 - unused pad
#   Q208 - I/O pin 97
#   F256 - I/O pin T13
#
bit 323 O 1 BSC107 322 1 Z
bit 322 C 1 *
bit 321 I 1 BSC107
#
# BSC group 106
#   T144 - I/O pin 67
#   Q208 - I/O pin 99
#   F256 - I/O pin R13
#
bit 320 O 1 BSC106 319 1 Z
bit 319 C 1 *
bit 318 I 1 BSC106
#
# BSC group 105
#   T144 - I/O pin 69
#   Q208 - I/O pin 101
#   F256 - I/O pin T14
#
bit 317 O 1 BSC105 316 1 Z
bit 316 C 1 *
bit 315 I 1 BSC105
#
# BSC group 104
#   T144 - I/O pin 70
#   Q208 - I/O pin 102
#   F256 - I/O pin R14
#
bit 314 O 1 BSC104 313 1 Z
bit 313 C 1 *
bit 312 I 1 BSC104
#
# BSC group 103
#   T144 - I/O pin 71
#   Q208 - I/O pin 103
#   F256 - I/O pin M11
#
bit 311 O 1 BSC103 310 1 Z
bit 310 C 1 *
bit 309 I 1 BSC103
#
# BSC group 102
#   T144 - I/O pin 72
#   Q208 - I/O pin 104
#   F256 - I/O pin L11
#
bit 308 O 1 BSC102 307 1 Z
bit 307 C 1 *
bit 306 I 1 BSC102
#
# BSC group 101
#   T144 - I/O pin 73
#   Q208 - I/O pin 105
#   F256 - I/O pin N12
#
bit 305 O 1 BSC101 304 1 Z
bit 304 C 1 *
bit 303 I 1 BSC101
#
# BSC group 100
#   T144 - I/O pin 74
#   Q208 - I/O pin 106
#   F256 - I/O pin M12
#
bit 302 O 1 BSC100 301 1 Z
bit 301 C 1 *
bit 300 I 1 BSC100
#
# BSC group 99
#   T144 - unused pad
#   Q208 - unused pad
#   F256 - I/O pin L12
#
bit 299 O 1 BSC099 298 1 Z
bit 298 C 1 *
bit 297 I 1 BSC099
#
# BSC group 98
#   T144 - unused pad
#   Q208 - unused pad
#   F256 - I/O pin K13
#
bit 296 O 1 BSC098 295 1 Z
bit 295 C 1 *
bit 294 I 1 BSC098
#
# BSC group 97
#   T144 - I/O pin 75
#   Q208 - I/O pin 107
#   F256 - I/O pin N13
#
bit 293 O 1 BSC097 292 1 Z
bit 292 C 1 *
bit 291 I 1 BSC097
#
# BSC group 96
#   T144 - I/O pin 76
#   Q208 - I/O pin 108
#   F256 - I/O pin N14
#
bit 290 O 1 BSC096 289 1 Z
bit 289 C 1 *
bit 288 I 1 BSC096
#
# BSC group 95
#   T144 - unused pad
#   Q208 - I/O pin 110
#   F256 - I/O pin P15
#
bit 287 O 1 BSC095 286 1 Z
bit 286 C 1 *
bit 285 I 1 BSC095
#
# BSC group 94
#   T144 - unused pad
#   Q208 - I/O pin 112
#   F256 - I/O pin P16
#
bit 284 O 1 BSC094 283 1 Z
bit 283 C 1 *
bit 282 I 1 BSC094
#
# BSC group 93
#   T144 - unused pad
#   Q208 - I/O pin 113
#   F256 - I/O pin N15
#
bit 281 O 1 BSC093 280 1 Z
bit 280 C 1 *
bit 279 I 1 BSC093
#
# BSC group 92
#   T144 - unused pad
#   Q208 - I/O pin 114
#   F256 - I/O pin N16
#
bit 278 O 1 BSC092 277 1 Z
bit 277 C 1 *
bit 276 I 1 BSC092
#
# BSC group 91
#   T144 - unused pad
#   Q208 - unused pad
#   F256 - I/O pin P14
#
bit 275 O 1 BSC091 274 1 Z
bit 274 C 1 *
bit 273 I 1 BSC091
#
# BSC group 90
#   T144 - unused pad
#   Q208 - I/O pin 115
#   F256 - unused pad
#
bit 272 O 1 BSC090 271 1 Z
bit 271 C 1 *
bit 270 I 1 BSC090
#
# BSC group 89
#   T144 - unused pad
#   Q208 - I/O pin 116
#   F256 - unused pad
#
bit 269 O 1 BSC089 268 1 Z
bit 268 C 1 *
bit 267 I 1 BSC089
#
# BSC group 88
#   T144 - I/O pin 79
#   Q208 - I/O pin 117
#   F256 - I/O pin M14
#
bit 266 O 1 BSC088 265 1 Z
bit 265 C 1 *
bit 264 I 1 BSC088
#
# BSC group 87
#   T144 - unused pad
#   Q208 - unused pad
#   F256 - I/O pin M15
#
bit 263 O 1 BSC087 262 1 Z
bit 262 C 1 *
bit 261 I 1 BSC087
#
# BSC group 86
#   T144 - unused pad
#   Q208 - unused pad
#   F256 - I/O pin M16
#
bit 260 O 1 BSC086 259 1 Z
bit 259 C 1 *
bit 258 I 1 BSC086
#
# BSC group 85
#   T144 - unused pad
#   Q208 - I/O pin 118
#   F256 - unused pad
#
bit 257 O 1 BSC085 256 1 Z
bit 256 C 1 *
bit 255 I 1 BSC085
#
# BSC group 84
#   T144 - unused pad
#   Q208 - unused pad
#   F256 - I/O pin L14
#
bit 254 O 1 BSC084 253 1 Z
bit 253 C 1 *
bit 252 I 1 BSC084
#
# BSC group 83
#   T144 - unused pad
#   Q208 - unused pad
#   F256 - I/O pin L15
#
bit 251 O 1 BSC083 250 1 Z
bit 250 C 1 *
bit 249 I 1 BSC083
#
# BSC group 82
#   T144 - unused pad
#   Q208 - unused pad
#   F256 - I/O pin L16
#
bit 248 O 1 BSC082 247 1 Z
bit 247 C 1 *
bit 246 I 1 BSC082
#
# BSC group 81 (nSTATUS)
#   T144 - untestable Family-specific pin 82
#   Q208 - untestable Family-specific pin 121
#   F256 - untestable Family-specific pin M13
#
bit 245 O 1 *
bit 244 O 1 *
bit 243 O 1 *
#
# BSC group 80 (CONF_DONE)
#   T144 - untestable Family-specific pin 83
#   Q208 - untestable Family-specific pin 123
#   F256 - untestable Family-specific pin L13
#
bit 242 O 1 *
bit 241 O 1 *
bit 240 O 1 *
#
# BSC group 79 (MSEL1)
#   T144 - Family-specific input pin 84
#   Q208 - Family-specific input pin 125
#   F256 - Family-specific input pin K12
#
bit 239 O 1 *
bit 238 O 1 *
bit 237 I 1 BSC079
#
# BSC group 78 (MSEL0)
#   T144 - Family-specific input pin 85
#   Q208 - Family-specific input pin 126
#   F256 - Family-specific input pin J13
#
bit 236 O 1 *
bit 235 O 1 *
bit 234 I 1 BSC078
#
# BSC group 77
#   T144 - I/O pin 86
#   Q208 - I/O pin 127
#   F256 - I/O pin K16
#
bit 233 O 1 BSC077 232 1 Z
bit 232 C 1 *
bit 231 I 1 BSC077
#
# BSC group 76
#   T144 - I/O pin 87
#   Q208 - I/O pin 128
#   F256 - I/O pin K15
#
bit 230 O 1 BSC076 229 1 Z
bit 229 C 1 *
bit 228 I 1 BSC076
#
# BSC group 75 (CLK7)
#   T144 - Family-specific input pin 88
#   Q208 - Family-specific input pin 129
#   F256 - Family-specific input pin J16
#
bit 227 O 1 *
bit 226 O 1 *
bit 225 I 1 BSC075
#
# BSC group 74 (CLK6)
#   T144 - Family-specific input pin 89
#   Q208 - Family-specific input pin 130
#   F256 - Family-specific input pin J15
#
bit 224 O 1 *
bit 223 O 1 *
bit 222 I 1 BSC074
#
# BSC group 73 (CLK5)
#   T144 - Family-specific input pin 90
#   Q208 - Family-specific input pin 131
#   F256 - Family-specific input pin H15
#
bit 221 O 1 *
bit 220 O 1 *
bit 219 I 1 BSC073
#
# BSC group 72 (CLK4)
#   T144 - Family-specific input pin 91
#   Q208 - Family-specific input pin 132
#   F256 - Family-specific input pin H16
#
bit 218 O 1 *
bit 217 O 1 *
bit 216 I 1 BSC072
#
# BSC group 71
#   T144 - I/O pin 92
#   Q208 - I/O pin 133
#   F256 - I/O pin H12
#
bit 215 O 1 BSC071 214 1 Z
bit 214 C 1 *
bit 213 I 1 BSC071
#
# BSC group 70
#   T144 - I/O pin 93
#   Q208 - I/O pin 134
#   F256 - I/O pin J12
#
bit 212 O 1 BSC070 211 1 Z
bit 211 C 1 *
bit 210 I 1 BSC070
#
# BSC group 69
#   T144 - I/O pin 94
#   Q208 - I/O pin 135
#   F256 - I/O pin G16
#
bit 209 O 1 BSC069 208 1 Z
bit 208 C 1 *
bit 207 I 1 BSC069
#
# BSC group 68
#   T144 - I/O pin 96
#   Q208 - I/O pin 137
#   F256 - I/O pin G15
#
bit 206 O 1 BSC068 205 1 Z
bit 205 C 1 *
bit 204 I 1 BSC068
#
# BSC group 67
#   T144 - I/O pin 97
#   Q208 - I/O pin 138
#   F256 - I/O pin F15
#
bit 203 O 1 BSC067 202 1 Z
bit 202 C 1 *
bit 201 I 1 BSC067
#
# BSC group 66
#   T144 - unused pad
#   Q208 - I/O pin 139
#   F256 - I/O pin F16
#
bit 200 O 1 BSC066 199 1 Z
bit 199 C 1 *
bit 198 I 1 BSC066
#
# BSC group 65
#   T144 - unused pad
#   Q208 - I/O pin 141
#   F256 - I/O pin J11
#
bit 197 O 1 BSC065 196 1 Z
bit 196 C 1 *
bit 195 I 1 BSC065
#
# BSC group 64
#   T144 - unused pad
#   Q208 - I/O pin 142
#   F256 - I/O pin H11
#
bit 194 O 1 BSC064 193 1 Z
bit 193 C 1 *
bit 192 I 1 BSC064
#
# BSC group 63
#   T144 - unused pad
#   Q208 - unused pad
#   F256 - I/O pin G12
#
bit 191 O 1 BSC063 190 1 Z
bit 190 C 1 *
bit 189 I 1 BSC063
#
# BSC group 62
#   T144 - unused pad
#   Q208 - unused pad
#   F256 - I/O pin G13
#
bit 188 O 1 BSC062 187 1 Z
bit 187 C 1 *
bit 186 I 1 BSC062
#
# BSC group 61
#   T144 - unused pad
#   Q208 - I/O pin 143
#   F256 - I/O pin E13
#
bit 185 O 1 BSC061 184 1 Z
bit 184 C 1 *
bit 183 I 1 BSC061
#
# BSC group 60
#   T144 - unused pad
#   Q208 - I/O pin 144
#   F256 - I/O pin F13
#
bit 182 O 1 BSC060 181 1 Z
bit 181 C 1 *
bit 180 I 1 BSC060
#
# BSC group 59
#   T144 - I/O pin 99
#   Q208 - I/O pin 145
#   F256 - I/O pin H13
#
bit 179 O 1 BSC059 178 1 Z
bit 178 C 1 *
bit 177 I 1 BSC059
#
# BSC group 58
#   T144 - unused pad
#   Q208 - unused pad
#   F256 - I/O pin D15
#
bit 176 O 1 BSC058 175 1 Z
bit 175 C 1 *
bit 174 I 1 BSC058
#
# BSC group 57
#   T144 - unused pad
#   Q208 - unused pad
#   F256 - I/O pin D16
#
bit 173 O 1 BSC057 172 1 Z
bit 172 C 1 *
bit 171 I 1 BSC057
#
# BSC group 56
#   T144 - unused pad
#   Q208 - unused pad
#   F256 - I/O pin E15
#
bit 170 O 1 BSC056 169 1 Z
bit 169 C 1 *
bit 168 I 1 BSC056
#
# BSC group 55
#   T144 - unused pad
#   Q208 - unused pad
#   F256 - I/O pin E16
#
bit 167 O 1 BSC055 166 1 Z
bit 166 C 1 *
bit 165 I 1 BSC055
#
# BSC group 54
#   T144 - unused pad
#   Q208 - unused pad
#   F256 - I/O pin F14
#
bit 164 O 1 BSC054 163 1 Z
bit 163 C 1 *
bit 162 I 1 BSC054
#
# BSC group 53
#   T144 - I/O pin 100
#   Q208 - I/O pin 146
#   F256 - I/O pin C15
#
bit 161 O 1 BSC053 160 1 Z
bit 160 C 1 *
bit 159 I 1 BSC053
#
# BSC group 52
#   T144 - I/O pin 101
#   Q208 - I/O pin 147
#   F256 - I/O pin C16
#
bit 158 O 1 BSC052 157 1 Z
bit 157 C 1 *
bit 156 I 1 BSC052
#
# BSC group 51
#   T144 - unused pad
#   Q208 - I/O pin 149
#   F256 - I/O pin C14
#
bit 155 O 1 BSC051 154 1 Z
bit 154 C 1 *
bit 153 I 1 BSC051
#
# BSC group 50
#   T144 - unused pad
#   Q208 - I/O pin 150
#   F256 - I/O pin D13
#
bit 152 O 1 BSC050 151 1 Z
bit 151 C 1 *
bit 150 I 1 BSC050
#
# BSC group 49
#   T144 - I/O pin 103
#   Q208 - I/O pin 151
#   F256 - I/O pin E14
#
bit 149 O 1 BSC049 148 1 Z
bit 148 C 1 *
bit 147 I 1 BSC049
#
# BSC group 48
#   T144 - I/O pin 104
#   Q208 - I/O pin 152
#   F256 - I/O pin D14
#
bit 146 O 1 BSC048 145 1 Z
bit 145 C 1 *
bit 144 I 1 BSC048
#
# BSC group 47
#   T144 - I/O pin 112
#   Q208 - I/O pin 160
#   F256 - I/O pin B14
#
bit 143 O 1 BSC047 142 1 Z
bit 142 C 1 *
bit 141 I 1 BSC047
#
# BSC group 46
#   T144 - I/O pin 113
#   Q208 - I/O pin 161
#   F256 - I/O pin A14
#
bit 140 O 1 BSC046 139 1 Z
bit 139 C 1 *
bit 138 I 1 BSC046
#
# BSC group 45
#   T144 - I/O pin 114
#   Q208 - I/O pin 162
#   F256 - I/O pin C13
#
bit 137 O 1 BSC045 136 1 Z
bit 136 C 1 *
bit 135 I 1 BSC045
#
# BSC group 44
#   T144 - I/O pin 115
#   Q208 - I/O pin 163
#   F256 - I/O pin C12
#
bit 134 O 1 BSC044 133 1 Z
bit 133 C 1 *
bit 132 I 1 BSC044
#
# BSC group 43
#   T144 - unused pad
#   Q208 - I/O pin 164
#   F256 - I/O pin B13
#
bit 131 O 1 BSC043 130 1 Z
bit 130 C 1 *
bit 129 I 1 BSC043
#
# BSC group 42
#   T144 - unused pad
#   Q208 - I/O pin 165
#   F256 - I/O pin A13
#
bit 128 O 1 BSC042 127 1 Z
bit 127 C 1 *
bit 126 I 1 BSC042
#
# BSC group 41
#   T144 - I/O pin 118
#   Q208 - I/O pin 168
#   F256 - I/O pin B12
#
bit 125 O 1 BSC041 124 1 Z
bit 124 C 1 *
bit 123 I 1 BSC041
#
# BSC group 40
#   T144 - I/O pin 119
#   Q208 - I/O pin 169
#   F256 - I/O pin A12
#
bit 122 O 1 BSC040 121 1 Z
bit 121 C 1 *
bit 120 I 1 BSC040
#
# BSC group 39
#   T144 - I/O pin 120
#   Q208 - I/O pin 170
#   F256 - I/O pin C11
#
bit 119 O 1 BSC039 118 1 Z
bit 118 C 1 *
bit 117 I 1 BSC039
#
# BSC group 38
#   T144 - I/O pin 121
#   Q208 - I/O pin 171
#   F256 - I/O pin B11
#
bit 116 O 1 BSC038 115 1 Z
bit 115 C 1 *
bit 114 I 1 BSC038
#
# BSC group 37
#   T144 - I/O pin 122
#   Q208 - I/O pin 173
#   F256 - I/O pin A11
#
bit 113 O 1 BSC037 112 1 Z
bit 112 C 1 *
bit 111 I 1 BSC037
#
# BSC group 36
#   T144 - unused pad
#   Q208 - unused pad
#   F256 - I/O pin G10
#
bit 110 O 1 BSC036 109 1 Z
bit 109 C 1 *
bit 108 I 1 BSC036
#
# BSC group 35
#   T144 - unused pad
#   Q208 - unused pad
#   F256 - I/O pin G11
#
bit 107 O 1 BSC035 106 1 Z
bit 106 C 1 *
bit 105 I 1 BSC035
#
# BSC group 34
#   T144 - unused pad
#   Q208 - I/O pin 175
#   F256 - I/O pin B10
#
bit 104 O 1 BSC034 103 1 Z
bit 103 C 1 *
bit 102 I 1 BSC034
#
# BSC group 33
#   T144 - unused pad
#   Q208 - I/O pin 176
#   F256 - I/O pin A10
#
bit 101 O 1 BSC033 100 1 Z
bit 100 C 1 *
bit 99 I 1 BSC033
#
# BSC group 32
#   T144 - unused pad
#   Q208 - unused pad
#   F256 - I/O pin F10
#
bit 98 O 1 BSC032 97 1 Z
bit 97 C 1 *
bit 96 I 1 BSC032
#
# BSC group 31
#   T144 - unused pad
#   Q208 - unused pad
#   F256 - I/O pin F9
#
bit 95 O 1 BSC031 94 1 Z
bit 94 C 1 *
bit 93 I 1 BSC031
#
# BSC group 30
#   T144 - unused pad
#   Q208 - unused pad
#   F256 - I/O pin D9
#
bit 92 O 1 BSC030 91 1 Z
bit 91 C 1 *
bit 90 I 1 BSC030
#
# BSC group 29
#   T144 - I/O pin 125
#   Q208 - I/O pin 179
#   F256 - I/O pin D11
#
bit 89 O 1 BSC029 88 1 Z
bit 88 C 1 *
bit 87 I 1 BSC029
#
# BSC group 28
#   T144 - I/O pin 126
#   Q208 - I/O pin 180
#   F256 - I/O pin D10
#
bit 86 O 1 BSC028 85 1 Z
bit 85 C 1 *
bit 84 I 1 BSC028
#
# BSC group 27
#   T144 - unused pad
#   Q208 - I/O pin 181
#   F256 - I/O pin A9
#
bit 83 O 1 BSC027 82 1 Z
bit 82 C 1 *
bit 81 I 1 BSC027
#
# BSC group 26
#   T144 - unused pad
#   Q208 - I/O pin 182
#   F256 - I/O pin B9
#
bit 80 O 1 BSC026 79 1 Z
bit 79 C 1 *
bit 78 I 1 BSC026
#
# BSC group 25
#   T144 - unused pad
#   Q208 - unused pad
#   F256 - I/O pin A8
#
bit 77 O 1 BSC025 76 1 Z
bit 76 C 1 *
bit 75 I 1 BSC025
#
# BSC group 24
#   T144 - unused pad
#   Q208 - unused pad
#   F256 - I/O pin B8
#
bit 74 O 1 BSC024 73 1 Z
bit 73 C 1 *
bit 72 I 1 BSC024
#
# BSC group 23
#   T144 - unused pad
#   Q208 - unused pad
#   F256 - I/O pin A7
#
bit 71 O 1 BSC023 70 1 Z
bit 70 C 1 *
bit 69 I 1 BSC023
#
# BSC group 22
#   T144 - I/O pin 129
#   Q208 - I/O pin 185
#   F256 - I/O pin B7
#
bit 68 O 1 BSC022 67 1 Z
bit 67 C 1 *
bit 66 I 1 BSC022
#
# BSC group 21
#   T144 - unused pad
#   Q208 - I/O pin 187
#   F256 - I/O pin F7
#
bit 65 O 1 BSC021 64 1 Z
bit 64 C 1 *
bit 63 I 1 BSC021
#
# BSC group 20
#   T144 - unused pad
#   Q208 - I/O pin 188
#   F256 - F8
#
bit 62 O 1 BSC020 61 1 Z
bit 61 C 1 *
bit 60 I 1 BSC020
#
# BSC group 19
#   T144 - unused pad
#   Q208 - I/O pin 189
#   F256 - unused pad
#
bit 59 O 1 BSC019 58 1 Z
bit 58 C 1 *
bit 57 I 1 BSC019
#
# BSC group 18
#   T144 - unused pad
#   Q208 - I/O pad 191
#   F256 - unused pad
#
bit 56 O 1 BSC018 55 1 Z
bit 55 C 1 *
bit 54 I 1 BSC018
#
# BSC group 17
#   T144 - I/O pin 132
#   Q208 - I/O pin 192
#   F256 - I/O pin D8
#
bit 53 O 1 BSC017 52 1 Z
bit 52 C 1 *
bit 51 I 1 BSC017
#
# BSC group 16
#   T144 - I/O pin 133
#   Q208 - I/O pin 193
#   F256 - I/O pin B6
#
bit 50 O 1 BSC016 49 1 Z
bit 49 C 1 *
bit 48 I 1 BSC016
#
# BSC group 15
#   T144 - I/O pin 134
#   Q208 - I/O pin 195
#   F256 - I/O pin A6
#
bit 47 O 1 BSC015 46 1 Z
bit 46 C 1 *
bit 45 I 1 BSC015
#
# BSC group 14
#   T144 - unused pad
#   Q208 - unused pad
#   F256 - I/O pin G6
#
bit 44 O 1 BSC014 43 1 Z
bit 43 C 1 *
bit 42 I 1 BSC014
#
# BSC group 13
#   T144 - unused pad
#   Q208 - unused pad
#   F256 - I/O pin G7
#
bit 41 O 1 BSC013 40 1 Z
bit 40 C 1 *
bit 39 I 1 BSC013
#
# BSC group 12
#   T144 - unused pad
#   Q208 - unused pad
#   F256 - I/O pin D7
#
bit 38 O 1 BSC012 37 1 Z
bit 37 C 1 *
bit 36 I 1 BSC012
#
# BSC group 11
#   T144 - unused pad
#   Q208 - I/O pin 197
#   F256 - I/O pin D6
#
bit 35 O 1 BSC011 34 1 Z
bit 34 C 1 *
bit 33 I 1 BSC011
#
# BSC group 10
#   T144 - unused pad
#   Q208 - I/O pin 198
#   F256 - I/O pin C6
#
bit 32 O 1 BSC010 31 1 Z
bit 31 C 1 *
bit 30 I 1 BSC010
#
# BSC group 9
#   T144 - unused pad
#   Q208 - unused pad
#   F256 - I/O pin C5
#
bit 29 O 1 BSC009 28 1 Z
bit 28 C 1 *
bit 27 I 1 BSC009
#
# BSC group 8
#   T144 - unused pad
#   Q208 - unused pad
#   F256 - I/O pin C4
#
bit 26 O 1 BSC008 25 1 Z
bit 25 C 1 *
bit 24 I 1 BSC008
#
# BSC group 7
#   T144 - I/O pin 135
#   Q208 - I/O pin 199
#   F256 - I/O pin B5
#
bit 23 O 1 BSC007 22 1 Z
bit 22 C 1 *
bit 21 I 1 BSC007
#
# BSC group 6
#   T144 - I/O pin 136
#   Q208 - I/O pin 200
#   F256 - I/O pin A5
#
bit 20 O 1 BSC006 19 1 Z
bit 19 C 1 *
bit 18 I 1 BSC006
#
# BSC group 5
#   T144 - I/O pin 137
#   Q208 - I/O pin 201
#   F256 - I/O pin B4
#
bit 17 O 1 BSC005 16 1 Z
bit 16 C 1 *
bit 15 I 1 BSC005
#
# BSC group 4
#   T144 - I/O pin 139
#   Q208 - I/O pin 203
#   F256 - I/O pin A4
#
bit 14 O 1 BSC004 13 1 Z
bit 13 C 1 *
bit 12 I 1 BSC004
#
# BSC group 3
#   T144 - I/O pin 141
#   Q208 - I/O pin 205
#   F256 - I/O pin A3
#
bit 11 O 1 BSC003 10 1 Z
bit 10 C 1 *
bit 9 I 1 BSC003
#
# BSC group 2
#   T144 - I/O pin 142
#   Q208 - I/O pin 206
#   F256 - I/O pin B3
#
bit 8 O 1 BSC002 7 1 Z
bit 7 C 1 *
bit 6 I 1 BSC002
#
# BSC group 1
#   T144 - I/O pin 143
#   Q208 - I/O pin 207
#   F256 - I/O pin E6
#
bit 5 O 1 BSC001 4 1 Z
bit 4 C 1 *
bit 3 I 1 BSC001
#
# BSC group 0
#   T144 - I/O pin 144
#   Q208 - I/O pin 208
#   F256 - I/O pin F6
#
bit 2 O 1 BSC000 1 1 Z
bit 1 C 1 *
bit 0 I 1 BSC000
