signal ADDR1
signal ADDR2
signal ADDR3
signal ADDR4
signal ADDR5
signal ADDR6
signal ADDR7
signal ADDR8
signal ADDR9
signal ADDR10
signal ADDR11
signal ADDR12
signal ADDR13
signal ADDR14
signal ADDR15
signal ADDR16
signal ADDR17
signal ADDR18
signal ADDR19
signal AMS_B0
signal AMS_B1
signal AMS_B2
signal AMS_B3
signal AOE_B
signal ARDY
signal ARE_B
signal AWE_B
signal ABE_B0
signal ABE_B1
signal BG_B
signal BGH_B
signal BMODE0
signal BMODE1
signal BMODE2
signal BR_B
signal DATA0
signal DATA1
signal DATA2
signal DATA3
signal DATA4
signal DATA5
signal DATA6
signal DATA7
signal DATA8
signal DATA9
signal DATA10
signal DATA11
signal DATA12
signal DATA13
signal DATA14
signal DATA15
signal NMI
signal PF0
signal PF1
signal PF2
signal PF3
signal PF4
signal PF5
signal PF6
signal PF7
signal PF8
signal PF9
signal PF10
signal PF11
signal PF12
signal PF13
signal PF14
signal PF15
signal PG0
signal PG1
signal PG2
signal PG3
signal PG4
signal PG5
signal PG6
signal PG7
signal PG8
signal PG9
signal PG10
signal PG11
signal PG12
signal PG13
signal PG14
signal PG15
signal PH0
signal PH1
signal PH2
signal PH3
signal PH4
signal PH5
signal PH6
signal PH7
signal PH8
signal PH9
signal PH10
signal PH11
signal PH12
signal PH13
signal PH14
signal PH15
signal PJ0
signal PJ1
signal PJ2
signal PJ3
signal PJ4
signal PJ5
signal PJ6
signal PJ7
signal PJ8
signal PJ9
signal PJ10
signal PJ11
signal RESET_B
signal CLKOUT
signal SA10
signal SCAS_B
signal SCKE
signal SMS_B
signal SRAS_B
signal SWE_B
signal TDI
signal TDO
signal TCK
signal TMS
signal TRST_B
signal TEST
signal EMU_B
signal RTXI
signal RTXO
signal VDD_INT0
signal VDD_INT1
signal VDD_INT2
signal VDD_INT3
signal VDD_INT4
signal VDD_INT5
signal VDD_INT6
signal VDD_EXT0
signal VDD_EXT1
signal VDD_EXT2
signal VDD_EXT3
signal VDD_EXT4
signal VDD_EXT5
signal VDD_EXT6
signal VDD_EXT7
signal VDD_EXT8
signal VDD_EXT9
signal VDD_EXT10
signal VDD_EXT11
signal VDD_EXT12
signal VDD_EXT13
signal VDD_EXT14
signal VDD_EXT15
signal GND0
signal GND1
signal GND2
signal GND3
signal GND4
signal GND5
signal GND6
signal GND7
signal GND8
signal GND9
signal GND10
signal GND11
signal GND12
signal GND13
signal GND14
signal GND15
signal GND16
signal GND17
signal GND18
signal GND19
signal GND20
signal GND21
signal GND22
signal GND23
signal VDD_RTC
signal CLKIN
signal XTAL
signal CLKBUF
signal VROUT0

register	BSR	261
register	BR	1
register	DIR	32
register	DBGSTAT	16
register	DBGCTL	16
register	EMUIR	32
register	EMUDAT	32
register	EMUPC	32

instruction length 5

instruction BYPASS 11111 BR
instruction EXTEST 00000 BSR
instruction SAMPLE/PRELOAD 10000 BSR
instruction IDCODE 00010 DIR
instruction DBGSTAT_SCAN 01100 DBGSTAT
instruction DBGCTL_SCAN 00100 DBGCTL
instruction EMUIR_SCAN 01000 EMUIR
instruction EMUDAT_SCAN 10100 EMUDAT
instruction EMUPC_SCAN 11110 EMUPC

bit 260 C 0 *
bit 259 O 1 DATA0 260 0 Z
bit 258 I 1 DATA0
bit 257 O 1 DATA1 260 0 Z
bit 256 I 1 DATA1
bit 255 O 1 DATA2 260 0 Z
bit 254 I 1 DATA2
bit 253 O 1 DATA3 260 0 Z
bit 252 I 1 DATA3
bit 251 O 1 DATA4 260 0 Z
bit 250 I 1 DATA4
bit 249 O 1 DATA5 260 0 Z
bit 248 I 1 DATA5
bit 247 O 1 DATA6 260 0 Z
bit 246 I 1 DATA6
bit 245 O 1 DATA7 260 0 Z
bit 244 I 1 DATA7
bit 243 O 1 DATA8 260 0 Z
bit 242 I 1 DATA8
bit 241 O 1 DATA9 260 0 Z
bit 240 I 1 DATA9
bit 239 O 1 DATA10 260 0 Z
bit 238 I 1 DATA10
bit 237 O 1 DATA11 260 0 Z
bit 236 I 1 DATA11
bit 235 O 1 DATA12 260 0 Z
bit 234 I 1 DATA12
bit 233 O 1 DATA13 260 0 Z
bit 232 I 1 DATA13
bit 231 O 1 DATA14 260 0 Z
bit 230 I 1 DATA14
bit 229 O 1 DATA15 260 0 Z
bit 228 I 1 DATA15
bit 227 I 1 TEST
bit 226 I 1 BMODE0
bit 225 I 1 BMODE1
bit 224 I 1 BMODE2
bit 223 C 0 *
bit 222 O 1 PF0 223 0 Z
bit 221 I 1 PF0
bit 220 C 0 *
bit 219 O 1 PF1 220 0 Z
bit 218 I 1 PF1
bit 217 C 0 *
bit 216 O 1 PF2 217 0 Z
bit 215 I 1 PF2
bit 214 C 0 *
bit 213 O 1 PF3 214 0 Z
bit 212 I 1 PF3
bit 211 C 0 *
bit 210 O 1 PF4 211 0 Z
bit 209 I 1 PF4
bit 208 C 0 *
bit 207 O 1 PF5 208 0 Z
bit 206 I 1 PF5
bit 205 C 0 *
bit 204 O 1 PF6 205 0 Z
bit 203 I 1 PF6
bit 202 C 0 *
bit 201 O 1 PF7 202 0 Z
bit 200 I 1 PF7
bit 199 C 0 *
bit 198 O 1 PF8 199 0 Z
bit 197 I 1 PF8
bit 196 C 0 *
bit 195 O 1 PF9 196 0 Z
bit 194 I 1 PF9
bit 193 C 0 *
bit 192 O 1 PF10 193 0 Z
bit 191 I 1 PF10
bit 190 C 0 *
bit 189 O 1 PF11 190 0 Z
bit 188 I 1 PF11
bit 187 C 0 *
bit 186 O 1 PF12 187 0 Z
bit 185 I 1 PF12
bit 184 C 0 *
bit 183 O 1 PF13 184 0 Z
bit 182 I 1 PF13
bit 181 C 0 *
bit 180 O 1 PF14 181 0 Z
bit 179 I 1 PF14
bit 178 C 0 *
bit 177 O 1 PF15 178 0 Z
bit 176 I 1 PF15
bit 175 C 0 *
bit 174 O 1 PG0 175 0 Z
bit 173 I 1 PG0
bit 172 C 0 *
bit 171 O 1 PG1 172 0 Z
bit 170 I 1 PG1
bit 169 C 0 *
bit 168 O 1 PG2 169 0 Z
bit 167 I 1 PG2
bit 166 C 0 *
bit 165 O 1 PG3 166 0 Z
bit 164 I 1 PG3
bit 163 C 0 *
bit 162 O 1 PG4 163 0 Z
bit 161 I 1 PG4
bit 160 C 0 *
bit 159 O 1 PG5 160 0 Z
bit 158 I 1 PG5
bit 157 C 0 *
bit 156 O 1 PG6 157 0 Z
bit 155 I 1 PG6
bit 154 C 0 *
bit 153 O 1 PG7 154 0 Z
bit 152 I 1 PG7
bit 151 C 0 *
bit 150 O 1 PG10 151 0 Z
bit 149 I 1 PG10
bit 148 C 0 *
bit 147 O 1 PG11 148 0 Z
bit 146 I 1 PG11
bit 145 C 0 *
bit 144 O 1 PG12 145 0 Z
bit 143 I 1 PG12
bit 142 C 0 *
bit 141 O 1 PG8 142 0 Z
bit 140 I 1 PG8
bit 139 C 0 *
bit 138 O 1 PG9 139 0 Z
bit 137 I 1 PG9
bit 136 C 0 *
bit 135 O 1 PG13 136 0 Z
bit 134 I 1 PG13
bit 133 C 0 *
bit 132 O 1 PG14 133 0 Z
bit 131 I 1 PG14
bit 130 C 0 *
bit 129 O 1 PG15 130 0 Z
bit 128 I 1 PG15
bit 127 C 0 *
bit 126 O 1 PH0 127 0 Z
bit 125 I 1 PH0
bit 124 C 0 *
bit 123 O 1 PH1 124 0 Z
bit 122 I 1 PH1
bit 121 C 0 *
bit 120 O 1 PH2 121 0 Z
bit 119 I 1 PH2
bit 118 C 0 *
bit 117 O 1 PH3 118 0 Z
bit 116 I 1 PH3
bit 115 C 0 *
bit 114 O 1 PH4 115 0 Z
bit 113 I 1 PH4
bit 112 C 0 *
bit 111 O 1 PH5 112 0 Z
bit 110 I 1 PH5
bit 109 C 0 *
bit 108 O 1 PH6 109 0 Z
bit 107 I 1 PH6
bit 106 C 0 *
bit 105 O 1 PH7 106 0 Z
bit 104 I 1 PH7
bit 103 C 0 *
bit 102 O 1 PH8 103 0 Z
bit 101 I 1 PH8
bit 100 C 0 *
bit 99 O 1 PH9 100 0 Z
bit 98 I 1 PH9
bit 97 C 0 *
bit 96 O 1 PH10 97 0 Z
bit 95 I 1 PH10
bit 94 C 0 *
bit 93 O 1 PH11 94 0 Z
bit 92 I 1 PH11
bit 91 C 0 *
bit 90 O 1 PH12 91 0 Z
bit 89 I 1 PH12
bit 88 C 0 *
bit 87 O 1 PH13 88 0 Z
bit 86 I 1 PH13
bit 85 C 0 *
bit 84 O 1 PH14 85 0 Z
bit 83 I 1 PH14
bit 82 C 0 *
bit 81 O 1 PH15 82 0 Z
bit 80 I 1 PH15
bit 79 C 0 *
bit 78 O 1 PJ0 79 0 Z
bit 77 I 1 PJ0
bit 76 C 0 *
bit 75 O 1 PJ1 76 0 Z
bit 74 I 1 PJ1
bit 73 C 0 *
bit 72 O 1 PJ6 73 0 Z
bit 71 I 1 PJ6
bit 70 C 0 *
bit 69 O 1 PJ7 70 0 Z
bit 68 I 1 PJ7
bit 67 C 0 *
bit 66 O 1 PJ8 67 0 Z
bit 65 I 1 PJ8
bit 64 C 0 *
bit 63 O 1 PJ4 64 0 Z
bit 62 I 1 PJ4
bit 61 C 0 *
bit 60 O 1 PJ5 61 0 Z
bit 59 I 1 PJ5
bit 58 C 0 *
bit 57 O 1 PJ9 58 0 Z
bit 56 I 1 PJ9
bit 55 C 0 *
bit 54 O 1 PJ10 55 0 Z
bit 53 I 1 PJ10
bit 52 C 0 *
bit 51 O 1 PJ11 52 0 Z
bit 50 I 1 PJ11
bit 49 C 0 *
bit 48 O 1 PJ2 49 0 Z
bit 47 I 1 PJ2
bit 46 C 0 *
bit 45 O 1 PJ3 46 0 Z
bit 44 I 1 PJ3
bit 43 I 1 NMI
bit 42 I 1 RESET_B
bit 41 O 1 SCKE 39 0 Z
bit 40 O 1 SMS_B 39 0 Z
bit 39 C 0 *
bit 38 O 1 CLKOUT 39 0 Z
bit 37 O 1 SRAS_B 39 0 Z
bit 36 O 1 SCAS_B 39 0 Z
bit 35 O 1 SWE_B 39 0 Z
bit 34 O 1 SA10 39 0 Z
bit 33 I 1 BR_B
bit 32 I 1 ARDY
bit 31 O 1 AMS_B0 27 0 Z
bit 30 O 1 AMS_B1 27 0 Z
bit 29 O 1 AMS_B2 27 0 Z
bit 28 O 1 AMS_B3 27 0 Z
bit 27 C 0 *
bit 26 O 1 AOE_B 27 0 Z
bit 25 O 1 ARE_B 27 0 Z
bit 24 O 1 AWE_B 27 0 Z
bit 23 O 1 ABE_B0 17 0 Z
bit 22 O 1 ABE_B1 17 0 Z
bit 21 O 1 ADDR1 17 0 Z
bit 20 O 1 ADDR2 17 0 Z
bit 19 O 1 ADDR3 17 0 Z
bit 18 O 1 ADDR4 17 0 Z
bit 17 C 0 *
bit 16 O 1 ADDR5 17 0 Z
bit 15 O 1 ADDR6 17 0 Z
bit 14 O 1 ADDR7 17 0 Z
bit 13 O 1 ADDR8 17 0 Z
bit 12 O 1 ADDR9 17 0 Z
bit 11 O 1 ADDR10 17 0 Z
bit 10 O 1 ADDR11 17 0 Z
bit 9 O 1 ADDR12 17 0 Z
bit 8 O 1 ADDR13 17 0 Z
bit 7 O 1 ADDR14 17 0 Z
bit 6 O 1 ADDR15 17 0 Z
bit 5 O 1 ADDR16 17 0 Z
bit 4 O 1 ADDR17 17 0 Z
bit 3 O 1 ADDR18 17 0 Z
bit 2 O 1 ADDR19 17 0 Z
bit 1 O 1 BGH_B
bit 0 O 1 BG_B
