#
# $Id: ppc440gx 619 2004-11-16 21:51:27Z telka $
#
# JTAG declarations for IBM PPC440GX
# Copyright (C) 2002 ETC s.r.o.
#
# This program is free software; you can redistribute it and/or
# modify it under the terms of the GNU General Public License
# as published by the Free Software Foundation; either version 2
# of the License, or (at your option) any later version.
#
# This program is distributed in the hope that it will be useful,
# but WITHOUT ANY WARRANTY; without even the implied warranty of
# MERCHANTABILITY or FITNESS FOR A PARTICULAR PURPOSE.  See the
# GNU General Public License for more details.
#
# You should have received a copy of the GNU General Public License
# along with this program; if not, write to the Free Software
# Foundation, Inc., 59 Temple Place - Suite 330, Boston, MA
# 02111-1307, USA.
#
# Written by Marcel Telka <marcel@telka.sk>, 2002.
#


signal DMAACK0               N05
signal DMAACK1               P07
signal DMAACK2               P06
signal DMAACK3               P11
signal DMAEOT0               R16
signal DMAEOT1               P15
signal DMAEOT2               P16
signal DMAEOT3               M16
signal DMAREQ0               R03
signal DMAREQ1               M11
signal DMAREQ2               N11
signal DMAREQ3               P01
signal EBCADR0               D11
signal EBCADR1               C11
signal EBCADR10              C20
signal EBCADR11              A16
signal EBCADR12              A13
signal EBCADR13              B14
signal EBCADR14              C14
signal EBCADR15              D14
signal EBCADR16              B20
signal EBCADR17              L15
signal EBCADR18              L21
signal EBCADR19              L22
signal EBCADR2               B11
signal EBCADR20              M22
signal EBCADR21 M01
signal EBCADR22  L24
signal EBCADR23  P24
signal EBCADR24  T19
signal EBCADR25  R24
signal EBCADR26  U22
signal EBCADR27  U24
signal EBCADR28  N03
signal EBCADR29  V20
signal EBCADR3   A12
signal EBCADR30  V23
signal EBCADR31  V21
signal EBCADR4   A19
signal EBCADR5   D18
signal EBCADR6   E11
signal EBCADR7   M03
signal EBCADR8   N01
signal EBCADR9   E14
signal EBCBE0_N  T18
signal EBCBE1_N  V19
signal EBCBE2_N  W22
signal EBCBE3_N  W24
signal EBCBLAST_N C07
signal EBCCS0_N  E17
signal EBCCS1_N  L10
signal EBCCS2_N  V04
signal EBCCS3_N  T24
signal EBCCS4_N  L03
signal EBCCS5_N  T03
signal EBCCS6_N  L13
signal EBCCS7_N  U03
signal EBCDATA0  H24
signal EBCDATA1  H22
signal EBCDATA10 J19
signal EBCDATA11 J18
signal EBCDATA12 J17
signal EBCDATA13 J15
signal EBCDATA14 J14
signal EBCDATA15 J13
signal EBCDATA16 J12
signal EBCDATA17 J11
signal EBCDATA18 J10
signal EBCDATA19 J09
signal EBCDATA2  H20
signal EBCDATA20 L14
signal EBCDATA21 K24
signal EBCDATA22 K22
signal EBCDATA23 K20
signal EBCDATA24 K18
signal EBCDATA25 K16
signal EBCDATA26 K14
signal EBCDATA27 K11
signal EBCDATA28 K09
signal EBCDATA29 L19
signal EBCDATA3  G20
signal EBCDATA30 L17
signal EBCDATA31 L16
signal EBCDATA4  G19
signal EBCDATA5  H18
signal EBCDATA6  J23
signal EBCDATA7  J22
signal EBCDATA8  J21
signal EBCDATA9  J20
signal EBCOE_N   M09
signal EBCPAR0   T23
signal EBCPAR1   T22
signal EBCPAR2   W20
signal EBCPAR3   U20
signal EBCREADY  N07
signal EBCRNW    P05
signal EBCWE_N   P02
signal EBMIBUSREQ AA24  
signal EBMICK       U18
signal EBMIERR      P21
signal EBMIEXTACK_N          AA22  
signal EBMIEXTREQ_N          AB23  
signal EBMIHOLDACK           Y21
signal EBMIHOLDREQ           Y23
signal EBMIRESET_N           T17
signal ENETCOL               J07
signal ENETCRS               K07
signal ENETMDCK              J08
signal ENETMDIO              L05
signal ENETRXCK              J02
signal ENETRXD0              G03
signal ENETRXD1              E01
signal ENETRXD2              A07
signal ENETRXD3              H09
signal ENETRXDV              K01
signal ENETRXER              K03
signal ENETTXCK              J06
signal ENETTXD0              L09
signal ENETTXD1              K05
signal ENETTXD2              J04
signal ENETTXD3              J03
signal ENETTXEN              L06
signal ENETTXER              C05
signal GMC1RXCTL             P04
signal GMC1TXCTL             L07
signal GMCREFCLK             L01
signal IIC0SCK               G11
signal IIC0SDATA             G13
signal IIC1SCK_GPIO16        H11
signal IIC1SDATA_GPIO17      H14
signal IRQ0_GPIO0            N18
signal IRQ10_GPIO10          V18
signal IRQ1_GPIO1            L20
signal IRQ2_GPIO2            P20
signal IRQ3_GPIO3            L18
signal IRQ4_GPIO4            N14
signal IRQ5_GPIO5            M20
signal IRQ6_GPIO6            M14
signal IRQ7_GPIO7            P18
signal IRQ8_GPIO8            N20
signal IRQ9_GPIO9            P22
signal JTAGTCK               V22
signal JTAGTDI               Y24
signal JTAGTDO               Y22
signal JTAGTMS               AB22  
signal JTAGTRST_N            N24
signal LSSD_RE               L02
signal LTIDRINH2             A05
signal LTITESTEN             M05
signal MEMADR0               Y19
signal MEMADR1               AD20
signal MEMADR10              W16
signal MEMADR11              Y11
signal MEMADR12              V10
signal MEMADR2               Y20
signal MEMADR3               AB20
signal MEMADR4               AD18
signal MEMADR5               AD16
signal MEMADR6               AB18
signal MEMADR7               Y14
signal MEMADR8               V13
signal MEMADR9               V11
signal MEMBA0                AA16
signal MEMBA1                AD09
signal MEMBSEL0_N            AB15  
signal MEMBSEL1_N            W14
signal MEMBSEL2_N            AD11  
signal MEMBSEL3_N            AD05  
signal MEMCAS_N              AB05  
signal MEMCKE0               AD17  
signal MEMCKE1               AB10  
signal MEMCKE2               Y09
signal MEMCKE3               W09
signal MEMDATA0              AD21  
signal MEMDATA1              AB21  
signal MEMDATA10             Y17
signal MEMDATA11 AB16  
signal MEMDATA12 AC18  
signal MEMDATA13 Y18
signal MEMDATA14 R14
signal MEMDATA15 AB17  
signal MEMDATA16 AA14  
signal MEMDATA17 AD15  
signal MEMDATA18 T15
signal MEMDATA19 V15
signal MEMDATA2  AC22  
signal MEMDATA20 Y16
signal MEMDATA21 U14
signal MEMDATA22 T13
signal MEMDATA23 Y15
signal MEMDATA24 AD13  
signal MEMDATA25 AD14  
signal MEMDATA26 V14
signal MEMDATA27 Y13
signal MEMDATA28 P12
signal MEMDATA29 AB12  
signal MEMDATA3  AA20  
signal MEMDATA30 Y12
signal MEMDATA31 V12
signal MEMDATA32 W11
signal MEMDATA33 AD12  
signal MEMDATA34 Y10
signal MEMDATA35 T12
signal MEMDATA36 U11
signal MEMDATA37 T11
signal MEMDATA38 T10
signal MEMDATA39 AD10  
signal MEMDATA4  U16
signal MEMDATA40 AB08  
signal MEMDATA41 AD08  
signal MEMDATA42 R11
signal MEMDATA43 Y07
signal MEMDATA44 AC07  
signal MEMDATA45 AB09  
signal MEMDATA46 Y06
signal MEMDATA47 Y08
signal MEMDATA48 AA01  
signal MEMDATA49 AA03  
signal MEMDATA5  V17
signal MEMDATA50 AB02  
signal MEMDATA51 Y01
signal MEMDATA52 AB03  
signal MEMDATA53 Y02
signal MEMDATA54 V07
signal MEMDATA55 V01
signal MEMDATA56 T08
signal MEMDATA57 U07
signal MEMDATA58 W01
signal MEMDATA59 W03
signal MEMDATA6  AD19  
signal MEMDATA60 V06
signal MEMDATA61 T07
signal MEMDATA62 W05
signal MEMDATA63 U05
signal MEMDATA7  AB19  
signal MEMDATA8  W18
signal MEMDATA9  V16
signal MEMDM0       T16
signal MEMDM1       AA18  
signal MEMDM2       AB14  
signal MEMDM3       P13
signal MEMDM4       AA09  
signal MEMDM5       AA07  
signal MEMDM6       Y03
signal MEMDM7       V03
signal MEMDM8       AC05  
signal MEMDQS0   AC20  
signal MEMDQS1   AC16  
signal MEMDQS2   AC14  
signal MEMDQS3   AB13  
signal MEMDQS4   AC11  
signal MEMDQS5   AC09  
signal MEMDQS6   Y04
signal MEMDQS7   T01
signal MEMDQS8   AA05  
signal MEMECC0   AB07  
signal MEMECC1   AB06  
signal MEMECC2   AD06  
signal MEMECC3   W07
signal MEMECC4   U09
signal MEMECC5   AC03  
signal MEMECC6   AB04  
signal MEMECC7   AD04  
signal MEMRAS_N  AD07  
signal MEMSYSCK  V09
signal MEMSYSCK_N V08
signal MEMVREFR1 T14
signal MEMVREFR2 T09
signal MEMWE_N   Y05
signal PCIACK64_N D09
signal PCIAD0       C17
signal PCIAD1       B09
signal PCIAD10   C15
signal PCIAD11   E15
signal PCIAD12   G15
signal PCIAD13   B16
signal PCIAD14   C16
signal PCIAD15   D16
signal PCIAD16   E18
signal PCIAD17   E19
signal PCIAD18   F18
signal PCIAD19   G18
signal PCIAD2       G10
signal PCIAD20   D20
signal PCIAD21   A20
signal PCIAD22   A21
signal PCIAD23   C21
signal PCIAD24   F22
signal PCIAD25   B22
signal PCIAD26   G21
signal PCIAD27   E23
signal PCIAD28   C23
signal PCIAD29   F24
signal PCIAD3       E10
signal PCIAD30   D22
signal PCIAD31   D24
signal PCIAD32   H03
signal PCIAD33   H01
signal PCIAD34   L08
signal PCIAD35   F01
signal PCIAD36   D01
signal PCIAD37   J05
signal PCIAD38   H05
signal PCIAD39   G02
signal PCIAD4       C10
signal PCIAD40   E02
signal PCIAD41   C02
signal PCIAD42   A08
signal PCIAD43   G05
signal PCIAD44   F03
signal PCIAD45   D03
signal PCIAD46   B03
signal PCIAD47   H07
signal PCIAD48   G04
signal PCIAD49   E04
signal PCIAD5       A10
signal PCIAD50   C04
signal PCIAD51   A04
signal PCIAD52   F05
signal PCIAD53   D05
signal PCIAD54   B05
signal PCIAD55   C09
signal PCIAD56   E06
signal PCIAD57   C06
signal PCIAD58   A06
signal PCIAD59   F07
signal PCIAD6       F11
signal PCIAD60   E07
signal PCIAD61   D07
signal PCIAD62   B07
signal PCIAD63   E08
signal PCIAD7       G12
signal PCIAD8       G14
signal PCIAD9       A15
signal PCICLK       E03
signal PCIC_BE0_N F14
signal PCIC_BE1_N E16
signal PCIC_BE2_N C19
signal PCIC_BE3_N F20
signal PCIC_BE4_N C08
signal PCIC_BE5_N C03
signal PCIC_BE6_N G09
signal PCIC_BE7_N F09
signal PCIDEVSEL_N        E13
signal PCIFRAME_N A11
signal PCIGNT0_N E22
signal PCIGNT1_N_IRQ12    C22
signal PCIGNT2_N N22
signal PCIGNT3_N M18
signal PCIGNT4_N R22
signal PCIGNT5_N P19
signal PCIIDSEL  G07
signal PCIINTA_N M07
signal PCIIRDY_N E12
signal PCIM66EN  A14
signal PCIPAR       F16
signal PCIPAR64  L04
signal PCIPERR_N A17
signal PCIREQ0_N E24
signal PCIREQ1_N_IRQ11    E21
signal PCIREQ2_N E20
signal PCIREQ3_N R20
signal PCIREQ4_N G23
signal PCIREQ5_N R18
signal PCIREQ64_N E09
signal PCIRST_N  M24
signal PCISERR_N A18
signal PCISTOP_N L12
signal PCITRDY_N C12
signal PCIX133UP G08
signal PCIXCAP   L23
signal SYSCKTK   U01
signal SYSCLK       G22
signal SYSERROR   T02
signal SYSHALT_N  V05
signal SYSMEMPLLG AA11
signal SYSMEMPLLV AB11
signal SYSPCIPLLG            J01
signal SYSPCIPLLV            G01
signal SYSPLLG               J24
signal SYSPLLV               G24
signal SYSRESET_N            P10
signal TRACEBR0_GPIO18       N16
signal TRACEBR1_GPIO19       P17
signal TRACEBR2_GPIO20       T20
signal TRACECK               R05
signal TRACEES0_GPIO21       T21
signal TRACEES1_GPIO22       P23
signal TRACEES2_GPIO23       N09
signal TRACEES3_GPIO24       P08
signal TRACEES4_GPIO25       T05
signal TRACETE1_GPIO11       P14
signal TRACETS0_GPIO26       T04
signal TRACETS1_GPIO27       P03
signal TRACETS2_GPIO28       R07
signal TRACETS3_GPIO29       P09
signal TRACETS4_GPIO30       R09
signal TRACETS5_GPIO31       T06
signal TRACETS6              R01
signal UART0CTS_N            C13
signal UART0DCD_N            V24
signal UART0DSR_N            V02
signal UART0DTR_N            B18
signal UART0RI_N             H16
signal UART0RTS_N            G16
signal UART0RX               G17
signal UART0TX               L11
signal UART1DSR_CTS_GPIO14_N G06
signal UART1RTS_DTR_GPIO15_N E05
signal UART1RX_GPIO12        C18
signal UART1TX_GPIO13        J16
signal UARTSERCK             A09
signal P_GND                 B06 B10 B13 B17 B21 D04 D08 D12 D15 D19 D23 F02 F10 F13 F17 F21 H04 H08 H12 H15 H23 K02 K06 K10 K13 K17 K21 M04 M08 M12 M15 M19 M23 N02 N06 N10 N13 N17 N21 R04 R08 R12 R15 R19 R23 U02 U10 U13 U17 U21 W04 W08 W12 W15 W23 AA02 AA06 AA10 AA13 AA17 AA21 AC04 AC08 AC12 AC15 AC19
signal P_VDD B08 B15 D06 D13 D21 F04 F12 F19 H02 H17 K12 K15 K23 M06 M10 M13 M21 N04 N12 N15 N19 R02 R10 R13 U08 U23 W06 W13 W21 AA04 AA12 AA19 AC10 AC17
signal P_VDD2                B04 B12 B19 D02 D10 D17 F08 F15 F23 H06 H10 H13 H21 K04 K08 K19 M02 M17 N08 N23 R06 R17 R21 U04 U19 W02 AA23
signal P_VDD3                U12 U15 W10 W17 AA08 AA15 AC06 AC13 AC21


# mandatory data registers
register    BSR  769 # Boundary Scan Register
register    BR     1 # Bypass Register

# optional data registers
register    DIR	  32 # Device Identification Register

instruction length 8

# mandatory instructions
instruction EXTEST         00000000	BSR
instruction SAMPLE/PRELOAD 11110010	BSR
instruction BYPASS         11111111	BR

# optional instructions
instruction CLAMP  11110110	BR
instruction HIGHZ  11110101	BR
instruction IDCODE 11110011	DIR



# Boundary Scan Register bit definition
bit   0 B ? PCIAD31 1 0 Z
bit   1 C 0 PCIAD31
bit   2 B ? PCIAD30 3 0 Z
bit   3 C 0 PCIAD30
bit   4 B ? PCIAD28 5 0 Z
bit   5 C 0 PCIAD28
bit   6 B ? PCIREQ0_N 7 0 Z
bit   7 C 0 PCIREQ0_N
bit   8 I ? PCIREQ1_N_IRQ11
bit   9 B ? PCIGNT1_N_IRQ12 10 0 Z
bit  10 C 0 PCIGNT1_N_IRQ12
bit  11 B ? PCIAD27 12 0 Z
bit  12 C 0 PCIAD27
bit  13 B ? PCIAD19 14 0 Z
bit  14 C 0 PCIAD19
bit  15 B ? PCIGNT0_N 16 0 Z
bit  16 C 0 PCIGNT0_N
bit  17 B ? PCIAD29 18 0 Z
bit  18 C 0 PCIAD29
bit  19 B ? PCIAD24 20 0 Z
bit  20 C 0 PCIAD24
bit  21 I ? SYSCLK
bit  22 B ? PCIC_BE3_N 23 0 Z
bit  23 C 0 PCIC_BE3_N
bit  24 B ? PCIAD26 25 0 Z
bit  25 C 0 PCIAD26
bit  26 B ? PCIREQ4_N 27 0 Z
bit  27 C 0 PCIREQ4_N
bit  28 I ? PCIXCAP
bit  29 B ? DMAEOT3 30 0 Z
bit  30 C 0 DMAEOT3
bit  31 O ? PCIRST_N 32 0 Z
bit  32 C 0 PCIRST_N
bit  33 O ? PCIGNT3_N 34 0 Z
bit  34 C 0 PCIGNT3_N
bit  35 B ? IRQ5_GPIO5 36 0 Z
bit  36 C 0 IRQ5_GPIO5
bit  37 B ? IRQ1_GPIO1 38 0 Z
bit  38 C 0 IRQ1_GPIO1
bit  39 B ? IRQ3_GPIO3 40 0 Z
bit  40 C 0 IRQ3_GPIO3
bit  41 B ? IRQ6_GPIO6 42 0 Z
bit  42 C 0 IRQ6_GPIO6
bit  43 B ? IRQ4_GPIO4 44 0 Z
bit  44 C 0 IRQ4_GPIO4
bit  45 B ? IRQ0_GPIO0 46 0 Z
bit  46 C 0 IRQ0_GPIO0
bit  47 B ? IRQ2_GPIO2 48 0 Z
bit  48 C 0 IRQ2_GPIO2
bit  49 O ? PCIGNT2_N 50 0 Z
bit  50 C 0 PCIGNT2_N
bit  51 B ? IRQ8_GPIO8 52 0 Z
bit  52 C 0 IRQ8_GPIO8
bit  53 B ? IRQ7_GPIO7 54 0 Z
bit  54 C 0 IRQ7_GPIO7
bit  55 O ? PCIGNT5_N 56 0 Z
bit  56 C 0 PCIGNT5_N
bit  57 B ? TRACETE1_GPIO11 58 0 Z
bit  58 C 0 TRACETE1_GPIO11
bit  59 O ? PCIGNT4_N 60 0 Z
bit  60 C 0 PCIGNT4_N
bit  61 B ? PCIREQ3_N 62 0 Z
bit  62 C 0 PCIREQ3_N
bit  63 B ? TRACEBR0_GPIO18 64 0 Z
bit  64 C 0 TRACEBR0_GPIO18
bit  65 B ? TRACEBR1_GPIO19 66 0 Z
bit  66 C 0 TRACEBR1_GPIO19
bit  67 B ? TRACEBR2_GPIO20 68 0 Z
bit  68 C 0 TRACEBR2_GPIO20
bit  69 B ? TRACEES0_GPIO21 70 0 Z
bit  70 C 0 TRACEES0_GPIO21
bit  71 B ? TRACEES1_GPIO22 72 0 Z
bit  72 C 0 TRACEES1_GPIO22
bit  73 B ? IRQ9_GPIO9 74 0 Z
bit  74 C 0 IRQ9_GPIO9
bit  75 B ? PCIREQ5_N 76 0 Z
bit  76 C 0 PCIREQ5_N
bit  77 B ? DMAEOT2 78 0 Z
bit  78 C 0 DMAEOT2
bit  79 B ? DMAEOT0 80 0 Z
bit  80 C 0 DMAEOT0
bit  81 B ? EBMIERR 82 0 Z
bit  82 C 0 EBMIERR
bit  83 B ? DMAEOT1 84 0 Z
bit  84 C 0 DMAEOT1
bit  85 O ? EBMICK 86 0 Z
bit  86 C 0 EBMICK
bit  87 O ? EBMIRESET_N 88 0 Z
bit  88 C 0 EBMIRESET_N
bit  89 I ? UART0DCD_N
bit  90 B ? IRQ10_GPIO10 91 0 Z
bit  91 C 0 IRQ10_GPIO10
bit  92 B ? EBMIHOLDREQ 93 0 Z
bit  93 C 0 EBMIHOLDREQ
bit  94 O ? EBMIHOLDACK 95 0 Z
bit  95 C 0 EBMIHOLDACK
bit  96 B ? EBMIEXTREQ_N 97 0 Z
bit  97 C 0 EBMIEXTREQ_N
bit  98 O ? EBMIEXTACK_N 99 0 Z
bit  99 C 0 EBMIEXTACK_N
bit 100 O ? EBMIBUSREQ 101 0 Z
bit 101 C 0 EBMIBUSREQ
bit 102 B ? PCIAD51 103 0 Z
bit 103 C 0 PCIAD51
bit 104 B ? PCIAD50 105 0 Z
bit 105 C 0 PCIAD50
bit 106 B ? PCIAD46 107 0 Z
bit 107 C 0 PCIAD46
bit 108 B ? PCIAD53 109 0 Z
bit 109 C 0 PCIAD53
bit 110 B ? UART1RTS_DTR_GPIO15_N 111 0 Z
bit 111 C 0 UART1RTS_DTR_GPIO15_N
bit 112 B ? PCIAD54 113 0 Z
bit 113 C 0 PCIAD54
bit 114 B ? ENETTXER 115 0 Z
bit 115 C 0 ENETTXER
bit 116 B ? ENETRXD2 117 0 Z
bit 117 C 0 ENETRXD2
bit 118 B ? ENETRXD3 119 0 Z
bit 119 C 0 ENETRXD3
bit 120 O ? PCIX133UP 121 0 Z
bit 121 C 0 PCIX133UP
bit 122 B ? PCIAD58 123 0 Z
bit 123 C 0 PCIAD58
bit 124 B ? PCIAD57 125 0 Z
bit 125 C 0 PCIAD57
bit 126 I ? UARTSERCK
bit 127 B ? PCIAD59 128 0 Z
bit 128 C 0 PCIAD59
bit 129 B ? PCIC_BE6_N 130 0 Z
bit 130 C 0 PCIC_BE6_N
bit 131 B ? PCIAD63 132 0 Z
bit 132 C 0 PCIAD63
bit 133 B ? PCIAD56 134 0 Z
bit 134 C 0 PCIAD56
bit 135 B ? PCIAD55 136 0 Z
bit 136 C 0 PCIAD55
bit 137 B ? PCIAD1 138 0 Z
bit 138 C 0 PCIAD1
bit 139 B ? PCIAD61 140 0 Z
bit 140 C 0 PCIAD61
bit 141 B ? PCIAD62 142 0 Z
bit 142 C 0 PCIAD62
bit 143 B ? PCIAD60 144 0 Z
bit 144 C 0 PCIAD60
bit 145 B ? PCIAD42 146 0 Z
bit 146 C 0 PCIAD42
bit 147 B ? PCIC_BE4_N 148 0 Z
bit 148 C 0 PCIC_BE4_N
bit 149 B ? PCIAD5 150 0 Z
bit 150 C 0 PCIAD5
bit 151 B ? PCIC_BE7_N 152 0 Z
bit 152 C 0 PCIC_BE7_N
bit 153 B ? PCIAD2 154 0 Z
bit 154 C 0 PCIAD2
bit 155 B ? PCIACK64_N 156 0 Z
bit 156 C 0 PCIACK64_N
bit 157 B ? PCIREQ64_N 158 0 Z
bit 158 C 0 PCIREQ64_N
bit 159 B ? PCIAD3 160 0 Z
bit 160 C 0 PCIAD3
bit 161 B ? PCIAD4 162 0 Z
bit 162 C 0 PCIAD4
bit 163 B ? PCIFRAME_N 164 0 Z
bit 164 C 0 PCIFRAME_N
bit 165 B ? PCIAD6 166 0 Z
bit 166 C 0 PCIAD6
bit 167 B ? PCIAD7 168 0 Z
bit 168 C 0 PCIAD7
bit 169 B ? PCIIRDY_N 170 0 Z
bit 170 C 0 PCIIRDY_N
bit 171 B ? PCITRDY_N 172 0 Z
bit 172 C 0 PCITRDY_N
bit 173 B ? PCISTOP_N 174 0 Z
bit 174 C 0 PCISTOP_N
bit 175 I ? UART0CTS_N
bit 176 B ? PCIDEVSEL_N 177 0 Z
bit 177 C 0 PCIDEVSEL_N
bit 178 B ? PCIAD8 179 0 Z
bit 179 C 0 PCIAD8
bit 180 B ? PCIC_BE0_N 181 0 Z
bit 181 C 0 PCIC_BE0_N
bit 182 I ? PCIM66EN
bit 183 B ? PCIAD10 184 0 Z
bit 184 C 0 PCIAD10
bit 185 B ? PCIAD11 186 0 Z
bit 186 C 0 PCIAD11
bit 187 B ? PCIC_BE1_N 188 0 Z
bit 188 C 0 PCIC_BE1_N
bit 189 B ? PCIAD15 190 0 Z
bit 190 C 0 PCIAD15
bit 191 B ? PCIAD12 192 0 Z
bit 192 C 0 PCIAD12
bit 193 B ? PCIPAR 194 0 Z
bit 194 C 0 PCIPAR
bit 195 B ? PCIAD9 196 0 Z
bit 196 C 0 PCIAD9
bit 197 B ? PCIAD0 198 0 Z
bit 198 C 0 PCIAD0
bit 199 B ? PCIPERR_N 200 0 Z
bit 200 C 0 PCIPERR_N
bit 201 B ? PCIAD16 202 0 Z
bit 202 C 0 PCIAD16
bit 203 O ? UART0DTR_N 204 0 Z
bit 204 C 0 UART0DTR_N
bit 205 B ? PCIAD13 206 0 Z
bit 206 C 0 PCIAD13
bit 207 B ? PCIAD14 208 0 Z
bit 208 C 0 PCIAD14
bit 209 B ? PCIAD17 210 0 Z
bit 210 C 0 PCIAD17
bit 211 O ? UART0RTS_N 212 0 Z
bit 212 C 0 UART0RTS_N
bit 213 B ? PCIAD18 214 0 Z
bit 214 C 0 PCIAD18
bit 215 B ? UART1RX_GPIO12 216 0 Z
bit 216 C 0 UART1RX_GPIO12
bit 217 B ? PCIC_BE2_N 218 0 Z
bit 218 C 0 PCIC_BE2_N
bit 219 I ? UART0RX
bit 220 I ? UART0RI_N
bit 221 B ? PCISERR_N 222 0 Z
bit 222 C 0 PCISERR_N
bit 223 B ? UART1TX_GPIO13 224 0 Z
bit 224 C 0 UART1TX_GPIO13
bit 225 B ? PCIREQ2_N 226 0 Z
bit 226 C 0 PCIREQ2_N
bit 227 B ? PCIAD20 228 0 Z
bit 228 C 0 PCIAD20
bit 229 B ? PCIAD21 230 0 Z
bit 230 C 0 PCIAD21
bit 231 B ? PCIAD25 232 0 Z
bit 232 C 0 PCIAD25
bit 233 B ? PCIAD23 234 0 Z
bit 234 C 0 PCIAD23
bit 235 B ? PCIAD22 236 0 Z
bit 236 C 0 PCIAD22
bit 237 B ? MEMDATA48 238 0 Z
bit 238 C 0 MEMDATA48
bit 239 B ? MEMDATA49 240 0 Z
bit 240 C 0 MEMDATA49
bit 241 B ? MEMDATA50 242 0 Z
bit 242 C 0 MEMDATA50
bit 243 B ? MEMDATA51 244 0 Z
bit 244 C 0 MEMDATA51
bit 245 B ? MEMDQS6 246 0 Z
bit 246 C 0 MEMDQS6
bit 247 B ? MEMDATA52 248 0 Z
bit 248 C 0 MEMDATA52
bit 249 B ? MEMDATA53 250 0 Z
bit 250 C 0 MEMDATA53
bit 251 B ? MEMDATA54 252 0 Z
bit 252 C 0 MEMDATA54
bit 253 O ? MEMDM6 254 0 Z
bit 254 C 0 MEMDM6
bit 255 B ? MEMDATA55 256 0 Z
bit 256 C 0 MEMDATA55
bit 257 B ? MEMDATA56 258 0 Z
bit 258 C 0 MEMDATA56
bit 259 B ? MEMDATA57 260 0 Z
bit 260 C 0 MEMDATA57
bit 261 B ? MEMDATA58 262 0 Z
bit 262 C 0 MEMDATA58
bit 263 B ? MEMDATA59 264 0 Z
bit 264 C 0 MEMDATA59
bit 265 B ? MEMDQS7 266 0 Z
bit 266 C 0 MEMDQS7
bit 267 I ? MEMDM7 268 0 Z
bit 268 C 0 MEMDM7
bit 269 B ? MEMDATA60 270 0 Z
bit 270 C 0 MEMDATA60
bit 271 B ? MEMDATA61 272 0 Z
bit 272 C 0 MEMDATA61
bit 273 B ? MEMDATA63 274 0 Z
bit 274 C 0 MEMDATA63
bit 275 B ? MEMDATA62 276 0 Z
bit 276 C 0 MEMDATA62
bit 277 O ? SYSERROR 278 0 Z
bit 278 C 0 SYSERROR
bit 279 I ? UART0DSR_N
bit 280 I ? SYSHALT_N
bit 281 B ? SYSRESET_N 282 0 Z
bit 282 C 0 SYSRESET_N
bit 283 I ? SYSCKTK
bit 284 I ? GMC1RXCTL
bit 285 B ? TRACETS6 286 0 Z
bit 286 C 0 TRACETS6
bit 287 B ? TRACETS5_GPIO31 288 0 Z
bit 288 C 0 TRACETS5_GPIO31
bit 289 B ? TRACETS4_GPIO30 290 0 Z
bit 290 C 0 TRACETS4_GPIO30
bit 291 B ? TRACETS3_GPIO29 292 0 Z
bit 292 C 0 TRACETS3_GPIO29
bit 293 B ? TRACETS2_GPIO28 294 0 Z
bit 294 C 0 TRACETS2_GPIO28
bit 295 B ? TRACETS1_GPIO27 296 0 Z
bit 296 C 0 TRACETS1_GPIO27
bit 297 B ? TRACETS0_GPIO26 298 0 Z
bit 298 C 0 TRACETS0_GPIO26
bit 299 B ? TRACEES4_GPIO25 300 0 Z
bit 300 C 0 TRACEES4_GPIO25
bit 301 B ? TRACEES3_GPIO24 302 0 Z
bit 302 C 0 TRACEES3_GPIO24
bit 303 B ? TRACEES2_GPIO23 304 0 Z
bit 304 C 0 TRACEES2_GPIO23
bit 305 O ? TRACECK 306 0 Z
bit 306 C 0 TRACECK
bit 307 I ? DMAREQ0
bit 308 B ? DMAREQ3 309 0 Z
bit 309 C 0 DMAREQ3
bit 310 B ? DMAACK3 311 0 Z
bit 311 C 0 DMAACK3
bit 312 B ? DMAACK2 313 0 Z
bit 313 C 0 DMAACK2
bit 314 O ? DMAACK1 315 0 Z
bit 315 C 0 DMAACK1
bit 316 O ? DMAACK0 317 0 Z
bit 317 C 0 DMAACK0
bit 318 I ? DMAREQ2
bit 319 I ? DMAREQ1
bit 320 B ? GMC1TXCTL 321 0 Z
bit 321 C 0 GMC1TXCTL
bit 322 B ? ENETMDIO 323 0 Z
bit 323 C 0 ENETMDIO
bit 324 O ? PCIINTA_N 325 0 Z
bit 325 C 0 PCIINTA_N
bit 326 O ? ENETTXEN 327 0 Z
bit 327 C 0 ENETTXEN
bit 328 O ? UART0TX 329 0 Z
bit 329 C 0 UART0TX
bit 330 I ? GMCREFCLK
bit 331 B ? ENETRXER 332 0 Z
bit 332 C 0 ENETRXER
bit 333 O ? ENETTXD1 334 0 Z
bit 334 C 0 ENETTXD1
bit 335 B ? PCIAD34 336 0 Z
bit 336 C 0 PCIAD34
bit 337 B ? PCIAD37 338 0 Z
bit 338 C 0 PCIAD37
bit 339 O ? ENETTXD2 340 0 Z
bit 340 C 0 ENETTXD2
bit 341 B ? ENETCRS 342 0 Z
bit 342 C 0 ENETCRS
bit 343 O ? ENETTXD0 344 0 Z
bit 344 C 0 ENETTXD0
bit 345 I ? ENETTXCK
bit 346 B ? ENETRXDV 347 0 Z
bit 347 C 0 ENETRXDV
bit 348 B ? PCIPAR64 349 0 Z
bit 349 C 0 PCIPAR64
bit 350 B ? PCIAD32 351 0 Z
bit 351 C 0 PCIAD32
bit 352 B ? PCIAD33 353 0 Z
bit 353 C 0 PCIAD33
bit 354 B ? PCIAD43 355 0 Z
bit 355 C 0 PCIAD43
bit 356 B ? PCIAD39 357 0 Z
bit 357 C 0 PCIAD39
bit 358 B ? PCIAD48 359 0 Z
bit 359 C 0 PCIAD48
bit 360 B ? ENETRXCK 361 0 Z
bit 361 C 0 ENETRXCK
bit 362 O ? ENETTXD3 363 0 Z
bit 363 C 0 ENETTXD3
bit 364 B ? PCIAD52 365 0 Z
bit 365 C 0 PCIAD52
bit 366 B ? PCIAD38 367 0 Z
bit 367 C 0 PCIAD38
bit 368 B ? ENETCOL 369 0 Z
bit 369 C 0 ENETCOL
bit 370 B ? UART1DSR_CTS_GPIO14_N 371 0 Z
bit 371 C 0 UART1DSR_CTS_GPIO14_N
bit 372 B ? ENETRXD0 373 0 Z
bit 373 C 0 ENETRXD0
bit 374 B ? PCIAD44 375 0 Z
bit 375 C 0 PCIAD44
bit 376 B ? PCIAD35 377 0 Z
bit 377 C 0 PCIAD35
bit 378 B ? PCIAD47 379 0 Z
bit 379 C 0 PCIAD47
bit 380 O ? ENETMDCK 381 0 Z
bit 381 C 0 ENETMDCK
bit 382 I ? PCICLK
bit 383 I ? PCIIDSEL
bit 384 B ? PCIAD40 385 0 Z
bit 385 C 0 PCIAD40
bit 386 B ? PCIC_BE5_N 387 0 Z
bit 387 C 0 PCIC_BE5_N
bit 388 B ? PCIAD49 389 0 Z
bit 389 C 0 PCIAD49
bit 390 B ? ENETRXD1 391 0 Z
bit 391 C 0 ENETRXD1
bit 392 B ? PCIAD41 393 0 Z
bit 393 C 0 PCIAD41
bit 394 B ? PCIAD45 395 0 Z
bit 395 C 0 PCIAD45
bit 396 B ? PCIAD36 397 0 Z
bit 397 C 0 PCIAD36
bit 398 B ? MEMDATA0 399 0 Z
bit 399 C 0 MEMDATA0
bit 400 B ? MEMDATA1 401 0 Z
bit 401 C 0 MEMDATA1
bit 402 B ? MEMDATA2 403 0 Z
bit 403 C 0 MEMDATA2
bit 404 O ? MEMADR1 405 0 Z
bit 405 C 0 MEMADR1
bit 406 B ? MEMDATA3 407 0 Z
bit 407 C 0 MEMDATA3
bit 408 O ? MEMADR2 409 0 Z
bit 409 C 0 MEMADR2
bit 410 B ? MEMDQS0 411 0 Z
bit 411 C 0 MEMDQS0
bit 412 O ? MEMDM0 413 0 Z
bit 413 C 0 MEMDM0
bit 414 O ? MEMADR3 415 0 Z
bit 415 C 0 MEMADR3
bit 416 O ? MEMADR4 417 0 Z
bit 417 C 0 MEMADR4
bit 418 B ? MEMDATA4 419 0 Z
bit 419 C 0 MEMDATA4
bit 420 B ? MEMDATA5 421 0 Z
bit 421 C 0 MEMDATA5
bit 422 B ? MEMDATA6 423 0 Z
bit 423 C 0 MEMDATA6
bit 424 B ? MEMDATA7 425 0 Z
bit 425 C 0 MEMDATA7
bit 426 O ? MEMADR5 427 0 Z
bit 427 C 0 MEMADR5
bit 428 O ? MEMADR6 429 0 Z
bit 429 C 0 MEMADR6
bit 430 B ? MEMDATA8 431 0 Z
bit 431 C 0 MEMDATA8
bit 432 B ? MEMDATA9 433 0 Z
bit 433 C 0 MEMDATA9
bit 434 B ? MEMDATA10 435 0 Z
bit 435 C 0 MEMDATA10
bit 436 O ? MEMADR0 437 0 Z
bit 437 C 0 MEMADR0
bit 438 B ? MEMDATA11 439 0 Z
bit 439 C 0 MEMDATA11
bit 440 B ? MEMDQS1 441 0 Z
bit 441 C 0 MEMDQS1
bit 442 O ? MEMDM1 443 0 Z
bit 443 C 0 MEMDM1
bit 444 B ? MEMDATA12 445 0 Z
bit 445 C 0 MEMDATA12
bit 446 B ? MEMDATA13 447 0 Z
bit 447 C 0 MEMDATA13
bit 448 B ? MEMDATA14 449 0 Z
bit 449 C 0 MEMDATA14
bit 450 O ? MEMCKE0 451 0 Z
bit 451 C 0 MEMCKE0
bit 452 B ? MEMDATA15 453 0 Z
bit 453 C 0 MEMDATA15
bit 454 B ? MEMDATA16 455 0 Z
bit 455 C 0 MEMDATA16
bit 456 B ? MEMDATA17 457 0 Z
bit 457 C 0 MEMDATA17
bit 458 O ? MEMADR10 459 0 Z
bit 459 C 0 MEMADR10
bit 460 B ? MEMDATA18 461 0 Z
bit 461 C 0 MEMDATA18
bit 462 B ? MEMDATA19 463 0 Z
bit 463 C 0 MEMDATA19
bit 464 O ? MEMDM2 465 0 Z
bit 465 C 0 MEMDM2
bit 466 B ? MEMDQS2 467 0 Z
bit 467 C 0 MEMDQS2
bit 468 O ? MEMBA0 469 0 Z
bit 469 C 0 MEMBA0
bit 470 B ? MEMDATA20 471 0 Z
bit 471 C 0 MEMDATA20
bit 472 B ? MEMDATA21 473 0 Z
bit 473 C 0 MEMDATA21
bit 474 B ? MEMDATA22 475 0 Z
bit 475 C 0 MEMDATA22
bit 476 B ? MEMDATA23 477 0 Z
bit 477 C 0 MEMDATA23
bit 478 O ? MEMBSEL0_N 479 0 Z
bit 479 C 0 MEMBSEL0_N
bit 480 B ? MEMDATA24 481 0 Z
bit 481 C 0 MEMDATA24
bit 482 B ? MEMDATA25 483 0 Z
bit 483 C 0 MEMDATA25
bit 484 O ? MEMBSEL1_N 485 0 Z
bit 485 C 0 MEMBSEL1_N
bit 486 B ? MEMDATA26 487 0 Z
bit 487 C 0 MEMDATA26
bit 488 B ? MEMDATA27 489 0 Z
bit 489 C 0 MEMDATA27
bit 490 B ? MEMDQS3 491 0 Z
bit 491 C 0 MEMDQS3
bit 492 O ? MEMADR7 493 0 Z
bit 493 C 0 MEMADR7
bit 494 O ? MEMADR8 495 0 Z
bit 495 C 0 MEMADR8
bit 496 O ? MEMDM3 497 0 Z
bit 497 C 0 MEMDM3
bit 498 B ? MEMDATA28 499 0 Z
bit 499 C 0 MEMDATA28
bit 500 O ? MEMADR9 501 0 Z
bit 501 C 0 MEMADR9
bit 502 O ? MEMADR11 503 0 Z
bit 503 C 0 MEMADR11
bit 504 B ? MEMDATA29 505 0 Z
bit 505 C 0 MEMDATA29
bit 506 B ? MEMDATA30 507 0 Z
bit 507 C 0 MEMDATA30
bit 508 B ? MEMDATA31 509 0 Z
bit 509 C 0 MEMDATA31
bit 510 B ? MEMDATA32 511 0 Z
bit 511 C 0 MEMDATA32
bit 512 O ? MEMBSEL2_N 513 0 Z
bit 513 C 0 MEMBSEL2_N
bit 514 B ? MEMDATA33 515 0 Z
bit 515 C 0 MEMDATA33
bit 516 O ? MEMCKE1 517 0 Z
bit 517 C 0 MEMCKE1
bit 518 B ? MEMDATA34 519 0 Z
bit 519 C 0 MEMDATA34
bit 520 B ? MEMDATA35 521 0 Z
bit 521 C 0 MEMDATA35
bit 522 B ? MEMDATA36 523 0 Z
bit 523 C 0 MEMDATA36
bit 524 O ? MEMCKE2 525 0 Z
bit 525 C 0 MEMCKE2
bit 526 O ? MEMDM4 527 0 Z
bit 527 C 0 MEMDM4
bit 528 B ? MEMDQS4 529 0 Z
bit 529 C 0 MEMDQS4
bit 530 O ? MEMADR12 531 0 Z
bit 531 C 0 MEMADR12
bit 532 B ? MEMDATA37 533 0 Z
bit 533 C 0 MEMDATA37
bit 534 B ? MEMDATA38 535 0 Z
bit 535 C 0 MEMDATA38
bit 536 O ? MEMCKE3 537 0 Z
bit 537 C 0 MEMCKE3
bit 538 B ? MEMDATA39 539 0 Z
bit 539 C 0 MEMDATA39
bit 540 B ? MEMDATA40 541 0 Z
bit 541 C 0 MEMDATA40
bit 542 B ? MEMDATA41 543 0 Z
bit 543 C 0 MEMDATA41
bit 544 B ? MEMDATA42 545 0 Z
bit 545 C 0 MEMDATA42
bit 546 B ? MEMDATA43 547 0 Z
bit 547 C 0 MEMDATA43
bit 548 B ? MEMDATA44 549 0 Z
bit 549 C 0 MEMDATA44
bit 550 O ? MEMDM5 551 0 Z
bit 551 C 0 MEMDM5
bit 552 B ? MEMDQS5 553 0 Z
bit 553 C 0 MEMDQS5
bit 554 B ? MEMDATA45 555 0 Z
bit 555 C 0 MEMDATA45
bit 556 B ? MEMDATA46 557 0 Z
bit 557 C 0 MEMDATA46
bit 558 B ? MEMDATA47 559 0 Z
bit 559 C 0 MEMDATA47
bit 560 O ? MEMSYSCK 561 0 Z
bit 561 C 0 MEMSYSCK
bit 562 B ? MEMECC0 563 0 Z
bit 563 C 0 MEMECC0
bit 564 O ? MEMBA1 565 0 Z
bit 565 C 0 MEMBA1
bit 566 B ? MEMECC1 567 0 Z
bit 567 C 0 MEMECC1
bit 568 B ? MEMECC2 569 0 Z
bit 569 C 0 MEMECC2
bit 570 B ? MEMECC3 571 0 Z
bit 571 C 0 MEMECC3
bit 572 B ? MEMECC4 573 0 Z
bit 573 C 0 MEMECC4
bit 574 O ? MEMRAS_N 575 0 Z
bit 575 C 0 MEMRAS_N
bit 576 O ? MEMCAS_N 577 0 Z
bit 577 C 0 MEMCAS_N
bit 578 O ? MEMDM8 579 0 Z
bit 579 C 0 MEMDM8
bit 580 O ? MEMWE_N 581 0 Z
bit 581 C 0 MEMWE_N
bit 582 B ? MEMDQS8 583 0 Z
bit 583 C 0 MEMDQS8
bit 584 O ? MEMBSEL3_N 585 0 Z
bit 585 C 0 MEMBSEL3_N
bit 586 B ? MEMECC5 587 0 Z
bit 587 C 0 MEMECC5
bit 588 B ? MEMECC6 589 0 Z
bit 589 C 0 MEMECC6
bit 590 B ? MEMECC7 591 0 Z
bit 591 C 0 MEMECC7
bit 592 B ? EBCDATA12 593 0 Z
bit 593 C 0 EBCDATA12
bit 594 B ? EBCDATA5 595 0 Z
bit 595 C 0 EBCDATA5
bit 596 B ? EBCDATA4 597 0 Z
bit 597 C 0 EBCDATA4
bit 598 B ? EBCDATA11 599 0 Z
bit 599 C 0 EBCDATA11
bit 600 B ? EBCDATA2 601 0 Z
bit 601 C 0 EBCDATA2
bit 602 B ? EBCDATA7 603 0 Z
bit 603 C 0 EBCDATA7
bit 604 B ? EBCDATA6 605 0 Z
bit 605 C 0 EBCDATA6
bit 606 B ? EBCDATA3 607 0 Z
bit 607 C 0 EBCDATA3
bit 608 B ? EBCADR17 609 0 Z
bit 609 C 0 EBCADR17
bit 610 B ? EBCDATA0 611 0 Z
bit 611 C 0 EBCDATA0
bit 612 B ? EBCDATA1 613 0 Z
bit 613 C 0 EBCDATA1
bit 614 B ? EBCADR18 615 0 Z
bit 615 C 0 EBCADR18
bit 616 B ? EBCDATA21 617 0 Z
bit 617 C 0 EBCDATA21
bit 618 B ? EBCDATA10 619 0 Z
bit 619 C 0 EBCDATA10
bit 620 B ? EBCDATA25 621 0 Z
bit 621 C 0 EBCDATA25
bit 622 B ? EBCDATA31 623 0 Z
bit 623 C 0 EBCDATA31
bit 624 B ? EBCDATA24 625 0 Z
bit 625 C 0 EBCDATA24
bit 626 B ? EBCADR19 627 0 Z
bit 627 C 0 EBCADR19
bit 628 B ? EBCDATA8 629 0 Z
bit 629 C 0 EBCDATA8
bit 630 B ? EBCDATA9 631 0 Z
bit 631 C 0 EBCDATA9
bit 632 B ? EBCDATA30 633 0 Z
bit 633 C 0 EBCDATA30
bit 634 B ? EBCDATA23 635 0 Z
bit 635 C 0 EBCDATA23
bit 636 B ? EBCDATA22 637 0 Z
bit 637 C 0 EBCDATA22
bit 638 B ? EBCADR22 639 0 Z
bit 639 C 0 EBCADR22
bit 640 B ? EBCDATA20 641 0 Z
bit 641 C 0 EBCDATA20
bit 642 B ? EBCDATA29 643 0 Z
bit 643 C 0 EBCDATA29
bit 644 B ? EBCADR20 645 0 Z
bit 645 C 0 EBCADR20
bit 646 B ? EBCADR23 647 0 Z
bit 647 C 0 EBCADR23
bit 648 B ? EBCADR24 649 0 Z
bit 649 C 0 EBCADR24
bit 650 B ? EBCADR25 651 0 Z
bit 651 C 0 EBCADR25
bit 652 B ? EBCADR26 653 0 Z
bit 653 C 0 EBCADR26
bit 654 B ? EBCADR27 655 0 Z
bit 655 C 0 EBCADR27
bit 656 B ? EBCADR29 657 0 Z
bit 657 C 0 EBCADR29
bit 658 B ? EBCADR30 659 0 Z
bit 659 C 0 EBCADR30
bit 660 B ? EBCADR31 661 0 Z
bit 661 C 0 EBCADR31
bit 662 B ? EBCPAR0 663 0 Z
bit 663 C 0 EBCPAR0
bit 664 B ? EBCPAR1 665 0 Z
bit 665 C 0 EBCPAR1
bit 666 B ? EBCPAR2 667 0 Z
bit 667 C 0 EBCPAR2
bit 668 B ? EBCPAR3 669 0 Z
bit 669 C 0 EBCPAR3
bit 670 B ? EBCBE0_N 671 0 Z
bit 671 C 0 EBCBE0_N
bit 672 B ? EBCBE1_N 673 0 Z
bit 673 C 0 EBCBE1_N
bit 674 O ? EBCCS3_N 675 0 Z
bit 675 C 0 EBCCS3_N
bit 676 B ? EBCBE2_N 677 0 Z
bit 677 C 0 EBCBE2_N
bit 678 B ? EBCBE3_N 679 0 Z
bit 679 C 0 EBCBE3_N
bit 680 B ? EBCDATA19 681 0 Z
bit 681 C 0 EBCDATA19
bit 682 B ? EBCBLAST_N 683 0 Z
bit 683 C 0 EBCBLAST_N
bit 684 B ? EBCDATA27 685 0 Z
bit 685 C 0 EBCDATA27
bit 686 B ? EBCADR0 687 0 Z
bit 687 C 0 EBCADR0
bit 688 B ? EBCDATA18 689 0 Z
bit 689 C 0 EBCDATA18
bit 690 B ? EBCDATA17 691 0 Z
bit 691 C 0 EBCDATA17
bit 692 B ? EBCADR1 693 0 Z
bit 693 C 0 EBCADR1
bit 694 B ? EBCADR2 695 0 Z
bit 695 C 0 EBCADR2
bit 696 B ? IIC1SCK_GPIO16 697 0 Z
bit 697 C 0 IIC1SCK_GPIO16
bit 698 B ? EBCDATA16 699 0 Z
bit 699 C 0 EBCDATA16
bit 700 B ? EBCADR3 701 0 Z
bit 701 C 0 EBCADR3
bit 702 B ? EBCADR6 703 0 Z
bit 703 C 0 EBCADR6
bit 704 B ? IIC0SCK 705 0 Z
bit 705 C 0 IIC0SCK
bit 706 O ? EBCCS6_N 707 0 Z
bit 707 C 0 EBCCS6_N
bit 708 B ? IIC0SDATA 709 0 Z
bit 709 C 0 IIC0SDATA
bit 710 B ? EBCADR9 711 0 Z
bit 711 C 0 EBCADR9
bit 712 B ? EBCADR12 713 0 Z
bit 713 C 0 EBCADR12
bit 714 B ? EBCDATA15 715 0 Z
bit 715 C 0 EBCDATA15
bit 716 B ? IIC1SDATA_GPIO17 717 0 Z
bit 717 C 0 IIC1SDATA_GPIO17
bit 718 B ? EBCADR13 719 0 Z
bit 719 C 0 EBCADR13
bit 720 B ? EBCADR14 721 0 Z
bit 721 C 0 EBCADR14
bit 722 B ? EBCDATA14 723 0 Z
bit 723 C 0 EBCDATA14
bit 724 B ? EBCDATA13 725 0 Z
bit 725 C 0 EBCDATA13
bit 726 B ? EBCADR15 727 0 Z
bit 727 C 0 EBCADR15
bit 728 B ? EBCDATA26 729 0 Z
bit 729 C 0 EBCDATA26
bit 730 B ? EBCADR5 731 0 Z
bit 731 C 0 EBCADR5
bit 732 O ? EBCCS0_N 733 0 Z
bit 733 C 0 EBCCS0_N
bit 734 B ? EBCADR11 735 0 Z
bit 735 C 0 EBCADR11
bit 736 B ? EBCADR4 737 0 Z
bit 737 C 0 EBCADR4
bit 738 B ? EBCADR10 739 0 Z
bit 739 C 0 EBCADR10
bit 740 B ? EBCADR16 741 0 Z
bit 741 C 0 EBCADR16
bit 742 O ? EBCCS5_N 743 0 Z
bit 743 C 0 EBCCS5_N
bit 744 O ? EBCCS2_N 745 0 Z
bit 745 C 0 EBCCS2_N
bit 746 O ? EBCCS7_N 747 0 Z
bit 747 C 0 EBCCS7_N
bit 748 O ? EBCWE_N 749 0 Z
bit 749 C 0 EBCWE_N
bit 750 B ? EBCADR8 751 0 Z
bit 751 C 0 EBCADR8
bit 752 B ? EBCADR28 753 0 Z
bit 753 C 0 EBCADR28
bit 754 B ? EBCRNW 755 0 Z
bit 755 C 0 EBCRNW
bit 756 I ? EBCREADY
bit 757 B ? EBCADR7 758 0 Z
bit 758 C 0 EBCADR7
bit 759 B ? EBCADR21 760 0 Z
bit 760 C 0 EBCADR21
bit 761 O ? EBCOE_N 762 0 Z
bit 762 C 0 EBCOE_N
bit 763 O ? EBCCS4_N 764 0 Z
bit 764 C 0 EBCCS4_N
bit 765 B ? EBCDATA28 766 0 Z
bit 766 C 0 EBCDATA28
bit 767 O ? EBCCS1_N 768 0 Z
bit 768 C 0 EBCCS1_N
