signal GND1
signal GND2
signal GND3
signal GND4
signal GND5
signal GND6
signal GND7
signal GND8
signal GND9
signal GND10
signal GND11
signal GND12
signal GND13
signal GND14
signal GND15
signal GND16
signal CCLK_P72
signal DONE_P71
signal HSWAP_EN_P142
signal M0_P38
signal M1_P37
signal M2_P39
signal PROG_B
signal TCK
signal TDI
signal TDO
signal TMS
signal VCCAUX1
signal VCCAUX2
signal VCCAUX3
signal VCCAUX4
signal VCCINT1
signal VCCINT2
signal VCCINT3
signal VCCINT4
signal VCCO011
signal VCCO012
signal VCCO013
signal VCCO231
signal VCCO232
signal VCCO233
signal VCCO451
signal VCCO452
signal VCCO453
signal VCCO671
signal VCCO672
signal VCCO673
signal IO_P1
signal IO_P2
signal IO_P4
signal IO_P5
signal IO_P6
signal IO_P7
signal IO_P8
signal IO_P10
signal IO_P11
signal IO_P12
signal IO_P13
signal IO_P14
signal IO_P15
signal IO_P17
signal IO_P18
signal IO_P20
signal IO_P21
signal IO_P23
signal IO_P24
signal IO_P25
signal IO_P26
signal IO_P27
signal IO_P28
signal IO_P30
signal IO_P31
signal IO_P32
signal IO_P33
signal IO_P35
signal IO_P36
signal IO_P40
signal IO_P41
signal IO_P44
signal IO_P46
signal IO_P47
signal IO_P50
signal IO_P51
signal IO_P52
signal IO_P53
signal IO_P55
signal IO_P56
signal IO_P57
signal IO_P58
signal IO_P59
signal IO_P60
signal IO_P63
signal IO_P65
signal IO_P68
signal IO_P69
signal IO_P70
signal IO_P73
signal IO_P74
signal IO_P76
signal IO_P77
signal IO_P78
signal IO_P79
signal IO_P80
signal IO_P82
signal IO_P83
signal IO_P84
signal IO_P85
signal IO_P86
signal IO_P87
signal IO_P89
signal IO_P90
signal IO_P92
signal IO_P93
signal IO_P95
signal IO_P96
signal IO_P97
signal IO_P98
signal IO_P99
signal IO_P100
signal IO_P102
signal IO_P103
signal IO_P104
signal IO_P105
signal IO_P107
signal IO_P108
signal IO_P112
signal IO_P113
signal IO_P116
signal IO_P118
signal IO_P119
signal IO_P122
signal IO_P123
signal IO_P124
signal IO_P125
signal IO_P127
signal IO_P128
signal IO_P129
signal IO_P130
signal IO_P131
signal IO_P132
signal IO_P135
signal IO_P137
signal IO_P140

register	BSR	815
register	BR	1
register	DIR	32

instruction length 6

instruction EXTEST 000000 BSR
instruction SAMPLE/PRELOAD 000001 BSR
instruction IDCODE 001001 DIR
instruction BYPASS 111111 BR

bit 814 I 1 IO_P108
bit 813 O 1 IO_P108 812 1 Z
bit 812 C 1 *
bit 811 I 1 IO_P107
bit 810 O 1 IO_P107 809 1 Z
bit 809 C 1 *
bit 808 O 1 *
bit 807 O 1 *
bit 806 O 1 *
bit 805 O 1 *
bit 804 O 1 *
bit 803 O 1 *
bit 802 O 1 *
bit 801 O 1 *
bit 800 O 1 *
bit 799 O 1 *
bit 798 O 1 *
bit 797 O 1 *
bit 796 O 1 *
bit 795 O 1 *
bit 794 O 1 *
bit 793 O 1 *
bit 792 O 1 *
bit 791 O 1 *
bit 790 O 1 *
bit 789 O 1 *
bit 788 O 1 *
bit 787 O 1 *
bit 786 O 1 *
bit 785 O 1 *
bit 784 I 1 IO_P105
bit 783 O 1 IO_P105 782 1 Z
bit 782 C 1 *
bit 781 I 1 IO_P104
bit 780 O 1 IO_P104 779 1 Z
bit 779 C 1 *
bit 778 I 1 IO_P103
bit 777 O 1 IO_P103 776 1 Z
bit 776 C 1 *
bit 775 I 1 IO_P102
bit 774 O 1 IO_P102 773 1 Z
bit 773 C 1 *
bit 772 I 1 IO_P100
bit 771 O 1 IO_P100 770 1 Z
bit 770 C 1 *
bit 769 I 1 IO_P99
bit 768 O 1 IO_P99 767 1 Z
bit 767 C 1 *
bit 766 I 1 IO_P98
bit 765 O 1 IO_P98 764 1 Z
bit 764 C 1 *
bit 763 I 1 IO_P97
bit 762 O 1 IO_P97 761 1 Z
bit 761 C 1 *
bit 760 I 1 IO_P96
bit 759 O 1 IO_P96 758 1 Z
bit 758 C 1 *
bit 757 I 1 IO_P95
bit 756 O 1 IO_P95 755 1 Z
bit 755 C 1 *
bit 754 O 1 *
bit 753 O 1 *
bit 752 O 1 *
bit 751 O 1 *
bit 750 O 1 *
bit 749 O 1 *
bit 748 O 1 *
bit 747 O 1 *
bit 746 O 1 *
bit 745 O 1 *
bit 744 O 1 *
bit 743 O 1 *
bit 742 O 1 *
bit 741 O 1 *
bit 740 O 1 *
bit 739 O 1 *
bit 738 O 1 *
bit 737 O 1 *
bit 736 O 1 *
bit 735 O 1 *
bit 734 O 1 *
bit 733 O 1 *
bit 732 O 1 *
bit 731 O 1 *
bit 730 O 1 *
bit 729 O 1 *
bit 728 O 1 *
bit 727 O 1 *
bit 726 O 1 *
bit 725 O 1 *
bit 724 I 1 IO_P93
bit 723 O 1 IO_P93 722 1 Z
bit 722 C 1 *
bit 721 I 1 IO_P92
bit 720 O 1 IO_P92 719 1 Z
bit 719 C 1 *
bit 718 I 1 IO_P90
bit 717 O 1 IO_P90 716 1 Z
bit 716 C 1 *
bit 715 I 1 IO_P89
bit 714 O 1 IO_P89 713 1 Z
bit 713 C 1 *
bit 712 O 1 *
bit 711 O 1 *
bit 710 O 1 *
bit 709 O 1 *
bit 708 O 1 *
bit 707 O 1 *
bit 706 O 1 *
bit 705 O 1 *
bit 704 O 1 *
bit 703 O 1 *
bit 702 O 1 *
bit 701 O 1 *
bit 700 O 1 *
bit 699 O 1 *
bit 698 O 1 *
bit 697 O 1 *
bit 696 O 1 *
bit 695 O 1 *
bit 694 O 1 *
bit 693 O 1 *
bit 692 O 1 *
bit 691 O 1 *
bit 690 O 1 *
bit 689 O 1 *
bit 688 O 1 *
bit 687 O 1 *
bit 686 O 1 *
bit 685 O 1 *
bit 684 O 1 *
bit 683 O 1 *
bit 682 I 1 IO_P87
bit 681 O 1 IO_P87 680 1 Z
bit 680 C 1 *
bit 679 I 1 IO_P86
bit 678 O 1 IO_P86 677 1 Z
bit 677 C 1 *
bit 676 I 1 IO_P85
bit 675 O 1 IO_P85 674 1 Z
bit 674 C 1 *
bit 673 I 1 IO_P84
bit 672 O 1 IO_P84 671 1 Z
bit 671 C 1 *
bit 670 I 1 IO_P83
bit 669 O 1 IO_P83 668 1 Z
bit 668 C 1 *
bit 667 I 1 IO_P82
bit 666 O 1 IO_P82 665 1 Z
bit 665 C 1 *
bit 664 I 1 IO_P80
bit 663 O 1 IO_P80 662 1 Z
bit 662 C 1 *
bit 661 I 1 IO_P79
bit 660 O 1 IO_P79 659 1 Z
bit 659 C 1 *
bit 658 I 1 IO_P78
bit 657 O 1 IO_P78 656 1 Z
bit 656 C 1 *
bit 655 I 1 IO_P77
bit 654 O 1 IO_P77 653 1 Z
bit 653 C 1 *
bit 652 I 1 IO_P76
bit 651 O 1 IO_P76 650 1 Z
bit 650 C 1 *
bit 649 O 1 *
bit 648 O 1 *
bit 647 O 1 *
bit 646 O 1 *
bit 645 O 1 *
bit 644 O 1 *
bit 643 O 1 *
bit 642 O 1 *
bit 641 O 1 *
bit 640 O 1 *
bit 639 O 1 *
bit 638 O 1 *
bit 637 O 1 *
bit 636 O 1 *
bit 635 O 1 *
bit 634 O 1 *
bit 633 O 1 *
bit 632 O 1 *
bit 631 O 1 *
bit 630 O 1 *
bit 629 O 1 *
bit 628 I 1 IO_P74
bit 627 O 1 IO_P74 626 1 Z
bit 626 C 1 *
bit 625 I 1 IO_P73
bit 624 O 1 IO_P73 623 1 Z
bit 623 C 1 *
bit 622 I 1 CCLK_P72
bit 621 O 1 CCLK_P72 620 1 Z
bit 620 C 1 *
bit 619 I 1 DONE_P71
bit 618 O 1 DONE_P71 617 1 Z
bit 617 C 1 *
bit 616 I 1 IO_P70
bit 615 O 1 IO_P70 614 1 Z
bit 614 C 1 *
bit 613 I 1 IO_P69
bit 612 O 1 IO_P69 611 1 Z
bit 611 C 1 *
bit 610 I 1 IO_P68
bit 609 O 1 IO_P68 608 1 Z
bit 608 C 1 *
bit 607 O 1 *
bit 606 O 1 *
bit 605 O 1 *
bit 604 O 1 *
bit 603 O 1 *
bit 602 O 1 *
bit 601 O 1 *
bit 600 O 1 *
bit 599 O 1 *
bit 598 O 1 *
bit 597 O 1 *
bit 596 O 1 *
bit 595 O 1 *
bit 594 O 1 *
bit 593 O 1 *
bit 592 O 1 *
bit 591 O 1 *
bit 590 O 1 *
bit 589 O 1 *
bit 588 O 1 *
bit 587 O 1 *
bit 586 O 1 *
bit 585 O 1 *
bit 584 O 1 *
bit 583 O 1 *
bit 582 O 1 *
bit 581 O 1 *
bit 580 O 1 *
bit 579 O 1 *
bit 578 O 1 *
bit 577 O 1 *
bit 576 O 1 *
bit 575 O 1 *
bit 574 O 1 *
bit 573 O 1 *
bit 572 O 1 *
bit 571 O 1 *
bit 570 O 1 *
bit 569 O 1 *
bit 568 O 1 *
bit 567 O 1 *
bit 566 O 1 *
bit 565 O 1 *
bit 564 O 1 *
bit 563 O 1 *
bit 562 O 1 *
bit 561 O 1 *
bit 560 O 1 *
bit 559 O 1 *
bit 558 O 1 *
bit 557 O 1 *
bit 556 O 1 *
bit 555 O 1 *
bit 554 O 1 *
bit 553 I 1 IO_P65
bit 552 O 1 IO_P65 551 1 Z
bit 551 C 1 *
bit 550 I 1 IO_P63
bit 549 O 1 IO_P63 548 1 Z
bit 548 C 1 *
bit 547 O 1 *
bit 546 O 1 *
bit 545 O 1 *
bit 544 O 1 *
bit 543 O 1 *
bit 542 O 1 *
bit 541 O 1 *
bit 540 O 1 *
bit 539 O 1 *
bit 538 O 1 *
bit 537 O 1 *
bit 536 O 1 *
bit 535 O 1 *
bit 534 O 1 *
bit 533 O 1 *
bit 532 I 1 IO_P60
bit 531 O 1 IO_P60 530 1 Z
bit 530 C 1 *
bit 529 I 1 IO_P59
bit 528 O 1 IO_P59 527 1 Z
bit 527 C 1 *
bit 526 O 1 *
bit 525 O 1 *
bit 524 O 1 *
bit 523 I 1 IO_P58
bit 522 O 1 IO_P58 521 1 Z
bit 521 C 1 *
bit 520 I 1 IO_P57
bit 519 O 1 IO_P57 518 1 Z
bit 518 C 1 *
bit 517 I 1 IO_P56
bit 516 O 1 IO_P56 515 1 Z
bit 515 C 1 *
bit 514 I 1 IO_P55
bit 513 O 1 IO_P55 512 1 Z
bit 512 C 1 *
bit 511 O 1 *
bit 510 O 1 *
bit 509 O 1 *
bit 508 I 1 IO_P53
bit 507 O 1 IO_P53 506 1 Z
bit 506 C 1 *
bit 505 I 1 IO_P52
bit 504 O 1 IO_P52 503 1 Z
bit 503 C 1 *
bit 502 I 1 IO_P51
bit 501 O 1 IO_P51 500 1 Z
bit 500 C 1 *
bit 499 I 1 IO_P50
bit 498 O 1 IO_P50 497 1 Z
bit 497 C 1 *
bit 496 O 1 *
bit 495 O 1 *
bit 494 O 1 *
bit 493 O 1 *
bit 492 O 1 *
bit 491 O 1 *
bit 490 O 1 *
bit 489 O 1 *
bit 488 O 1 *
bit 487 O 1 *
bit 486 O 1 *
bit 485 O 1 *
bit 484 O 1 *
bit 483 O 1 *
bit 482 O 1 *
bit 481 O 1 *
bit 480 O 1 *
bit 479 O 1 *
bit 478 I 1 IO_P47
bit 477 O 1 IO_P47 476 1 Z
bit 476 C 1 *
bit 475 I 1 IO_P46
bit 474 O 1 IO_P46 473 1 Z
bit 473 C 1 *
bit 472 I 1 IO_P44
bit 471 O 1 IO_P44 470 1 Z
bit 470 C 1 *
bit 469 O 1 *
bit 468 O 1 *
bit 467 O 1 *
bit 466 O 1 *
bit 465 O 1 *
bit 464 O 1 *
bit 463 O 1 *
bit 462 O 1 *
bit 461 O 1 *
bit 460 O 1 *
bit 459 O 1 *
bit 458 O 1 *
bit 457 O 1 *
bit 456 O 1 *
bit 455 O 1 *
bit 454 O 1 *
bit 453 O 1 *
bit 452 O 1 *
bit 451 O 1 *
bit 450 O 1 *
bit 449 O 1 *
bit 448 O 1 *
bit 447 O 1 *
bit 446 O 1 *
bit 445 O 1 *
bit 444 O 1 *
bit 443 O 1 *
bit 442 O 1 *
bit 441 O 1 *
bit 440 O 1 *
bit 439 O 1 *
bit 438 O 1 *
bit 437 O 1 *
bit 436 O 1 *
bit 435 O 1 *
bit 434 O 1 *
bit 433 O 1 *
bit 432 O 1 *
bit 431 O 1 *
bit 430 O 1 *
bit 429 O 1 *
bit 428 O 1 *
bit 427 O 1 *
bit 426 O 1 *
bit 425 O 1 *
bit 424 O 1 *
bit 423 O 1 *
bit 422 O 1 *
bit 421 O 1 *
bit 420 O 1 *
bit 419 O 1 *
bit 418 O 1 *
bit 417 O 1 *
bit 416 O 1 *
bit 415 O 1 *
bit 414 O 1 *
bit 413 O 1 *
bit 412 I 1 IO_P41
bit 411 O 1 IO_P41 410 1 Z
bit 410 C 1 *
bit 409 I 1 IO_P40
bit 408 O 1 IO_P40 407 1 Z
bit 407 C 1 *
bit 406 I 1 M2_P39
bit 405 I 1 M0_P38
bit 404 I 1 M1_P37
bit 403 I 1 IO_P36
bit 402 O 1 IO_P36 401 1 Z
bit 401 C 1 *
bit 400 I 1 IO_P35
bit 399 O 1 IO_P35 398 1 Z
bit 398 C 1 *
bit 397 O 1 *
bit 396 O 1 *
bit 395 O 1 *
bit 394 O 1 *
bit 393 O 1 *
bit 392 O 1 *
bit 391 O 1 *
bit 390 O 1 *
bit 389 O 1 *
bit 388 O 1 *
bit 387 O 1 *
bit 386 O 1 *
bit 385 O 1 *
bit 384 O 1 *
bit 383 O 1 *
bit 382 O 1 *
bit 381 O 1 *
bit 380 O 1 *
bit 379 O 1 *
bit 378 O 1 *
bit 377 O 1 *
bit 376 O 1 *
bit 375 O 1 *
bit 374 O 1 *
bit 373 I 1 IO_P33
bit 372 O 1 IO_P33 371 1 Z
bit 371 C 1 *
bit 370 I 1 IO_P32
bit 369 O 1 IO_P32 368 1 Z
bit 368 C 1 *
bit 367 I 1 IO_P31
bit 366 O 1 IO_P31 365 1 Z
bit 365 C 1 *
bit 364 I 1 IO_P30
bit 363 O 1 IO_P30 362 1 Z
bit 362 C 1 *
bit 361 I 1 IO_P28
bit 360 O 1 IO_P28 359 1 Z
bit 359 C 1 *
bit 358 I 1 IO_P27
bit 357 O 1 IO_P27 356 1 Z
bit 356 C 1 *
bit 355 I 1 IO_P26
bit 354 O 1 IO_P26 353 1 Z
bit 353 C 1 *
bit 352 I 1 IO_P25
bit 351 O 1 IO_P25 350 1 Z
bit 350 C 1 *
bit 349 I 1 IO_P24
bit 348 O 1 IO_P24 347 1 Z
bit 347 C 1 *
bit 346 I 1 IO_P23
bit 345 O 1 IO_P23 344 1 Z
bit 344 C 1 *
bit 343 O 1 *
bit 342 O 1 *
bit 341 O 1 *
bit 340 O 1 *
bit 339 O 1 *
bit 338 O 1 *
bit 337 O 1 *
bit 336 O 1 *
bit 335 O 1 *
bit 334 O 1 *
bit 333 O 1 *
bit 332 O 1 *
bit 331 O 1 *
bit 330 O 1 *
bit 329 O 1 *
bit 328 O 1 *
bit 327 O 1 *
bit 326 O 1 *
bit 325 O 1 *
bit 324 O 1 *
bit 323 O 1 *
bit 322 O 1 *
bit 321 O 1 *
bit 320 O 1 *
bit 319 O 1 *
bit 318 O 1 *
bit 317 O 1 *
bit 316 O 1 *
bit 315 O 1 *
bit 314 O 1 *
bit 313 I 1 IO_P21
bit 312 O 1 IO_P21 311 1 Z
bit 311 C 1 *
bit 310 I 1 IO_P20
bit 309 O 1 IO_P20 308 1 Z
bit 308 C 1 *
bit 307 I 1 IO_P18
bit 306 O 1 IO_P18 305 1 Z
bit 305 C 1 *
bit 304 I 1 IO_P17
bit 303 O 1 IO_P17 302 1 Z
bit 302 C 1 *
bit 301 O 1 *
bit 300 O 1 *
bit 299 O 1 *
bit 298 O 1 *
bit 297 O 1 *
bit 296 O 1 *
bit 295 O 1 *
bit 294 O 1 *
bit 293 O 1 *
bit 292 O 1 *
bit 291 O 1 *
bit 290 O 1 *
bit 289 O 1 *
bit 288 O 1 *
bit 287 O 1 *
bit 286 O 1 *
bit 285 O 1 *
bit 284 O 1 *
bit 283 O 1 *
bit 282 O 1 *
bit 281 O 1 *
bit 280 O 1 *
bit 279 O 1 *
bit 278 O 1 *
bit 277 O 1 *
bit 276 O 1 *
bit 275 O 1 *
bit 274 O 1 *
bit 273 O 1 *
bit 272 O 1 *
bit 271 I 1 IO_P15
bit 270 O 1 IO_P15 269 1 Z
bit 269 C 1 *
bit 268 I 1 IO_P14
bit 267 O 1 IO_P14 266 1 Z
bit 266 C 1 *
bit 265 I 1 IO_P13
bit 264 O 1 IO_P13 263 1 Z
bit 263 C 1 *
bit 262 I 1 IO_P12
bit 261 O 1 IO_P12 260 1 Z
bit 260 C 1 *
bit 259 I 1 IO_P11
bit 258 O 1 IO_P11 257 1 Z
bit 257 C 1 *
bit 256 I 1 IO_P10
bit 255 O 1 IO_P10 254 1 Z
bit 254 C 1 *
bit 253 I 1 IO_P8
bit 252 O 1 IO_P8 251 1 Z
bit 251 C 1 *
bit 250 I 1 IO_P7
bit 249 O 1 IO_P7 248 1 Z
bit 248 C 1 *
bit 247 I 1 IO_P6
bit 246 O 1 IO_P6 245 1 Z
bit 245 C 1 *
bit 244 I 1 IO_P5
bit 243 O 1 IO_P5 242 1 Z
bit 242 C 1 *
bit 241 I 1 IO_P4
bit 240 O 1 IO_P4 239 1 Z
bit 239 C 1 *
bit 238 O 1 *
bit 237 O 1 *
bit 236 O 1 *
bit 235 O 1 *
bit 234 O 1 *
bit 233 O 1 *
bit 232 O 1 *
bit 231 O 1 *
bit 230 O 1 *
bit 229 O 1 *
bit 228 O 1 *
bit 227 O 1 *
bit 226 O 1 *
bit 225 O 1 *
bit 224 O 1 *
bit 223 O 1 *
bit 222 O 1 *
bit 221 O 1 *
bit 220 O 1 *
bit 219 O 1 *
bit 218 O 1 *
bit 217 I 1 IO_P2
bit 216 O 1 IO_P2 215 1 Z
bit 215 C 1 *
bit 214 I 1 IO_P1
bit 213 O 1 IO_P1 212 1 Z
bit 212 C 1 *
bit 211 O 1 *
bit 210 I 1 HSWAP_EN_P142
bit 209 O 1 *
bit 208 O 1 *
bit 207 O 1 *
bit 206 I 1 IO_P141
bit 205 O 1 IO_P141 204 1 Z
bit 204 C 1 *
bit 203 I 1 IO_P140
bit 202 O 1 IO_P140 201 1 Z
bit 201 C 1 *
bit 200 O 1 *
bit 199 O 1 *
bit 198 O 1 *
bit 197 O 1 *
bit 196 O 1 *
bit 195 O 1 *
bit 194 O 1 *
bit 193 O 1 *
bit 192 O 1 *
bit 191 O 1 *
bit 190 O 1 *
bit 189 O 1 *
bit 188 O 1 *
bit 187 O 1 *
bit 186 O 1 *
bit 185 O 1 *
bit 184 O 1 *
bit 183 O 1 *
bit 182 O 1 *
bit 181 O 1 *
bit 180 O 1 *
bit 179 O 1 *
bit 178 O 1 *
bit 177 O 1 *
bit 176 O 1 *
bit 175 O 1 *
bit 174 O 1 *
bit 173 O 1 *
bit 172 O 1 *
bit 171 O 1 *
bit 170 O 1 *
bit 169 O 1 *
bit 168 O 1 *
bit 167 O 1 *
bit 166 O 1 *
bit 165 O 1 *
bit 164 O 1 *
bit 163 O 1 *
bit 162 O 1 *
bit 161 O 1 *
bit 160 O 1 *
bit 159 O 1 *
bit 158 O 1 *
bit 157 O 1 *
bit 156 O 1 *
bit 155 O 1 *
bit 154 O 1 *
bit 153 O 1 *
bit 152 O 1 *
bit 151 O 1 *
bit 150 O 1 *
bit 149 O 1 *
bit 148 O 1 *
bit 147 O 1 *
bit 146 I 1 IO_P137
bit 145 O 1 IO_P137 144 1 Z
bit 144 C 1 *
bit 143 I 1 IO_P135
bit 142 O 1 IO_P135 141 1 Z
bit 141 C 1 *
bit 140 O 1 *
bit 139 O 1 *
bit 138 O 1 *
bit 137 O 1 *
bit 136 O 1 *
bit 135 O 1 *
bit 134 O 1 *
bit 133 O 1 *
bit 132 O 1 *
bit 131 O 1 *
bit 130 O 1 *
bit 129 O 1 *
bit 128 O 1 *
bit 127 O 1 *
bit 126 O 1 *
bit 125 I 1 IO_P132
bit 124 O 1 IO_P132 123 1 Z
bit 123 C 1 *
bit 122 I 1 IO_P131
bit 121 O 1 IO_P131 120 1 Z
bit 120 C 1 *
bit 119 O 1 *
bit 118 O 1 *
bit 117 O 1 *
bit 116 I 1 IO_P130
bit 115 O 1 IO_P130 114 1 Z
bit 114 C 1 *
bit 113 I 1 IO_P129
bit 112 O 1 IO_P129 111 1 Z
bit 111 C 1 *
bit 110 I 1 IO_P128
bit 109 O 1 IO_P128 108 1 Z
bit 108 C 1 *
bit 107 I 1 IO_P127
bit 106 O 1 IO_P127 105 1 Z
bit 105 C 1 *
bit 104 O 1 *
bit 103 O 1 *
bit 102 O 1 *
bit 101 I 1 IO_P125
bit 100 O 1 IO_P125 99 1 Z
bit 99 C 1 *
bit 98 I 1 IO_P124
bit 97 O 1 IO_P124 96 1 Z
bit 96 C 1 *
bit 95 I 1 IO_P123
bit 94 O 1 IO_P123 93 1 Z
bit 93 C 1 *
bit 92 I 1 IO_P122
bit 91 O 1 IO_P122 90 1 Z
bit 90 C 1 *
bit 89 O 1 *
bit 88 O 1 *
bit 87 O 1 *
bit 86 O 1 *
bit 85 O 1 *
bit 84 O 1 *
bit 83 O 1 *
bit 82 O 1 *
bit 81 O 1 *
bit 80 O 1 *
bit 79 O 1 *
bit 78 O 1 *
bit 77 O 1 *
bit 76 O 1 *
bit 75 O 1 *
bit 74 O 1 *
bit 73 O 1 *
bit 72 O 1 *
bit 71 I 1 IO_P119
bit 70 O 1 IO_P119 69 1 Z
bit 69 C 1 *
bit 68 I 1 IO_P118
bit 67 O 1 IO_P118 66 1 Z
bit 66 C 1 *
bit 65 I 1 IO_P116
bit 64 O 1 IO_P116 63 1 Z
bit 63 C 1 *
bit 62 O 1 *
bit 61 O 1 *
bit 60 O 1 *
bit 59 O 1 *
bit 58 O 1 *
bit 57 O 1 *
bit 56 O 1 *
bit 55 O 1 *
bit 54 O 1 *
bit 53 O 1 *
bit 52 O 1 *
bit 51 O 1 *
bit 50 O 1 *
bit 49 O 1 *
bit 48 O 1 *
bit 47 O 1 *
bit 46 O 1 *
bit 45 O 1 *
bit 44 O 1 *
bit 43 O 1 *
bit 42 O 1 *
bit 41 O 1 *
bit 40 O 1 *
bit 39 O 1 *
bit 38 O 1 *
bit 37 O 1 *
bit 36 O 1 *
bit 35 O 1 *
bit 34 O 1 *
bit 33 O 1 *
bit 32 O 1 *
bit 31 O 1 *
bit 30 O 1 *
bit 29 O 1 *
bit 28 O 1 *
bit 27 O 1 *
bit 26 O 1 *
bit 25 O 1 *
bit 24 O 1 *
bit 23 O 1 *
bit 22 O 1 *
bit 21 O 1 *
bit 20 O 1 *
bit 19 O 1 *
bit 18 O 1 *
bit 17 O 1 *
bit 16 O 1 *
bit 15 O 1 *
bit 14 O 1 *
bit 13 O 1 *
bit 12 O 1 *
bit 11 O 1 *
bit 10 O 1 *
bit 9 O 1 *
bit 8 O 1 *
bit 7 O 1 *
bit 6 O 1 *
bit 5 I 1 IO_P113
bit 4 O 1 IO_P113 3 1 Z
bit 3 C 1 *
bit 2 I 1 IO_P112
bit 1 O 1 IO_P112 0 1 Z
bit 0 C 1 *
