signal GND1
signal GND2
signal GND3
signal GND4
signal GND5
signal GND6
signal GND7
signal GND8
signal GND9
signal GND10
signal GND11
signal GND12
signal GND13
signal GND14
signal GND15
signal GND16
signal CCLK_P72
signal DONE_P71
signal HSWAP_EN_P142
signal M0_P38
signal M1_P37
signal M2_P39
signal PROG_B
signal TCK
signal TDI
signal TDO
signal TMS
signal VCCAUX1
signal VCCAUX2
signal VCCAUX3
signal VCCAUX4
signal VCCINT1
signal VCCINT2
signal VCCINT3
signal VCCINT4
signal VCCO011
signal VCCO012
signal VCCO013
signal VCCO231
signal VCCO232
signal VCCO233
signal VCCO451
signal VCCO452
signal VCCO453
signal VCCO671
signal VCCO672
signal VCCO673
signal IO_P1
signal IO_P2
signal IO_P4
signal IO_P5
signal IO_P6
signal IO_P7
signal IO_P8
signal IO_P10
signal IO_P11
signal IO_P12
signal IO_P13
signal IO_P14
signal IO_P15
signal IO_P17
signal IO_P18
signal IO_P20
signal IO_P21
signal IO_P23
signal IO_P24
signal IO_P25
signal IO_P26
signal IO_P27
signal IO_P28
signal IO_P30
signal IO_P31
signal IO_P32
signal IO_P33
signal IO_P35
signal IO_P36
signal IO_P40
signal IO_P41
signal IO_P44
signal IO_P46
signal IO_P47
signal IO_P50
signal IO_P51
signal IO_P52
signal IO_P53
signal IO_P55
signal IO_P56
signal IO_P57
signal IO_P58
signal IO_P59
signal IO_P60
signal IO_P63
signal IO_P65
signal IO_P68
signal IO_P69
signal IO_P70
signal IO_P73
signal IO_P74
signal IO_P76
signal IO_P77
signal IO_P78
signal IO_P79
signal IO_P80
signal IO_P82
signal IO_P83
signal IO_P84
signal IO_P85
signal IO_P86
signal IO_P87
signal IO_P89
signal IO_P90
signal IO_P92
signal IO_P93
signal IO_P95
signal IO_P96
signal IO_P97
signal IO_P98
signal IO_P99
signal IO_P100
signal IO_P102
signal IO_P103
signal IO_P104
signal IO_P105
signal IO_P107
signal IO_P108
signal IO_P112
signal IO_P113
signal IO_P116
signal IO_P118
signal IO_P119
signal IO_P122
signal IO_P123
signal IO_P124
signal IO_P125
signal IO_P127
signal IO_P128
signal IO_P129
signal IO_P130
signal IO_P131
signal IO_P132
signal IO_P135
signal IO_P137
signal IO_P140

register	BSR	599
register	BR	1
register	DIR	32

instruction length 6

instruction EXTEST 000000 BSR
instruction SAMPLE/PRELOAD 000001 BSR
instruction IDCODE 001001 DIR
instruction BYPASS 111111 BR

bit 598 I 1 IO_P108
bit 597 O 1 IO_P108 596 1 Z
bit 596 C 1 *
bit 595 I 1 IO_P107
bit 594 O 1 IO_P107 593 1 Z
bit 593 C 1 *
bit 592 O 1 *
bit 591 O 1 *
bit 590 O 1 *
bit 589 O 1 *
bit 588 O 1 *
bit 587 O 1 *
bit 586 O 1 *
bit 585 O 1 *
bit 584 O 1 *
bit 583 O 1 *
bit 582 O 1 *
bit 581 O 1 *
bit 580 O 1 *
bit 579 O 1 *
bit 578 O 1 *
bit 577 O 1 *
bit 576 O 1 *
bit 575 O 1 *
bit 574 I 1 IO_P105
bit 573 O 1 IO_P105 572 1 Z
bit 572 C 1 *
bit 571 I 1 IO_P104
bit 570 O 1 IO_P104 569 1 Z
bit 569 C 1 *
bit 568 I 1 IO_P103
bit 567 O 1 IO_P103 566 1 Z
bit 566 C 1 *
bit 565 I 1 IO_P102
bit 564 O 1 IO_P102 563 1 Z
bit 563 C 1 *
bit 562 I 1 IO_P100
bit 561 O 1 IO_P100 560 1 Z
bit 560 C 1 *
bit 559 I 1 IO_P99
bit 558 O 1 IO_P99 557 1 Z
bit 557 C 1 *
bit 556 I 1 IO_P98
bit 555 O 1 IO_P98 554 1 Z
bit 554 C 1 *
bit 553 I 1 IO_P97
bit 552 O 1 IO_P97 551 1 Z
bit 551 C 1 *
bit 550 I 1 IO_P96
bit 549 O 1 IO_P96 548 1 Z
bit 548 C 1 *
bit 547 I 1 IO_P95
bit 546 O 1 IO_P95 545 1 Z
bit 545 C 1 *
bit 544 O 1 *
bit 543 O 1 *
bit 542 O 1 *
bit 541 O 1 *
bit 540 O 1 *
bit 539 O 1 *
bit 538 O 1 *
bit 537 O 1 *
bit 536 O 1 *
bit 535 O 1 *
bit 534 O 1 *
bit 533 O 1 *
bit 532 I 1 IO_P93
bit 531 O 1 IO_P93 530 1 Z
bit 530 C 1 *
bit 529 I 1 IO_P92
bit 528 O 1 IO_P92 527 1 Z
bit 527 C 1 *
bit 526 I 1 IO_P90
bit 525 O 1 IO_P90 524 1 Z
bit 524 C 1 *
bit 523 I 1 IO_P89
bit 522 O 1 IO_P89 521 1 Z
bit 521 C 1 *
bit 520 O 1 *
bit 519 O 1 *
bit 518 O 1 *
bit 517 O 1 *
bit 516 O 1 *
bit 515 O 1 *
bit 514 O 1 *
bit 513 O 1 *
bit 512 O 1 *
bit 511 O 1 *
bit 510 O 1 *
bit 509 O 1 *
bit 508 I 1 IO_P87
bit 507 O 1 IO_P87 506 1 Z
bit 506 C 1 *
bit 505 I 1 IO_P86
bit 504 O 1 IO_P86 503 1 Z
bit 503 C 1 *
bit 502 I 1 IO_P85
bit 501 O 1 IO_P85 500 1 Z
bit 500 C 1 *
bit 499 I 1 IO_P84
bit 498 O 1 IO_P84 497 1 Z
bit 497 C 1 *
bit 496 I 1 IO_P83
bit 495 O 1 IO_P83 494 1 Z
bit 494 C 1 *
bit 493 I 1 IO_P82
bit 492 O 1 IO_P82 491 1 Z
bit 491 C 1 *
bit 490 I 1 IO_P80
bit 489 O 1 IO_P80 488 1 Z
bit 488 C 1 *
bit 487 I 1 IO_P79
bit 486 O 1 IO_P79 485 1 Z
bit 485 C 1 *
bit 484 I 1 IO_P78
bit 483 O 1 IO_P78 482 1 Z
bit 482 C 1 *
bit 481 I 1 IO_P77
bit 480 O 1 IO_P77 479 1 Z
bit 479 C 1 *
bit 478 I 1 IO_P76
bit 477 O 1 IO_P76 476 1 Z
bit 476 C 1 *
bit 475 O 1 *
bit 474 O 1 *
bit 473 O 1 *
bit 472 O 1 *
bit 471 O 1 *
bit 470 O 1 *
bit 469 O 1 *
bit 468 O 1 *
bit 467 O 1 *
bit 466 O 1 *
bit 465 O 1 *
bit 464 O 1 *
bit 463 O 1 *
bit 462 O 1 *
bit 461 O 1 *
bit 460 I 1 IO_P74
bit 459 O 1 IO_P74 458 1 Z
bit 458 C 1 *
bit 457 I 1 IO_P73
bit 456 O 1 IO_P73 455 1 Z
bit 455 C 1 *
bit 454 I 1 CCLK_P72
bit 453 O 1 CCLK_P72 452 1 Z
bit 452 C 1 *
bit 451 I 1 DONE_P71
bit 450 O 1 DONE_P71 449 1 Z
bit 449 C 1 *
bit 448 I 1 IO_P70
bit 447 O 1 IO_P70 446 1 Z
bit 446 C 1 *
bit 445 I 1 IO_P69
bit 444 O 1 IO_P69 443 1 Z
bit 443 C 1 *
bit 442 I 1 IO_P68
bit 441 O 1 IO_P68 440 1 Z
bit 440 C 1 *
bit 439 O 1 *
bit 438 O 1 *
bit 437 O 1 *
bit 436 O 1 *
bit 435 O 1 *
bit 434 O 1 *
bit 433 O 1 *
bit 432 O 1 *
bit 431 O 1 *
bit 430 O 1 *
bit 429 O 1 *
bit 428 O 1 *
bit 427 O 1 *
bit 426 O 1 *
bit 425 O 1 *
bit 424 O 1 *
bit 423 O 1 *
bit 422 O 1 *
bit 421 O 1 *
bit 420 O 1 *
bit 419 O 1 *
bit 418 O 1 *
bit 417 O 1 *
bit 416 O 1 *
bit 415 I 1 IO_P65
bit 414 O 1 IO_P65 413 1 Z
bit 413 C 1 *
bit 412 I 1 IO_P63
bit 411 O 1 IO_P63 410 1 Z
bit 410 C 1 *
bit 409 O 1 *
bit 408 O 1 *
bit 407 O 1 *
bit 406 O 1 *
bit 405 O 1 *
bit 404 O 1 *
bit 403 O 1 *
bit 402 O 1 *
bit 401 O 1 *
bit 400 O 1 *
bit 399 O 1 *
bit 398 O 1 *
bit 397 O 1 *
bit 396 O 1 *
bit 395 O 1 *
bit 394 I 1 IO_P60
bit 393 O 1 IO_P60 392 1 Z
bit 392 C 1 *
bit 391 I 1 IO_P59
bit 390 O 1 IO_P59 389 1 Z
bit 389 C 1 *
bit 388 O 1 *
bit 387 O 1 *
bit 386 O 1 *
bit 385 I 1 IO_P58
bit 384 O 1 IO_P58 383 1 Z
bit 383 C 1 *
bit 382 I 1 IO_P57
bit 381 O 1 IO_P57 380 1 Z
bit 380 C 1 *
bit 379 I 1 IO_P56
bit 378 O 1 IO_P56 377 1 Z
bit 377 C 1 *
bit 376 I 1 IO_P55
bit 375 O 1 IO_P55 374 1 Z
bit 374 C 1 *
bit 373 O 1 *
bit 372 O 1 *
bit 371 O 1 *
bit 370 I 1 IO_P53
bit 369 O 1 IO_P53 368 1 Z
bit 368 C 1 *
bit 367 I 1 IO_P52
bit 366 O 1 IO_P52 365 1 Z
bit 365 C 1 *
bit 364 I 1 IO_P51
bit 363 O 1 IO_P51 362 1 Z
bit 362 C 1 *
bit 361 I 1 IO_P50
bit 360 O 1 IO_P50 359 1 Z
bit 359 C 1 *
bit 358 O 1 *
bit 357 O 1 *
bit 356 O 1 *
bit 355 O 1 *
bit 354 O 1 *
bit 353 O 1 *
bit 352 O 1 *
bit 351 O 1 *
bit 350 O 1 *
bit 349 O 1 *
bit 348 O 1 *
bit 347 O 1 *
bit 346 O 1 *
bit 345 O 1 *
bit 344 O 1 *
bit 343 O 1 *
bit 342 O 1 *
bit 341 O 1 *
bit 340 I 1 IO_P47
bit 339 O 1 IO_P47 338 1 Z
bit 338 C 1 *
bit 337 I 1 IO_P46
bit 336 O 1 IO_P46 335 1 Z
bit 335 C 1 *
bit 334 I 1 IO_P44
bit 333 O 1 IO_P44 332 1 Z
bit 332 C 1 *
bit 331 O 1 *
bit 330 O 1 *
bit 329 O 1 *
bit 328 O 1 *
bit 327 O 1 *
bit 326 O 1 *
bit 325 O 1 *
bit 324 O 1 *
bit 323 O 1 *
bit 322 O 1 *
bit 321 O 1 *
bit 320 O 1 *
bit 319 O 1 *
bit 318 O 1 *
bit 317 O 1 *
bit 316 O 1 *
bit 315 O 1 *
bit 314 O 1 *
bit 313 O 1 *
bit 312 O 1 *
bit 311 O 1 *
bit 310 O 1 *
bit 309 O 1 *
bit 308 O 1 *
bit 307 O 1 *
bit 306 O 1 *
bit 305 O 1 *
bit 304 I 1 IO_P41
bit 303 O 1 IO_P41 302 1 Z
bit 302 C 1 *
bit 301 I 1 IO_P40
bit 300 O 1 IO_P40 299 1 Z
bit 299 C 1 *
bit 298 I 1 M2_P39
bit 297 I 1 M0_P38
bit 296 I 1 M1_P37
bit 295 I 1 IO_P36
bit 294 O 1 IO_P36 293 1 Z
bit 293 C 1 *
bit 292 I 1 IO_P35
bit 291 O 1 IO_P35 290 1 Z
bit 290 C 1 *
bit 289 O 1 *
bit 288 O 1 *
bit 287 O 1 *
bit 286 O 1 *
bit 285 O 1 *
bit 284 O 1 *
bit 283 O 1 *
bit 282 O 1 *
bit 281 O 1 *
bit 280 O 1 *
bit 279 O 1 *
bit 278 O 1 *
bit 277 O 1 *
bit 276 O 1 *
bit 275 O 1 *
bit 274 O 1 *
bit 273 O 1 *
bit 272 O 1 *
bit 271 I 1 IO_P33
bit 270 O 1 IO_P33 269 1 Z
bit 269 C 1 *
bit 268 I 1 IO_P32
bit 267 O 1 IO_P32 266 1 Z
bit 266 C 1 *
bit 265 I 1 IO_P31
bit 264 O 1 IO_P31 263 1 Z
bit 263 C 1 *
bit 262 I 1 IO_P30
bit 261 O 1 IO_P30 260 1 Z
bit 260 C 1 *
bit 259 I 1 IO_P28
bit 258 O 1 IO_P28 257 1 Z
bit 257 C 1 *
bit 256 I 1 IO_P27
bit 255 O 1 IO_P27 254 1 Z
bit 254 C 1 *
bit 253 I 1 IO_P26
bit 252 O 1 IO_P26 251 1 Z
bit 251 C 1 *
bit 250 I 1 IO_P25
bit 249 O 1 IO_P25 248 1 Z
bit 248 C 1 *
bit 247 I 1 IO_P24
bit 246 O 1 IO_P24 245 1 Z
bit 245 C 1 *
bit 244 I 1 IO_P23
bit 243 O 1 IO_P23 242 1 Z
bit 242 C 1 *
bit 241 O 1 *
bit 240 O 1 *
bit 239 O 1 *
bit 238 O 1 *
bit 237 O 1 *
bit 236 O 1 *
bit 235 O 1 *
bit 234 O 1 *
bit 233 O 1 *
bit 232 O 1 *
bit 231 O 1 *
bit 230 O 1 *
bit 229 I 1 IO_P21
bit 228 O 1 IO_P21 227 1 Z
bit 227 C 1 *
bit 226 I 1 IO_P20
bit 225 O 1 IO_P20 224 1 Z
bit 224 C 1 *
bit 223 I 1 IO_P18
bit 222 O 1 IO_P18 221 1 Z
bit 221 C 1 *
bit 220 I 1 IO_P17
bit 219 O 1 IO_P17 218 1 Z
bit 218 C 1 *
bit 217 O 1 *
bit 216 O 1 *
bit 215 O 1 *
bit 214 O 1 *
bit 213 O 1 *
bit 212 O 1 *
bit 211 O 1 *
bit 210 O 1 *
bit 209 O 1 *
bit 208 O 1 *
bit 207 O 1 *
bit 206 O 1 *
bit 205 I 1 IO_P15
bit 204 O 1 IO_P15 203 1 Z
bit 203 C 1 *
bit 202 I 1 IO_P14
bit 201 O 1 IO_P14 200 1 Z
bit 200 C 1 *
bit 199 I 1 IO_P13
bit 198 O 1 IO_P13 197 1 Z
bit 197 C 1 *
bit 196 I 1 IO_P12
bit 195 O 1 IO_P12 194 1 Z
bit 194 C 1 *
bit 193 I 1 IO_P11
bit 192 O 1 IO_P11 191 1 Z
bit 191 C 1 *
bit 190 I 1 IO_P10
bit 189 O 1 IO_P10 188 1 Z
bit 188 C 1 *
bit 187 I 1 IO_P8
bit 186 O 1 IO_P8 185 1 Z
bit 185 C 1 *
bit 184 I 1 IO_P7
bit 183 O 1 IO_P7 182 1 Z
bit 182 C 1 *
bit 181 I 1 IO_P6
bit 180 O 1 IO_P6 179 1 Z
bit 179 C 1 *
bit 178 I 1 IO_P5
bit 177 O 1 IO_P5 176 1 Z
bit 176 C 1 *
bit 175 I 1 IO_P4
bit 174 O 1 IO_P4 173 1 Z
bit 173 C 1 *
bit 172 O 1 *
bit 171 O 1 *
bit 170 O 1 *
bit 169 O 1 *
bit 168 O 1 *
bit 167 O 1 *
bit 166 O 1 *
bit 165 O 1 *
bit 164 O 1 *
bit 163 O 1 *
bit 162 O 1 *
bit 161 O 1 *
bit 160 O 1 *
bit 159 O 1 *
bit 158 O 1 *
bit 157 I 1 IO_P2
bit 156 O 1 IO_P2 155 1 Z
bit 155 C 1 *
bit 154 I 1 IO_P1
bit 153 O 1 IO_P1 152 1 Z
bit 152 C 1 *
bit 151 O 1 *
bit 150 I 1 HSWAP_EN_P142
bit 149 O 1 *
bit 148 O 1 *
bit 147 O 1 *
bit 146 I 1 IO_P141
bit 145 O 1 IO_P141 144 1 Z
bit 144 C 1 *
bit 143 I 1 IO_P140
bit 142 O 1 IO_P140 141 1 Z
bit 141 C 1 *
bit 140 O 1 *
bit 139 O 1 *
bit 138 O 1 *
bit 137 O 1 *
bit 136 O 1 *
bit 135 O 1 *
bit 134 O 1 *
bit 133 O 1 *
bit 132 O 1 *
bit 131 O 1 *
bit 130 O 1 *
bit 129 O 1 *
bit 128 O 1 *
bit 127 O 1 *
bit 126 O 1 *
bit 125 O 1 *
bit 124 O 1 *
bit 123 O 1 *
bit 122 O 1 *
bit 121 O 1 *
bit 120 O 1 *
bit 119 O 1 *
bit 118 O 1 *
bit 117 O 1 *
bit 116 I 1 IO_P137
bit 115 O 1 IO_P137 114 1 Z
bit 114 C 1 *
bit 113 I 1 IO_P135
bit 112 O 1 IO_P135 111 1 Z
bit 111 C 1 *
bit 110 O 1 *
bit 109 O 1 *
bit 108 O 1 *
bit 107 O 1 *
bit 106 O 1 *
bit 105 O 1 *
bit 104 O 1 *
bit 103 O 1 *
bit 102 O 1 *
bit 101 O 1 *
bit 100 O 1 *
bit 99 O 1 *
bit 98 O 1 *
bit 97 O 1 *
bit 96 O 1 *
bit 95 I 1 IO_P132
bit 94 O 1 IO_P132 93 1 Z
bit 93 C 1 *
bit 92 I 1 IO_P131
bit 91 O 1 IO_P131 90 1 Z
bit 90 C 1 *
bit 89 O 1 *
bit 88 O 1 *
bit 87 O 1 *
bit 86 I 1 IO_P130
bit 85 O 1 IO_P130 84 1 Z
bit 84 C 1 *
bit 83 I 1 IO_P129
bit 82 O 1 IO_P129 81 1 Z
bit 81 C 1 *
bit 80 I 1 IO_P128
bit 79 O 1 IO_P128 78 1 Z
bit 78 C 1 *
bit 77 I 1 IO_P127
bit 76 O 1 IO_P127 75 1 Z
bit 75 C 1 *
bit 74 O 1 *
bit 73 O 1 *
bit 72 O 1 *
bit 71 I 1 IO_P125
bit 70 O 1 IO_P125 69 1 Z
bit 69 C 1 *
bit 68 I 1 IO_P124
bit 67 O 1 IO_P124 66 1 Z
bit 66 C 1 *
bit 65 I 1 IO_P123
bit 64 O 1 IO_P123 63 1 Z
bit 63 C 1 *
bit 62 I 1 IO_P122
bit 61 O 1 IO_P122 60 1 Z
bit 60 C 1 *
bit 59 O 1 *
bit 58 O 1 *
bit 57 O 1 *
bit 56 O 1 *
bit 55 O 1 *
bit 54 O 1 *
bit 53 O 1 *
bit 52 O 1 *
bit 51 O 1 *
bit 50 O 1 *
bit 49 O 1 *
bit 48 O 1 *
bit 47 O 1 *
bit 46 O 1 *
bit 45 O 1 *
bit 44 O 1 *
bit 43 O 1 *
bit 42 O 1 *
bit 41 I 1 IO_P119
bit 40 O 1 IO_P119 39 1 Z
bit 39 C 1 *
bit 38 I 1 IO_P118
bit 37 O 1 IO_P118 36 1 Z
bit 36 C 1 *
bit 35 I 1 IO_P116
bit 34 O 1 IO_P116 33 1 Z
bit 33 C 1 *
bit 32 O 1 *
bit 31 O 1 *
bit 30 O 1 *
bit 29 O 1 *
bit 28 O 1 *
bit 27 O 1 *
bit 26 O 1 *
bit 25 O 1 *
bit 24 O 1 *
bit 23 O 1 *
bit 22 O 1 *
bit 21 O 1 *
bit 20 O 1 *
bit 19 O 1 *
bit 18 O 1 *
bit 17 O 1 *
bit 16 O 1 *
bit 15 O 1 *
bit 14 O 1 *
bit 13 O 1 *
bit 12 O 1 *
bit 11 O 1 *
bit 10 O 1 *
bit 9 O 1 *
bit 8 O 1 *
bit 7 O 1 *
bit 6 O 1 *
bit 5 I 1 IO_P113
bit 4 O 1 IO_P113 3 1 Z
bit 3 C 1 *
bit 2 I 1 IO_P112
bit 1 O 1 IO_P112 0 1 Z
bit 0 C 1 *
