signal GND1
signal GND2
signal GND3
signal GND4
signal GND5
signal GND6
signal GND7
signal GND8
signal GND9
signal GND10
signal GND11
signal GND12
signal GND13
signal GND14
signal GND15
signal GND16
signal GND17
signal GND18
signal GND19
signal GND20
signal GND21
signal GND22
signal GND23
signal GND24
signal GND25
signal GND26
signal GND27
signal GND28
signal GND29
signal GND30
signal GND31
signal GND32
signal GND33
signal GND34
signal GND35
signal GND36
signal GND37
signal GND38
signal GND39
signal GND40
signal GND41
signal GND42
signal GND43
signal GND44
signal GND45
signal GND46
signal GND47
signal GND48
signal GND49
signal GND50
signal GND51
signal GND52
signal CCLK_AA22
signal DONE_AB21
signal HSWAP_EN_B3
signal M0_AB2
signal M1_AA1
signal M2_AB3
signal PROG_B
signal TCK
signal TDI
signal TDO
signal TMS
signal VCCAUX1
signal VCCAUX2
signal VCCAUX3
signal VCCAUX4
signal VCCAUX5
signal VCCAUX6
signal VCCAUX7
signal VCCAUX8
signal VCCINT1
signal VCCINT2
signal VCCINT3
signal VCCINT4
signal VCCINT5
signal VCCINT6
signal VCCINT7
signal VCCINT8
signal VCCINT9
signal VCCINT10
signal VCCINT11
signal VCCINT12
signal VCCO01
signal VCCO02
signal VCCO03
signal VCCO04
signal VCCO05
signal VCCO11
signal VCCO12
signal VCCO13
signal VCCO14
signal VCCO15
signal VCCO21
signal VCCO22
signal VCCO23
signal VCCO24
signal VCCO25
signal VCCO31
signal VCCO32
signal VCCO33
signal VCCO34
signal VCCO35
signal VCCO41
signal VCCO42
signal VCCO43
signal VCCO44
signal VCCO45
signal VCCO51
signal VCCO52
signal VCCO53
signal VCCO54
signal VCCO55
signal VCCO61
signal VCCO62
signal VCCO63
signal VCCO64
signal VCCO65
signal VCCO71
signal VCCO72
signal VCCO73
signal VCCO74
signal VCCO75
signal IO_A3
signal IO_A4
signal IO_A5
signal IO_A8
signal IO_A9
signal IO_A10
signal IO_A11
signal IO_A12
signal IO_A13
signal IO_A14
signal IO_A15
signal IO_A18
signal IO_A19
signal IO_B4
signal IO_B5
signal IO_B6
signal IO_B8
signal IO_B9
signal IO_B10
signal IO_B11
signal IO_B12
signal IO_B13
signal IO_B14
signal IO_B15
signal IO_B17
signal IO_B18
signal IO_B19
signal IO_B20
signal IO_C1
signal IO_C2
signal IO_C3
signal IO_C4
signal IO_C5
signal IO_C6
signal IO_C7
signal IO_C10
signal IO_C11
signal IO_C12
signal IO_C13
signal IO_C17
signal IO_C18
signal IO_C19
signal IO_C20
signal IO_C21
signal IO_C22
signal IO_D1
signal IO_D2
signal IO_D3
signal IO_D4
signal IO_D5
signal IO_D6
signal IO_D7
signal IO_D9
signal IO_D10
signal IO_D11
signal IO_D12
signal IO_D13
signal IO_D14
signal IO_D15
signal IO_D17
signal IO_D18
signal IO_D19
signal IO_D20
signal IO_D21
signal IO_D22
signal IO_E1
signal IO_E2
signal IO_E3
signal IO_E4
signal IO_E6
signal IO_E7
signal IO_E9
signal IO_E10
signal IO_E11
signal IO_E12
signal IO_E13
signal IO_E14
signal IO_E15
signal IO_E16
signal IO_E17
signal IO_E18
signal IO_E19
signal IO_E20
signal IO_E21
signal IO_E22
signal IO_F2
signal IO_F3
signal IO_F4
signal IO_F5
signal IO_F6
signal IO_F7
signal IO_F9
signal IO_F10
signal IO_F11
signal IO_F12
signal IO_F13
signal IO_F16
signal IO_F17
signal IO_F18
signal IO_F19
signal IO_F20
signal IO_F21
signal IO_G1
signal IO_G2
signal IO_G5
signal IO_G6
signal IO_G17
signal IO_G18
signal IO_G19
signal IO_G21
signal IO_G22
signal IO_H5
signal IO_K1
signal IO_K2
signal IO_K3
signal IO_K4
signal IO_K19
signal IO_K20
signal IO_K21
signal IO_K22
signal IO_L1
signal IO_L2
signal IO_L3
signal IO_L4
signal IO_L5
signal IO_L6
signal IO_L17
signal IO_L18
signal IO_L19
signal IO_L20
signal IO_L21
signal IO_L22
signal IO_M1
signal IO_M2
signal IO_M3
signal IO_M4
signal IO_M5
signal IO_M6
signal IO_M17
signal IO_M18
signal IO_M19
signal IO_M20
signal IO_M21
signal IO_M22
signal IO_N1
signal IO_N2
signal IO_N3
signal IO_N4
signal IO_N19
signal IO_N20
signal IO_N21
signal IO_N22
signal IO_R18
signal IO_T1
signal IO_T2
signal IO_T4
signal IO_T5
signal IO_T6
signal IO_T17
signal IO_T18
signal IO_T21
signal IO_T22
signal IO_U2
signal IO_U3
signal IO_U4
signal IO_U5
signal IO_U6
signal IO_U7
signal IO_U10
signal IO_U11
signal IO_U12
signal IO_U13
signal IO_U14
signal IO_U16
signal IO_U17
signal IO_U18
signal IO_U19
signal IO_U20
signal IO_U21
signal IO_V1
signal IO_V2
signal IO_V3
signal IO_V4
signal IO_V5
signal IO_V6
signal IO_V7
signal IO_V8
signal IO_V9
signal IO_V10
signal IO_V11
signal IO_V12
signal IO_V13
signal IO_V14
signal IO_V16
signal IO_V17
signal IO_V18
signal IO_V19
signal IO_V20
signal IO_V21
signal IO_V22
signal IO_W1
signal IO_W2
signal IO_W3
signal IO_W4
signal IO_W5
signal IO_W6
signal IO_W8
signal IO_W9
signal IO_W10
signal IO_W11
signal IO_W12
signal IO_W13
signal IO_W14
signal IO_W16
signal IO_W17
signal IO_W18
signal IO_W19
signal IO_W20
signal IO_W21
signal IO_W22
signal IO_Y1
signal IO_Y2
signal IO_Y3
signal IO_Y4
signal IO_Y5
signal IO_Y6
signal IO_Y10
signal IO_Y11
signal IO_Y12
signal IO_Y13
signal IO_Y16
signal IO_Y17
signal IO_Y18
signal IO_Y19
signal IO_Y20
signal IO_Y21
signal IO_Y22
signal IO_AA3
signal IO_AA4
signal IO_AA5
signal IO_AA6
signal IO_AA8
signal IO_AA9
signal IO_AA10
signal IO_AA11
signal IO_AA12
signal IO_AA13
signal IO_AA14
signal IO_AA15
signal IO_AA17
signal IO_AA18
signal IO_AA20
signal IO_AB4
signal IO_AB5
signal IO_AB8
signal IO_AB9
signal IO_AB10
signal IO_AB11
signal IO_AB12
signal IO_AB13
signal IO_AB14
signal IO_AB15
signal IO_AB18

register	BSR	815
register	BR	1
register	DIR	32

instruction length 6

instruction EXTEST 000000 BSR
instruction SAMPLE/PRELOAD 000001 BSR
instruction IDCODE 001001 DIR
instruction BYPASS 111111 BR

bit 814 I 1 IO_C20
bit 813 O 1 IO_C20 812 1 Z
bit 812 C 1 *
bit 811 I 1 IO_C21
bit 810 O 1 IO_C21 809 1 Z
bit 809 C 1 *
bit 808 O 1 *
bit 807 O 1 *
bit 806 O 1 *
bit 805 I 1 IO_C22
bit 804 O 1 IO_C22 803 1 Z
bit 803 C 1 *
bit 802 I 1 IO_D20
bit 801 O 1 IO_D20 800 1 Z
bit 800 C 1 *
bit 799 I 1 IO_D19
bit 798 O 1 IO_D19 797 1 Z
bit 797 C 1 *
bit 796 I 1 IO_D21
bit 795 O 1 IO_D21 794 1 Z
bit 794 C 1 *
bit 793 I 1 IO_D22
bit 792 O 1 IO_D22 791 1 Z
bit 791 C 1 *
bit 790 I 1 IO_E18
bit 789 O 1 IO_E18 788 1 Z
bit 788 C 1 *
bit 787 I 1 IO_F18
bit 786 O 1 IO_F18 785 1 Z
bit 785 C 1 *
bit 784 I 1 IO_E19
bit 783 O 1 IO_E19 782 1 Z
bit 782 C 1 *
bit 781 I 1 IO_E20
bit 780 O 1 IO_E20 779 1 Z
bit 779 C 1 *
bit 778 I 1 IO_E21
bit 777 O 1 IO_E21 776 1 Z
bit 776 C 1 *
bit 775 I 1 IO_E22
bit 774 O 1 IO_E22 773 1 Z
bit 773 C 1 *
bit 772 I 1 IO_G17
bit 771 O 1 IO_G17 770 1 Z
bit 770 C 1 *
bit 769 I 1 IO_G18
bit 768 O 1 IO_G18 767 1 Z
bit 767 C 1 *
bit 766 I 1 IO_F19
bit 765 O 1 IO_F19 764 1 Z
bit 764 C 1 *
bit 763 I 1 IO_G19
bit 762 O 1 IO_G19 761 1 Z
bit 761 C 1 *
bit 760 I 1 IO_F20
bit 759 O 1 IO_F20 758 1 Z
bit 758 C 1 *
bit 757 I 1 IO_F21
bit 756 O 1 IO_F21 755 1 Z
bit 755 C 1 *
bit 754 I 1 IO_G21
bit 753 O 1 IO_G21 752 1 Z
bit 752 C 1 *
bit 751 I 1 IO_G22
bit 750 O 1 IO_G22 749 1 Z
bit 749 C 1 *
bit 748 I 1 IO_K19
bit 747 O 1 IO_K19 746 1 Z
bit 746 C 1 *
bit 745 I 1 IO_K20
bit 744 O 1 IO_K20 743 1 Z
bit 743 C 1 *
bit 742 I 1 IO_K21
bit 741 O 1 IO_K21 740 1 Z
bit 740 C 1 *
bit 739 I 1 IO_K22
bit 738 O 1 IO_K22 737 1 Z
bit 737 C 1 *
bit 736 I 1 IO_L17
bit 735 O 1 IO_L17 734 1 Z
bit 734 C 1 *
bit 733 I 1 IO_L18
bit 732 O 1 IO_L18 731 1 Z
bit 731 C 1 *
bit 730 I 1 IO_L19
bit 729 O 1 IO_L19 728 1 Z
bit 728 C 1 *
bit 727 I 1 IO_L20
bit 726 O 1 IO_L20 725 1 Z
bit 725 C 1 *
bit 724 I 1 IO_L21
bit 723 O 1 IO_L21 722 1 Z
bit 722 C 1 *
bit 721 I 1 IO_L22
bit 720 O 1 IO_L22 719 1 Z
bit 719 C 1 *
bit 718 I 1 IO_M22
bit 717 O 1 IO_M22 716 1 Z
bit 716 C 1 *
bit 715 I 1 IO_M21
bit 714 O 1 IO_M21 713 1 Z
bit 713 C 1 *
bit 712 I 1 IO_M20
bit 711 O 1 IO_M20 710 1 Z
bit 710 C 1 *
bit 709 I 1 IO_M19
bit 708 O 1 IO_M19 707 1 Z
bit 707 C 1 *
bit 706 I 1 IO_M18
bit 705 O 1 IO_M18 704 1 Z
bit 704 C 1 *
bit 703 I 1 IO_M17
bit 702 O 1 IO_M17 701 1 Z
bit 701 C 1 *
bit 700 I 1 IO_N22
bit 699 O 1 IO_N22 698 1 Z
bit 698 C 1 *
bit 697 I 1 IO_N21
bit 696 O 1 IO_N21 695 1 Z
bit 695 C 1 *
bit 694 I 1 IO_N20
bit 693 O 1 IO_N20 692 1 Z
bit 692 C 1 *
bit 691 I 1 IO_N19
bit 690 O 1 IO_N19 689 1 Z
bit 689 C 1 *
bit 688 I 1 IO_T22
bit 687 O 1 IO_T22 686 1 Z
bit 686 C 1 *
bit 685 I 1 IO_T21
bit 684 O 1 IO_T21 683 1 Z
bit 683 C 1 *
bit 682 I 1 IO_R18
bit 681 O 1 IO_R18 680 1 Z
bit 680 C 1 *
bit 679 I 1 IO_T18
bit 678 O 1 IO_T18 677 1 Z
bit 677 C 1 *
bit 676 I 1 IO_U21
bit 675 O 1 IO_U21 674 1 Z
bit 674 C 1 *
bit 673 I 1 IO_U20
bit 672 O 1 IO_U20 671 1 Z
bit 671 C 1 *
bit 670 I 1 IO_T17
bit 669 O 1 IO_T17 668 1 Z
bit 668 C 1 *
bit 667 I 1 IO_U18
bit 666 O 1 IO_U18 665 1 Z
bit 665 C 1 *
bit 664 I 1 IO_V22
bit 663 O 1 IO_V22 662 1 Z
bit 662 C 1 *
bit 661 I 1 IO_V21
bit 660 O 1 IO_V21 659 1 Z
bit 659 C 1 *
bit 658 I 1 IO_U19
bit 657 O 1 IO_U19 656 1 Z
bit 656 C 1 *
bit 655 I 1 IO_V20
bit 654 O 1 IO_V20 653 1 Z
bit 653 C 1 *
bit 652 I 1 IO_W21
bit 651 O 1 IO_W21 650 1 Z
bit 650 C 1 *
bit 649 I 1 IO_W20
bit 648 O 1 IO_W20 647 1 Z
bit 647 C 1 *
bit 646 I 1 IO_V19
bit 645 O 1 IO_V19 644 1 Z
bit 644 C 1 *
bit 643 I 1 IO_W19
bit 642 O 1 IO_W19 641 1 Z
bit 641 C 1 *
bit 640 I 1 IO_W22
bit 639 O 1 IO_W22 638 1 Z
bit 638 C 1 *
bit 637 I 1 IO_Y22
bit 636 O 1 IO_Y22 635 1 Z
bit 635 C 1 *
bit 634 I 1 IO_Y21
bit 633 O 1 IO_Y21 632 1 Z
bit 632 C 1 *
bit 631 O 1 *
bit 630 O 1 *
bit 629 O 1 *
bit 628 I 1 IO_Y20
bit 627 O 1 IO_Y20 626 1 Z
bit 626 C 1 *
bit 625 I 1 IO_Y19
bit 624 O 1 IO_Y19 623 1 Z
bit 623 C 1 *
bit 622 I 1 CCLK_AA22
bit 621 O 1 CCLK_AA22 620 1 Z
bit 620 C 1 *
bit 619 I 1 DONE_AB21
bit 618 O 1 DONE_AB21 617 1 Z
bit 617 C 1 *
bit 616 I 1 IO_V18
bit 615 O 1 IO_V18 614 1 Z
bit 614 C 1 *
bit 613 I 1 IO_AA20
bit 612 O 1 IO_AA20 611 1 Z
bit 611 C 1 *
bit 610 I 1 IO_AB20
bit 609 O 1 IO_AB20 608 1 Z
bit 608 C 1 *
bit 607 I 1 IO_W18
bit 606 O 1 IO_W18 605 1 Z
bit 605 C 1 *
bit 604 I 1 IO_Y18
bit 603 O 1 IO_Y18 602 1 Z
bit 602 C 1 *
bit 601 I 1 IO_U17
bit 600 O 1 IO_U17 599 1 Z
bit 599 C 1 *
bit 598 I 1 IO_AA18
bit 597 O 1 IO_AA18 596 1 Z
bit 596 C 1 *
bit 595 I 1 IO_AB18
bit 594 O 1 IO_AB18 593 1 Z
bit 593 C 1 *
bit 592 I 1 IO_V17
bit 591 O 1 IO_V17 590 1 Z
bit 590 C 1 *
bit 589 I 1 IO_W17
bit 588 O 1 IO_W17 587 1 Z
bit 587 C 1 *
bit 586 I 1 IO_U16
bit 585 O 1 IO_U16 584 1 Z
bit 584 C 1 *
bit 583 I 1 IO_Y17
bit 582 O 1 IO_Y17 581 1 Z
bit 581 C 1 *
bit 580 I 1 IO_AA17
bit 579 O 1 IO_AA17 578 1 Z
bit 578 C 1 *
bit 577 I 1 IO_V16
bit 576 O 1 IO_V16 575 1 Z
bit 575 C 1 *
bit 574 I 1 IO_W16
bit 573 O 1 IO_W16 572 1 Z
bit 572 C 1 *
bit 571 I 1 IO_Y16
bit 570 O 1 IO_Y16 569 1 Z
bit 569 C 1 *
bit 568 I 1 IO_AA15
bit 567 O 1 IO_AA15 566 1 Z
bit 566 C 1 *
bit 565 I 1 IO_AB15
bit 564 O 1 IO_AB15 563 1 Z
bit 563 C 1 *
bit 562 I 1 IO_U14
bit 561 O 1 IO_U14 560 1 Z
bit 560 C 1 *
bit 559 I 1 IO_V14
bit 558 O 1 IO_V14 557 1 Z
bit 557 C 1 *
bit 556 I 1 IO_W14
bit 555 O 1 IO_W14 554 1 Z
bit 554 C 1 *
bit 553 I 1 IO_AA14
bit 552 O 1 IO_AA14 551 1 Z
bit 551 C 1 *
bit 550 I 1 IO_AB14
bit 549 O 1 IO_AB14 548 1 Z
bit 548 C 1 *
bit 547 I 1 IO_U13
bit 546 O 1 IO_U13 545 1 Z
bit 545 C 1 *
bit 544 I 1 IO_V13
bit 543 O 1 IO_V13 542 1 Z
bit 542 C 1 *
bit 541 I 1 IO_W13
bit 540 O 1 IO_W13 539 1 Z
bit 539 C 1 *
bit 538 I 1 IO_Y13
bit 537 O 1 IO_Y13 536 1 Z
bit 536 C 1 *
bit 535 I 1 IO_AA13
bit 534 O 1 IO_AA13 533 1 Z
bit 533 C 1 *
bit 532 I 1 IO_U12
bit 531 O 1 IO_U12 530 1 Z
bit 530 C 1 *
bit 529 I 1 IO_V12
bit 528 O 1 IO_V12 527 1 Z
bit 527 C 1 *
bit 526 I 1 IO_AB13
bit 525 O 1 IO_AB13 524 1 Z
bit 524 C 1 *
bit 523 I 1 IO_W12
bit 522 O 1 IO_W12 521 1 Z
bit 521 C 1 *
bit 520 I 1 IO_Y12
bit 519 O 1 IO_Y12 518 1 Z
bit 518 C 1 *
bit 517 I 1 IO_AA12
bit 516 O 1 IO_AA12 515 1 Z
bit 515 C 1 *
bit 514 I 1 IO_AB12
bit 513 O 1 IO_AB12 512 1 Z
bit 512 C 1 *
bit 511 I 1 IO_AB11
bit 510 O 1 IO_AB11 509 1 Z
bit 509 C 1 *
bit 508 I 1 IO_AA11
bit 507 O 1 IO_AA11 506 1 Z
bit 506 C 1 *
bit 505 I 1 IO_Y11
bit 504 O 1 IO_Y11 503 1 Z
bit 503 C 1 *
bit 502 I 1 IO_W11
bit 501 O 1 IO_W11 500 1 Z
bit 500 C 1 *
bit 499 I 1 IO_V11
bit 498 O 1 IO_V11 497 1 Z
bit 497 C 1 *
bit 496 I 1 IO_U11
bit 495 O 1 IO_U11 494 1 Z
bit 494 C 1 *
bit 493 I 1 IO_AB10
bit 492 O 1 IO_AB10 491 1 Z
bit 491 C 1 *
bit 490 I 1 IO_AA10
bit 489 O 1 IO_AA10 488 1 Z
bit 488 C 1 *
bit 487 I 1 IO_Y10
bit 486 O 1 IO_Y10 485 1 Z
bit 485 C 1 *
bit 484 I 1 IO_W10
bit 483 O 1 IO_W10 482 1 Z
bit 482 C 1 *
bit 481 I 1 IO_V10
bit 480 O 1 IO_V10 479 1 Z
bit 479 C 1 *
bit 478 I 1 IO_AB9
bit 477 O 1 IO_AB9 476 1 Z
bit 476 C 1 *
bit 475 I 1 IO_AA9
bit 474 O 1 IO_AA9 473 1 Z
bit 473 C 1 *
bit 472 I 1 IO_W9
bit 471 O 1 IO_W9 470 1 Z
bit 470 C 1 *
bit 469 I 1 IO_V9
bit 468 O 1 IO_V9 467 1 Z
bit 467 C 1 *
bit 466 I 1 IO_U10
bit 465 O 1 IO_U10 464 1 Z
bit 464 C 1 *
bit 463 I 1 IO_AB8
bit 462 O 1 IO_AB8 461 1 Z
bit 461 C 1 *
bit 460 I 1 IO_AA8
bit 459 O 1 IO_AA8 458 1 Z
bit 458 C 1 *
bit 457 I 1 IO_W8
bit 456 O 1 IO_W8 455 1 Z
bit 455 C 1 *
bit 454 I 1 IO_V8
bit 453 O 1 IO_V8 452 1 Z
bit 452 C 1 *
bit 451 I 1 IO_V7
bit 450 O 1 IO_V7 449 1 Z
bit 449 C 1 *
bit 448 I 1 IO_AA6
bit 447 O 1 IO_AA6 446 1 Z
bit 446 C 1 *
bit 445 I 1 IO_Y6
bit 444 O 1 IO_Y6 443 1 Z
bit 443 C 1 *
bit 442 I 1 IO_W6
bit 441 O 1 IO_W6 440 1 Z
bit 440 C 1 *
bit 439 I 1 IO_V6
bit 438 O 1 IO_V6 437 1 Z
bit 437 C 1 *
bit 436 I 1 IO_U7
bit 435 O 1 IO_U7 434 1 Z
bit 434 C 1 *
bit 433 I 1 IO_AB5
bit 432 O 1 IO_AB5 431 1 Z
bit 431 C 1 *
bit 430 I 1 IO_AA5
bit 429 O 1 IO_AA5 428 1 Z
bit 428 C 1 *
bit 427 I 1 IO_Y5
bit 426 O 1 IO_Y5 425 1 Z
bit 425 C 1 *
bit 424 I 1 IO_W5
bit 423 O 1 IO_W5 422 1 Z
bit 422 C 1 *
bit 421 I 1 IO_U6
bit 420 O 1 IO_U6 419 1 Z
bit 419 C 1 *
bit 418 I 1 IO_AB4
bit 417 O 1 IO_AB4 416 1 Z
bit 416 C 1 *
bit 415 I 1 IO_AA4
bit 414 O 1 IO_AA4 413 1 Z
bit 413 C 1 *
bit 412 I 1 IO_Y4
bit 411 O 1 IO_Y4 410 1 Z
bit 410 C 1 *
bit 409 I 1 IO_AA3
bit 408 O 1 IO_AA3 407 1 Z
bit 407 C 1 *
bit 406 I 1 M2_AB3
bit 405 I 1 M0_AB2
bit 404 I 1 M1_AA1
bit 403 I 1 IO_Y3
bit 402 O 1 IO_Y3 401 1 Z
bit 401 C 1 *
bit 400 I 1 IO_Y2
bit 399 O 1 IO_Y2 398 1 Z
bit 398 C 1 *
bit 397 O 1 *
bit 396 O 1 *
bit 395 O 1 *
bit 394 I 1 IO_Y1
bit 393 O 1 IO_Y1 392 1 Z
bit 392 C 1 *
bit 391 I 1 IO_W4
bit 390 O 1 IO_W4 389 1 Z
bit 389 C 1 *
bit 388 I 1 IO_W3
bit 387 O 1 IO_W3 386 1 Z
bit 386 C 1 *
bit 385 I 1 IO_W2
bit 384 O 1 IO_W2 383 1 Z
bit 383 C 1 *
bit 382 I 1 IO_W1
bit 381 O 1 IO_W1 380 1 Z
bit 380 C 1 *
bit 379 I 1 IO_V5
bit 378 O 1 IO_V5 377 1 Z
bit 377 C 1 *
bit 376 I 1 IO_U5
bit 375 O 1 IO_U5 374 1 Z
bit 374 C 1 *
bit 373 I 1 IO_V4
bit 372 O 1 IO_V4 371 1 Z
bit 371 C 1 *
bit 370 I 1 IO_V3
bit 369 O 1 IO_V3 368 1 Z
bit 368 C 1 *
bit 367 I 1 IO_V2
bit 366 O 1 IO_V2 365 1 Z
bit 365 C 1 *
bit 364 I 1 IO_V1
bit 363 O 1 IO_V1 362 1 Z
bit 362 C 1 *
bit 361 I 1 IO_T6
bit 360 O 1 IO_T6 359 1 Z
bit 359 C 1 *
bit 358 I 1 IO_T5
bit 357 O 1 IO_T5 356 1 Z
bit 356 C 1 *
bit 355 I 1 IO_U4
bit 354 O 1 IO_U4 353 1 Z
bit 353 C 1 *
bit 352 I 1 IO_T4
bit 351 O 1 IO_T4 350 1 Z
bit 350 C 1 *
bit 349 I 1 IO_U3
bit 348 O 1 IO_U3 347 1 Z
bit 347 C 1 *
bit 346 I 1 IO_U2
bit 345 O 1 IO_U2 344 1 Z
bit 344 C 1 *
bit 343 I 1 IO_T2
bit 342 O 1 IO_T2 341 1 Z
bit 341 C 1 *
bit 340 I 1 IO_T1
bit 339 O 1 IO_T1 338 1 Z
bit 338 C 1 *
bit 337 I 1 IO_N4
bit 336 O 1 IO_N4 335 1 Z
bit 335 C 1 *
bit 334 I 1 IO_N3
bit 333 O 1 IO_N3 332 1 Z
bit 332 C 1 *
bit 331 I 1 IO_N2
bit 330 O 1 IO_N2 329 1 Z
bit 329 C 1 *
bit 328 I 1 IO_N1
bit 327 O 1 IO_N1 326 1 Z
bit 326 C 1 *
bit 325 I 1 IO_M6
bit 324 O 1 IO_M6 323 1 Z
bit 323 C 1 *
bit 322 I 1 IO_M5
bit 321 O 1 IO_M5 320 1 Z
bit 320 C 1 *
bit 319 I 1 IO_M4
bit 318 O 1 IO_M4 317 1 Z
bit 317 C 1 *
bit 316 I 1 IO_M3
bit 315 O 1 IO_M3 314 1 Z
bit 314 C 1 *
bit 313 I 1 IO_M2
bit 312 O 1 IO_M2 311 1 Z
bit 311 C 1 *
bit 310 I 1 IO_M1
bit 309 O 1 IO_M1 308 1 Z
bit 308 C 1 *
bit 307 I 1 IO_L1
bit 306 O 1 IO_L1 305 1 Z
bit 305 C 1 *
bit 304 I 1 IO_L2
bit 303 O 1 IO_L2 302 1 Z
bit 302 C 1 *
bit 301 I 1 IO_L3
bit 300 O 1 IO_L3 299 1 Z
bit 299 C 1 *
bit 298 I 1 IO_L4
bit 297 O 1 IO_L4 296 1 Z
bit 296 C 1 *
bit 295 I 1 IO_L5
bit 294 O 1 IO_L5 293 1 Z
bit 293 C 1 *
bit 292 I 1 IO_L6
bit 291 O 1 IO_L6 290 1 Z
bit 290 C 1 *
bit 289 I 1 IO_K1
bit 288 O 1 IO_K1 287 1 Z
bit 287 C 1 *
bit 286 I 1 IO_K2
bit 285 O 1 IO_K2 284 1 Z
bit 284 C 1 *
bit 283 I 1 IO_K3
bit 282 O 1 IO_K3 281 1 Z
bit 281 C 1 *
bit 280 I 1 IO_K4
bit 279 O 1 IO_K4 278 1 Z
bit 278 C 1 *
bit 277 I 1 IO_G1
bit 276 O 1 IO_G1 275 1 Z
bit 275 C 1 *
bit 274 I 1 IO_G2
bit 273 O 1 IO_G2 272 1 Z
bit 272 C 1 *
bit 271 I 1 IO_H5
bit 270 O 1 IO_H5 269 1 Z
bit 269 C 1 *
bit 268 I 1 IO_G5
bit 267 O 1 IO_G5 266 1 Z
bit 266 C 1 *
bit 265 I 1 IO_F2
bit 264 O 1 IO_F2 263 1 Z
bit 263 C 1 *
bit 262 I 1 IO_F3
bit 261 O 1 IO_F3 260 1 Z
bit 260 C 1 *
bit 259 I 1 IO_G6
bit 258 O 1 IO_G6 257 1 Z
bit 257 C 1 *
bit 256 I 1 IO_F5
bit 255 O 1 IO_F5 254 1 Z
bit 254 C 1 *
bit 253 I 1 IO_E1
bit 252 O 1 IO_E1 251 1 Z
bit 251 C 1 *
bit 250 I 1 IO_E2
bit 249 O 1 IO_E2 248 1 Z
bit 248 C 1 *
bit 247 I 1 IO_F4
bit 246 O 1 IO_F4 245 1 Z
bit 245 C 1 *
bit 244 I 1 IO_E3
bit 243 O 1 IO_E3 242 1 Z
bit 242 C 1 *
bit 241 I 1 IO_D3
bit 240 O 1 IO_D3 239 1 Z
bit 239 C 1 *
bit 238 I 1 IO_D2
bit 237 O 1 IO_D2 236 1 Z
bit 236 C 1 *
bit 235 I 1 IO_E4
bit 234 O 1 IO_E4 233 1 Z
bit 233 C 1 *
bit 232 I 1 IO_D4
bit 231 O 1 IO_D4 230 1 Z
bit 230 C 1 *
bit 229 I 1 IO_D1
bit 228 O 1 IO_D1 227 1 Z
bit 227 C 1 *
bit 226 I 1 IO_C1
bit 225 O 1 IO_C1 224 1 Z
bit 224 C 1 *
bit 223 I 1 IO_C2
bit 222 O 1 IO_C2 221 1 Z
bit 221 C 1 *
bit 220 O 1 *
bit 219 O 1 *
bit 218 O 1 *
bit 217 I 1 IO_C3
bit 216 O 1 IO_C3 215 1 Z
bit 215 C 1 *
bit 214 I 1 IO_C4
bit 213 O 1 IO_C4 212 1 Z
bit 212 C 1 *
bit 211 O 1 *
bit 210 I 1 HSWAP_EN_B3
bit 209 I 1 IO_A3
bit 208 O 1 IO_A3 207 1 Z
bit 207 C 1 *
bit 206 I 1 IO_B4
bit 205 O 1 IO_B4 204 1 Z
bit 204 C 1 *
bit 203 I 1 IO_A4
bit 202 O 1 IO_A4 201 1 Z
bit 201 C 1 *
bit 200 I 1 IO_D5
bit 199 O 1 IO_D5 198 1 Z
bit 198 C 1 *
bit 197 I 1 IO_C5
bit 196 O 1 IO_C5 195 1 Z
bit 195 C 1 *
bit 194 I 1 IO_F6
bit 193 O 1 IO_F6 192 1 Z
bit 192 C 1 *
bit 191 I 1 IO_B5
bit 190 O 1 IO_B5 189 1 Z
bit 189 C 1 *
bit 188 I 1 IO_A5
bit 187 O 1 IO_A5 186 1 Z
bit 186 C 1 *
bit 185 I 1 IO_E6
bit 184 O 1 IO_E6 183 1 Z
bit 183 C 1 *
bit 182 I 1 IO_D6
bit 181 O 1 IO_D6 180 1 Z
bit 180 C 1 *
bit 179 I 1 IO_F7
bit 178 O 1 IO_F7 177 1 Z
bit 177 C 1 *
bit 176 I 1 IO_C6
bit 175 O 1 IO_C6 174 1 Z
bit 174 C 1 *
bit 173 I 1 IO_B6
bit 172 O 1 IO_B6 171 1 Z
bit 171 C 1 *
bit 170 I 1 IO_E7
bit 169 O 1 IO_E7 168 1 Z
bit 168 C 1 *
bit 167 I 1 IO_D7
bit 166 O 1 IO_D7 165 1 Z
bit 165 C 1 *
bit 164 I 1 IO_C7
bit 163 O 1 IO_C7 162 1 Z
bit 162 C 1 *
bit 161 I 1 IO_B8
bit 160 O 1 IO_B8 159 1 Z
bit 159 C 1 *
bit 158 I 1 IO_A8
bit 157 O 1 IO_A8 156 1 Z
bit 156 C 1 *
bit 155 I 1 IO_F9
bit 154 O 1 IO_F9 153 1 Z
bit 153 C 1 *
bit 152 I 1 IO_E9
bit 151 O 1 IO_E9 150 1 Z
bit 150 C 1 *
bit 149 I 1 IO_D9
bit 148 O 1 IO_D9 147 1 Z
bit 147 C 1 *
bit 146 I 1 IO_B9
bit 145 O 1 IO_B9 144 1 Z
bit 144 C 1 *
bit 143 I 1 IO_A9
bit 142 O 1 IO_A9 141 1 Z
bit 141 C 1 *
bit 140 I 1 IO_F10
bit 139 O 1 IO_F10 138 1 Z
bit 138 C 1 *
bit 137 I 1 IO_E10
bit 136 O 1 IO_E10 135 1 Z
bit 135 C 1 *
bit 134 I 1 IO_D10
bit 133 O 1 IO_D10 132 1 Z
bit 132 C 1 *
bit 131 I 1 IO_C10
bit 130 O 1 IO_C10 129 1 Z
bit 129 C 1 *
bit 128 I 1 IO_B10
bit 127 O 1 IO_B10 126 1 Z
bit 126 C 1 *
bit 125 I 1 IO_F11
bit 124 O 1 IO_F11 123 1 Z
bit 123 C 1 *
bit 122 I 1 IO_E11
bit 121 O 1 IO_E11 120 1 Z
bit 120 C 1 *
bit 119 I 1 IO_A10
bit 118 O 1 IO_A10 117 1 Z
bit 117 C 1 *
bit 116 I 1 IO_D11
bit 115 O 1 IO_D11 114 1 Z
bit 114 C 1 *
bit 113 I 1 IO_C11
bit 112 O 1 IO_C11 111 1 Z
bit 111 C 1 *
bit 110 I 1 IO_B11
bit 109 O 1 IO_B11 108 1 Z
bit 108 C 1 *
bit 107 I 1 IO_A11
bit 106 O 1 IO_A11 105 1 Z
bit 105 C 1 *
bit 104 I 1 IO_A12
bit 103 O 1 IO_A12 102 1 Z
bit 102 C 1 *
bit 101 I 1 IO_B12
bit 100 O 1 IO_B12 99 1 Z
bit 99 C 1 *
bit 98 I 1 IO_C12
bit 97 O 1 IO_C12 96 1 Z
bit 96 C 1 *
bit 95 I 1 IO_D12
bit 94 O 1 IO_D12 93 1 Z
bit 93 C 1 *
bit 92 I 1 IO_E12
bit 91 O 1 IO_E12 90 1 Z
bit 90 C 1 *
bit 89 I 1 IO_F12
bit 88 O 1 IO_F12 87 1 Z
bit 87 C 1 *
bit 86 I 1 IO_A13
bit 85 O 1 IO_A13 84 1 Z
bit 84 C 1 *
bit 83 I 1 IO_B13
bit 82 O 1 IO_B13 81 1 Z
bit 81 C 1 *
bit 80 I 1 IO_C13
bit 79 O 1 IO_C13 78 1 Z
bit 78 C 1 *
bit 77 I 1 IO_D13
bit 76 O 1 IO_D13 75 1 Z
bit 75 C 1 *
bit 74 I 1 IO_E13
bit 73 O 1 IO_E13 72 1 Z
bit 72 C 1 *
bit 71 I 1 IO_A14
bit 70 O 1 IO_A14 69 1 Z
bit 69 C 1 *
bit 68 I 1 IO_B14
bit 67 O 1 IO_B14 66 1 Z
bit 66 C 1 *
bit 65 I 1 IO_D14
bit 64 O 1 IO_D14 63 1 Z
bit 63 C 1 *
bit 62 I 1 IO_E14
bit 61 O 1 IO_E14 60 1 Z
bit 60 C 1 *
bit 59 I 1 IO_F13
bit 58 O 1 IO_F13 57 1 Z
bit 57 C 1 *
bit 56 I 1 IO_B15
bit 55 O 1 IO_B15 54 1 Z
bit 54 C 1 *
bit 53 I 1 IO_A15
bit 52 O 1 IO_A15 51 1 Z
bit 51 C 1 *
bit 50 I 1 IO_D15
bit 49 O 1 IO_D15 48 1 Z
bit 48 C 1 *
bit 47 I 1 IO_E15
bit 46 O 1 IO_E15 45 1 Z
bit 45 C 1 *
bit 44 I 1 IO_E16
bit 43 O 1 IO_E16 42 1 Z
bit 42 C 1 *
bit 41 I 1 IO_B17
bit 40 O 1 IO_B17 39 1 Z
bit 39 C 1 *
bit 38 I 1 IO_C17
bit 37 O 1 IO_C17 36 1 Z
bit 36 C 1 *
bit 35 I 1 IO_D17
bit 34 O 1 IO_D17 33 1 Z
bit 33 C 1 *
bit 32 I 1 IO_E17
bit 31 O 1 IO_E17 30 1 Z
bit 30 C 1 *
bit 29 I 1 IO_F16
bit 28 O 1 IO_F16 27 1 Z
bit 27 C 1 *
bit 26 I 1 IO_A18
bit 25 O 1 IO_A18 24 1 Z
bit 24 C 1 *
bit 23 I 1 IO_B18
bit 22 O 1 IO_B18 21 1 Z
bit 21 C 1 *
bit 20 I 1 IO_C18
bit 19 O 1 IO_C18 18 1 Z
bit 18 C 1 *
bit 17 I 1 IO_D18
bit 16 O 1 IO_D18 15 1 Z
bit 15 C 1 *
bit 14 I 1 IO_F17
bit 13 O 1 IO_F17 12 1 Z
bit 12 C 1 *
bit 11 I 1 IO_A19
bit 10 O 1 IO_A19 9 1 Z
bit 9 C 1 *
bit 8 I 1 IO_B19
bit 7 O 1 IO_B19 6 1 Z
bit 6 C 1 *
bit 5 I 1 IO_C19
bit 4 O 1 IO_C19 3 1 Z
bit 3 C 1 *
bit 2 I 1 IO_B20
bit 1 O 1 IO_B20 0 1 Z
bit 0 C 1 *
