signal GND1
signal GND2
signal GND3
signal GND4
signal GND5
signal GND6
signal GND7
signal GND8
signal GND9
signal GND10
signal GND11
signal GND12
signal GND13
signal GND14
signal GND15
signal GND16
signal GND17
signal GND18
signal GND19
signal GND20
signal GND21
signal GND22
signal GND23
signal GND24
signal GND25
signal GND26
signal GND27
signal GND28
signal GND29
signal GND30
signal GND31
signal GND32
signal CCLK_PAD134
signal DONE_PAD133
signal HSWAP_EN_PAD25
signal M0_PAD83
signal M1_PAD82
signal M2_PAD84
signal PROG_B
signal TCK
signal TDI
signal TDO
signal TMS
signal VCCAUX1
signal VCCAUX2
signal VCCAUX3
signal VCCAUX4
signal VCCAUX5
signal VCCAUX6
signal VCCAUX7
signal VCCAUX8
signal VCCINT1
signal VCCINT2
signal VCCINT3
signal VCCINT4
signal VCCINT5
signal VCCINT6
signal VCCINT7
signal VCCINT8
signal VCCO01
signal VCCO02
signal VCCO03
signal VCCO04
signal VCCO11
signal VCCO12
signal VCCO13
signal VCCO14
signal VCCO21
signal VCCO22
signal VCCO23
signal VCCO24
signal VCCO31
signal VCCO32
signal VCCO33
signal VCCO34
signal VCCO41
signal VCCO42
signal VCCO43
signal VCCO44
signal VCCO51
signal VCCO52
signal VCCO53
signal VCCO54
signal VCCO61
signal VCCO62
signal VCCO63
signal VCCO64
signal VCCO71
signal VCCO72
signal VCCO73
signal VCCO74
signal IO_PAD2
signal IO_PAD3
signal IO_PAD4
signal IO_PAD6
signal IO_PAD8
signal IO_PAD9
signal IO_PAD10
signal IO_PAD14
signal IO_PAD16
signal IO_PAD17
signal IO_PAD18
signal IO_PAD19
signal IO_PAD22
signal IO_PAD23
signal IO_PAD24
signal IO_PAD29
signal IO_PAD30
signal IO_PAD32
signal IO_PAD34
signal IO_PAD35
signal IO_PAD36
signal IO_PAD37
signal IO_PAD38
signal IO_PAD40
signal IO_PAD42
signal IO_PAD44
signal IO_PAD46
signal IO_PAD47
signal IO_PAD48
signal IO_PAD51
signal IO_PAD53
signal IO_PAD56
signal IO_PAD58
signal IO_PAD61
signal IO_PAD62
signal IO_PAD63
signal IO_PAD65
signal IO_PAD67
signal IO_PAD69
signal IO_PAD71
signal IO_PAD72
signal IO_PAD73
signal IO_PAD74
signal IO_PAD75
signal IO_PAD77
signal IO_PAD79
signal IO_PAD80
signal IO_PAD85
signal IO_PAD86
signal IO_PAD89
signal IO_PAD90
signal IO_PAD91
signal IO_PAD92
signal IO_PAD93
signal IO_PAD95
signal IO_PAD97
signal IO_PAD100
signal IO_PAD101
signal IO_PAD103
signal IO_PAD105
signal IO_PAD106
signal IO_PAD107
signal IO_PAD110
signal IO_PAD111
signal IO_PAD112
signal IO_PAD114
signal IO_PAD116
signal IO_PAD117
signal IO_PAD118
signal IO_PAD122
signal IO_PAD124
signal IO_PAD125
signal IO_PAD126
signal IO_PAD127
signal IO_PAD130
signal IO_PAD131
signal IO_PAD132
signal IO_PAD137
signal IO_PAD138
signal IO_PAD140
signal IO_PAD142
signal IO_PAD143
signal IO_PAD144
signal IO_PAD145
signal IO_PAD146
signal IO_PAD148
signal IO_PAD150
signal IO_PAD152
signal IO_PAD154
signal IO_PAD155
signal IO_PAD156
signal IO_PAD159
signal IO_PAD161
signal IO_PAD164
signal IO_PAD166
signal IO_PAD169
signal IO_PAD170
signal IO_PAD171
signal IO_PAD173
signal IO_PAD175
signal IO_PAD177
signal IO_PAD179
signal IO_PAD180
signal IO_PAD181
signal IO_PAD182
signal IO_PAD183
signal IO_PAD185
signal IO_PAD187
signal IO_PAD188
signal IO_PAD193
signal IO_PAD194
signal IO_PAD197
signal IO_PAD198
signal IO_PAD199
signal IO_PAD200
signal IO_PAD201
signal IO_PAD203
signal IO_PAD205
signal IO_PAD208
signal IO_PAD209
signal IO_PAD211
signal IO_PAD213
signal IO_PAD214

register	BSR	383
register	BR	1
register	DIR	32

instruction length 6

instruction EXTEST 000000 BSR
instruction SAMPLE/PRELOAD 000001 BSR
instruction IDCODE 001001 DIR
instruction BYPASS 111111 BR

bit 382 I 1 IO_PAD188
bit 381 O 1 IO_PAD188 380 1 Z
bit 380 C 1 *
bit 379 I 1 IO_PAD187
bit 378 O 1 IO_PAD187 377 1 Z
bit 377 C 1 *
bit 376 I 1 IO_PAD185
bit 375 O 1 IO_PAD185 374 1 Z
bit 374 C 1 *
bit 373 I 1 IO_PAD183
bit 372 O 1 IO_PAD183 371 1 Z
bit 371 C 1 *
bit 370 I 1 IO_PAD182
bit 369 O 1 IO_PAD182 368 1 Z
bit 368 C 1 *
bit 367 I 1 IO_PAD181
bit 366 O 1 IO_PAD181 365 1 Z
bit 365 C 1 *
bit 364 I 1 IO_PAD180
bit 363 O 1 IO_PAD180 362 1 Z
bit 362 C 1 *
bit 361 I 1 IO_PAD179
bit 360 O 1 IO_PAD179 359 1 Z
bit 359 C 1 *
bit 358 I 1 IO_PAD177
bit 357 O 1 IO_PAD177 356 1 Z
bit 356 C 1 *
bit 355 I 1 IO_PAD175
bit 354 O 1 IO_PAD175 353 1 Z
bit 353 C 1 *
bit 352 I 1 IO_PAD173
bit 351 O 1 IO_PAD173 350 1 Z
bit 350 C 1 *
bit 349 I 1 IO_PAD171
bit 348 O 1 IO_PAD171 347 1 Z
bit 347 C 1 *
bit 346 I 1 IO_PAD170
bit 345 O 1 IO_PAD170 344 1 Z
bit 344 C 1 *
bit 343 I 1 IO_PAD169
bit 342 O 1 IO_PAD169 341 1 Z
bit 341 C 1 *
bit 340 I 1 IO_PAD166
bit 339 O 1 IO_PAD166 338 1 Z
bit 338 C 1 *
bit 337 I 1 IO_PAD164
bit 336 O 1 IO_PAD164 335 1 Z
bit 335 C 1 *
bit 334 I 1 IO_PAD161
bit 333 O 1 IO_PAD161 332 1 Z
bit 332 C 1 *
bit 331 I 1 IO_PAD159
bit 330 O 1 IO_PAD159 329 1 Z
bit 329 C 1 *
bit 328 I 1 IO_PAD156
bit 327 O 1 IO_PAD156 326 1 Z
bit 326 C 1 *
bit 325 I 1 IO_PAD155
bit 324 O 1 IO_PAD155 323 1 Z
bit 323 C 1 *
bit 322 I 1 IO_PAD154
bit 321 O 1 IO_PAD154 320 1 Z
bit 320 C 1 *
bit 319 I 1 IO_PAD152
bit 318 O 1 IO_PAD152 317 1 Z
bit 317 C 1 *
bit 316 I 1 IO_PAD150
bit 315 O 1 IO_PAD150 314 1 Z
bit 314 C 1 *
bit 313 I 1 IO_PAD148
bit 312 O 1 IO_PAD148 311 1 Z
bit 311 C 1 *
bit 310 I 1 IO_PAD146
bit 309 O 1 IO_PAD146 308 1 Z
bit 308 C 1 *
bit 307 I 1 IO_PAD145
bit 306 O 1 IO_PAD145 305 1 Z
bit 305 C 1 *
bit 304 I 1 IO_PAD144
bit 303 O 1 IO_PAD144 302 1 Z
bit 302 C 1 *
bit 301 I 1 IO_PAD143
bit 300 O 1 IO_PAD143 299 1 Z
bit 299 C 1 *
bit 298 I 1 IO_PAD142
bit 297 O 1 IO_PAD142 296 1 Z
bit 296 C 1 *
bit 295 I 1 IO_PAD140
bit 294 O 1 IO_PAD140 293 1 Z
bit 293 C 1 *
bit 292 I 1 IO_PAD138
bit 291 O 1 IO_PAD138 290 1 Z
bit 290 C 1 *
bit 289 I 1 IO_PAD137
bit 288 O 1 IO_PAD137 287 1 Z
bit 287 C 1 *
bit 286 I 1 CCLK_PAD134
bit 285 O 1 CCLK_PAD134 284 1 Z
bit 284 C 1 *
bit 283 I 1 DONE_PAD133
bit 282 O 1 DONE_PAD133 281 1 Z
bit 281 C 1 *
bit 280 I 1 IO_PAD132
bit 279 O 1 IO_PAD132 278 1 Z
bit 278 C 1 *
bit 277 I 1 IO_PAD131
bit 276 O 1 IO_PAD131 275 1 Z
bit 275 C 1 *
bit 274 I 1 IO_PAD130
bit 273 O 1 IO_PAD130 272 1 Z
bit 272 C 1 *
bit 271 I 1 IO_PAD127
bit 270 O 1 IO_PAD127 269 1 Z
bit 269 C 1 *
bit 268 I 1 IO_PAD126
bit 267 O 1 IO_PAD126 266 1 Z
bit 266 C 1 *
bit 265 I 1 IO_PAD125
bit 264 O 1 IO_PAD125 263 1 Z
bit 263 C 1 *
bit 262 I 1 IO_PAD124
bit 261 O 1 IO_PAD124 260 1 Z
bit 260 C 1 *
bit 259 I 1 IO_PAD122
bit 258 O 1 IO_PAD122 257 1 Z
bit 257 C 1 *
bit 256 I 1 IO_PAD118
bit 255 O 1 IO_PAD118 254 1 Z
bit 254 C 1 *
bit 253 I 1 IO_PAD117
bit 252 O 1 IO_PAD117 251 1 Z
bit 251 C 1 *
bit 250 I 1 IO_PAD116
bit 249 O 1 IO_PAD116 248 1 Z
bit 248 C 1 *
bit 247 I 1 IO_PAD114
bit 246 O 1 IO_PAD114 245 1 Z
bit 245 C 1 *
bit 244 I 1 IO_PAD112
bit 243 O 1 IO_PAD112 242 1 Z
bit 242 C 1 *
bit 241 I 1 IO_PAD111
bit 240 O 1 IO_PAD111 239 1 Z
bit 239 C 1 *
bit 238 I 1 IO_PAD110
bit 237 O 1 IO_PAD110 236 1 Z
bit 236 C 1 *
bit 235 I 1 IO_PAD107
bit 234 O 1 IO_PAD107 233 1 Z
bit 233 C 1 *
bit 232 I 1 IO_PAD106
bit 231 O 1 IO_PAD106 230 1 Z
bit 230 C 1 *
bit 229 I 1 IO_PAD105
bit 228 O 1 IO_PAD105 227 1 Z
bit 227 C 1 *
bit 226 I 1 IO_PAD103
bit 225 O 1 IO_PAD103 224 1 Z
bit 224 C 1 *
bit 223 I 1 IO_PAD101
bit 222 O 1 IO_PAD101 221 1 Z
bit 221 C 1 *
bit 220 I 1 IO_PAD100
bit 219 O 1 IO_PAD100 218 1 Z
bit 218 C 1 *
bit 217 I 1 IO_PAD97
bit 216 O 1 IO_PAD97 215 1 Z
bit 215 C 1 *
bit 214 I 1 IO_PAD95
bit 213 O 1 IO_PAD95 212 1 Z
bit 212 C 1 *
bit 211 I 1 IO_PAD93
bit 210 O 1 IO_PAD93 209 1 Z
bit 209 C 1 *
bit 208 I 1 IO_PAD92
bit 207 O 1 IO_PAD92 206 1 Z
bit 206 C 1 *
bit 205 I 1 IO_PAD91
bit 204 O 1 IO_PAD91 203 1 Z
bit 203 C 1 *
bit 202 I 1 IO_PAD90
bit 201 O 1 IO_PAD90 200 1 Z
bit 200 C 1 *
bit 199 I 1 IO_PAD89
bit 198 O 1 IO_PAD89 197 1 Z
bit 197 C 1 *
bit 196 I 1 IO_PAD86
bit 195 O 1 IO_PAD86 194 1 Z
bit 194 C 1 *
bit 193 I 1 IO_PAD85
bit 192 O 1 IO_PAD85 191 1 Z
bit 191 C 1 *
bit 190 I 1 M2_PAD84
bit 189 I 1 M0_PAD83
bit 188 I 1 M1_PAD82
bit 187 I 1 IO_PAD80
bit 186 O 1 IO_PAD80 185 1 Z
bit 185 C 1 *
bit 184 I 1 IO_PAD79
bit 183 O 1 IO_PAD79 182 1 Z
bit 182 C 1 *
bit 181 I 1 IO_PAD77
bit 180 O 1 IO_PAD77 179 1 Z
bit 179 C 1 *
bit 178 I 1 IO_PAD75
bit 177 O 1 IO_PAD75 176 1 Z
bit 176 C 1 *
bit 175 I 1 IO_PAD74
bit 174 O 1 IO_PAD74 173 1 Z
bit 173 C 1 *
bit 172 I 1 IO_PAD73
bit 171 O 1 IO_PAD73 170 1 Z
bit 170 C 1 *
bit 169 I 1 IO_PAD72
bit 168 O 1 IO_PAD72 167 1 Z
bit 167 C 1 *
bit 166 I 1 IO_PAD71
bit 165 O 1 IO_PAD71 164 1 Z
bit 164 C 1 *
bit 163 I 1 IO_PAD69
bit 162 O 1 IO_PAD69 161 1 Z
bit 161 C 1 *
bit 160 I 1 IO_PAD67
bit 159 O 1 IO_PAD67 158 1 Z
bit 158 C 1 *
bit 157 I 1 IO_PAD65
bit 156 O 1 IO_PAD65 155 1 Z
bit 155 C 1 *
bit 154 I 1 IO_PAD63
bit 153 O 1 IO_PAD63 152 1 Z
bit 152 C 1 *
bit 151 I 1 IO_PAD62
bit 150 O 1 IO_PAD62 149 1 Z
bit 149 C 1 *
bit 148 I 1 IO_PAD61
bit 147 O 1 IO_PAD61 146 1 Z
bit 146 C 1 *
bit 145 I 1 IO_PAD58
bit 144 O 1 IO_PAD58 143 1 Z
bit 143 C 1 *
bit 142 I 1 IO_PAD56
bit 141 O 1 IO_PAD56 140 1 Z
bit 140 C 1 *
bit 139 I 1 IO_PAD53
bit 138 O 1 IO_PAD53 137 1 Z
bit 137 C 1 *
bit 136 I 1 IO_PAD51
bit 135 O 1 IO_PAD51 134 1 Z
bit 134 C 1 *
bit 133 I 1 IO_PAD48
bit 132 O 1 IO_PAD48 131 1 Z
bit 131 C 1 *
bit 130 I 1 IO_PAD47
bit 129 O 1 IO_PAD47 128 1 Z
bit 128 C 1 *
bit 127 I 1 IO_PAD46
bit 126 O 1 IO_PAD46 125 1 Z
bit 125 C 1 *
bit 124 I 1 IO_PAD44
bit 123 O 1 IO_PAD44 122 1 Z
bit 122 C 1 *
bit 121 I 1 IO_PAD42
bit 120 O 1 IO_PAD42 119 1 Z
bit 119 C 1 *
bit 118 I 1 IO_PAD40
bit 117 O 1 IO_PAD40 116 1 Z
bit 116 C 1 *
bit 115 I 1 IO_PAD38
bit 114 O 1 IO_PAD38 113 1 Z
bit 113 C 1 *
bit 112 I 1 IO_PAD37
bit 111 O 1 IO_PAD37 110 1 Z
bit 110 C 1 *
bit 109 I 1 IO_PAD36
bit 108 O 1 IO_PAD36 107 1 Z
bit 107 C 1 *
bit 106 I 1 IO_PAD35
bit 105 O 1 IO_PAD35 104 1 Z
bit 104 C 1 *
bit 103 I 1 IO_PAD34
bit 102 O 1 IO_PAD34 101 1 Z
bit 101 C 1 *
bit 100 I 1 IO_PAD32
bit 99 O 1 IO_PAD32 98 1 Z
bit 98 C 1 *
bit 97 I 1 IO_PAD30
bit 96 O 1 IO_PAD30 95 1 Z
bit 95 C 1 *
bit 94 I 1 IO_PAD29
bit 93 O 1 IO_PAD29 92 1 Z
bit 92 C 1 *
bit 91 O 1 *
bit 90 I 1 HSWAP_EN_PAD25
bit 89 I 1 IO_PAD24
bit 88 O 1 IO_PAD24 87 1 Z
bit 87 C 1 *
bit 86 I 1 IO_PAD23
bit 85 O 1 IO_PAD23 84 1 Z
bit 84 C 1 *
bit 83 I 1 IO_PAD22
bit 82 O 1 IO_PAD22 81 1 Z
bit 81 C 1 *
bit 80 I 1 IO_PAD19
bit 79 O 1 IO_PAD19 78 1 Z
bit 78 C 1 *
bit 77 I 1 IO_PAD18
bit 76 O 1 IO_PAD18 75 1 Z
bit 75 C 1 *
bit 74 I 1 IO_PAD17
bit 73 O 1 IO_PAD17 72 1 Z
bit 72 C 1 *
bit 71 I 1 IO_PAD16
bit 70 O 1 IO_PAD16 69 1 Z
bit 69 C 1 *
bit 68 I 1 IO_PAD14
bit 67 O 1 IO_PAD14 66 1 Z
bit 66 C 1 *
bit 65 I 1 IO_PAD10
bit 64 O 1 IO_PAD10 63 1 Z
bit 63 C 1 *
bit 62 I 1 IO_PAD9
bit 61 O 1 IO_PAD9 60 1 Z
bit 60 C 1 *
bit 59 I 1 IO_PAD8
bit 58 O 1 IO_PAD8 57 1 Z
bit 57 C 1 *
bit 56 I 1 IO_PAD6
bit 55 O 1 IO_PAD6 54 1 Z
bit 54 C 1 *
bit 53 I 1 IO_PAD4
bit 52 O 1 IO_PAD4 51 1 Z
bit 51 C 1 *
bit 50 I 1 IO_PAD3
bit 49 O 1 IO_PAD3 48 1 Z
bit 48 C 1 *
bit 47 I 1 IO_PAD2
bit 46 O 1 IO_PAD2 45 1 Z
bit 45 C 1 *
bit 44 I 1 IO_PAD215
bit 43 O 1 IO_PAD215 42 1 Z
bit 42 C 1 *
bit 41 I 1 IO_PAD214
bit 40 O 1 IO_PAD214 39 1 Z
bit 39 C 1 *
bit 38 I 1 IO_PAD213
bit 37 O 1 IO_PAD213 36 1 Z
bit 36 C 1 *
bit 35 I 1 IO_PAD211
bit 34 O 1 IO_PAD211 33 1 Z
bit 33 C 1 *
bit 32 I 1 IO_PAD209
bit 31 O 1 IO_PAD209 30 1 Z
bit 30 C 1 *
bit 29 I 1 IO_PAD208
bit 28 O 1 IO_PAD208 27 1 Z
bit 27 C 1 *
bit 26 I 1 IO_PAD205
bit 25 O 1 IO_PAD205 24 1 Z
bit 24 C 1 *
bit 23 I 1 IO_PAD203
bit 22 O 1 IO_PAD203 21 1 Z
bit 21 C 1 *
bit 20 I 1 IO_PAD201
bit 19 O 1 IO_PAD201 18 1 Z
bit 18 C 1 *
bit 17 I 1 IO_PAD200
bit 16 O 1 IO_PAD200 15 1 Z
bit 15 C 1 *
bit 14 I 1 IO_PAD199
bit 13 O 1 IO_PAD199 12 1 Z
bit 12 C 1 *
bit 11 I 1 IO_PAD198
bit 10 O 1 IO_PAD198 9 1 Z
bit 9 C 1 *
bit 8 I 1 IO_PAD197
bit 7 O 1 IO_PAD197 6 1 Z
bit 6 C 1 *
bit 5 I 1 IO_PAD194
bit 4 O 1 IO_PAD194 3 1 Z
bit 3 C 1 *
bit 2 I 1 IO_PAD193
bit 1 O 1 IO_PAD193 0 1 Z
bit 0 C 1 *
