signal ADDR2
signal ADDR3
signal ADDR4
signal ADDR5
signal ADDR6
signal ADDR7
signal ADDR8
signal ADDR9
signal ADDR10
signal ADDR11
signal ADDR12
signal ADDR13
signal ADDR14
signal ADDR15
signal ADDR16
signal ADDR17
signal ADDR18
signal ADDR19
signal ADDR20
signal ADDR21
signal ADDR22
signal ADDR23
signal ADDR24
signal ADDR25
signal DATA0
signal DATA1
signal DATA2
signal DATA3
signal DATA4
signal DATA5
signal DATA6
signal DATA7
signal DATA8
signal DATA9
signal DATA10
signal DATA11
signal DATA12
signal DATA13
signal DATA14
signal DATA15
signal DATA16
signal DATA17
signal DATA18
signal DATA19
signal DATA20
signal DATA21
signal DATA22
signal DATA23
signal DATA24
signal DATA25
signal DATA26
signal DATA27
signal DATA28
signal DATA29
signal DATA30
signal DATA31
signal AMS_B0
signal AMS_B1
signal AMS_B2
signal AMS_B3
signal AOE_B
signal ARDY
signal ARE_B
signal AWE_B
signal ABE_B0
signal ABE_B1
signal ABE_B2
signal ABE_B3
signal BG_B
signal BGH_B
signal BMODE0
signal BMODE1
signal BR_B
signal BY_PASS
signal PPI1_DATA0
signal PPI1_DATA1
signal PPI1_DATA2
signal PPI1_DATA3
signal PPI1_DATA4
signal PPI1_DATA5
signal PPI1_DATA6
signal PPI1_DATA7
signal PPI1_DATA8
signal PPI1_DATA9
signal PPI1_DATA10
signal PPI1_DATA11
signal PPI1_DATA12
signal PPI1_DATA13
signal PPI1_DATA14
signal PPI1_DATA15
signal PPI2_DATA0
signal PPI2_DATA1
signal PPI2_DATA2
signal PPI2_DATA3
signal PPI2_DATA4
signal PPI2_DATA5
signal PPI2_DATA6
signal PPI2_DATA7
signal PPI2_DATA8
signal PPI2_DATA9
signal PPI2_DATA10
signal PPI2_DATA11
signal PPI2_DATA12
signal PPI2_DATA13
signal PPI2_DATA14
signal PPI2_DATA15
signal DR0PRI
signal DR0SEC
signal DR1PRI
signal DR1SEC
signal DT0PRI
signal DT0SEC
signal DT1PRI
signal DT1SEC
signal MISO
signal MOSI
signal NMI_0
signal NMI_1
signal PF0
signal PF1
signal PF2
signal PF3
signal PF4
signal PF5
signal PF6
signal PF7
signal PF8
signal PF9
signal PF10
signal PF11
signal PF12
signal PF13
signal PF14
signal PF15
signal RESET_B
signal RFS0
signal RFS1
signal RSCLK0
signal RSCLK1
signal TSCLK0
signal TSCLK1
signal RX
signal TX
signal SA10
signal SCAS_B
signal SCK
signal SCKE
signal SLEEP
signal SMS_B0
signal SMS_B1
signal SMS_B2
signal SMS_B3
signal SRAS_B
signal SWE_B
signal SCLK0
signal SCLK1
signal TCK
signal TDI
signal TDO
signal TMS
signal TRST_B
signal EMU_B
signal TEST
signal TFS0
signal TFS1
signal PPI1_CLK
signal PPI2_CLK
signal PPI1_SYNC1
signal PPI1_SYNC2
signal PPI1_SYNC3
signal PPI2_SYNC1
signal PPI2_SYNC2
signal PPI2_SYNC3
signal VDD_INT0
signal VDD_INT1
signal VDD_INT2
signal VDD_INT3
signal VDD_INT4
signal VDD_INT5
signal VDD_INT6
signal VDD_INT7
signal VDD_INT8
signal GND_INT0
signal GND_INT1
signal GND_INT2
signal GND_INT3
signal GND_INT4
signal GND_INT5
signal GND_INT6
signal VDD_EXT0
signal VDD_EXT1
signal VDD_EXT2
signal VDD_EXT3
signal VDD_EXT4
signal VDD_EXT5
signal VDD_EXT6
signal VDD_EXT7
signal VDD_EXT8
signal VDD_EXT9
signal VDD_EXT10
signal VDD_EXT11
signal VDD_EXT12
signal VDD_EXT13
signal VDD_EXT14
signal VDD_EXT15
signal VDD_EXT16
signal VDD_EXT17
signal VDD_EXT18
signal CLKIN
signal XTAL
signal VREF_FLT
signal VREG
signal PSMON_VDD
signal PSMON_GND
signal GND_EXT0
signal GND_EXT1
signal GND_EXT2
signal GND_EXT3
signal GND_EXT4
signal GND_EXT5
signal GND_EXT6
signal GND_EXT7
signal GND_EXT8
signal GND_EXT9
signal GND_EXT10
signal GND_EXT11
signal GND_EXT12
signal GND_EXT13
signal GND_EXT14
signal GND_EXT15
signal GND_EXT16
signal GND_EXT17
signal GND_EXT18

register	BSR	355
register	BR	1
register	DIR	32
register	DBGSTAT	16
register	DBGCTL	16
register	EMUIR	32
register	EMUDAT	32
register	EMUPC	32

instruction length 5

instruction BYPASS 11111 BR
instruction EXTEST 00000 BSR
instruction SAMPLE/PRELOAD 10000 BSR
instruction IDCODE 00010 DIR
instruction DBGSTAT_SCAN 01100 DBGSTAT
instruction DBGCTL_SCAN 00100 DBGCTL
instruction EMUIR_SCAN 01000 EMUIR
instruction EMUDAT_SCAN 10100 EMUDAT
instruction EMUPC_SCAN 11110 EMUPC

bit 354 I 1 TEST
bit 353 I 1 BMODE1
bit 352 I 1 BMODE0
bit 351 O 1 SLEEP
bit 350 I 1 NMI_0
bit 349 C 0 *
bit 348 O 1 MISO 349 0 Z
bit 347 I 1 MISO
bit 346 C 0 *
bit 345 O 1 MOSI 346 0 Z
bit 344 I 1 MOSI
bit 343 C 0 *
bit 342 O 1 SCK 343 0 Z
bit 341 I 1 SCK
bit 340 C 0 *
bit 339 O 1 RX 340 0 Z
bit 338 I 1 RX
bit 337 C 0 *
bit 336 O 1 TX 337 0 Z
bit 335 I 1 TX
bit 334 C 0 *
bit 333 O 1 RSCLK1 334 0 Z
bit 332 I 1 RSCLK1
bit 331 C 0 *
bit 330 O 1 RFS1 331 0 Z
bit 329 I 1 RFS1
bit 328 C 0 *
bit 327 O 1 DR1SEC 328 0 Z
bit 326 I 1 DR1SEC
bit 325 C 0 *
bit 324 O 1 DR1PRI 325 0 Z
bit 323 I 1 DR1PRI
bit 322 C 0 *
bit 321 O 1 TSCLK1 322 0 Z
bit 320 I 1 TSCLK1
bit 319 C 0 *
bit 318 O 1 TFS1 319 0 Z
bit 317 I 1 TFS1
bit 316 C 0 *
bit 315 O 1 DT1SEC 316 0 Z
bit 314 I 1 DT1SEC
bit 313 C 0 *
bit 312 O 1 DT1PRI 313 0 Z
bit 311 I 1 DT1PRI
bit 310 C 0 *
bit 309 O 1 RSCLK0 310 0 Z
bit 308 I 1 RSCLK0
bit 307 C 0 *
bit 306 O 1 RFS0 307 0 Z
bit 305 I 1 RFS0
bit 304 C 0 *
bit 303 O 1 DR0SEC 304 0 Z
bit 302 I 1 DR0SEC
bit 301 C 0 *
bit 300 O 1 DR0PRI 301 0 Z
bit 299 I 1 DR0PRI
bit 298 C 0 *
bit 297 O 1 TSCLK0 298 0 Z
bit 296 I 1 TSCLK0
bit 295 C 0 *
bit 294 O 1 TFS0 295 0 Z
bit 293 I 1 TFS0
bit 292 C 0 *
bit 291 O 1 DT0SEC 292 0 Z
bit 290 I 1 DT0SEC
bit 289 C 0 *
bit 288 O 1 DT0PRI 289 0 Z
bit 287 I 1 DT0PRI
bit 286 O 1 DATA31 254 0 Z
bit 285 I 1 DATA31
bit 284 O 1 DATA30 254 0 Z
bit 283 I 1 DATA30
bit 282 O 1 DATA29 254 0 Z
bit 281 I 1 DATA29
bit 280 O 1 DATA28 254 0 Z
bit 279 I 1 DATA28
bit 278 O 1 DATA27 254 0 Z
bit 277 I 1 DATA27
bit 276 O 1 DATA26 254 0 Z
bit 275 I 1 DATA26
bit 274 O 1 DATA25 254 0 Z
bit 273 I 1 DATA25
bit 272 O 1 DATA24 254 0 Z
bit 271 I 1 DATA24
bit 270 O 1 DATA23 254 0 Z
bit 269 I 1 DATA23
bit 268 O 1 DATA22 254 0 Z
bit 267 I 1 DATA22
bit 266 O 1 DATA21 254 0 Z
bit 265 I 1 DATA21
bit 264 O 1 DATA20 254 0 Z
bit 263 I 1 DATA20
bit 262 O 1 DATA19 254 0 Z
bit 261 I 1 DATA19
bit 260 O 1 DATA18 254 0 Z
bit 259 I 1 DATA18
bit 258 O 1 DATA17 254 0 Z
bit 257 I 1 DATA17
bit 256 O 1 DATA16 254 0 Z
bit 255 I 1 DATA16
bit 254 C 0 *
bit 253 O 1 DATA15 221 0 Z
bit 252 I 1 DATA15
bit 251 O 1 DATA14 221 0 Z
bit 250 I 1 DATA14
bit 249 O 1 DATA13 221 0 Z
bit 248 I 1 DATA13
bit 247 O 1 DATA12 221 0 Z
bit 246 I 1 DATA12
bit 245 O 1 DATA11 221 0 Z
bit 244 I 1 DATA11
bit 243 O 1 DATA10 221 0 Z
bit 242 I 1 DATA10
bit 241 O 1 DATA9 221 0 Z
bit 240 I 1 DATA9
bit 239 O 1 DATA8 221 0 Z
bit 238 I 1 DATA8
bit 237 O 1 DATA7 221 0 Z
bit 236 I 1 DATA7
bit 235 O 1 DATA6 221 0 Z
bit 234 I 1 DATA6
bit 233 O 1 DATA5 221 0 Z
bit 232 I 1 DATA5
bit 231 O 1 DATA4 221 0 Z
bit 230 I 1 DATA4
bit 229 O 1 DATA3 221 0 Z
bit 228 I 1 DATA3
bit 227 O 1 DATA2 221 0 Z
bit 226 I 1 DATA2
bit 225 O 1 DATA1 221 0 Z
bit 224 I 1 DATA1
bit 223 O 1 DATA0 221 0 Z
bit 222 I 1 DATA0
bit 221 C 0 *
bit 220 O 1 ADDR2 219 0 Z
bit 219 C 0 *
bit 218 O 1 ADDR3 219 0 Z
bit 217 O 1 ADDR4 219 0 Z
bit 216 O 1 ADDR5 219 0 Z
bit 215 O 1 ADDR6 219 0 Z
bit 214 O 1 ADDR7 219 0 Z
bit 213 O 1 ADDR8 219 0 Z
bit 212 O 1 ABE_B3 219 0 Z
bit 211 O 1 ABE_B2 219 0 Z
bit 210 O 1 ABE_B1 219 0 Z
bit 209 O 1 ABE_B0 219 0 Z
bit 208 O 1 BGH_B
bit 207 O 1 BG_B
bit 206 I 1 BR_B
bit 205 O 1 SA10 194 0 Z
bit 204 O 1 SCLK1 194 0 Z
bit 203 O 1 SCLK0 194 0 Z
bit 202 O 1 SWE_B 194 0 Z
bit 201 O 1 SCAS_B 194 0 Z
bit 200 O 1 SCKE 194 0 Z
bit 199 O 1 SRAS_B 194 0 Z
bit 198 O 1 SMS_B3 194 0 Z
bit 197 O 1 SMS_B2 194 0 Z
bit 196 O 1 SMS_B1 194 0 Z
bit 195 O 1 SMS_B0 194 0 Z
bit 194 C 0 *
bit 193 I 1 ARDY
bit 192 O 1 ARE_B 189 0 Z
bit 191 O 1 AOE_B 189 0 Z
bit 190 O 1 AWE_B 189 0 Z
bit 189 C 0 *
bit 188 O 1 AMS_B0 189 0 Z
bit 187 O 1 AMS_B1 189 0 Z
bit 186 O 1 AMS_B2 189 0 Z
bit 185 O 1 AMS_B3 189 0 Z
bit 184 O 1 ADDR9 175 0 Z
bit 183 O 1 ADDR10 175 0 Z
bit 182 O 1 ADDR11 175 0 Z
bit 181 O 1 ADDR12 175 0 Z
bit 180 O 1 ADDR13 175 0 Z
bit 179 O 1 ADDR14 175 0 Z
bit 178 O 1 ADDR15 175 0 Z
bit 177 O 1 ADDR16 175 0 Z
bit 176 O 1 ADDR17 175 0 Z
bit 175 C 0 *
bit 174 O 1 ADDR18 175 0 Z
bit 173 O 1 ADDR19 175 0 Z
bit 172 O 1 ADDR20 175 0 Z
bit 171 O 1 ADDR21 175 0 Z
bit 170 O 1 ADDR22 175 0 Z
bit 169 O 1 ADDR23 175 0 Z
bit 168 O 1 ADDR24 175 0 Z
bit 167 O 1 ADDR25 175 0 Z
bit 166 I 1 PPI2_CLK
bit 165 I 1 PPI1_CLK
bit 164 C 0 *
bit 163 O 1 PPI1_SYNC3 164 0 Z
bit 162 I 1 PPI1_SYNC3
bit 161 C 0 *
bit 160 O 1 PPI1_SYNC2 161 0 Z
bit 159 I 1 PPI1_SYNC2
bit 158 C 0 *
bit 157 O 1 PPI1_SYNC1 158 0 Z
bit 156 I 1 PPI1_SYNC1
bit 155 C 0 *
bit 154 O 1 PPI1_DATA15 155 0 Z
bit 153 I 1 PPI1_DATA15
bit 152 C 0 *
bit 151 O 1 PPI1_DATA14 152 0 Z
bit 150 I 1 PPI1_DATA14
bit 149 C 0 *
bit 148 O 1 PPI1_DATA13 149 0 Z
bit 147 I 1 PPI1_DATA13
bit 146 C 0 *
bit 145 O 1 PPI1_DATA12 146 0 Z
bit 144 I 1 PPI1_DATA12
bit 143 C 0 *
bit 142 O 1 PPI1_DATA11 143 0 Z
bit 141 I 1 PPI1_DATA11
bit 140 C 0 *
bit 139 O 1 PPI1_DATA10 140 0 Z
bit 138 I 1 PPI1_DATA10
bit 137 I 1 RESET_B
bit 136 I 1 BY_PASS
bit 135 C 0 *
bit 134 O 1 PPI1_DATA9 135 0 Z
bit 133 I 1 PPI1_DATA9
bit 132 C 0 *
bit 131 O 1 PPI1_DATA8 132 0 Z
bit 130 I 1 PPI1_DATA8
bit 129 C 0 *
bit 128 O 1 PPI1_DATA7 129 0 Z
bit 127 I 1 PPI1_DATA7
bit 126 C 0 *
bit 125 O 1 PPI1_DATA6 126 0 Z
bit 124 I 1 PPI1_DATA6
bit 123 C 0 *
bit 122 O 1 PPI1_DATA5 123 0 Z
bit 121 I 1 PPI1_DATA5
bit 120 C 0 *
bit 119 O 1 PPI1_DATA4 120 0 Z
bit 118 I 1 PPI1_DATA4
bit 117 C 0 *
bit 116 O 1 PPI1_DATA3 117 0 Z
bit 115 I 1 PPI1_DATA3
bit 114 C 0 *
bit 113 O 1 PPI1_DATA2 114 0 Z
bit 112 I 1 PPI1_DATA2
bit 111 C 0 *
bit 110 O 1 PPI1_DATA1 111 0 Z
bit 109 I 1 PPI1_DATA1
bit 108 C 0 *
bit 107 O 1 PPI1_DATA0 108 0 Z
bit 106 I 1 PPI1_DATA0
bit 105 C 0 *
bit 104 O 1 PPI2_SYNC3 105 0 Z
bit 103 I 1 PPI2_SYNC3
bit 102 C 0 *
bit 101 O 1 PPI2_SYNC2 102 0 Z
bit 100 I 1 PPI2_SYNC2
bit 99 C 0 *
bit 98 O 1 PPI2_SYNC1 99 0 Z
bit 97 I 1 PPI2_SYNC1
bit 96 C 0 *
bit 95 O 1 PPI2_DATA15 96 0 Z
bit 94 I 1 PPI2_DATA15
bit 93 C 0 *
bit 92 O 1 PPI2_DATA14 93 0 Z
bit 91 I 1 PPI2_DATA14
bit 90 C 0 *
bit 89 O 1 PPI2_DATA13 90 0 Z
bit 88 I 1 PPI2_DATA13
bit 87 C 0 *
bit 86 O 1 PPI2_DATA12 87 0 Z
bit 85 I 1 PPI2_DATA12
bit 84 C 0 *
bit 83 O 1 PPI2_DATA11 84 0 Z
bit 82 I 1 PPI2_DATA11
bit 81 C 0 *
bit 80 O 1 PPI2_DATA10 81 0 Z
bit 79 I 1 PPI2_DATA10
bit 78 C 0 *
bit 77 O 1 PPI2_DATA9 78 0 Z
bit 76 I 1 PPI2_DATA9
bit 75 C 0 *
bit 74 O 1 PPI2_DATA8 75 0 Z
bit 73 I 1 PPI2_DATA8
bit 72 C 0 *
bit 71 O 1 PPI2_DATA7 72 0 Z
bit 70 I 1 PPI2_DATA7
bit 69 C 0 *
bit 68 O 1 PPI2_DATA6 69 0 Z
bit 67 I 1 PPI2_DATA6
bit 66 C 0 *
bit 65 O 1 PPI2_DATA5 66 0 Z
bit 64 I 1 PPI2_DATA5
bit 63 C 0 *
bit 62 O 1 PPI2_DATA4 63 0 Z
bit 61 I 1 PPI2_DATA4
bit 60 C 0 *
bit 59 O 1 PPI2_DATA3 60 0 Z
bit 58 I 1 PPI2_DATA3
bit 57 C 0 *
bit 56 O 1 PPI2_DATA2 57 0 Z
bit 55 I 1 PPI2_DATA2
bit 54 C 0 *
bit 53 O 1 PPI2_DATA1 54 0 Z
bit 52 I 1 PPI2_DATA1
bit 51 C 0 *
bit 50 O 1 PPI2_DATA0 51 0 Z
bit 49 I 1 PPI2_DATA0
bit 48 C 0 *
bit 47 O 1 PF0 48 0 Z
bit 46 I 1 PF0
bit 45 C 0 *
bit 44 O 1 PF1 45 0 Z
bit 43 I 1 PF1
bit 42 C 0 *
bit 41 O 1 PF2 42 0 Z
bit 40 I 1 PF2
bit 39 C 0 *
bit 38 O 1 PF3 39 0 Z
bit 37 I 1 PF3
bit 36 C 0 *
bit 35 O 1 PF4 36 0 Z
bit 34 I 1 PF4
bit 33 C 0 *
bit 32 O 1 PF5 33 0 Z
bit 31 I 1 PF5
bit 30 C 0 *
bit 29 O 1 PF6 30 0 Z
bit 28 I 1 PF6
bit 27 C 0 *
bit 26 O 1 PF7 27 0 Z
bit 25 I 1 PF7
bit 24 C 0 *
bit 23 O 1 PF8 24 0 Z
bit 22 I 1 PF8
bit 21 C 0 *
bit 20 O 1 PF9 21 0 Z
bit 19 I 1 PF9
bit 18 C 0 *
bit 17 O 1 PF10 18 0 Z
bit 16 I 1 PF10
bit 15 C 0 *
bit 14 O 1 PF11 15 0 Z
bit 13 I 1 PF11
bit 12 C 0 *
bit 11 O 1 PF12 12 0 Z
bit 10 I 1 PF12
bit 9 C 0 *
bit 8 O 1 PF13 9 0 Z
bit 7 I 1 PF13
bit 6 C 0 *
bit 5 O 1 PF14 6 0 Z
bit 4 I 1 PF14
bit 3 C 0 *
bit 2 O 1 PF15 3 0 Z
bit 1 I 1 PF15
bit 0 I 1 NMI_1
