#
# $Id: xc3s1000 747 2007-11-10 00:31:50Z arniml $
#
# JTAG declarations for XC3S1000
#
# This program is free software; you can redistribute it and/or
# modify it under the terms of the GNU General Public License
# as published by the Free Software Foundation; either version 2
# of the License, or (at your option) any later version.
#
# This program is distributed in the hope that it will be useful,
# but WITHOUT ANY WARRANTY; without even the implied warranty of
# MERCHANTABILITY or FITNESS FOR A PARTICULAR PURPOSE.  See the
# GNU General Public License for more details.
#
# You should have received a copy of the GNU General Public License
# along with this program; if not, write to the Free Software
# Foundation, Inc., 59 Temple Place - Suite 330, Boston, MA
# 02111-1307, USA.
#
# Written by Arnim Laeuger <arniml@users.sourceforge.net>
#
# Note:
#   The signals defined in this file are generic for any XC3S1000.
#   Signalnames according to Xilinx' package tables are set in the
#   package specific scripts.
#

signal CCLK_PAD349
signal DONE_PAD348
signal HSWAP_EN_PAD70
signal IO_PAD10
signal IO_PAD100
signal IO_PAD102
signal IO_PAD104
signal IO_PAD105
signal IO_PAD106
signal IO_PAD108
signal IO_PAD110
signal IO_PAD111
signal IO_PAD112
signal IO_PAD113
signal IO_PAD114
signal IO_PAD115
signal IO_PAD116
signal IO_PAD117
signal IO_PAD118
signal IO_PAD119
signal IO_PAD12
signal IO_PAD120
signal IO_PAD121
signal IO_PAD122
signal IO_PAD124
signal IO_PAD126
signal IO_PAD128
signal IO_PAD13
signal IO_PAD130
signal IO_PAD132
signal IO_PAD133
signal IO_PAD134
signal IO_PAD136
signal IO_PAD138
signal IO_PAD139
signal IO_PAD14
signal IO_PAD140
signal IO_PAD141
signal IO_PAD143
signal IO_PAD145
signal IO_PAD146
signal IO_PAD147
signal IO_PAD149
signal IO_PAD151
signal IO_PAD153
signal IO_PAD155
signal IO_PAD157
signal IO_PAD158
signal IO_PAD159
signal IO_PAD16
signal IO_PAD160
signal IO_PAD161
signal IO_PAD162
signal IO_PAD163
signal IO_PAD164
signal IO_PAD165
signal IO_PAD166
signal IO_PAD167
signal IO_PAD168
signal IO_PAD169
signal IO_PAD171
signal IO_PAD173
signal IO_PAD174
signal IO_PAD175
signal IO_PAD177
signal IO_PAD179
signal IO_PAD18
signal IO_PAD181
signal IO_PAD183
signal IO_PAD184
signal IO_PAD185
signal IO_PAD186
signal IO_PAD187
signal IO_PAD189
signal IO_PAD191
signal IO_PAD192
signal IO_PAD193
signal IO_PAD195
signal IO_PAD196
signal IO_PAD197
signal IO_PAD199
signal IO_PAD2
signal IO_PAD20
signal IO_PAD200
signal IO_PAD201
signal IO_PAD202
signal IO_PAD203
signal IO_PAD204
signal IO_PAD210
signal IO_PAD211
signal IO_PAD214
signal IO_PAD215
signal IO_PAD216
signal IO_PAD218
signal IO_PAD219
signal IO_PAD22
signal IO_PAD220
signal IO_PAD221
signal IO_PAD222
signal IO_PAD224
signal IO_PAD226
signal IO_PAD227
signal IO_PAD228
signal IO_PAD229
signal IO_PAD23
signal IO_PAD230
signal IO_PAD232
signal IO_PAD234
signal IO_PAD236
signal IO_PAD238
signal IO_PAD239
signal IO_PAD24
signal IO_PAD240
signal IO_PAD241
signal IO_PAD242
signal IO_PAD243
signal IO_PAD244
signal IO_PAD245
signal IO_PAD246
signal IO_PAD248
signal IO_PAD249
signal IO_PAD250
signal IO_PAD251
signal IO_PAD252
signal IO_PAD254
signal IO_PAD256
signal IO_PAD257
signal IO_PAD258
signal IO_PAD26
signal IO_PAD260
signal IO_PAD262
signal IO_PAD264
signal IO_PAD266
signal IO_PAD267
signal IO_PAD268
signal IO_PAD270
signal IO_PAD271
signal IO_PAD272
signal IO_PAD274
signal IO_PAD276
signal IO_PAD277
signal IO_PAD278
signal IO_PAD28
signal IO_PAD280
signal IO_PAD281
signal IO_PAD282
signal IO_PAD284
signal IO_PAD286
signal IO_PAD287
signal IO_PAD288
signal IO_PAD29
signal IO_PAD290
signal IO_PAD291
signal IO_PAD292
signal IO_PAD294
signal IO_PAD296
signal IO_PAD298
signal IO_PAD3
signal IO_PAD30
signal IO_PAD300
signal IO_PAD301
signal IO_PAD302
signal IO_PAD304
signal IO_PAD306
signal IO_PAD307
signal IO_PAD308
signal IO_PAD309
signal IO_PAD31
signal IO_PAD310
signal IO_PAD312
signal IO_PAD313
signal IO_PAD314
signal IO_PAD315
signal IO_PAD316
signal IO_PAD317
signal IO_PAD318
signal IO_PAD319
signal IO_PAD32
signal IO_PAD320
signal IO_PAD322
signal IO_PAD324
signal IO_PAD326
signal IO_PAD328
signal IO_PAD329
signal IO_PAD330
signal IO_PAD331
signal IO_PAD332
signal IO_PAD334
signal IO_PAD336
signal IO_PAD337
signal IO_PAD338
signal IO_PAD339
signal IO_PAD34
signal IO_PAD340
signal IO_PAD342
signal IO_PAD343
signal IO_PAD345
signal IO_PAD346
signal IO_PAD347
signal IO_PAD35
signal IO_PAD353
signal IO_PAD354
signal IO_PAD355
signal IO_PAD356
signal IO_PAD357
signal IO_PAD358
signal IO_PAD36
signal IO_PAD360
signal IO_PAD361
signal IO_PAD362
signal IO_PAD364
signal IO_PAD365
signal IO_PAD366
signal IO_PAD368
signal IO_PAD37
signal IO_PAD370
signal IO_PAD371
signal IO_PAD372
signal IO_PAD373
signal IO_PAD374
signal IO_PAD376
signal IO_PAD378
signal IO_PAD38
signal IO_PAD380
signal IO_PAD382
signal IO_PAD383
signal IO_PAD384
signal IO_PAD386
signal IO_PAD388
signal IO_PAD389
signal IO_PAD39
signal IO_PAD390
signal IO_PAD391
signal IO_PAD392
signal IO_PAD393
signal IO_PAD394
signal IO_PAD395
signal IO_PAD396
signal IO_PAD397
signal IO_PAD398
signal IO_PAD399
signal IO_PAD4
signal IO_PAD40
signal IO_PAD400
signal IO_PAD402
signal IO_PAD404
signal IO_PAD406
signal IO_PAD408
signal IO_PAD41
signal IO_PAD410
signal IO_PAD411
signal IO_PAD412
signal IO_PAD414
signal IO_PAD416
signal IO_PAD417
signal IO_PAD418
signal IO_PAD419
signal IO_PAD42
signal IO_PAD421
signal IO_PAD423
signal IO_PAD424
signal IO_PAD425
signal IO_PAD427
signal IO_PAD429
signal IO_PAD431
signal IO_PAD433
signal IO_PAD435
signal IO_PAD436
signal IO_PAD437
signal IO_PAD438
signal IO_PAD439
signal IO_PAD44
signal IO_PAD440
signal IO_PAD441
signal IO_PAD442
signal IO_PAD443
signal IO_PAD444
signal IO_PAD445
signal IO_PAD446
signal IO_PAD447
signal IO_PAD449
signal IO_PAD451
signal IO_PAD452
signal IO_PAD453
signal IO_PAD455
signal IO_PAD457
signal IO_PAD459
signal IO_PAD46
signal IO_PAD461
signal IO_PAD462
signal IO_PAD463
signal IO_PAD464
signal IO_PAD465
signal IO_PAD467
signal IO_PAD469
signal IO_PAD470
signal IO_PAD471
signal IO_PAD473
signal IO_PAD474
signal IO_PAD475
signal IO_PAD477
signal IO_PAD478
signal IO_PAD479
signal IO_PAD48
signal IO_PAD480
signal IO_PAD481
signal IO_PAD482
signal IO_PAD488
signal IO_PAD489
signal IO_PAD491
signal IO_PAD492
signal IO_PAD493
signal IO_PAD495
signal IO_PAD496
signal IO_PAD497
signal IO_PAD498
signal IO_PAD499
signal IO_PAD50
signal IO_PAD501
signal IO_PAD503
signal IO_PAD504
signal IO_PAD505
signal IO_PAD506
signal IO_PAD507
signal IO_PAD509
signal IO_PAD51
signal IO_PAD511
signal IO_PAD513
signal IO_PAD515
signal IO_PAD516
signal IO_PAD517
signal IO_PAD518
signal IO_PAD519
signal IO_PAD52
signal IO_PAD520
signal IO_PAD521
signal IO_PAD522
signal IO_PAD523
signal IO_PAD525
signal IO_PAD526
signal IO_PAD527
signal IO_PAD528
signal IO_PAD529
signal IO_PAD53
signal IO_PAD531
signal IO_PAD533
signal IO_PAD534
signal IO_PAD535
signal IO_PAD537
signal IO_PAD539
signal IO_PAD54
signal IO_PAD541
signal IO_PAD543
signal IO_PAD544
signal IO_PAD545
signal IO_PAD547
signal IO_PAD548
signal IO_PAD549
signal IO_PAD551
signal IO_PAD553
signal IO_PAD554
signal IO_PAD555
signal IO_PAD56
signal IO_PAD58
signal IO_PAD59
signal IO_PAD6
signal IO_PAD60
signal IO_PAD61
signal IO_PAD62
signal IO_PAD64
signal IO_PAD65
signal IO_PAD67
signal IO_PAD68
signal IO_PAD69
signal IO_PAD75
signal IO_PAD76
signal IO_PAD77
signal IO_PAD78
signal IO_PAD79
signal IO_PAD8
signal IO_PAD80
signal IO_PAD82
signal IO_PAD83
signal IO_PAD84
signal IO_PAD86
signal IO_PAD87
signal IO_PAD88
signal IO_PAD9
signal IO_PAD90
signal IO_PAD92
signal IO_PAD93
signal IO_PAD94
signal IO_PAD95
signal IO_PAD96
signal IO_PAD98
signal M0_PAD412
signal M1_PAD411
signal M2_PAD413


register	BYPASS		1
register	BSR		1187
register	DEVICE_ID	32

instruction length 6

instruction	IDCODE		001001	DEVICE_ID
instruction	SAMPLE/PRELOAD	000001	BSR
instruction	INTEST		000111	BSR
instruction	HIGHZ		001010	BYPASS
instruction	BYPASS		111111	BYPASS
instruction	USERCODE	001000	DEVICE_ID
instruction	EXTEST		000000	BSR

bit  0 C 1 *
bit  1 O ? IO_PAD488 0 1 Z
bit  2 I ? IO_PAD488
bit  3 C 1 *
bit  4 O ? IO_PAD489 3 1 Z
bit  5 I ? IO_PAD489
bit  6 C 1 *
bit  7 O ? IO_PAD491 6 1 Z
bit  8 I ? IO_PAD491
bit  9 C 1 *
bit 10 O ? IO_PAD492 9 1 Z
bit 11 I ? IO_PAD492
bit 12 C 1 *
bit 13 O ? IO_PAD493 12 1 Z
bit 14 I ? IO_PAD493
bit 15 C 1 *
bit 16 O ? IO_PAD495 15 1 Z
bit 17 I ? IO_PAD495
bit 18 C 1 *
bit 19 O ? IO_PAD496 18 1 Z
bit 20 I ? IO_PAD496
bit 21 C 1 *
bit 22 O ? IO_PAD497 21 1 Z
bit 23 I ? IO_PAD497
bit 24 C 1 *
bit 25 O ? IO_PAD498 24 1 Z
bit 26 I ? IO_PAD498
bit 27 C 1 *
bit 28 O ? IO_PAD499 27 1 Z
bit 29 I ? IO_PAD499
bit 30 C 1 *
bit 31 O ? IO_PAD501 30 1 Z
bit 32 I ? IO_PAD501
bit 33 C 1 *
bit 34 O ? IO_PAD503 33 1 Z
bit 35 I ? IO_PAD503
bit 36 C 1 *
bit 37 O ? IO_PAD504 36 1 Z
bit 38 I ? IO_PAD504
bit 39 C 1 *
bit 40 O ? IO_PAD505 39 1 Z
bit 41 I ? IO_PAD505
bit 42 C 1 *
bit 43 O ? IO_PAD506 42 1 Z
bit 44 I ? IO_PAD506
bit 45 C 1 *
bit 46 O ? IO_PAD507 45 1 Z
bit 47 I ? IO_PAD507
bit 48 C 1 *
bit 49 O ? IO_PAD509 48 1 Z
bit 50 I ? IO_PAD509
bit 51 C 1 *
bit 52 O ? IO_PAD511 51 1 Z
bit 53 I ? IO_PAD511
bit 54 C 1 *
bit 55 O ? IO_PAD513 54 1 Z
bit 56 I ? IO_PAD513
bit 57 C 1 *
bit 58 O ? IO_PAD515 57 1 Z
bit 59 I ? IO_PAD515
bit 60 C 1 *
bit 61 O ? IO_PAD516 60 1 Z
bit 62 I ? IO_PAD516
bit 63 C 1 *
bit 64 O ? IO_PAD517 63 1 Z
bit 65 I ? IO_PAD517
bit 66 C 1 *
bit 67 O ? IO_PAD518 66 1 Z
bit 68 I ? IO_PAD518
bit 69 C 1 *
bit 70 O ? IO_PAD519 69 1 Z
bit 71 I ? IO_PAD519
bit 72 C 1 *
bit 73 O ? IO_PAD520 72 1 Z
bit 74 I ? IO_PAD520
bit 75 C 1 *
bit 76 O ? IO_PAD521 75 1 Z
bit 77 I ? IO_PAD521
bit 78 C 1 *
bit 79 O ? IO_PAD522 78 1 Z
bit 80 I ? IO_PAD522
bit 81 C 1 *
bit 82 O ? IO_PAD523 81 1 Z
bit 83 I ? IO_PAD523
bit 84 C 1 *
bit 85 O ? IO_PAD525 84 1 Z
bit 86 I ? IO_PAD525
bit 87 C 1 *
bit 88 O ? IO_PAD526 87 1 Z
bit 89 I ? IO_PAD526
bit 90 C 1 *
bit 91 O ? IO_PAD527 90 1 Z
bit 92 I ? IO_PAD527
bit 93 C 1 *
bit 94 O ? IO_PAD528 93 1 Z
bit 95 I ? IO_PAD528
bit 96 C 1 *
bit 97 O ? IO_PAD529 96 1 Z
bit 98 I ? IO_PAD529
bit 99 C 1 *
bit 100 O ? IO_PAD531 99 1 Z
bit 101 I ? IO_PAD531
bit 102 C 1 *
bit 103 O ? IO_PAD533 102 1 Z
bit 104 I ? IO_PAD533
bit 105 C 1 *
bit 106 O ? IO_PAD534 105 1 Z
bit 107 I ? IO_PAD534
bit 108 C 1 *
bit 109 O ? IO_PAD535 108 1 Z
bit 110 I ? IO_PAD535
bit 111 C 1 *
bit 112 O ? IO_PAD537 111 1 Z
bit 113 I ? IO_PAD537
bit 114 C 1 *
bit 115 O ? IO_PAD539 114 1 Z
bit 116 I ? IO_PAD539
bit 117 C 1 *
bit 118 O ? IO_PAD541 117 1 Z
bit 119 I ? IO_PAD541
bit 120 C 1 *
bit 121 O ? IO_PAD543 120 1 Z
bit 122 I ? IO_PAD543
bit 123 C 1 *
bit 124 O ? IO_PAD544 123 1 Z
bit 125 I ? IO_PAD544
bit 126 C 1 *
bit 127 O ? IO_PAD545 126 1 Z
bit 128 I ? IO_PAD545
bit 129 C 1 *
bit 130 O ? IO_PAD547 129 1 Z
bit 131 I ? IO_PAD547
bit 132 C 1 *
bit 133 O ? IO_PAD548 132 1 Z
bit 134 I ? IO_PAD548
bit 135 C 1 *
bit 136 O ? IO_PAD549 135 1 Z
bit 137 I ? IO_PAD549
bit 138 C 1 *
bit 139 O ? IO_PAD551 138 1 Z
bit 140 I ? IO_PAD551
bit 141 C 1 *
bit 142 O ? IO_PAD553 141 1 Z
bit 143 I ? IO_PAD553
bit 144 C 1 *
bit 145 O ? IO_PAD554 144 1 Z
bit 146 I ? IO_PAD554
bit 147 C 1 *
bit 148 O ? IO_PAD555 147 1 Z
bit 149 I ? IO_PAD555
bit 150 C 1 *
bit 151 O ? IO_PAD2 150 1 Z
bit 152 I ? IO_PAD2
bit 153 C 1 *
bit 154 O ? IO_PAD3 153 1 Z
bit 155 I ? IO_PAD3
bit 156 C 1 *
bit 157 O ? IO_PAD4 156 1 Z
bit 158 I ? IO_PAD4
bit 159 C 1 *
bit 160 O ? IO_PAD6 159 1 Z
bit 161 I ? IO_PAD6
bit 162 C 1 *
bit 163 O ? IO_PAD8 162 1 Z
bit 164 I ? IO_PAD8
bit 165 C 1 *
bit 166 O ? IO_PAD9 165 1 Z
bit 167 I ? IO_PAD9
bit 168 C 1 *
bit 169 O ? IO_PAD10 168 1 Z
bit 170 I ? IO_PAD10
bit 171 C 1 *
bit 172 O ? IO_PAD12 171 1 Z
bit 173 I ? IO_PAD12
bit 174 C 1 *
bit 175 O ? IO_PAD13 174 1 Z
bit 176 I ? IO_PAD13
bit 177 C 1 *
bit 178 O ? IO_PAD14 177 1 Z
bit 179 I ? IO_PAD14
bit 180 C 1 *
bit 181 O ? IO_PAD16 180 1 Z
bit 182 I ? IO_PAD16
bit 183 C 1 *
bit 184 O ? IO_PAD18 183 1 Z
bit 185 I ? IO_PAD18
bit 186 C 1 *
bit 187 O ? IO_PAD20 186 1 Z
bit 188 I ? IO_PAD20
bit 189 C 1 *
bit 190 O ? IO_PAD22 189 1 Z
bit 191 I ? IO_PAD22
bit 192 C 1 *
bit 193 O ? IO_PAD23 192 1 Z
bit 194 I ? IO_PAD23
bit 195 C 1 *
bit 196 O ? IO_PAD24 195 1 Z
bit 197 I ? IO_PAD24
bit 198 C 1 *
bit 199 O ? IO_PAD26 198 1 Z
bit 200 I ? IO_PAD26
bit 201 C 1 *
bit 202 O ? IO_PAD28 201 1 Z
bit 203 I ? IO_PAD28
bit 204 C 1 *
bit 205 O ? IO_PAD29 204 1 Z
bit 206 I ? IO_PAD29
bit 207 C 1 *
bit 208 O ? IO_PAD30 207 1 Z
bit 209 I ? IO_PAD30
bit 210 C 1 *
bit 211 O ? IO_PAD31 210 1 Z
bit 212 I ? IO_PAD31
bit 213 C 1 *
bit 214 O ? IO_PAD32 213 1 Z
bit 215 I ? IO_PAD32
bit 216 C 1 *
bit 217 O ? IO_PAD34 216 1 Z
bit 218 I ? IO_PAD34
bit 219 C 1 *
bit 220 O ? IO_PAD35 219 1 Z
bit 221 I ? IO_PAD35
bit 222 C 1 *
bit 223 O ? IO_PAD36 222 1 Z
bit 224 I ? IO_PAD36
bit 225 C 1 *
bit 226 O ? IO_PAD37 225 1 Z
bit 227 I ? IO_PAD37
bit 228 C 1 *
bit 229 O ? IO_PAD38 228 1 Z
bit 230 I ? IO_PAD38
bit 231 C 1 *
bit 232 O ? IO_PAD39 231 1 Z
bit 233 I ? IO_PAD39
bit 234 C 1 *
bit 235 O ? IO_PAD40 234 1 Z
bit 236 I ? IO_PAD40
bit 237 C 1 *
bit 238 O ? IO_PAD41 237 1 Z
bit 239 I ? IO_PAD41
bit 240 C 1 *
bit 241 O ? IO_PAD42 240 1 Z
bit 242 I ? IO_PAD42
bit 243 C 1 *
bit 244 O ? IO_PAD44 243 1 Z
bit 245 I ? IO_PAD44
bit 246 C 1 *
bit 247 O ? IO_PAD46 246 1 Z
bit 248 I ? IO_PAD46
bit 249 C 1 *
bit 250 O ? IO_PAD48 249 1 Z
bit 251 I ? IO_PAD48
bit 252 C 1 *
bit 253 O ? IO_PAD50 252 1 Z
bit 254 I ? IO_PAD50
bit 255 C 1 *
bit 256 O ? IO_PAD51 255 1 Z
bit 257 I ? IO_PAD51
bit 258 C 1 *
bit 259 O ? IO_PAD52 258 1 Z
bit 260 I ? IO_PAD52
bit 261 C 1 *
bit 262 O ? IO_PAD53 261 1 Z
bit 263 I ? IO_PAD53
bit 264 C 1 *
bit 265 O ? IO_PAD54 264 1 Z
bit 266 I ? IO_PAD54
bit 267 C 1 *
bit 268 O ? IO_PAD56 267 1 Z
bit 269 I ? IO_PAD56
bit 270 C 1 *
bit 271 O ? IO_PAD58 270 1 Z
bit 272 I ? IO_PAD58
bit 273 C 1 *
bit 274 O ? IO_PAD59 273 1 Z
bit 275 I ? IO_PAD59
bit 276 C 1 *
bit 277 O ? IO_PAD60 276 1 Z
bit 278 I ? IO_PAD60
bit 279 C 1 *
bit 280 O ? IO_PAD61 279 1 Z
bit 281 I ? IO_PAD61
bit 282 C 1 *
bit 283 O ? IO_PAD62 282 1 Z
bit 284 I ? IO_PAD62
bit 285 C 1 *
bit 286 O ? IO_PAD64 285 1 Z
bit 287 I ? IO_PAD64
bit 288 C 1 *
bit 289 O ? IO_PAD65 288 1 Z
bit 290 I ? IO_PAD65
bit 291 C 1 *
bit 292 O ? IO_PAD67 291 1 Z
bit 293 I ? IO_PAD67
bit 294 C 1 *
bit 295 O ? IO_PAD68 294 1 Z
bit 296 I ? IO_PAD68
bit 297 C 1 *
bit 298 O ? IO_PAD69 297 1 Z
bit 299 I ? IO_PAD69
bit 300 I ? HSWAP_EN_PAD70
bit 301 X 1 *
bit 302 C 1 *
bit 303 O ? IO_PAD75 302 1 Z
bit 304 I ? IO_PAD75
bit 305 C 1 *
bit 306 O ? IO_PAD76 305 1 Z
bit 307 I ? IO_PAD76
bit 308 C 1 *
bit 309 O ? IO_PAD77 308 1 Z
bit 310 I ? IO_PAD77
bit 311 C 1 *
bit 312 O ? IO_PAD78 311 1 Z
bit 313 I ? IO_PAD78
bit 314 C 1 *
bit 315 O ? IO_PAD79 314 1 Z
bit 316 I ? IO_PAD79
bit 317 C 1 *
bit 318 O ? IO_PAD80 317 1 Z
bit 319 I ? IO_PAD80
bit 320 C 1 *
bit 321 O ? IO_PAD82 320 1 Z
bit 322 I ? IO_PAD82
bit 323 C 1 *
bit 324 O ? IO_PAD83 323 1 Z
bit 325 I ? IO_PAD83
bit 326 C 1 *
bit 327 O ? IO_PAD84 326 1 Z
bit 328 I ? IO_PAD84
bit 329 C 1 *
bit 330 O ? IO_PAD86 329 1 Z
bit 331 I ? IO_PAD86
bit 332 C 1 *
bit 333 O ? IO_PAD87 332 1 Z
bit 334 I ? IO_PAD87
bit 335 C 1 *
bit 336 O ? IO_PAD88 335 1 Z
bit 337 I ? IO_PAD88
bit 338 C 1 *
bit 339 O ? IO_PAD90 338 1 Z
bit 340 I ? IO_PAD90
bit 341 C 1 *
bit 342 O ? IO_PAD92 341 1 Z
bit 343 I ? IO_PAD92
bit 344 C 1 *
bit 345 O ? IO_PAD93 344 1 Z
bit 346 I ? IO_PAD93
bit 347 C 1 *
bit 348 O ? IO_PAD94 347 1 Z
bit 349 I ? IO_PAD94
bit 350 C 1 *
bit 351 O ? IO_PAD95 350 1 Z
bit 352 I ? IO_PAD95
bit 353 C 1 *
bit 354 O ? IO_PAD96 353 1 Z
bit 355 I ? IO_PAD96
bit 356 C 1 *
bit 357 O ? IO_PAD98 356 1 Z
bit 358 I ? IO_PAD98
bit 359 C 1 *
bit 360 O ? IO_PAD100 359 1 Z
bit 361 I ? IO_PAD100
bit 362 C 1 *
bit 363 O ? IO_PAD102 362 1 Z
bit 364 I ? IO_PAD102
bit 365 C 1 *
bit 366 O ? IO_PAD104 365 1 Z
bit 367 I ? IO_PAD104
bit 368 C 1 *
bit 369 O ? IO_PAD105 368 1 Z
bit 370 I ? IO_PAD105
bit 371 C 1 *
bit 372 O ? IO_PAD106 371 1 Z
bit 373 I ? IO_PAD106
bit 374 C 1 *
bit 375 O ? IO_PAD108 374 1 Z
bit 376 I ? IO_PAD108
bit 377 C 1 *
bit 378 O ? IO_PAD110 377 1 Z
bit 379 I ? IO_PAD110
bit 380 C 1 *
bit 381 O ? IO_PAD111 380 1 Z
bit 382 I ? IO_PAD111
bit 383 C 1 *
bit 384 O ? IO_PAD112 383 1 Z
bit 385 I ? IO_PAD112
bit 386 C 1 *
bit 387 O ? IO_PAD113 386 1 Z
bit 388 I ? IO_PAD113
bit 389 C 1 *
bit 390 O ? IO_PAD114 389 1 Z
bit 391 I ? IO_PAD114
bit 392 C 1 *
bit 393 O ? IO_PAD115 392 1 Z
bit 394 I ? IO_PAD115
bit 395 C 1 *
bit 396 O ? IO_PAD116 395 1 Z
bit 397 I ? IO_PAD116
bit 398 C 1 *
bit 399 O ? IO_PAD117 398 1 Z
bit 400 I ? IO_PAD117
bit 401 C 1 *
bit 402 O ? IO_PAD118 401 1 Z
bit 403 I ? IO_PAD118
bit 404 C 1 *
bit 405 O ? IO_PAD119 404 1 Z
bit 406 I ? IO_PAD119
bit 407 C 1 *
bit 408 O ? IO_PAD120 407 1 Z
bit 409 I ? IO_PAD120
bit 410 C 1 *
bit 411 O ? IO_PAD121 410 1 Z
bit 412 I ? IO_PAD121
bit 413 C 1 *
bit 414 O ? IO_PAD122 413 1 Z
bit 415 I ? IO_PAD122
bit 416 C 1 *
bit 417 O ? IO_PAD124 416 1 Z
bit 418 I ? IO_PAD124
bit 419 C 1 *
bit 420 O ? IO_PAD126 419 1 Z
bit 421 I ? IO_PAD126
bit 422 C 1 *
bit 423 O ? IO_PAD128 422 1 Z
bit 424 I ? IO_PAD128
bit 425 C 1 *
bit 426 O ? IO_PAD130 425 1 Z
bit 427 I ? IO_PAD130
bit 428 C 1 *
bit 429 O ? IO_PAD132 428 1 Z
bit 430 I ? IO_PAD132
bit 431 C 1 *
bit 432 O ? IO_PAD133 431 1 Z
bit 433 I ? IO_PAD133
bit 434 C 1 *
bit 435 O ? IO_PAD134 434 1 Z
bit 436 I ? IO_PAD134
bit 437 C 1 *
bit 438 O ? IO_PAD136 437 1 Z
bit 439 I ? IO_PAD136
bit 440 C 1 *
bit 441 O ? IO_PAD138 440 1 Z
bit 442 I ? IO_PAD138
bit 443 C 1 *
bit 444 O ? IO_PAD139 443 1 Z
bit 445 I ? IO_PAD139
bit 446 C 1 *
bit 447 O ? IO_PAD140 446 1 Z
bit 448 I ? IO_PAD140
bit 449 C 1 *
bit 450 O ? IO_PAD141 449 1 Z
bit 451 I ? IO_PAD141
bit 452 C 1 *
bit 453 O ? IO_PAD143 452 1 Z
bit 454 I ? IO_PAD143
bit 455 C 1 *
bit 456 O ? IO_PAD145 455 1 Z
bit 457 I ? IO_PAD145
bit 458 C 1 *
bit 459 O ? IO_PAD146 458 1 Z
bit 460 I ? IO_PAD146
bit 461 C 1 *
bit 462 O ? IO_PAD147 461 1 Z
bit 463 I ? IO_PAD147
bit 464 C 1 *
bit 465 O ? IO_PAD149 464 1 Z
bit 466 I ? IO_PAD149
bit 467 C 1 *
bit 468 O ? IO_PAD151 467 1 Z
bit 469 I ? IO_PAD151
bit 470 C 1 *
bit 471 O ? IO_PAD153 470 1 Z
bit 472 I ? IO_PAD153
bit 473 C 1 *
bit 474 O ? IO_PAD155 473 1 Z
bit 475 I ? IO_PAD155
bit 476 C 1 *
bit 477 O ? IO_PAD157 476 1 Z
bit 478 I ? IO_PAD157
bit 479 C 1 *
bit 480 O ? IO_PAD158 479 1 Z
bit 481 I ? IO_PAD158
bit 482 C 1 *
bit 483 O ? IO_PAD159 482 1 Z
bit 484 I ? IO_PAD159
bit 485 C 1 *
bit 486 O ? IO_PAD160 485 1 Z
bit 487 I ? IO_PAD160
bit 488 C 1 *
bit 489 O ? IO_PAD161 488 1 Z
bit 490 I ? IO_PAD161
bit 491 C 1 *
bit 492 O ? IO_PAD162 491 1 Z
bit 493 I ? IO_PAD162
bit 494 C 1 *
bit 495 O ? IO_PAD163 494 1 Z
bit 496 I ? IO_PAD163
bit 497 C 1 *
bit 498 O ? IO_PAD164 497 1 Z
bit 499 I ? IO_PAD164
bit 500 C 1 *
bit 501 O ? IO_PAD165 500 1 Z
bit 502 I ? IO_PAD165
bit 503 C 1 *
bit 504 O ? IO_PAD166 503 1 Z
bit 505 I ? IO_PAD166
bit 506 C 1 *
bit 507 O ? IO_PAD167 506 1 Z
bit 508 I ? IO_PAD167
bit 509 C 1 *
bit 510 O ? IO_PAD168 509 1 Z
bit 511 I ? IO_PAD168
bit 512 C 1 *
bit 513 O ? IO_PAD169 512 1 Z
bit 514 I ? IO_PAD169
bit 515 C 1 *
bit 516 O ? IO_PAD171 515 1 Z
bit 517 I ? IO_PAD171
bit 518 C 1 *
bit 519 O ? IO_PAD173 518 1 Z
bit 520 I ? IO_PAD173
bit 521 C 1 *
bit 522 O ? IO_PAD174 521 1 Z
bit 523 I ? IO_PAD174
bit 524 C 1 *
bit 525 O ? IO_PAD175 524 1 Z
bit 526 I ? IO_PAD175
bit 527 C 1 *
bit 528 O ? IO_PAD177 527 1 Z
bit 529 I ? IO_PAD177
bit 530 C 1 *
bit 531 O ? IO_PAD179 530 1 Z
bit 532 I ? IO_PAD179
bit 533 C 1 *
bit 534 O ? IO_PAD181 533 1 Z
bit 535 I ? IO_PAD181
bit 536 C 1 *
bit 537 O ? IO_PAD183 536 1 Z
bit 538 I ? IO_PAD183
bit 539 C 1 *
bit 540 O ? IO_PAD184 539 1 Z
bit 541 I ? IO_PAD184
bit 542 C 1 *
bit 543 O ? IO_PAD185 542 1 Z
bit 544 I ? IO_PAD185
bit 545 C 1 *
bit 546 O ? IO_PAD186 545 1 Z
bit 547 I ? IO_PAD186
bit 548 C 1 *
bit 549 O ? IO_PAD187 548 1 Z
bit 550 I ? IO_PAD187
bit 551 C 1 *
bit 552 O ? IO_PAD189 551 1 Z
bit 553 I ? IO_PAD189
bit 554 C 1 *
bit 555 O ? IO_PAD191 554 1 Z
bit 556 I ? IO_PAD191
bit 557 C 1 *
bit 558 O ? IO_PAD192 557 1 Z
bit 559 I ? IO_PAD192
bit 560 C 1 *
bit 561 O ? IO_PAD193 560 1 Z
bit 562 I ? IO_PAD193
bit 563 C 1 *
bit 564 O ? IO_PAD195 563 1 Z
bit 565 I ? IO_PAD195
bit 566 C 1 *
bit 567 O ? IO_PAD196 566 1 Z
bit 568 I ? IO_PAD196
bit 569 C 1 *
bit 570 O ? IO_PAD197 569 1 Z
bit 571 I ? IO_PAD197
bit 572 C 1 *
bit 573 O ? IO_PAD199 572 1 Z
bit 574 I ? IO_PAD199
bit 575 C 1 *
bit 576 O ? IO_PAD200 575 1 Z
bit 577 I ? IO_PAD200
bit 578 C 1 *
bit 579 O ? IO_PAD201 578 1 Z
bit 580 I ? IO_PAD201
bit 581 C 1 *
bit 582 O ? IO_PAD202 581 1 Z
bit 583 I ? IO_PAD202
bit 584 C 1 *
bit 585 O ? IO_PAD203 584 1 Z
bit 586 I ? IO_PAD203
bit 587 C 1 *
bit 588 O ? IO_PAD204 587 1 Z
bit 589 I ? IO_PAD204
bit 590 I ? M1_PAD207
bit 591 I ? M0_PAD208
bit 592 I ? M2_PAD209
bit 593 C 1 *
bit 594 O ? IO_PAD210 593 1 Z
bit 595 I ? IO_PAD210
bit 596 C 1 *
bit 597 O ? IO_PAD211 596 1 Z
bit 598 I ? IO_PAD211
bit 599 C 1 *
bit 600 O ? IO_PAD214 599 1 Z
bit 601 I ? IO_PAD214
bit 602 C 1 *
bit 603 O ? IO_PAD215 602 1 Z
bit 604 I ? IO_PAD215
bit 605 C 1 *
bit 606 O ? IO_PAD216 605 1 Z
bit 607 I ? IO_PAD216
bit 608 C 1 *
bit 609 O ? IO_PAD218 608 1 Z
bit 610 I ? IO_PAD218
bit 611 C 1 *
bit 612 O ? IO_PAD219 611 1 Z
bit 613 I ? IO_PAD219
bit 614 C 1 *
bit 615 O ? IO_PAD220 614 1 Z
bit 616 I ? IO_PAD220
bit 617 C 1 *
bit 618 O ? IO_PAD221 617 1 Z
bit 619 I ? IO_PAD221
bit 620 C 1 *
bit 621 O ? IO_PAD222 620 1 Z
bit 622 I ? IO_PAD222
bit 623 C 1 *
bit 624 O ? IO_PAD224 623 1 Z
bit 625 I ? IO_PAD224
bit 626 C 1 *
bit 627 O ? IO_PAD226 626 1 Z
bit 628 I ? IO_PAD226
bit 629 C 1 *
bit 630 O ? IO_PAD227 629 1 Z
bit 631 I ? IO_PAD227
bit 632 C 1 *
bit 633 O ? IO_PAD228 632 1 Z
bit 634 I ? IO_PAD228
bit 635 C 1 *
bit 636 O ? IO_PAD229 635 1 Z
bit 637 I ? IO_PAD229
bit 638 C 1 *
bit 639 O ? IO_PAD230 638 1 Z
bit 640 I ? IO_PAD230
bit 641 C 1 *
bit 642 O ? IO_PAD232 641 1 Z
bit 643 I ? IO_PAD232
bit 644 C 1 *
bit 645 O ? IO_PAD234 644 1 Z
bit 646 I ? IO_PAD234
bit 647 C 1 *
bit 648 O ? IO_PAD236 647 1 Z
bit 649 I ? IO_PAD236
bit 650 C 1 *
bit 651 O ? IO_PAD238 650 1 Z
bit 652 I ? IO_PAD238
bit 653 C 1 *
bit 654 O ? IO_PAD239 653 1 Z
bit 655 I ? IO_PAD239
bit 656 C 1 *
bit 657 O ? IO_PAD240 656 1 Z
bit 658 I ? IO_PAD240
bit 659 C 1 *
bit 660 O ? IO_PAD241 659 1 Z
bit 661 I ? IO_PAD241
bit 662 C 1 *
bit 663 O ? IO_PAD242 662 1 Z
bit 664 I ? IO_PAD242
bit 665 C 1 *
bit 666 O ? IO_PAD243 665 1 Z
bit 667 I ? IO_PAD243
bit 668 C 1 *
bit 669 O ? IO_PAD244 668 1 Z
bit 670 I ? IO_PAD244
bit 671 C 1 *
bit 672 O ? IO_PAD245 671 1 Z
bit 673 I ? IO_PAD245
bit 674 C 1 *
bit 675 O ? IO_PAD246 674 1 Z
bit 676 I ? IO_PAD246
bit 677 C 1 *
bit 678 O ? IO_PAD248 677 1 Z
bit 679 I ? IO_PAD248
bit 680 C 1 *
bit 681 O ? IO_PAD249 680 1 Z
bit 682 I ? IO_PAD249
bit 683 C 1 *
bit 684 O ? IO_PAD250 683 1 Z
bit 685 I ? IO_PAD250
bit 686 C 1 *
bit 687 O ? IO_PAD251 686 1 Z
bit 688 I ? IO_PAD251
bit 689 C 1 *
bit 690 O ? IO_PAD252 689 1 Z
bit 691 I ? IO_PAD252
bit 692 C 1 *
bit 693 O ? IO_PAD254 692 1 Z
bit 694 I ? IO_PAD254
bit 695 C 1 *
bit 696 O ? IO_PAD256 695 1 Z
bit 697 I ? IO_PAD256
bit 698 C 1 *
bit 699 O ? IO_PAD257 698 1 Z
bit 700 I ? IO_PAD257
bit 701 C 1 *
bit 702 O ? IO_PAD258 701 1 Z
bit 703 I ? IO_PAD258
bit 704 C 1 *
bit 705 O ? IO_PAD260 704 1 Z
bit 706 I ? IO_PAD260
bit 707 C 1 *
bit 708 O ? IO_PAD262 707 1 Z
bit 709 I ? IO_PAD262
bit 710 C 1 *
bit 711 O ? IO_PAD264 710 1 Z
bit 712 I ? IO_PAD264
bit 713 C 1 *
bit 714 O ? IO_PAD266 713 1 Z
bit 715 I ? IO_PAD266
bit 716 C 1 *
bit 717 O ? IO_PAD267 716 1 Z
bit 718 I ? IO_PAD267
bit 719 C 1 *
bit 720 O ? IO_PAD268 719 1 Z
bit 721 I ? IO_PAD268
bit 722 C 1 *
bit 723 O ? IO_PAD270 722 1 Z
bit 724 I ? IO_PAD270
bit 725 C 1 *
bit 726 O ? IO_PAD271 725 1 Z
bit 727 I ? IO_PAD271
bit 728 C 1 *
bit 729 O ? IO_PAD272 728 1 Z
bit 730 I ? IO_PAD272
bit 731 C 1 *
bit 732 O ? IO_PAD274 731 1 Z
bit 733 I ? IO_PAD274
bit 734 C 1 *
bit 735 O ? IO_PAD276 734 1 Z
bit 736 I ? IO_PAD276
bit 737 C 1 *
bit 738 O ? IO_PAD277 737 1 Z
bit 739 I ? IO_PAD277
bit 740 C 1 *
bit 741 O ? IO_PAD278 740 1 Z
bit 742 I ? IO_PAD278
bit 743 C 1 *
bit 744 O ? IO_PAD280 743 1 Z
bit 745 I ? IO_PAD280
bit 746 C 1 *
bit 747 O ? IO_PAD281 746 1 Z
bit 748 I ? IO_PAD281
bit 749 C 1 *
bit 750 O ? IO_PAD282 749 1 Z
bit 751 I ? IO_PAD282
bit 752 C 1 *
bit 753 O ? IO_PAD284 752 1 Z
bit 754 I ? IO_PAD284
bit 755 C 1 *
bit 756 O ? IO_PAD286 755 1 Z
bit 757 I ? IO_PAD286
bit 758 C 1 *
bit 759 O ? IO_PAD287 758 1 Z
bit 760 I ? IO_PAD287
bit 761 C 1 *
bit 762 O ? IO_PAD288 761 1 Z
bit 763 I ? IO_PAD288
bit 764 C 1 *
bit 765 O ? IO_PAD290 764 1 Z
bit 766 I ? IO_PAD290
bit 767 C 1 *
bit 768 O ? IO_PAD291 767 1 Z
bit 769 I ? IO_PAD291
bit 770 C 1 *
bit 771 O ? IO_PAD292 770 1 Z
bit 772 I ? IO_PAD292
bit 773 C 1 *
bit 774 O ? IO_PAD294 773 1 Z
bit 775 I ? IO_PAD294
bit 776 C 1 *
bit 777 O ? IO_PAD296 776 1 Z
bit 778 I ? IO_PAD296
bit 779 C 1 *
bit 780 O ? IO_PAD298 779 1 Z
bit 781 I ? IO_PAD298
bit 782 C 1 *
bit 783 O ? IO_PAD300 782 1 Z
bit 784 I ? IO_PAD300
bit 785 C 1 *
bit 786 O ? IO_PAD301 785 1 Z
bit 787 I ? IO_PAD301
bit 788 C 1 *
bit 789 O ? IO_PAD302 788 1 Z
bit 790 I ? IO_PAD302
bit 791 C 1 *
bit 792 O ? IO_PAD304 791 1 Z
bit 793 I ? IO_PAD304
bit 794 C 1 *
bit 795 O ? IO_PAD306 794 1 Z
bit 796 I ? IO_PAD306
bit 797 C 1 *
bit 798 O ? IO_PAD307 797 1 Z
bit 799 I ? IO_PAD307
bit 800 C 1 *
bit 801 O ? IO_PAD308 800 1 Z
bit 802 I ? IO_PAD308
bit 803 C 1 *
bit 804 O ? IO_PAD309 803 1 Z
bit 805 I ? IO_PAD309
bit 806 C 1 *
bit 807 O ? IO_PAD310 806 1 Z
bit 808 I ? IO_PAD310
bit 809 C 1 *
bit 810 O ? IO_PAD312 809 1 Z
bit 811 I ? IO_PAD312
bit 812 C 1 *
bit 813 O ? IO_PAD313 812 1 Z
bit 814 I ? IO_PAD313
bit 815 C 1 *
bit 816 O ? IO_PAD314 815 1 Z
bit 817 I ? IO_PAD314
bit 818 C 1 *
bit 819 O ? IO_PAD315 818 1 Z
bit 820 I ? IO_PAD315
bit 821 C 1 *
bit 822 O ? IO_PAD316 821 1 Z
bit 823 I ? IO_PAD316
bit 824 C 1 *
bit 825 O ? IO_PAD317 824 1 Z
bit 826 I ? IO_PAD317
bit 827 C 1 *
bit 828 O ? IO_PAD318 827 1 Z
bit 829 I ? IO_PAD318
bit 830 C 1 *
bit 831 O ? IO_PAD319 830 1 Z
bit 832 I ? IO_PAD319
bit 833 C 1 *
bit 834 O ? IO_PAD320 833 1 Z
bit 835 I ? IO_PAD320
bit 836 C 1 *
bit 837 O ? IO_PAD322 836 1 Z
bit 838 I ? IO_PAD322
bit 839 C 1 *
bit 840 O ? IO_PAD324 839 1 Z
bit 841 I ? IO_PAD324
bit 842 C 1 *
bit 843 O ? IO_PAD326 842 1 Z
bit 844 I ? IO_PAD326
bit 845 C 1 *
bit 846 O ? IO_PAD328 845 1 Z
bit 847 I ? IO_PAD328
bit 848 C 1 *
bit 849 O ? IO_PAD329 848 1 Z
bit 850 I ? IO_PAD329
bit 851 C 1 *
bit 852 O ? IO_PAD330 851 1 Z
bit 853 I ? IO_PAD330
bit 854 C 1 *
bit 855 O ? IO_PAD331 854 1 Z
bit 856 I ? IO_PAD331
bit 857 C 1 *
bit 858 O ? IO_PAD332 857 1 Z
bit 859 I ? IO_PAD332
bit 860 C 1 *
bit 861 O ? IO_PAD334 860 1 Z
bit 862 I ? IO_PAD334
bit 863 C 1 *
bit 864 O ? IO_PAD336 863 1 Z
bit 865 I ? IO_PAD336
bit 866 C 1 *
bit 867 O ? IO_PAD337 866 1 Z
bit 868 I ? IO_PAD337
bit 869 C 1 *
bit 870 O ? IO_PAD338 869 1 Z
bit 871 I ? IO_PAD338
bit 872 C 1 *
bit 873 O ? IO_PAD339 872 1 Z
bit 874 I ? IO_PAD339
bit 875 C 1 *
bit 876 O ? IO_PAD340 875 1 Z
bit 877 I ? IO_PAD340
bit 878 C 1 *
bit 879 O ? IO_PAD342 878 1 Z
bit 880 I ? IO_PAD342
bit 881 C 1 *
bit 882 O ? IO_PAD343 881 1 Z
bit 883 I ? IO_PAD343
bit 884 C 1 *
bit 885 O ? IO_PAD345 884 1 Z
bit 886 I ? IO_PAD345
bit 887 C 1 *
bit 888 O ? IO_PAD346 887 1 Z
bit 889 I ? IO_PAD346
bit 890 C 1 *
bit 891 O ? IO_PAD347 890 1 Z
bit 892 I ? IO_PAD347
bit 893 C 1 *
bit 894 O ? DONE_PAD348 893 1 Z
bit 895 I ? DONE_PAD348
bit 896 C 1 *
bit 897 O ? CCLK_PAD349 896 1 Z
bit 898 I ? CCLK_PAD349
bit 899 C 1 *
bit 900 O ? IO_PAD353 899 1 Z
bit 901 I ? IO_PAD353
bit 902 C 1 *
bit 903 O ? IO_PAD354 902 1 Z
bit 904 I ? IO_PAD354
bit 905 C 1 *
bit 906 O ? IO_PAD355 905 1 Z
bit 907 I ? IO_PAD355
bit 908 C 1 *
bit 909 O ? IO_PAD356 908 1 Z
bit 910 I ? IO_PAD356
bit 911 C 1 *
bit 912 O ? IO_PAD357 911 1 Z
bit 913 I ? IO_PAD357
bit 914 C 1 *
bit 915 O ? IO_PAD358 914 1 Z
bit 916 I ? IO_PAD358
bit 917 C 1 *
bit 918 O ? IO_PAD360 917 1 Z
bit 919 I ? IO_PAD360
bit 920 C 1 *
bit 921 O ? IO_PAD361 920 1 Z
bit 922 I ? IO_PAD361
bit 923 C 1 *
bit 924 O ? IO_PAD362 923 1 Z
bit 925 I ? IO_PAD362
bit 926 C 1 *
bit 927 O ? IO_PAD364 926 1 Z
bit 928 I ? IO_PAD364
bit 929 C 1 *
bit 930 O ? IO_PAD365 929 1 Z
bit 931 I ? IO_PAD365
bit 932 C 1 *
bit 933 O ? IO_PAD366 932 1 Z
bit 934 I ? IO_PAD366
bit 935 C 1 *
bit 936 O ? IO_PAD368 935 1 Z
bit 937 I ? IO_PAD368
bit 938 C 1 *
bit 939 O ? IO_PAD370 938 1 Z
bit 940 I ? IO_PAD370
bit 941 C 1 *
bit 942 O ? IO_PAD371 941 1 Z
bit 943 I ? IO_PAD371
bit 944 C 1 *
bit 945 O ? IO_PAD372 944 1 Z
bit 946 I ? IO_PAD372
bit 947 C 1 *
bit 948 O ? IO_PAD373 947 1 Z
bit 949 I ? IO_PAD373
bit 950 C 1 *
bit 951 O ? IO_PAD374 950 1 Z
bit 952 I ? IO_PAD374
bit 953 C 1 *
bit 954 O ? IO_PAD376 953 1 Z
bit 955 I ? IO_PAD376
bit 956 C 1 *
bit 957 O ? IO_PAD378 956 1 Z
bit 958 I ? IO_PAD378
bit 959 C 1 *
bit 960 O ? IO_PAD380 959 1 Z
bit 961 I ? IO_PAD380
bit 962 C 1 *
bit 963 O ? IO_PAD382 962 1 Z
bit 964 I ? IO_PAD382
bit 965 C 1 *
bit 966 O ? IO_PAD383 965 1 Z
bit 967 I ? IO_PAD383
bit 968 C 1 *
bit 969 O ? IO_PAD384 968 1 Z
bit 970 I ? IO_PAD384
bit 971 C 1 *
bit 972 O ? IO_PAD386 971 1 Z
bit 973 I ? IO_PAD386
bit 974 C 1 *
bit 975 O ? IO_PAD388 974 1 Z
bit 976 I ? IO_PAD388
bit 977 C 1 *
bit 978 O ? IO_PAD389 977 1 Z
bit 979 I ? IO_PAD389
bit 980 C 1 *
bit 981 O ? IO_PAD390 980 1 Z
bit 982 I ? IO_PAD390
bit 983 C 1 *
bit 984 O ? IO_PAD391 983 1 Z
bit 985 I ? IO_PAD391
bit 986 C 1 *
bit 987 O ? IO_PAD392 986 1 Z
bit 988 I ? IO_PAD392
bit 989 C 1 *
bit 990 O ? IO_PAD393 989 1 Z
bit 991 I ? IO_PAD393
bit 992 C 1 *
bit 993 O ? IO_PAD394 992 1 Z
bit 994 I ? IO_PAD394
bit 995 C 1 *
bit 996 O ? IO_PAD395 995 1 Z
bit 997 I ? IO_PAD395
bit 998 C 1 *
bit 999 O ? IO_PAD396 998 1 Z
bit 1000 I ? IO_PAD396
bit 1001 C 1 *
bit 1002 O ? IO_PAD397 1001 1 Z
bit 1003 I ? IO_PAD397
bit 1004 C 1 *
bit 1005 O ? IO_PAD398 1004 1 Z
bit 1006 I ? IO_PAD398
bit 1007 C 1 *
bit 1008 O ? IO_PAD399 1007 1 Z
bit 1009 I ? IO_PAD399
bit 1010 C 1 *
bit 1011 O ? IO_PAD400 1010 1 Z
bit 1012 I ? IO_PAD400
bit 1013 C 1 *
bit 1014 O ? IO_PAD402 1013 1 Z
bit 1015 I ? IO_PAD402
bit 1016 C 1 *
bit 1017 O ? IO_PAD404 1016 1 Z
bit 1018 I ? IO_PAD404
bit 1019 C 1 *
bit 1020 O ? IO_PAD406 1019 1 Z
bit 1021 I ? IO_PAD406
bit 1022 C 1 *
bit 1023 O ? IO_PAD408 1022 1 Z
bit 1024 I ? IO_PAD408
bit 1025 C 1 *
bit 1026 O ? IO_PAD410 1025 1 Z
bit 1027 I ? IO_PAD410
bit 1028 C 1 *
bit 1029 O ? IO_PAD411 1028 1 Z
bit 1030 I ? IO_PAD411
bit 1031 C 1 *
bit 1032 O ? IO_PAD412 1031 1 Z
bit 1033 I ? IO_PAD412
bit 1034 C 1 *
bit 1035 O ? IO_PAD414 1034 1 Z
bit 1036 I ? IO_PAD414
bit 1037 C 1 *
bit 1038 O ? IO_PAD416 1037 1 Z
bit 1039 I ? IO_PAD416
bit 1040 C 1 *
bit 1041 O ? IO_PAD417 1040 1 Z
bit 1042 I ? IO_PAD417
bit 1043 C 1 *
bit 1044 O ? IO_PAD418 1043 1 Z
bit 1045 I ? IO_PAD418
bit 1046 C 1 *
bit 1047 O ? IO_PAD419 1046 1 Z
bit 1048 I ? IO_PAD419
bit 1049 C 1 *
bit 1050 O ? IO_PAD421 1049 1 Z
bit 1051 I ? IO_PAD421
bit 1052 C 1 *
bit 1053 O ? IO_PAD423 1052 1 Z
bit 1054 I ? IO_PAD423
bit 1055 C 1 *
bit 1056 O ? IO_PAD424 1055 1 Z
bit 1057 I ? IO_PAD424
bit 1058 C 1 *
bit 1059 O ? IO_PAD425 1058 1 Z
bit 1060 I ? IO_PAD425
bit 1061 C 1 *
bit 1062 O ? IO_PAD427 1061 1 Z
bit 1063 I ? IO_PAD427
bit 1064 C 1 *
bit 1065 O ? IO_PAD429 1064 1 Z
bit 1066 I ? IO_PAD429
bit 1067 C 1 *
bit 1068 O ? IO_PAD431 1067 1 Z
bit 1069 I ? IO_PAD431
bit 1070 C 1 *
bit 1071 O ? IO_PAD433 1070 1 Z
bit 1072 I ? IO_PAD433
bit 1073 C 1 *
bit 1074 O ? IO_PAD435 1073 1 Z
bit 1075 I ? IO_PAD435
bit 1076 C 1 *
bit 1077 O ? IO_PAD436 1076 1 Z
bit 1078 I ? IO_PAD436
bit 1079 C 1 *
bit 1080 O ? IO_PAD437 1079 1 Z
bit 1081 I ? IO_PAD437
bit 1082 C 1 *
bit 1083 O ? IO_PAD438 1082 1 Z
bit 1084 I ? IO_PAD438
bit 1085 C 1 *
bit 1086 O ? IO_PAD439 1085 1 Z
bit 1087 I ? IO_PAD439
bit 1088 C 1 *
bit 1089 O ? IO_PAD440 1088 1 Z
bit 1090 I ? IO_PAD440
bit 1091 C 1 *
bit 1092 O ? IO_PAD441 1091 1 Z
bit 1093 I ? IO_PAD441
bit 1094 C 1 *
bit 1095 O ? IO_PAD442 1094 1 Z
bit 1096 I ? IO_PAD442
bit 1097 C 1 *
bit 1098 O ? IO_PAD443 1097 1 Z
bit 1099 I ? IO_PAD443
bit 1100 C 1 *
bit 1101 O ? IO_PAD444 1100 1 Z
bit 1102 I ? IO_PAD444
bit 1103 C 1 *
bit 1104 O ? IO_PAD445 1103 1 Z
bit 1105 I ? IO_PAD445
bit 1106 C 1 *
bit 1107 O ? IO_PAD446 1106 1 Z
bit 1108 I ? IO_PAD446
bit 1109 C 1 *
bit 1110 O ? IO_PAD447 1109 1 Z
bit 1111 I ? IO_PAD447
bit 1112 C 1 *
bit 1113 O ? IO_PAD449 1112 1 Z
bit 1114 I ? IO_PAD449
bit 1115 C 1 *
bit 1116 O ? IO_PAD451 1115 1 Z
bit 1117 I ? IO_PAD451
bit 1118 C 1 *
bit 1119 O ? IO_PAD452 1118 1 Z
bit 1120 I ? IO_PAD452
bit 1121 C 1 *
bit 1122 O ? IO_PAD453 1121 1 Z
bit 1123 I ? IO_PAD453
bit 1124 C 1 *
bit 1125 O ? IO_PAD455 1124 1 Z
bit 1126 I ? IO_PAD455
bit 1127 C 1 *
bit 1128 O ? IO_PAD457 1127 1 Z
bit 1129 I ? IO_PAD457
bit 1130 C 1 *
bit 1131 O ? IO_PAD459 1130 1 Z
bit 1132 I ? IO_PAD459
bit 1133 C 1 *
bit 1134 O ? IO_PAD461 1133 1 Z
bit 1135 I ? IO_PAD461
bit 1136 C 1 *
bit 1137 O ? IO_PAD462 1136 1 Z
bit 1138 I ? IO_PAD462
bit 1139 C 1 *
bit 1140 O ? IO_PAD463 1139 1 Z
bit 1141 I ? IO_PAD463
bit 1142 C 1 *
bit 1143 O ? IO_PAD464 1142 1 Z
bit 1144 I ? IO_PAD464
bit 1145 C 1 *
bit 1146 O ? IO_PAD465 1145 1 Z
bit 1147 I ? IO_PAD465
bit 1148 C 1 *
bit 1149 O ? IO_PAD467 1148 1 Z
bit 1150 I ? IO_PAD467
bit 1151 C 1 *
bit 1152 O ? IO_PAD469 1151 1 Z
bit 1153 I ? IO_PAD469
bit 1154 C 1 *
bit 1155 O ? IO_PAD470 1154 1 Z
bit 1156 I ? IO_PAD470
bit 1157 C 1 *
bit 1158 O ? IO_PAD471 1157 1 Z
bit 1159 I ? IO_PAD471
bit 1160 C 1 *
bit 1161 O ? IO_PAD473 1160 1 Z
bit 1162 I ? IO_PAD473
bit 1163 C 1 *
bit 1164 O ? IO_PAD474 1163 1 Z
bit 1165 I ? IO_PAD474
bit 1166 C 1 *
bit 1167 O ? IO_PAD475 1166 1 Z
bit 1168 I ? IO_PAD475
bit 1169 C 1 *
bit 1170 O ? IO_PAD477 1169 1 Z
bit 1171 I ? IO_PAD477
bit 1172 C 1 *
bit 1173 O ? IO_PAD478 1172 1 Z
bit 1174 I ? IO_PAD478
bit 1175 C 1 *
bit 1176 O ? IO_PAD479 1175 1 Z
bit 1177 I ? IO_PAD479
bit 1178 C 1 *
bit 1179 O ? IO_PAD480 1178 1 Z
bit 1180 I ? IO_PAD480
bit 1181 C 1 *
bit 1182 O ? IO_PAD481 1181 1 Z
bit 1183 I ? IO_PAD481
bit 1184 C 1 *
bit 1185 O ? IO_PAD482 1184 1 Z
bit 1186 I ? IO_PAD482
