#
# $Id$
#
# JTAG declarations for EP1C12
#
# This program is free software; you can redistribute it and/or
# modify it under the terms of the GNU General Public License
# as published by the Free Software Foundation; either version 2
# of the License, or (at your option) any later version.
#
# This program is distributed in the hope that it will be useful,
# but WITHOUT ANY WARRANTY; without even the implied warranty of
# MERCHANTABILITY or FITNESS FOR A PARTICULAR PURPOSE.  See the
# GNU General Public License for more details.
#
# You should have received a copy of the GNU General Public License
# along with this program; if not, write to the Free Software
# Foundation, Inc., 59 Temple Place - Suite 330, Boston, MA
# 02111-1307, USA.
#
# Written by Arnim Laeuger <arniml@users.sourceforge.net>
#
# Note:
#   The signals defined in this file are generic for any EP1C12.
#   Signalnames according to Altera's package tables are set in the
#   package specific scripts.
#
#                  **Testing Differential Pin Pairs**
#   Refer to the note in the original bsd-files for issues related to
#   testing differential pin pairs!
#

register	BYPASS		1
register	BSR		774
register	IOCSR		4454
register	DEVICE_ID	32
register	USERCODE	32

instruction length 10
instruction	BYPASS		1111111111	BYPASS
instruction	IDCODE		0000000110	DEVICE_ID
instruction	USERCODE	0000000111	USERCODE
instruction	CLAMP		0000001010	BYPASS
instruction	SAMPLE/PRELOAD	0000000101	BSR
instruction	EXTEST		0000000000	BSR
instruction	CONFIG_IO	0000001101	IOCSR
instruction	HIGHZ		0000001011	BYPASS

signal	BSC0
signal	BSC1
signal	BSC10
signal	BSC100
signal	BSC101
signal	BSC102
signal	BSC103
signal	BSC104
signal	BSC105
signal	BSC106
signal	BSC107
signal	BSC108
signal	BSC109
signal	BSC11
signal	BSC110
signal	BSC111
signal	BSC112
signal	BSC113
signal	BSC114
signal	BSC115
signal	BSC116
signal	BSC117
signal	BSC118
signal	BSC119
signal	BSC12
signal	BSC120
signal	BSC121
signal	BSC122
signal	BSC123
signal	BSC124
signal	BSC125
signal	BSC126
signal	BSC127
signal	BSC128
signal	BSC129
signal	BSC13
signal	BSC130
signal	BSC131
signal	BSC132
signal	BSC133
signal	BSC134
signal	BSC135
signal	BSC136
signal	BSC137
signal	BSC138
signal	BSC139
signal	BSC14
signal	BSC140
signal	BSC141
signal	BSC142
signal	BSC143
signal	BSC144
signal	BSC145
signal	BSC146
signal	BSC147
signal	BSC148
signal	BSC149
signal	BSC15
signal	BSC150
signal	BSC151
signal	BSC152
signal	BSC153
signal	BSC154
signal	BSC155
signal	BSC156
signal	BSC157
signal	BSC158
signal	BSC159
signal	BSC16
signal	BSC160
signal	BSC161
signal	BSC162
signal	BSC163
signal	BSC164
signal	BSC165
signal	BSC166
signal	BSC167
signal	BSC168
signal	BSC169
signal	BSC17
signal	BSC170
signal	BSC171
signal	BSC172
signal	BSC173
signal	BSC174
signal	BSC175
signal	BSC176
signal	BSC177
signal	BSC178
signal	BSC179
signal	BSC18
signal	BSC180
signal	BSC181
signal	BSC182
signal	BSC183
signal	BSC184
signal	BSC185
signal	BSC186
signal	BSC187
signal	BSC188
signal	BSC189
signal	BSC19
signal	BSC190
signal	BSC191
signal	BSC192
signal	BSC193
signal	BSC194
signal	BSC195
signal	BSC196
signal	BSC197
signal	BSC198
signal	BSC199
signal	BSC2
signal	BSC20
signal	BSC200
signal	BSC201
signal	BSC202
signal	BSC203
signal	BSC204
signal	BSC205
signal	BSC206
signal	BSC207
signal	BSC208
signal	BSC209
signal	BSC21
signal	BSC210
signal	BSC211
signal	BSC212
signal	BSC213
signal	BSC214
signal	BSC215
signal	BSC216
signal	BSC217
signal	BSC218
signal	BSC22
signal	BSC228
signal	BSC229
signal	BSC23
signal	BSC230
signal	BSC231
signal	BSC232
signal	BSC233
signal	BSC234
signal	BSC235
signal	BSC236
signal	BSC237
signal	BSC238
signal	BSC239
signal	BSC24
signal	BSC240
signal	BSC241
signal	BSC242
signal	BSC243
signal	BSC244
signal	BSC245
signal	BSC246
signal	BSC247
signal	BSC248
signal	BSC249
signal	BSC25
signal	BSC250
signal	BSC251
signal	BSC252
signal	BSC253
signal	BSC254
signal	BSC255
signal	BSC256
signal	BSC257
signal	BSC26
signal	BSC27
signal	BSC28
signal	BSC29
signal	BSC3
signal	BSC30
signal	BSC31
signal	BSC32
signal	BSC33
signal	BSC34
signal	BSC35
signal	BSC36
signal	BSC37
signal	BSC38
signal	BSC39
signal	BSC4
signal	BSC40
signal	BSC41
signal	BSC42
signal	BSC43
signal	BSC44
signal	BSC45
signal	BSC46
signal	BSC47
signal	BSC48
signal	BSC49
signal	BSC5
signal	BSC50
signal	BSC51
signal	BSC52
signal	BSC53
signal	BSC54
signal	BSC55
signal	BSC56
signal	BSC57
signal	BSC58
signal	BSC59
signal	BSC6
signal	BSC60
signal	BSC61
signal	BSC62
signal	BSC63
signal	BSC64
signal	BSC65
signal	BSC66
signal	BSC67
signal	BSC68
signal	BSC69
signal	BSC7
signal	BSC70
signal	BSC71
signal	BSC72
signal	BSC73
signal	BSC74
signal	BSC75
signal	BSC76
signal	BSC77
signal	BSC78
signal	BSC79
signal	BSC8
signal	BSC80
signal	BSC81
signal	BSC82
signal	BSC83
signal	BSC84
signal	BSC85
signal	BSC86
signal	BSC87
signal	BSC88
signal	BSC89
signal	BSC9
signal	BSC90
signal	BSC91
signal	BSC96
signal	BSC97
signal	BSC98
signal	BSC99
signal	CLK0
signal	CLK2
signal	DATA0
signal	DCLK
signal	MSEL0
signal	MSEL1

bit  0 I ? BSC0
bit  1 C 1 *
bit  2 O ? BSC0 1 1 Z
bit  3 I ? BSC1
bit  4 C 1 *
bit  5 O ? BSC1 4 1 Z
bit  6 I ? BSC2
bit  7 C 1 *
bit  8 O ? BSC2 7 1 Z
bit  9 I ? BSC3
bit 10 C 1 *
bit 11 O ? BSC3 10 1 Z
bit 12 I ? BSC4
bit 13 C 1 *
bit 14 O ? BSC4 13 1 Z
bit 15 I ? BSC5
bit 16 C 1 *
bit 17 O ? BSC5 16 1 Z
bit 18 I ? BSC6
bit 19 C 1 *
bit 20 O ? BSC6 19 1 Z
bit 21 I ? BSC7
bit 22 C 1 *
bit 23 O ? BSC7 22 1 Z
bit 24 I ? BSC8
bit 25 C 1 *
bit 26 O ? BSC8 25 1 Z
bit 27 I ? BSC9
bit 28 C 1 *
bit 29 O ? BSC9 28 1 Z
bit 30 I ? BSC10
bit 31 C 1 *
bit 32 O ? BSC10 31 1 Z
bit 33 I ? BSC11
bit 34 C 1 *
bit 35 O ? BSC11 34 1 Z
bit 36 I ? BSC12
bit 37 C 1 *
bit 38 O ? BSC12 37 1 Z
bit 39 I ? BSC13
bit 40 C 1 *
bit 41 O ? BSC13 40 1 Z
bit 42 I ? BSC14
bit 43 C 1 *
bit 44 O ? BSC14 43 1 Z
bit 45 I ? BSC15
bit 46 C 1 *
bit 47 O ? BSC15 46 1 Z
bit 48 I ? BSC16
bit 49 C 1 *
bit 50 O ? BSC16 49 1 Z
bit 51 I ? BSC17
bit 52 C 1 *
bit 53 O ? BSC17 52 1 Z
bit 54 I ? BSC18
bit 55 C 1 *
bit 56 O ? BSC18 55 1 Z
bit 57 I ? BSC19
bit 58 C 1 *
bit 59 O ? BSC19 58 1 Z
bit 60 I ? BSC20
bit 61 C 1 *
bit 62 O ? BSC20 61 1 Z
bit 63 I ? BSC21
bit 64 C 1 *
bit 65 O ? BSC21 64 1 Z
bit 66 I ? BSC22
bit 67 C 1 *
bit 68 O ? BSC22 67 1 Z
bit 69 I ? BSC23
bit 70 C 1 *
bit 71 O ? BSC23 70 1 Z
bit 72 I ? BSC24
bit 73 C 1 *
bit 74 O ? BSC24 73 1 Z
bit 75 I ? BSC25
bit 76 C 1 *
bit 77 O ? BSC25 76 1 Z
bit 78 I ? BSC26
bit 79 C 1 *
bit 80 O ? BSC26 79 1 Z
bit 81 I ? BSC27
bit 82 C 1 *
bit 83 O ? BSC27 82 1 Z
bit 84 I ? BSC28
bit 85 C 1 *
bit 86 O ? BSC28 85 1 Z
bit 87 I ? BSC29
bit 88 C 1 *
bit 89 O ? BSC29 88 1 Z
bit 90 I ? BSC30
bit 91 C 1 *
bit 92 O ? BSC30 91 1 Z
bit 93 I ? BSC31
bit 94 C 1 *
bit 95 O ? BSC31 94 1 Z
bit 96 I ? BSC32
bit 97 C 1 *
bit 98 O ? BSC32 97 1 Z
bit 99 I ? BSC33
bit 100 C 1 *
bit 101 O ? BSC33 100 1 Z
bit 102 I ? BSC34
bit 103 C 1 *
bit 104 O ? BSC34 103 1 Z
bit 105 I ? BSC35
bit 106 C 1 *
bit 107 O ? BSC35 106 1 Z
bit 108 I ? BSC36
bit 109 C 1 *
bit 110 O ? BSC36 109 1 Z
bit 111 I ? BSC37
bit 112 C 1 *
bit 113 O ? BSC37 112 1 Z
bit 114 I ? BSC38
bit 115 C 1 *
bit 116 O ? BSC38 115 1 Z
bit 117 I ? BSC39
bit 118 C 1 *
bit 119 O ? BSC39 118 1 Z
bit 120 I ? BSC40
bit 121 C 1 *
bit 122 O ? BSC40 121 1 Z
bit 123 I ? BSC41
bit 124 C 1 *
bit 125 O ? BSC41 124 1 Z
bit 126 I ? BSC42
bit 127 C 1 *
bit 128 O ? BSC42 127 1 Z
bit 129 I ? BSC43
bit 130 C 1 *
bit 131 O ? BSC43 130 1 Z
bit 132 I ? BSC44
bit 133 C 1 *
bit 134 O ? BSC44 133 1 Z
bit 135 I ? BSC45
bit 136 C 1 *
bit 137 O ? BSC45 136 1 Z
bit 138 I ? BSC46
bit 139 C 1 *
bit 140 O ? BSC46 139 1 Z
bit 141 I ? BSC47
bit 142 C 1 *
bit 143 O ? BSC47 142 1 Z
bit 144 I ? BSC48
bit 145 C 1 *
bit 146 O ? BSC48 145 1 Z
bit 147 I ? BSC49
bit 148 C 1 *
bit 149 O ? BSC49 148 1 Z
bit 150 I ? BSC50
bit 151 C 1 *
bit 152 O ? BSC50 151 1 Z
bit 153 I ? BSC51
bit 154 C 1 *
bit 155 O ? BSC51 154 1 Z
bit 156 I ? BSC52
bit 157 C 1 *
bit 158 O ? BSC52 157 1 Z
bit 159 I ? BSC53
bit 160 C 1 *
bit 161 O ? BSC53 160 1 Z
bit 162 I ? BSC54
bit 163 C 1 *
bit 164 O ? BSC54 163 1 Z
bit 165 I ? BSC55
bit 166 C 1 *
bit 167 O ? BSC55 166 1 Z
bit 168 I ? BSC56
bit 169 C 1 *
bit 170 O ? BSC56 169 1 Z
bit 171 I ? BSC57
bit 172 C 1 *
bit 173 O ? BSC57 172 1 Z
bit 174 I ? BSC58
bit 175 C 1 *
bit 176 O ? BSC58 175 1 Z
bit 177 I ? BSC59
bit 178 C 1 *
bit 179 O ? BSC59 178 1 Z
bit 180 I ? BSC60
bit 181 C 1 *
bit 182 O ? BSC60 181 1 Z
bit 183 I ? BSC61
bit 184 C 1 *
bit 185 O ? BSC61 184 1 Z
bit 186 I ? BSC62
bit 187 C 1 *
bit 188 O ? BSC62 187 1 Z
bit 189 I ? BSC63
bit 190 C 1 *
bit 191 O ? BSC63 190 1 Z
bit 192 I ? BSC64
bit 193 C 1 *
bit 194 O ? BSC64 193 1 Z
bit 195 I ? BSC65
bit 196 C 1 *
bit 197 O ? BSC65 196 1 Z
bit 198 I ? BSC66
bit 199 C 1 *
bit 200 O ? BSC66 199 1 Z
bit 201 I ? BSC67
bit 202 C 1 *
bit 203 O ? BSC67 202 1 Z
bit 204 I ? BSC68
bit 205 C 1 *
bit 206 O ? BSC68 205 1 Z
bit 207 I ? BSC69
bit 208 C 1 *
bit 209 O ? BSC69 208 1 Z
bit 210 I ? BSC70
bit 211 C 1 *
bit 212 O ? BSC70 211 1 Z
bit 213 I ? BSC71
bit 214 C 1 *
bit 215 O ? BSC71 214 1 Z
bit 216 I ? BSC72
bit 217 C 1 *
bit 218 O ? BSC72 217 1 Z
bit 219 I ? BSC73
bit 220 C 1 *
bit 221 O ? BSC73 220 1 Z
bit 222 I ? BSC74
bit 223 C 1 *
bit 224 O ? BSC74 223 1 Z
bit 225 I ? BSC75
bit 226 C 1 *
bit 227 O ? BSC75 226 1 Z
bit 228 I ? BSC76
bit 229 C 1 *
bit 230 O ? BSC76 229 1 Z
bit 231 I ? BSC77
bit 232 C 1 *
bit 233 O ? BSC77 232 1 Z
bit 234 I ? BSC78
bit 235 C 1 *
bit 236 O ? BSC78 235 1 Z
bit 237 I ? BSC79
bit 238 C 1 *
bit 239 O ? BSC79 238 1 Z
bit 240 I ? BSC80
bit 241 C 1 *
bit 242 O ? BSC80 241 1 Z
bit 243 I ? BSC81
bit 244 C 1 *
bit 245 O ? BSC81 244 1 Z
bit 246 I ? BSC82
bit 247 C 1 *
bit 248 O ? BSC82 247 1 Z
bit 249 I ? BSC83
bit 250 C 1 *
bit 251 O ? BSC83 250 1 Z
bit 252 I ? BSC84
bit 253 C 1 *
bit 254 O ? BSC84 253 1 Z
bit 255 I ? BSC85
bit 256 C 1 *
bit 257 O ? BSC85 256 1 Z
bit 258 I ? BSC86
bit 259 C 1 *
bit 260 O ? BSC86 259 1 Z
bit 261 I ? BSC87
bit 262 C 1 *
bit 263 O ? BSC87 262 1 Z
bit 264 I ? BSC88
bit 265 C 1 *
bit 266 O ? BSC88 265 1 Z
bit 267 I ? BSC89
bit 268 C 1 *
bit 269 O ? BSC89 268 1 Z
bit 270 I ? BSC90
bit 271 C 1 *
bit 272 O ? BSC90 271 1 Z
bit 273 I ? BSC91
bit 274 C 1 *
bit 275 O ? BSC91 274 1 Z
bit 276 I ? CLK2
bit 277 X ? *
bit 278 X ? *
bit 279 X ? *
bit 280 X 1 *
bit 281 X ? *
bit 282 X ? *
bit 283 X 1 *
bit 284 X ? *
bit 285 X ? *
bit 286 X 1 *
bit 287 X ? *
bit 288 I ? BSC96
bit 289 C 1 *
bit 290 O ? BSC96 289 1 Z
bit 291 I ? BSC97
bit 292 C 1 *
bit 293 O ? BSC97 292 1 Z
bit 294 I ? BSC98
bit 295 C 1 *
bit 296 O ? BSC98 295 1 Z
bit 297 I ? BSC99
bit 298 C 1 *
bit 299 O ? BSC99 298 1 Z
bit 300 I ? BSC100
bit 301 C 1 *
bit 302 O ? BSC100 301 1 Z
bit 303 I ? BSC101
bit 304 C 1 *
bit 305 O ? BSC101 304 1 Z
bit 306 I ? BSC102
bit 307 C 1 *
bit 308 O ? BSC102 307 1 Z
bit 309 I ? BSC103
bit 310 C 1 *
bit 311 O ? BSC103 310 1 Z
bit 312 I ? BSC104
bit 313 C 1 *
bit 314 O ? BSC104 313 1 Z
bit 315 I ? BSC105
bit 316 C 1 *
bit 317 O ? BSC105 316 1 Z
bit 318 I ? BSC106
bit 319 C 1 *
bit 320 O ? BSC106 319 1 Z
bit 321 I ? BSC107
bit 322 C 1 *
bit 323 O ? BSC107 322 1 Z
bit 324 I ? BSC108
bit 325 C 1 *
bit 326 O ? BSC108 325 1 Z
bit 327 I ? BSC109
bit 328 C 1 *
bit 329 O ? BSC109 328 1 Z
bit 330 I ? BSC110
bit 331 C 1 *
bit 332 O ? BSC110 331 1 Z
bit 333 I ? BSC111
bit 334 C 1 *
bit 335 O ? BSC111 334 1 Z
bit 336 I ? BSC112
bit 337 C 1 *
bit 338 O ? BSC112 337 1 Z
bit 339 I ? BSC113
bit 340 C 1 *
bit 341 O ? BSC113 340 1 Z
bit 342 I ? BSC114
bit 343 C 1 *
bit 344 O ? BSC114 343 1 Z
bit 345 I ? BSC115
bit 346 C 1 *
bit 347 O ? BSC115 346 1 Z
bit 348 I ? BSC116
bit 349 C 1 *
bit 350 O ? BSC116 349 1 Z
bit 351 I ? BSC117
bit 352 C 1 *
bit 353 O ? BSC117 352 1 Z
bit 354 I ? BSC118
bit 355 C 1 *
bit 356 O ? BSC118 355 1 Z
bit 357 I ? BSC119
bit 358 C 1 *
bit 359 O ? BSC119 358 1 Z
bit 360 I ? BSC120
bit 361 C 1 *
bit 362 O ? BSC120 361 1 Z
bit 363 I ? BSC121
bit 364 C 1 *
bit 365 O ? BSC121 364 1 Z
bit 366 I ? BSC122
bit 367 C 1 *
bit 368 O ? BSC122 367 1 Z
bit 369 I ? BSC123
bit 370 C 1 *
bit 371 O ? BSC123 370 1 Z
bit 372 I ? BSC124
bit 373 C 1 *
bit 374 O ? BSC124 373 1 Z
bit 375 I ? BSC125
bit 376 C 1 *
bit 377 O ? BSC125 376 1 Z
bit 378 I ? BSC126
bit 379 C 1 *
bit 380 O ? BSC126 379 1 Z
bit 381 I ? BSC127
bit 382 C 1 *
bit 383 O ? BSC127 382 1 Z
bit 384 I ? BSC128
bit 385 C 1 *
bit 386 O ? BSC128 385 1 Z
bit 387 I ? BSC129
bit 388 C 1 *
bit 389 O ? BSC129 388 1 Z
bit 390 I ? BSC130
bit 391 C 1 *
bit 392 O ? BSC130 391 1 Z
bit 393 I ? BSC131
bit 394 C 1 *
bit 395 O ? BSC131 394 1 Z
bit 396 I ? BSC132
bit 397 C 1 *
bit 398 O ? BSC132 397 1 Z
bit 399 I ? BSC133
bit 400 C 1 *
bit 401 O ? BSC133 400 1 Z
bit 402 I ? BSC134
bit 403 C 1 *
bit 404 O ? BSC134 403 1 Z
bit 405 I ? BSC135
bit 406 C 1 *
bit 407 O ? BSC135 406 1 Z
bit 408 I ? BSC136
bit 409 C 1 *
bit 410 O ? BSC136 409 1 Z
bit 411 I ? BSC137
bit 412 C 1 *
bit 413 O ? BSC137 412 1 Z
bit 414 I ? BSC138
bit 415 C 1 *
bit 416 O ? BSC138 415 1 Z
bit 417 I ? BSC139
bit 418 C 1 *
bit 419 O ? BSC139 418 1 Z
bit 420 I ? BSC140
bit 421 C 1 *
bit 422 O ? BSC140 421 1 Z
bit 423 I ? BSC141
bit 424 C 1 *
bit 425 O ? BSC141 424 1 Z
bit 426 I ? BSC142
bit 427 C 1 *
bit 428 O ? BSC142 427 1 Z
bit 429 I ? BSC143
bit 430 C 1 *
bit 431 O ? BSC143 430 1 Z
bit 432 I ? BSC144
bit 433 C 1 *
bit 434 O ? BSC144 433 1 Z
bit 435 I ? BSC145
bit 436 C 1 *
bit 437 O ? BSC145 436 1 Z
bit 438 I ? BSC146
bit 439 C 1 *
bit 440 O ? BSC146 439 1 Z
bit 441 I ? BSC147
bit 442 C 1 *
bit 443 O ? BSC147 442 1 Z
bit 444 I ? BSC148
bit 445 C 1 *
bit 446 O ? BSC148 445 1 Z
bit 447 I ? BSC149
bit 448 C 1 *
bit 449 O ? BSC149 448 1 Z
bit 450 I ? BSC150
bit 451 C 1 *
bit 452 O ? BSC150 451 1 Z
bit 453 I ? BSC151
bit 454 C 1 *
bit 455 O ? BSC151 454 1 Z
bit 456 I ? BSC152
bit 457 C 1 *
bit 458 O ? BSC152 457 1 Z
bit 459 I ? BSC153
bit 460 C 1 *
bit 461 O ? BSC153 460 1 Z
bit 462 I ? BSC154
bit 463 C 1 *
bit 464 O ? BSC154 463 1 Z
bit 465 I ? BSC155
bit 466 C 1 *
bit 467 O ? BSC155 466 1 Z
bit 468 I ? BSC156
bit 469 C 1 *
bit 470 O ? BSC156 469 1 Z
bit 471 I ? BSC157
bit 472 C 1 *
bit 473 O ? BSC157 472 1 Z
bit 474 I ? BSC158
bit 475 C 1 *
bit 476 O ? BSC158 475 1 Z
bit 477 I ? BSC159
bit 478 C 1 *
bit 479 O ? BSC159 478 1 Z
bit 480 I ? BSC160
bit 481 C 1 *
bit 482 O ? BSC160 481 1 Z
bit 483 I ? BSC161
bit 484 C 1 *
bit 485 O ? BSC161 484 1 Z
bit 486 I ? BSC162
bit 487 C 1 *
bit 488 O ? BSC162 487 1 Z
bit 489 I ? BSC163
bit 490 C 1 *
bit 491 O ? BSC163 490 1 Z
bit 492 I ? BSC164
bit 493 C 1 *
bit 494 O ? BSC164 493 1 Z
bit 495 I ? BSC165
bit 496 C 1 *
bit 497 O ? BSC165 496 1 Z
bit 498 I ? BSC166
bit 499 C 1 *
bit 500 O ? BSC166 499 1 Z
bit 501 I ? BSC167
bit 502 C 1 *
bit 503 O ? BSC167 502 1 Z
bit 504 I ? BSC168
bit 505 C 1 *
bit 506 O ? BSC168 505 1 Z
bit 507 I ? BSC169
bit 508 C 1 *
bit 509 O ? BSC169 508 1 Z
bit 510 I ? BSC170
bit 511 C 1 *
bit 512 O ? BSC170 511 1 Z
bit 513 I ? BSC171
bit 514 C 1 *
bit 515 O ? BSC171 514 1 Z
bit 516 I ? BSC172
bit 517 C 1 *
bit 518 O ? BSC172 517 1 Z
bit 519 I ? BSC173
bit 520 C 1 *
bit 521 O ? BSC173 520 1 Z
bit 522 I ? BSC174
bit 523 C 1 *
bit 524 O ? BSC174 523 1 Z
bit 525 I ? BSC175
bit 526 C 1 *
bit 527 O ? BSC175 526 1 Z
bit 528 I ? BSC176
bit 529 C 1 *
bit 530 O ? BSC176 529 1 Z
bit 531 I ? BSC177
bit 532 C 1 *
bit 533 O ? BSC177 532 1 Z
bit 534 I ? BSC178
bit 535 C 1 *
bit 536 O ? BSC178 535 1 Z
bit 537 I ? BSC179
bit 538 C 1 *
bit 539 O ? BSC179 538 1 Z
bit 540 I ? BSC180
bit 541 C 1 *
bit 542 O ? BSC180 541 1 Z
bit 543 I ? BSC181
bit 544 C 1 *
bit 545 O ? BSC181 544 1 Z
bit 546 I ? BSC182
bit 547 C 1 *
bit 548 O ? BSC182 547 1 Z
bit 549 I ? BSC183
bit 550 C 1 *
bit 551 O ? BSC183 550 1 Z
bit 552 I ? BSC184
bit 553 C 1 *
bit 554 O ? BSC184 553 1 Z
bit 555 I ? BSC185
bit 556 C 1 *
bit 557 O ? BSC185 556 1 Z
bit 558 I ? BSC186
bit 559 C 1 *
bit 560 O ? BSC186 559 1 Z
bit 561 I ? BSC187
bit 562 C 1 *
bit 563 O ? BSC187 562 1 Z
bit 564 I ? BSC188
bit 565 C 1 *
bit 566 O ? BSC188 565 1 Z
bit 567 I ? BSC189
bit 568 C 1 *
bit 569 O ? BSC189 568 1 Z
bit 570 I ? BSC190
bit 571 C 1 *
bit 572 O ? BSC190 571 1 Z
bit 573 I ? BSC191
bit 574 C 1 *
bit 575 O ? BSC191 574 1 Z
bit 576 I ? BSC192
bit 577 C 1 *
bit 578 O ? BSC192 577 1 Z
bit 579 I ? BSC193
bit 580 C 1 *
bit 581 O ? BSC193 580 1 Z
bit 582 I ? BSC194
bit 583 C 1 *
bit 584 O ? BSC194 583 1 Z
bit 585 I ? BSC195
bit 586 C 1 *
bit 587 O ? BSC195 586 1 Z
bit 588 I ? BSC196
bit 589 C 1 *
bit 590 O ? BSC196 589 1 Z
bit 591 I ? BSC197
bit 592 C 1 *
bit 593 O ? BSC197 592 1 Z
bit 594 I ? BSC198
bit 595 C 1 *
bit 596 O ? BSC198 595 1 Z
bit 597 I ? BSC199
bit 598 C 1 *
bit 599 O ? BSC199 598 1 Z
bit 600 I ? BSC200
bit 601 C 1 *
bit 602 O ? BSC200 601 1 Z
bit 603 I ? BSC201
bit 604 C 1 *
bit 605 O ? BSC201 604 1 Z
bit 606 I ? BSC202
bit 607 C 1 *
bit 608 O ? BSC202 607 1 Z
bit 609 I ? BSC203
bit 610 C 1 *
bit 611 O ? BSC203 610 1 Z
bit 612 I ? BSC204
bit 613 C 1 *
bit 614 O ? BSC204 613 1 Z
bit 615 I ? BSC205
bit 616 C 1 *
bit 617 O ? BSC205 616 1 Z
bit 618 I ? BSC206
bit 619 C 1 *
bit 620 O ? BSC206 619 1 Z
bit 621 I ? BSC207
bit 622 C 1 *
bit 623 O ? BSC207 622 1 Z
bit 624 I ? BSC208
bit 625 C 1 *
bit 626 O ? BSC208 625 1 Z
bit 627 I ? BSC209
bit 628 C 1 *
bit 629 O ? BSC209 628 1 Z
bit 630 I ? BSC210
bit 631 C 1 *
bit 632 O ? BSC210 631 1 Z
bit 633 I ? BSC211
bit 634 C 1 *
bit 635 O ? BSC211 634 1 Z
bit 636 I ? BSC212
bit 637 C 1 *
bit 638 O ? BSC212 637 1 Z
bit 639 I ? BSC213
bit 640 C 1 *
bit 641 O ? BSC213 640 1 Z
bit 642 I ? BSC214
bit 643 C 1 *
bit 644 O ? BSC214 643 1 Z
bit 645 I ? BSC215
bit 646 C 1 *
bit 647 O ? BSC215 646 1 Z
bit 648 I ? BSC216
bit 649 C 1 *
bit 650 O ? BSC216 649 1 Z
bit 651 I ? BSC217
bit 652 C 1 *
bit 653 O ? BSC217 652 1 Z
bit 654 I ? BSC218
bit 655 C 1 *
bit 656 O ? BSC218 655 1 Z
bit 657 I ? DCLK
bit 658 C 1 *
bit 659 O ? DCLK 658 1 Z
bit 660 I ? MSEL1
bit 661 X ? *
bit 662 X ? *
bit 663 I ? MSEL0
bit 664 X ? *
bit 665 X ? *
bit 666 X ? *
bit 667 X 1 *
bit 668 X ? *
bit 669 X ? *
bit 670 X 1 *
bit 671 X ? *
bit 672 X ? *
bit 673 X 1 *
bit 674 X ? *
bit 675 I ? CLK0
bit 676 X ? *
bit 677 X ? *
bit 678 X ? *
bit 679 X 1 *
bit 680 X ? *
bit 681 I ? DATA0
bit 682 X ? *
bit 683 X ? *
bit 684 I ? BSC228
bit 685 C 1 *
bit 686 O ? BSC228 685 1 Z
bit 687 I ? BSC229
bit 688 C 1 *
bit 689 O ? BSC229 688 1 Z
bit 690 I ? BSC230
bit 691 C 1 *
bit 692 O ? BSC230 691 1 Z
bit 693 I ? BSC231
bit 694 C 1 *
bit 695 O ? BSC231 694 1 Z
bit 696 I ? BSC232
bit 697 C 1 *
bit 698 O ? BSC232 697 1 Z
bit 699 I ? BSC233
bit 700 C 1 *
bit 701 O ? BSC233 700 1 Z
bit 702 I ? BSC234
bit 703 C 1 *
bit 704 O ? BSC234 703 1 Z
bit 705 I ? BSC235
bit 706 C 1 *
bit 707 O ? BSC235 706 1 Z
bit 708 I ? BSC236
bit 709 C 1 *
bit 710 O ? BSC236 709 1 Z
bit 711 I ? BSC237
bit 712 C 1 *
bit 713 O ? BSC237 712 1 Z
bit 714 I ? BSC238
bit 715 C 1 *
bit 716 O ? BSC238 715 1 Z
bit 717 I ? BSC239
bit 718 C 1 *
bit 719 O ? BSC239 718 1 Z
bit 720 I ? BSC240
bit 721 C 1 *
bit 722 O ? BSC240 721 1 Z
bit 723 I ? BSC241
bit 724 C 1 *
bit 725 O ? BSC241 724 1 Z
bit 726 I ? BSC242
bit 727 C 1 *
bit 728 O ? BSC242 727 1 Z
bit 729 I ? BSC243
bit 730 C 1 *
bit 731 O ? BSC243 730 1 Z
bit 732 I ? BSC244
bit 733 C 1 *
bit 734 O ? BSC244 733 1 Z
bit 735 I ? BSC245
bit 736 C 1 *
bit 737 O ? BSC245 736 1 Z
bit 738 I ? BSC246
bit 739 C 1 *
bit 740 O ? BSC246 739 1 Z
bit 741 I ? BSC247
bit 742 C 1 *
bit 743 O ? BSC247 742 1 Z
bit 744 I ? BSC248
bit 745 C 1 *
bit 746 O ? BSC248 745 1 Z
bit 747 I ? BSC249
bit 748 C 1 *
bit 749 O ? BSC249 748 1 Z
bit 750 I ? BSC250
bit 751 C 1 *
bit 752 O ? BSC250 751 1 Z
bit 753 I ? BSC251
bit 754 C 1 *
bit 755 O ? BSC251 754 1 Z
bit 756 I ? BSC252
bit 757 C 1 *
bit 758 O ? BSC252 757 1 Z
bit 759 I ? BSC253
bit 760 C 1 *
bit 761 O ? BSC253 760 1 Z
bit 762 I ? BSC254
bit 763 C 1 *
bit 764 O ? BSC254 763 1 Z
bit 765 I ? BSC255
bit 766 C 1 *
bit 767 O ? BSC255 766 1 Z
bit 768 I ? BSC256
bit 769 C 1 *
bit 770 O ? BSC256 769 1 Z
bit 771 I ? BSC257
bit 772 C 1 *
bit 773 O ? BSC257 772 1 Z
