signal GND1
signal GND2
signal GND3
signal GND4
signal GND5
signal GND6
signal GND7
signal GND8
signal GND9
signal GND10
signal GND11
signal GND12
signal GND13
signal GND14
signal GND15
signal GND16
signal GND17
signal GND18
signal GND19
signal GND20
signal GND21
signal GND22
signal GND23
signal GND24
signal GND25
signal GND26
signal GND27
signal GND28
signal CCLK_P104
signal DONE_P103
signal HSWAP_EN_P206
signal M0_P55
signal M1_P54
signal M2_P56
signal PROG_B
signal TCK
signal TDI
signal TDO
signal TMS
signal VCCAUX1
signal VCCAUX2
signal VCCAUX3
signal VCCAUX4
signal VCCAUX5
signal VCCAUX6
signal VCCAUX7
signal VCCAUX8
signal VCCINT1
signal VCCINT2
signal VCCINT3
signal VCCINT4
signal VCCO01
signal VCCO02
signal VCCO11
signal VCCO12
signal VCCO21
signal VCCO22
signal VCCO31
signal VCCO32
signal VCCO41
signal VCCO42
signal VCCO51
signal VCCO52
signal VCCO61
signal VCCO62
signal VCCO71
signal VCCO72
signal IO_P2
signal IO_P3
signal IO_P4
signal IO_P5
signal IO_P7
signal IO_P9
signal IO_P10
signal IO_P11
signal IO_P12
signal IO_P13
signal IO_P15
signal IO_P16
signal IO_P18
signal IO_P19
signal IO_P20
signal IO_P21
signal IO_P22
signal IO_P24
signal IO_P26
signal IO_P27
signal IO_P28
signal IO_P29
signal IO_P31
signal IO_P33
signal IO_P34
signal IO_P35
signal IO_P36
signal IO_P37
signal IO_P39
signal IO_P40
signal IO_P42
signal IO_P43
signal IO_P44
signal IO_P45
signal IO_P46
signal IO_P48
signal IO_P50
signal IO_P51
signal IO_P52
signal IO_P57
signal IO_P58
signal IO_P61
signal IO_P62
signal IO_P63
signal IO_P64
signal IO_P65
signal IO_P67
signal IO_P68
signal IO_P71
signal IO_P72
signal IO_P74
signal IO_P76
signal IO_P77
signal IO_P78
signal IO_P79
signal IO_P80
signal IO_P81
signal IO_P83
signal IO_P85
signal IO_P86
signal IO_P87
signal IO_P90
signal IO_P92
signal IO_P93
signal IO_P94
signal IO_P95
signal IO_P96
signal IO_P97
signal IO_P100
signal IO_P101
signal IO_P102
signal IO_P106
signal IO_P107
signal IO_P108
signal IO_P109
signal IO_P111
signal IO_P113
signal IO_P114
signal IO_P115
signal IO_P116
signal IO_P117
signal IO_P119
signal IO_P120
signal IO_P122
signal IO_P123
signal IO_P124
signal IO_P125
signal IO_P126
signal IO_P128
signal IO_P130
signal IO_P131
signal IO_P132
signal IO_P133
signal IO_P135
signal IO_P137
signal IO_P138
signal IO_P139
signal IO_P140
signal IO_P141
signal IO_P143
signal IO_P144
signal IO_P146
signal IO_P147
signal IO_P148
signal IO_P149
signal IO_P150
signal IO_P152
signal IO_P154
signal IO_P155
signal IO_P156
signal IO_P161
signal IO_P162
signal IO_P165
signal IO_P166
signal IO_P167
signal IO_P168
signal IO_P169
signal IO_P171
signal IO_P172
signal IO_P175
signal IO_P176
signal IO_P178
signal IO_P180
signal IO_P181
signal IO_P182
signal IO_P183
signal IO_P184
signal IO_P185
signal IO_P187
signal IO_P189
signal IO_P190
signal IO_P191
signal IO_P194
signal IO_P196
signal IO_P197
signal IO_P198
signal IO_P199
signal IO_P200
signal IO_P203
signal IO_P204

register	BSR	815
register	BR	1
register	DIR	32

instruction length 6

instruction EXTEST 000000 BSR
instruction SAMPLE/PRELOAD 000001 BSR
instruction IDCODE 001001 DIR
instruction BYPASS 111111 BR

bit 814 I 1 IO_P156
bit 813 O 1 IO_P156 812 1 Z
bit 812 C 1 *
bit 811 I 1 IO_P155
bit 810 O 1 IO_P155 809 1 Z
bit 809 C 1 *
bit 808 O 1 *
bit 807 O 1 *
bit 806 O 1 *
bit 805 O 1 *
bit 804 O 1 *
bit 803 O 1 *
bit 802 O 1 *
bit 801 O 1 *
bit 800 O 1 *
bit 799 O 1 *
bit 798 O 1 *
bit 797 O 1 *
bit 796 O 1 *
bit 795 O 1 *
bit 794 O 1 *
bit 793 I 1 IO_P154
bit 792 O 1 IO_P154 791 1 Z
bit 791 C 1 *
bit 790 I 1 IO_P152
bit 789 O 1 IO_P152 788 1 Z
bit 788 C 1 *
bit 787 I 1 IO_P150
bit 786 O 1 IO_P150 785 1 Z
bit 785 C 1 *
bit 784 I 1 IO_P149
bit 783 O 1 IO_P149 782 1 Z
bit 782 C 1 *
bit 781 I 1 IO_P148
bit 780 O 1 IO_P148 779 1 Z
bit 779 C 1 *
bit 778 I 1 IO_P147
bit 777 O 1 IO_P147 776 1 Z
bit 776 C 1 *
bit 775 I 1 IO_P146
bit 774 O 1 IO_P146 773 1 Z
bit 773 C 1 *
bit 772 I 1 IO_P144
bit 771 O 1 IO_P144 770 1 Z
bit 770 C 1 *
bit 769 I 1 IO_P143
bit 768 O 1 IO_P143 767 1 Z
bit 767 C 1 *
bit 766 I 1 IO_P141
bit 765 O 1 IO_P141 764 1 Z
bit 764 C 1 *
bit 763 I 1 IO_P140
bit 762 O 1 IO_P140 761 1 Z
bit 761 C 1 *
bit 760 I 1 IO_P139
bit 759 O 1 IO_P139 758 1 Z
bit 758 C 1 *
bit 757 I 1 IO_P138
bit 756 O 1 IO_P138 755 1 Z
bit 755 C 1 *
bit 754 O 1 *
bit 753 O 1 *
bit 752 O 1 *
bit 751 O 1 *
bit 750 O 1 *
bit 749 O 1 *
bit 748 O 1 *
bit 747 O 1 *
bit 746 O 1 *
bit 745 O 1 *
bit 744 O 1 *
bit 743 O 1 *
bit 742 O 1 *
bit 741 O 1 *
bit 740 O 1 *
bit 739 O 1 *
bit 738 O 1 *
bit 737 O 1 *
bit 736 O 1 *
bit 735 O 1 *
bit 734 O 1 *
bit 733 O 1 *
bit 732 O 1 *
bit 731 O 1 *
bit 730 I 1 IO_P137
bit 729 O 1 IO_P137 728 1 Z
bit 728 C 1 *
bit 727 I 1 IO_P135
bit 726 O 1 IO_P135 725 1 Z
bit 725 C 1 *
bit 724 I 1 IO_P133
bit 723 O 1 IO_P133 722 1 Z
bit 722 C 1 *
bit 721 I 1 IO_P132
bit 720 O 1 IO_P132 719 1 Z
bit 719 C 1 *
bit 718 I 1 IO_P131
bit 717 O 1 IO_P131 716 1 Z
bit 716 C 1 *
bit 715 I 1 IO_P130
bit 714 O 1 IO_P130 713 1 Z
bit 713 C 1 *
bit 712 I 1 IO_P128
bit 711 O 1 IO_P128 710 1 Z
bit 710 C 1 *
bit 709 I 1 IO_P126
bit 708 O 1 IO_P126 707 1 Z
bit 707 C 1 *
bit 706 O 1 *
bit 705 O 1 *
bit 704 O 1 *
bit 703 O 1 *
bit 702 O 1 *
bit 701 O 1 *
bit 700 O 1 *
bit 699 O 1 *
bit 698 O 1 *
bit 697 O 1 *
bit 696 O 1 *
bit 695 O 1 *
bit 694 O 1 *
bit 693 O 1 *
bit 692 O 1 *
bit 691 O 1 *
bit 690 O 1 *
bit 689 O 1 *
bit 688 O 1 *
bit 687 O 1 *
bit 686 O 1 *
bit 685 O 1 *
bit 684 O 1 *
bit 683 O 1 *
bit 682 I 1 IO_P125
bit 681 O 1 IO_P125 680 1 Z
bit 680 C 1 *
bit 679 I 1 IO_P124
bit 678 O 1 IO_P124 677 1 Z
bit 677 C 1 *
bit 676 I 1 IO_P123
bit 675 O 1 IO_P123 674 1 Z
bit 674 C 1 *
bit 673 I 1 IO_P122
bit 672 O 1 IO_P122 671 1 Z
bit 671 C 1 *
bit 670 I 1 IO_P120
bit 669 O 1 IO_P120 668 1 Z
bit 668 C 1 *
bit 667 I 1 IO_P119
bit 666 O 1 IO_P119 665 1 Z
bit 665 C 1 *
bit 664 I 1 IO_P117
bit 663 O 1 IO_P117 662 1 Z
bit 662 C 1 *
bit 661 I 1 IO_P116
bit 660 O 1 IO_P116 659 1 Z
bit 659 C 1 *
bit 658 I 1 IO_P115
bit 657 O 1 IO_P115 656 1 Z
bit 656 C 1 *
bit 655 I 1 IO_P114
bit 654 O 1 IO_P114 653 1 Z
bit 653 C 1 *
bit 652 I 1 IO_P113
bit 651 O 1 IO_P113 650 1 Z
bit 650 C 1 *
bit 649 I 1 IO_P111
bit 648 O 1 IO_P111 647 1 Z
bit 647 C 1 *
bit 646 I 1 IO_P109
bit 645 O 1 IO_P109 644 1 Z
bit 644 C 1 *
bit 643 I 1 IO_P108
bit 642 O 1 IO_P108 641 1 Z
bit 641 C 1 *
bit 640 O 1 *
bit 639 O 1 *
bit 638 O 1 *
bit 637 O 1 *
bit 636 O 1 *
bit 635 O 1 *
bit 634 O 1 *
bit 633 O 1 *
bit 632 O 1 *
bit 631 O 1 *
bit 630 O 1 *
bit 629 O 1 *
bit 628 I 1 IO_P107
bit 627 O 1 IO_P107 626 1 Z
bit 626 C 1 *
bit 625 I 1 IO_P106
bit 624 O 1 IO_P106 623 1 Z
bit 623 C 1 *
bit 622 I 1 CCLK_P104
bit 621 O 1 CCLK_P104 620 1 Z
bit 620 C 1 *
bit 619 I 1 DONE_P103
bit 618 O 1 DONE_P103 617 1 Z
bit 617 C 1 *
bit 616 I 1 IO_P102
bit 615 O 1 IO_P102 614 1 Z
bit 614 C 1 *
bit 613 I 1 IO_P101
bit 612 O 1 IO_P101 611 1 Z
bit 611 C 1 *
bit 610 I 1 IO_P100
bit 609 O 1 IO_P100 608 1 Z
bit 608 C 1 *
bit 607 O 1 *
bit 606 O 1 *
bit 605 O 1 *
bit 604 O 1 *
bit 603 O 1 *
bit 602 O 1 *
bit 601 O 1 *
bit 600 O 1 *
bit 599 O 1 *
bit 598 O 1 *
bit 597 O 1 *
bit 596 O 1 *
bit 595 O 1 *
bit 594 O 1 *
bit 593 O 1 *
bit 592 O 1 *
bit 591 O 1 *
bit 590 O 1 *
bit 589 O 1 *
bit 588 O 1 *
bit 587 O 1 *
bit 586 O 1 *
bit 585 O 1 *
bit 584 O 1 *
bit 583 O 1 *
bit 582 O 1 *
bit 581 O 1 *
bit 580 O 1 *
bit 579 O 1 *
bit 578 O 1 *
bit 577 I 1 IO_P97
bit 576 O 1 IO_P97 575 1 Z
bit 575 C 1 *
bit 574 O 1 *
bit 573 O 1 *
bit 572 O 1 *
bit 571 I 1 IO_P96
bit 570 O 1 IO_P96 569 1 Z
bit 569 C 1 *
bit 568 O 1 *
bit 567 O 1 *
bit 566 O 1 *
bit 565 O 1 *
bit 564 O 1 *
bit 563 O 1 *
bit 562 I 1 IO_P95
bit 561 O 1 IO_P95 560 1 Z
bit 560 C 1 *
bit 559 I 1 IO_P94
bit 558 O 1 IO_P94 557 1 Z
bit 557 C 1 *
bit 556 I 1 IO_P93
bit 555 O 1 IO_P93 554 1 Z
bit 554 C 1 *
bit 553 I 1 IO_P92
bit 552 O 1 IO_P92 551 1 Z
bit 551 C 1 *
bit 550 I 1 IO_P90
bit 549 O 1 IO_P90 548 1 Z
bit 548 C 1 *
bit 547 O 1 *
bit 546 O 1 *
bit 545 O 1 *
bit 544 O 1 *
bit 543 O 1 *
bit 542 O 1 *
bit 541 O 1 *
bit 540 O 1 *
bit 539 O 1 *
bit 538 O 1 *
bit 537 O 1 *
bit 536 O 1 *
bit 535 O 1 *
bit 534 O 1 *
bit 533 O 1 *
bit 532 I 1 IO_P87
bit 531 O 1 IO_P87 530 1 Z
bit 530 C 1 *
bit 529 I 1 IO_P86
bit 528 O 1 IO_P86 527 1 Z
bit 527 C 1 *
bit 526 I 1 IO_P85
bit 525 O 1 IO_P85 524 1 Z
bit 524 C 1 *
bit 523 I 1 IO_P83
bit 522 O 1 IO_P83 521 1 Z
bit 521 C 1 *
bit 520 I 1 IO_P81
bit 519 O 1 IO_P81 518 1 Z
bit 518 C 1 *
bit 517 I 1 IO_P80
bit 516 O 1 IO_P80 515 1 Z
bit 515 C 1 *
bit 514 I 1 IO_P79
bit 513 O 1 IO_P79 512 1 Z
bit 512 C 1 *
bit 511 I 1 IO_P78
bit 510 O 1 IO_P78 509 1 Z
bit 509 C 1 *
bit 508 I 1 IO_P77
bit 507 O 1 IO_P77 506 1 Z
bit 506 C 1 *
bit 505 I 1 IO_P76
bit 504 O 1 IO_P76 503 1 Z
bit 503 C 1 *
bit 502 I 1 IO_P74
bit 501 O 1 IO_P74 500 1 Z
bit 500 C 1 *
bit 499 I 1 IO_P72
bit 498 O 1 IO_P72 497 1 Z
bit 497 C 1 *
bit 496 I 1 IO_P71
bit 495 O 1 IO_P71 494 1 Z
bit 494 C 1 *
bit 493 O 1 *
bit 492 O 1 *
bit 491 O 1 *
bit 490 O 1 *
bit 489 O 1 *
bit 488 O 1 *
bit 487 O 1 *
bit 486 O 1 *
bit 485 O 1 *
bit 484 O 1 *
bit 483 O 1 *
bit 482 O 1 *
bit 481 O 1 *
bit 480 O 1 *
bit 479 O 1 *
bit 478 I 1 IO_P68
bit 477 O 1 IO_P68 476 1 Z
bit 476 C 1 *
bit 475 I 1 IO_P67
bit 474 O 1 IO_P67 473 1 Z
bit 473 C 1 *
bit 472 I 1 IO_P65
bit 471 O 1 IO_P65 470 1 Z
bit 470 C 1 *
bit 469 I 1 IO_P64
bit 468 O 1 IO_P64 467 1 Z
bit 467 C 1 *
bit 466 I 1 IO_P63
bit 465 O 1 IO_P63 464 1 Z
bit 464 C 1 *
bit 463 O 1 *
bit 462 O 1 *
bit 461 O 1 *
bit 460 O 1 *
bit 459 O 1 *
bit 458 O 1 *
bit 457 O 1 *
bit 456 O 1 *
bit 455 O 1 *
bit 454 O 1 *
bit 453 O 1 *
bit 452 O 1 *
bit 451 O 1 *
bit 450 O 1 *
bit 449 O 1 *
bit 448 O 1 *
bit 447 O 1 *
bit 446 O 1 *
bit 445 O 1 *
bit 444 O 1 *
bit 443 O 1 *
bit 442 O 1 *
bit 441 O 1 *
bit 440 O 1 *
bit 439 O 1 *
bit 438 O 1 *
bit 437 O 1 *
bit 436 O 1 *
bit 435 O 1 *
bit 434 O 1 *
bit 433 I 1 IO_P62
bit 432 O 1 IO_P62 431 1 Z
bit 431 C 1 *
bit 430 I 1 IO_P61
bit 429 O 1 IO_P61 428 1 Z
bit 428 C 1 *
bit 427 O 1 *
bit 426 O 1 *
bit 425 O 1 *
bit 424 O 1 *
bit 423 O 1 *
bit 422 O 1 *
bit 421 O 1 *
bit 420 O 1 *
bit 419 O 1 *
bit 418 O 1 *
bit 417 O 1 *
bit 416 O 1 *
bit 415 O 1 *
bit 414 O 1 *
bit 413 O 1 *
bit 412 I 1 IO_P58
bit 411 O 1 IO_P58 410 1 Z
bit 410 C 1 *
bit 409 I 1 IO_P57
bit 408 O 1 IO_P57 407 1 Z
bit 407 C 1 *
bit 406 I 1 M2_P56
bit 405 I 1 M0_P55
bit 404 I 1 M1_P54
bit 403 I 1 IO_P52
bit 402 O 1 IO_P52 401 1 Z
bit 401 C 1 *
bit 400 I 1 IO_P51
bit 399 O 1 IO_P51 398 1 Z
bit 398 C 1 *
bit 397 O 1 *
bit 396 O 1 *
bit 395 O 1 *
bit 394 O 1 *
bit 393 O 1 *
bit 392 O 1 *
bit 391 O 1 *
bit 390 O 1 *
bit 389 O 1 *
bit 388 O 1 *
bit 387 O 1 *
bit 386 O 1 *
bit 385 O 1 *
bit 384 O 1 *
bit 383 O 1 *
bit 382 I 1 IO_P50
bit 381 O 1 IO_P50 380 1 Z
bit 380 C 1 *
bit 379 I 1 IO_P48
bit 378 O 1 IO_P48 377 1 Z
bit 377 C 1 *
bit 376 I 1 IO_P46
bit 375 O 1 IO_P46 374 1 Z
bit 374 C 1 *
bit 373 I 1 IO_P45
bit 372 O 1 IO_P45 371 1 Z
bit 371 C 1 *
bit 370 I 1 IO_P44
bit 369 O 1 IO_P44 368 1 Z
bit 368 C 1 *
bit 367 I 1 IO_P43
bit 366 O 1 IO_P43 365 1 Z
bit 365 C 1 *
bit 364 I 1 IO_P42
bit 363 O 1 IO_P42 362 1 Z
bit 362 C 1 *
bit 361 I 1 IO_P40
bit 360 O 1 IO_P40 359 1 Z
bit 359 C 1 *
bit 358 I 1 IO_P39
bit 357 O 1 IO_P39 356 1 Z
bit 356 C 1 *
bit 355 I 1 IO_P37
bit 354 O 1 IO_P37 353 1 Z
bit 353 C 1 *
bit 352 I 1 IO_P36
bit 351 O 1 IO_P36 350 1 Z
bit 350 C 1 *
bit 349 I 1 IO_P35
bit 348 O 1 IO_P35 347 1 Z
bit 347 C 1 *
bit 346 I 1 IO_P34
bit 345 O 1 IO_P34 344 1 Z
bit 344 C 1 *
bit 343 O 1 *
bit 342 O 1 *
bit 341 O 1 *
bit 340 O 1 *
bit 339 O 1 *
bit 338 O 1 *
bit 337 O 1 *
bit 336 O 1 *
bit 335 O 1 *
bit 334 O 1 *
bit 333 O 1 *
bit 332 O 1 *
bit 331 O 1 *
bit 330 O 1 *
bit 329 O 1 *
bit 328 O 1 *
bit 327 O 1 *
bit 326 O 1 *
bit 325 O 1 *
bit 324 O 1 *
bit 323 O 1 *
bit 322 O 1 *
bit 321 O 1 *
bit 320 O 1 *
bit 319 I 1 IO_P33
bit 318 O 1 IO_P33 317 1 Z
bit 317 C 1 *
bit 316 I 1 IO_P31
bit 315 O 1 IO_P31 314 1 Z
bit 314 C 1 *
bit 313 I 1 IO_P29
bit 312 O 1 IO_P29 311 1 Z
bit 311 C 1 *
bit 310 I 1 IO_P28
bit 309 O 1 IO_P28 308 1 Z
bit 308 C 1 *
bit 307 I 1 IO_P27
bit 306 O 1 IO_P27 305 1 Z
bit 305 C 1 *
bit 304 I 1 IO_P26
bit 303 O 1 IO_P26 302 1 Z
bit 302 C 1 *
bit 301 I 1 IO_P24
bit 300 O 1 IO_P24 299 1 Z
bit 299 C 1 *
bit 298 I 1 IO_P22
bit 297 O 1 IO_P22 296 1 Z
bit 296 C 1 *
bit 295 O 1 *
bit 294 O 1 *
bit 293 O 1 *
bit 292 O 1 *
bit 291 O 1 *
bit 290 O 1 *
bit 289 O 1 *
bit 288 O 1 *
bit 287 O 1 *
bit 286 O 1 *
bit 285 O 1 *
bit 284 O 1 *
bit 283 O 1 *
bit 282 O 1 *
bit 281 O 1 *
bit 280 O 1 *
bit 279 O 1 *
bit 278 O 1 *
bit 277 O 1 *
bit 276 O 1 *
bit 275 O 1 *
bit 274 O 1 *
bit 273 O 1 *
bit 272 O 1 *
bit 271 I 1 IO_P21
bit 270 O 1 IO_P21 269 1 Z
bit 269 C 1 *
bit 268 I 1 IO_P20
bit 267 O 1 IO_P20 266 1 Z
bit 266 C 1 *
bit 265 I 1 IO_P19
bit 264 O 1 IO_P19 263 1 Z
bit 263 C 1 *
bit 262 I 1 IO_P18
bit 261 O 1 IO_P18 260 1 Z
bit 260 C 1 *
bit 259 I 1 IO_P16
bit 258 O 1 IO_P16 257 1 Z
bit 257 C 1 *
bit 256 I 1 IO_P15
bit 255 O 1 IO_P15 254 1 Z
bit 254 C 1 *
bit 253 I 1 IO_P13
bit 252 O 1 IO_P13 251 1 Z
bit 251 C 1 *
bit 250 I 1 IO_P12
bit 249 O 1 IO_P12 248 1 Z
bit 248 C 1 *
bit 247 I 1 IO_P11
bit 246 O 1 IO_P11 245 1 Z
bit 245 C 1 *
bit 244 I 1 IO_P10
bit 243 O 1 IO_P10 242 1 Z
bit 242 C 1 *
bit 241 I 1 IO_P9
bit 240 O 1 IO_P9 239 1 Z
bit 239 C 1 *
bit 238 I 1 IO_P7
bit 237 O 1 IO_P7 236 1 Z
bit 236 C 1 *
bit 235 O 1 *
bit 234 O 1 *
bit 233 O 1 *
bit 232 O 1 *
bit 231 O 1 *
bit 230 O 1 *
bit 229 I 1 IO_P5
bit 228 O 1 IO_P5 227 1 Z
bit 227 C 1 *
bit 226 I 1 IO_P4
bit 225 O 1 IO_P4 224 1 Z
bit 224 C 1 *
bit 223 O 1 *
bit 222 O 1 *
bit 221 O 1 *
bit 220 O 1 *
bit 219 O 1 *
bit 218 O 1 *
bit 217 I 1 IO_P3
bit 216 O 1 IO_P3 215 1 Z
bit 215 C 1 *
bit 214 I 1 IO_P2
bit 213 O 1 IO_P2 212 1 Z
bit 212 C 1 *
bit 211 O 1 *
bit 210 I 1 HSWAP_EN_P206
bit 209 I 1 IO_P205
bit 208 O 1 IO_P205 207 1 Z
bit 207 C 1 *
bit 206 I 1 IO_P204
bit 205 O 1 IO_P204 204 1 Z
bit 204 C 1 *
bit 203 I 1 IO_P203
bit 202 O 1 IO_P203 201 1 Z
bit 201 C 1 *
bit 200 O 1 *
bit 199 O 1 *
bit 198 O 1 *
bit 197 O 1 *
bit 196 O 1 *
bit 195 O 1 *
bit 194 O 1 *
bit 193 O 1 *
bit 192 O 1 *
bit 191 O 1 *
bit 190 O 1 *
bit 189 O 1 *
bit 188 O 1 *
bit 187 O 1 *
bit 186 O 1 *
bit 185 O 1 *
bit 184 O 1 *
bit 183 O 1 *
bit 182 O 1 *
bit 181 O 1 *
bit 180 O 1 *
bit 179 O 1 *
bit 178 O 1 *
bit 177 O 1 *
bit 176 O 1 *
bit 175 O 1 *
bit 174 O 1 *
bit 173 O 1 *
bit 172 O 1 *
bit 171 O 1 *
bit 170 O 1 *
bit 169 O 1 *
bit 168 O 1 *
bit 167 O 1 *
bit 166 O 1 *
bit 165 O 1 *
bit 164 I 1 IO_P200
bit 163 O 1 IO_P200 162 1 Z
bit 162 C 1 *
bit 161 O 1 *
bit 160 O 1 *
bit 159 O 1 *
bit 158 O 1 *
bit 157 O 1 *
bit 156 O 1 *
bit 155 I 1 IO_P199
bit 154 O 1 IO_P199 153 1 Z
bit 153 C 1 *
bit 152 I 1 IO_P198
bit 151 O 1 IO_P198 150 1 Z
bit 150 C 1 *
bit 149 I 1 IO_P197
bit 148 O 1 IO_P197 147 1 Z
bit 147 C 1 *
bit 146 I 1 IO_P196
bit 145 O 1 IO_P196 144 1 Z
bit 144 C 1 *
bit 143 I 1 IO_P194
bit 142 O 1 IO_P194 141 1 Z
bit 141 C 1 *
bit 140 O 1 *
bit 139 O 1 *
bit 138 O 1 *
bit 137 O 1 *
bit 136 O 1 *
bit 135 O 1 *
bit 134 O 1 *
bit 133 O 1 *
bit 132 O 1 *
bit 131 O 1 *
bit 130 O 1 *
bit 129 O 1 *
bit 128 O 1 *
bit 127 O 1 *
bit 126 O 1 *
bit 125 I 1 IO_P191
bit 124 O 1 IO_P191 123 1 Z
bit 123 C 1 *
bit 122 I 1 IO_P190
bit 121 O 1 IO_P190 120 1 Z
bit 120 C 1 *
bit 119 I 1 IO_P189
bit 118 O 1 IO_P189 117 1 Z
bit 117 C 1 *
bit 116 I 1 IO_P187
bit 115 O 1 IO_P187 114 1 Z
bit 114 C 1 *
bit 113 I 1 IO_P185
bit 112 O 1 IO_P185 111 1 Z
bit 111 C 1 *
bit 110 I 1 IO_P184
bit 109 O 1 IO_P184 108 1 Z
bit 108 C 1 *
bit 107 I 1 IO_P183
bit 106 O 1 IO_P183 105 1 Z
bit 105 C 1 *
bit 104 I 1 IO_P182
bit 103 O 1 IO_P182 102 1 Z
bit 102 C 1 *
bit 101 I 1 IO_P181
bit 100 O 1 IO_P181 99 1 Z
bit 99 C 1 *
bit 98 I 1 IO_P180
bit 97 O 1 IO_P180 96 1 Z
bit 96 C 1 *
bit 95 I 1 IO_P178
bit 94 O 1 IO_P178 93 1 Z
bit 93 C 1 *
bit 92 I 1 IO_P176
bit 91 O 1 IO_P176 90 1 Z
bit 90 C 1 *
bit 89 I 1 IO_P175
bit 88 O 1 IO_P175 87 1 Z
bit 87 C 1 *
bit 86 O 1 *
bit 85 O 1 *
bit 84 O 1 *
bit 83 O 1 *
bit 82 O 1 *
bit 81 O 1 *
bit 80 O 1 *
bit 79 O 1 *
bit 78 O 1 *
bit 77 O 1 *
bit 76 O 1 *
bit 75 O 1 *
bit 74 O 1 *
bit 73 O 1 *
bit 72 O 1 *
bit 71 I 1 IO_P172
bit 70 O 1 IO_P172 69 1 Z
bit 69 C 1 *
bit 68 I 1 IO_P171
bit 67 O 1 IO_P171 66 1 Z
bit 66 C 1 *
bit 65 I 1 IO_P169
bit 64 O 1 IO_P169 63 1 Z
bit 63 C 1 *
bit 62 I 1 IO_P168
bit 61 O 1 IO_P168 60 1 Z
bit 60 C 1 *
bit 59 I 1 IO_P167
bit 58 O 1 IO_P167 57 1 Z
bit 57 C 1 *
bit 56 O 1 *
bit 55 O 1 *
bit 54 O 1 *
bit 53 O 1 *
bit 52 O 1 *
bit 51 O 1 *
bit 50 O 1 *
bit 49 O 1 *
bit 48 O 1 *
bit 47 O 1 *
bit 46 O 1 *
bit 45 O 1 *
bit 44 O 1 *
bit 43 O 1 *
bit 42 O 1 *
bit 41 O 1 *
bit 40 O 1 *
bit 39 O 1 *
bit 38 O 1 *
bit 37 O 1 *
bit 36 O 1 *
bit 35 O 1 *
bit 34 O 1 *
bit 33 O 1 *
bit 32 O 1 *
bit 31 O 1 *
bit 30 O 1 *
bit 29 O 1 *
bit 28 O 1 *
bit 27 O 1 *
bit 26 I 1 IO_P166
bit 25 O 1 IO_P166 24 1 Z
bit 24 C 1 *
bit 23 I 1 IO_P165
bit 22 O 1 IO_P165 21 1 Z
bit 21 C 1 *
bit 20 O 1 *
bit 19 O 1 *
bit 18 O 1 *
bit 17 O 1 *
bit 16 O 1 *
bit 15 O 1 *
bit 14 O 1 *
bit 13 O 1 *
bit 12 O 1 *
bit 11 O 1 *
bit 10 O 1 *
bit 9 O 1 *
bit 8 O 1 *
bit 7 O 1 *
bit 6 O 1 *
bit 5 I 1 IO_P162
bit 4 O 1 IO_P162 3 1 Z
bit 3 C 1 *
bit 2 I 1 IO_P161
bit 1 O 1 IO_P161 0 1 Z
bit 0 C 1 *
