#
# $Id: lh7a400 698 2007-11-06 19:23:57Z kawk $
#
# Copyright (C) 2004 IDK Chemnitz GmbH
#
# This program is free software; you can redistribute it and/or
# modify it under the terms of the GNU General Public License
# as published by the Free Software Foundation; either version 2
# of the License, or (at your option) any later version.
#
# This program is distributed in the hope that it will be useful,
# but WITHOUT ANY WARRANTY; without even the implied warranty of
# MERCHANTABILITY or FITNESS FOR A PARTICULAR PURPOSE.  See the
# GNU General Public License for more details.
#
# You should have received a copy of the GNU General Public License
# along with this program; if not, write to the Free Software
# Foundation, Inc., 59 Temple Place - Suite 330, Boston, MA
# 02111-1307, USA.
#
# Written by Marko Roessler <marko.roessler@indakom.de> , 2004.
#

# mandatory data registers
register	BSR	507
register	BR	1
register	IR	4
register	DIR	32

# see page 250 in [1]
instruction length 4
# mandatory instructions
instruction EXTEST		0000	BSR	# 
instruction SCAN_N              0010    BSR	# choose chain
instruction INTEST              1100    BSR	#
instruction IDCODE		1110	DIR	#
instruction BYPASS		1111	BR	# 
instruction CLAMP               0101    BSR	#
instruction HIGHZ               0111    BSR	#
instruction CLAMPZ              1001    BSR	#
instruction SAMPLE/PRELOAD	0011	BSR	# 



signal	CS6	B10
signal	CS7	C10
signal	nCS3	M12
signal	nCS2	P13
signal	nCS1	K10
signal	nCS0	K11
signal	nWE3	D10
signal	OSCEN	P14
signal	PA7	L3
signal	PA6	L2
signal	PA5	L1
signal	PA4	K5
signal	PA3	K3
signal	PA2	K2
signal	PA1	K1
signal	PA0	J5
signal	PB7	N3
signal	PB6	N2
signal	PB5	N1
signal	PB4	M4
signal	PB3	M2
signal	PB2	L7
signal	PB1	L5
signal	PB0	L4
signal	PC7	R2
signal	PC6	T2
signal	PC5	T1
signal	PC4	L8
signal	PC3	K6
signal	PC2	R1
signal	PC1	P2
signal	PC0	P1
signal	PD7	R10
signal	PD6	P10
signal	PD5	T9
signal	PD4	R9
signal	PD3	N11
signal	PD2	K8
signal	PD1	L11
signal	PD0	M11
signal	PE3	M10
signal	PE2	M9
signal	PE1	N10
signal	PE0	L10
signal	PF7	C5
signal	PF6	E6
signal	PF5	D6
signal	PF4	B5
signal	PF3	H8
signal	PF2	C6
signal	PF1	B6
signal	PF0	A6
signal	PG7	N4
signal	PG6	M8
signal	PG5	M7
signal	PG4	N6
signal	PG3	M6
signal	PG2	L6
signal	PG1	T3
signal	PG0	R3
signal	PH7	T5
signal	PH6	R5
signal	PH5	P5
signal	PH4	P8
signal	PH3	N7
signal	PH2	T4 
signal	PH1	R4
signal	PH0	P4
signal	IRTX2	F2
signal	IRRX2	F3
signal	UARTTXD2	F4
signal	UARTRXD2	J7
signal	UARTCTS2	E2
signal	UARTDCD2	E3
signal	UARTDSR2	E5
signal	XTAL32OUT	P15
signal	XTAL32IN	P16
signal	AC97IN	A4
signal	AC97CLK	C4
signal	AC97OUT	D5
signal	AC97SYNC	B4
signal	SSPRX	J1
signal	SSPFRM	J3
signal	SSPTX	J2
signal	SSPCLK	H4
signal	PGMCLK	J6
signal	PWM1	B7
signal	PWM0	C7
signal	PWMEN1 D7
signal	PWMEN0 E7
signal	COL7	H2
signal	COL6	H1
signal	COL5	G5
signal	COL4	G4
signal	COL3	G2
signal	COL2	G1
signal	COL1	F5
signal	COL0	F6
signal	BUZ	H3
signal	D31	D11
signal	D30	B11
signal 	D29	B12
signal	D28	G10
signal	D27	E12
signal	D26	C13
signal	D25	B13
signal	D24	A14
signal	D23	A16
signal	D22	F10
signal	D21	D14
signal	D20	H10
signal	D19	D16
signal	D18	E14
signal	D17	F12
signal	D16	F15
signal	D15	G12
signal	D14	G11
signal	D13	G15
signal	D12	H13
signal	D11	H15
signal	D10	J10
signal	D9	J13
signal	D8	J15
signal	D7	K12
signal	D6	H11
signal	D5	L14
signal	D4	L15
signal	D3	L16
signal	D2	N13
signal	D1	M15
signal	D0	L12
signal	A27	A8
signal	A26	F8
signal	A25	G8
signal	A24	A13 
signal	A23	A15
signal	A22	B16
signal	A21	C16
signal	A20	D15
signal	A19	F11
signal	A18	E13
signal	A17	E16
signal	A16	F14
signal	A15	F16
signal	A14	G13
signal	A13	G14
signal	A12	G16 
signal	A11	H14
signal	A10	H16
signal	A9	J9
signal	A8	J14 
signal	A7	J16
signal	A6	J8
signal	A5	K14
signal	A4	K15
signal	A3	K16
signal	A2	M13
signal	A1	N14
signal	A0	M16
signal	nBATCHG	D2
signal	nEXTPWR	C2
signal	BATOK	D1
signal	nPOR	D3
signal	MEDCHG	C3
signal	XTALIN	R13
signal	XTALOUT	T13
signal	nURESET	H6
signal	WAKEUP	D4
signal	nPWRFL	E4
signal	LCDLP	R8
signal	LCDDCLK	N9
signal	LCDFP	R6
signal	LCDM	P9
signal	LCDVD3	N8
signal	LCDVD2	T7
signal	LCDVD1	R7
signal	LCDVD0	P7
signal	nRAS	F9
signal	nCAS	C11
signal	nSWE	C12
signal	nSCS3	A12
signal	nSCS2	E11
signal	nSCS1	D13
signal	nSCS0	C14
signal	SCLK	A10
signal	SCKEN3	G9
signal	DQM0	A9
signal	DQM1	B9
signal	DQM2	D9
signal	DQM3	E9
signal	nWE0	C8
signal	nOE	D8
signal	MMCCLK	A3
signal	MMCCMD	B3
signal	MMCDATA	A2
signal	nTEST1	R15
signal	nTEST0	T12
signal	WIDTH1	R12
signal	WIDTH0	P11
signal	USBDP	T15
signal	USBDN	T16
signal	TDI	A1
signal	TDO	B2
signal	TMST	C1
signal	TCLK	B1
signal	VDD	G17 F1 K7 M1 M5 T6 R14 M14 J11 J12 F13 E10 B8
signal	VSS	H7 G3 K4 N5 P6 T14 R16 N16 K13 H9 C15 A11 E8 A5 F7
signal	VDDC	E1 J4 P3 T8 K9 L13 E15 D12 A7
signal	VSSC	C9 M3 L9 T10 N15 H12 B15 G6
signal	VDDA1	R11
signal	VSSA1	T11
signal	VDDA2	N12
signal	VSSA2	P12



bit 506 I 1 nEXTPWR
bit 505 I 1 MEDCHG
bit 504 I 1 BATOK
bit 503 I 1 nBATCHG
bit 502 I 1 WAKEUP
bit 501 I 1 UARTCTS2
bit 500 C 0 UARTCTS2
bit 499 O 1 UARTCTS2 500 0 Z
bit 498 I 1 UARTDCD2
bit 497 C 0 UARTDCD2
bit 496 O 1 UARTDCD2 497 0 Z
bit 495 I 1 nPWRFL
bit 494 I 1 UARTDSR2
bit 493 C 0 UARTDSR2
bit 492 O 1 UARTDSR2 493 0 Z
bit 491 I 1 IRTX2
bit 490 C 0 IRTX2
bit 489 O 1 IRTX2 490 0 Z
bit 488 I 1 IRRX2
bit 487 C 0 IRRX2
bit 486 O 1 IRRX2 487 0 Z
bit 485 I 1 UARTTXD2
bit 484 C 0 UARTTXD2
bit 483 O 1 UARTTXD2 484 0 Z
bit 482 I 1 UARTRXD2
bit 481 C 0 UARTRXD2
bit 480 O 1 UARTRXD2 481 0 Z
bit 479 I 1 COL0
bit 478 C 0 COL0
bit 477 O 1 COL0 478 0 Z
bit 476 I 1 COL1
bit 475 C 0 COL1
bit 474 O 1 COL1 475 0 Z
bit 473 I 1 COL2
bit 472 C 0 COL2
bit 471 O 1 COL2 472 0 Z
bit 470 I 1 COL3
bit 469 C 0 COL3
bit 468 O 1 COL3 469 0 Z
bit 467 I 1 COL4
bit 466 C 0 COL4
bit 465 O 1 COL4 466 0 Z
bit 464 I 1 COL5
bit 463 C 0 COL5
bit 462 O 1 COL5 463 0 Z
bit 461 I 1 COL6
bit 460 C 0 COL6
bit 459 O 1 COL6 460 0 Z
bit 458 I 1 COL7
bit 457 C 0 COL7
bit 456 O 1 COL7 457 0 Z
bit 455 I 1 BUZ
bit 454 C 0 BUZ
bit 453 O 1 BUZ 454 0 Z
bit 452 C 0 SSPCLK
bit 451 O 1 SSPCLK 452 0 Z
bit 450 C 0 PGMCLK
bit 449 O 1 PGMCLK 450 0 Z
bit 448 I 1 SSPRX
bit 447 C 0 SSPRX
bit 446 O 1 SSPRX 447 0 Z
bit 445 C 0 SSPTX
bit 444 O 1 SSPTX 445 0 Z
bit 443 C 0 SSPFRM
bit 442 O 1 SSPFRM 443 0 Z
bit 441 I 1 PA0
bit 440 C 0 PA0
bit 439 O 1 PA0 440 0 Z
bit 438 I 1 PA1
bit 437 C 0 PA1
bit 436 O 1 PA1 437 0 Z
bit 435 I 1 PA2
bit 434 C 0 PA2
bit 433 O 1 PA2 434 0 Z
bit 432 I 1 PA3
bit 431 C 0 PA3
bit 430 O 1 PA3 431 0 Z
bit 429 I 1 PA4
bit 428 C 0 PA4
bit 427 O 1 PA4 428 0 Z
bit 426 I 1 PA5
bit 425 C 0 PA5
bit 424 O 1 PA5 425 0 Z
bit 423 I 1 PA6
bit 422 C 0 PA6
bit 421 O 1 PA6 422 0 Z
bit 420 I 1 PA7
bit 419 C 0 PA7
bit 418 O 1 PA7 419 0 Z
bit 417 I 1 PB0
bit 416 C 0 PB0
bit 415 O 1 PB0 416 0 Z
bit 414 I 1 PB1
bit 413 C 0 PB1
bit 412 O 1 PB1 413 0 Z
bit 411 I 1 PB2
bit 410 C 0 PB2
bit 409 O 1 PB2 410 0 Z
bit 408 I 1 PB3
bit 407 C 0 PB3
bit 406 O 1 PB3 407 0 Z
bit 405 I 1 PB4
bit 404 C 0 PB4
bit 403 O 1 PB4 404 0 Z
bit 402 I 1 PB5
bit 401 C 0 PB5
bit 400 O 1 PB5 401 0 Z
bit 399 I 1 PB6
bit 398 C 0 PB6
bit 397 O 1 PB6 398 0 Z
bit 396 I 1 PB7
bit 395 C 0 PB7
bit 394 O 1 PB7 395 0 Z
bit 393 I 1 PC0
bit 392 C 0 PC0
bit 391 O 1 PC0 392 0 Z
bit 390 I 1 PC1
bit 389 C 0 PC1
bit 388 O 1 PC1 389 0 Z
bit 387 I 1 PC2
bit 386 C 0 PC2
bit 385 O 1 PC2 386 0 Z
bit 384 I 1 PC3
bit 383 C 0 PC3
bit 382 O 1 PC3 383 0 Z
bit 381 I 1 PC4
bit 380 C 0 PC4
bit 379 O 1 PC4 380 0 Z
bit 378 I 1 PC5
bit 377 C 0 PC5
bit 376 O 1 PC5 377 0 Z
bit 375 I 1 PC6
bit 374 C 0 PC6
bit 373 O 1 PC6 374 0 Z
bit 372 I 1 PC7
bit 371 C 0 PC7
bit 370 O 1 PC7 371 0 Z
bit 369 I 1 PG0
bit 368 C 0 PG0
bit 367 O 1 PG0 368 0 Z
bit 366 I 1 PG1
bit 365 C 0 PG1
bit 364 O 1 PG1 365 0 Z
bit 363 I 1 PG2
bit 362 C 0 PG2
bit 361 O 1 PG2 362 0 Z
bit 360 I 1 PG3
bit 359 C 0 PG3
bit 358 O 1 PG3 359 0 Z
bit 357 I 1 PG4
bit 356 C 0 PG4
bit 355 O 1 PG4 356 0 Z
bit 354 I 1 PG5
bit 353 C 0 PG5
bit 352 O 1 PG5 353 0 Z
bit 351 I 1 PG6
bit 350 C 0 PG6
bit 349 O 1 PG6 350 0 Z
bit 348 I 1 PG7
bit 347 C 0 PG7
bit 346 O 1 PG7 347 0 Z
bit 345 I 1 PH0
bit 344 C 0 PH0
bit 343 O 1 PH0 344 0 Z
bit 342 I 1 PH1
bit 341 C 0 PH1
bit 340 O 1 PH1 341 0 Z
bit 339 I 1 PH2
bit 338 C 0 PH2
bit 337 O 1 PH2 338 0 Z
bit 336 I 1 PH3
bit 335 C 0 PH3
bit 334 O 1 PH3 335 0 Z
bit 333 I 1 PH4
bit 332 C 0 PH4
bit 331 O 1 PH4 332 0 Z
bit 330 I 1 PH5
bit 329 C 0 PH5
bit 328 O 1 PH5 329 0 Z
bit 327 I 1 PH6
bit 326 C 0 PH6
bit 325 O 1 PH6 326 0 Z
bit 324 I 1 PH7
bit 323 C 0 PH7
bit 322 O 1 PH7 323 0 Z
bit 321 C 0 LCDFP
bit 320 O 1 LCDFP 321 0 Z
bit 319 C 0 LCDVD0
bit 318 O 1 LCDVD0 319 0 Z
bit 317 C 0 LCDVD1
bit 316 O 1 LCDVD1 317 0 Z
bit 315 C 0 LCDVD2
bit 314 O 1 LCDVD2 315 0 Z
bit 313 C 0 LCDVD3
bit 312 O 1 LCDVD3 313 0 Z
bit 311 I 1 PE0
bit 310 C 0 PE0
bit 309 O 1 PE0 310 0 Z
bit 308 C 0 LCDLP
bit 307 O 1 LCDLP 308 0 Z
bit 306 C 0 LCDM
bit 305 O 1 LCDM 306 0 Z
bit 304 C 0 LCDDCLK
bit 303 O 1 LCDDCLK 304 0 Z
bit 302 I 1 PE1
bit 301 C 0 PE1
bit 300 O 1 PE1 301 0 Z
bit 299 I 1 PE2
bit 298 C 0 PE2
bit 297 O 1 PE2 298 0 Z
bit 296 I 1 PE3
bit 295 C 0 PE3
bit 294 O 1 PE3 295 0 Z
bit 293 I 1 PD0
bit 292 C 0 PD0
bit 291 O 1 PD0 292 0 Z
bit 290 I 1 PD1
bit 289 C 0 PD1
bit 288 O 1 PD1 289 0 Z
bit 287 I 1 PD2
bit 286 C 0 PD2
bit 285 O 1 PD2 286 0 Z
bit 284 I 1 PD3
bit 283 C 0 PD3
bit 282 O 1 PD3 283 0 Z
bit 281 I 1 PD4
bit 280 C 0 PD4
bit 279 O 1 PD4 280 0 Z
bit 278 I 1 PD5
bit 277 C 0 PD5
bit 276 O 1 PD5 277 0 Z
bit 275 I 1 PD6
bit 274 C 0 PD6
bit 273 O 1 PD6 274 0 Z
bit 272 I 1 PD7
bit 271 C 0 PD7
bit 270 O 1 PD7 271 0 Z
bit 269 I 1 WIDTH0
bit 268 I 1 WIDTH1
bit 267 C 0 nCS0
bit 266 O 1 nCS0 267 0 Z
bit 265 C 0 nCS1
bit 264 O 1 nCS1 265 0 Z
bit 263 I 1 OSCEN
bit 262 C 0 OSCEN
bit 261 O 1 OSCEN 262 0 Z
bit 260 C 0 nCS2
bit 259 O 1 nCS2 260 0 Z
bit 258 C 0 nCS3
bit 257 O 1 nCS3 258 0 Z
bit 256 I 1 D0
bit 255 C 0 D0
bit 254 O 1 D0 255 0 Z
bit 253 C 0 A0
bit 252 O 1 A0 253 0 Z
bit 251 I 1 D1
bit 250 C 0 D1
bit 249 O 1 D1 250 0 Z
bit 248 C 0 A1
bit 247 O 1 A1 248 0 Z
bit 246 I 1 D2
bit 245 C 0 D2
bit 244 O 1 D2 245 0 Z
bit 243 C 0 A2
bit 242 O 1 A2 243 0 Z
bit 241 I 1 D3
bit 240 C 0 D3
bit 239 O 1 D3 240 0 Z
bit 238 C 0 A3
bit 237 O 1 A3 238 0 Z
bit 236 I 1 D4
bit 235 C 0 D4
bit 234 O 1 D4 235 0 Z
bit 233 C 0 A4
bit 232 O 1 A4 233 0 Z
bit 231 I 1 D5
bit 230 C 0 D5
bit 229 O 1 D5 230 0 Z
bit 228 C 0 A5
bit 227 O 1 A5 228 0 Z
bit 226 I 1 D6
bit 225 C 0 D6
bit 224 O 1 D6 225 0 Z
bit 223 C 0 A6
bit 222 O 1 A6 223 0 Z
bit 221 I 1 D7
bit 220 C 0 D7
bit 219 O 1 D7 220 0 Z
bit 218 C 0 A7
bit 217 O 1 A7 218 0 Z
bit 216 I 1 D8
bit 215 C 0 D8
bit 214 O 1 D8 215 0 Z
bit 213 C 0 A8
bit 212 O 1 A8 213 0 Z
bit 211 I 1 D9
bit 210 C 0 D9
bit 209 O 1 D9 210 0 Z
bit 208 C 0 A9
bit 207 O 1 A9 208 0 Z
bit 206 I 1 D10
bit 205 C 0 D10
bit 204 O 1 D10 205 0 Z
bit 203 C 0 A10
bit 202 O 1 A10 203 0 Z
bit 201 I 1 D11
bit 200 C 0 D11
bit 199 O 1 D11 200 0 Z
bit 198 C 0 A11
bit 197 O 1 A11 198 0 Z
bit 196 I 1 D12
bit 195 C 0 D12
bit 194 O 1 D12 195 0 Z
bit 193 C 0 A12
bit 192 O 1 A12 193 0 Z
bit 191 I 1 D13
bit 190 C 0 D13
bit 189 O 1 D13 190 0 Z
bit 188 C 0 A13
bit 187 O 1 A13 188 0 Z
bit 186 I 1 D14
bit 185 C 0 D14
bit 184 O 1 D14 185 0 Z
bit 183 C 0 A14
bit 182 O 1 A14 183 0 Z
bit 181 I 1 D15
bit 180 C 0 D15
bit 179 O 1 D15 180 0 Z
bit 178 C 0 A15
bit 177 O 1 A15 178 0 Z
bit 176 I 1 D16
bit 175 C 0 D16
bit 174 O 1 D16 175 0 Z
bit 173 C 0 A16
bit 172 O 1 A16 173 0 Z
bit 171 I 1 D17
bit 170 C 0 D17
bit 169 O 1 D17 170 0 Z
bit 168 C 0 A17
bit 167 O 1 A17 168 0 Z
bit 166 I 1 D18
bit 165 C 0 D18
bit 164 O 1 D18 165 0 Z
bit 163 C 0 A18
bit 162 O 1 A18 163 0 Z
bit 161 I 1 D19
bit 160 C 0 D19
bit 159 O 1 D19 160 0 Z
bit 158 C 0 A19
bit 157 O 1 A19 158 0 Z
bit 156 I 1 D20
bit 155 C 0 D20
bit 154 O 1 D20 155 0 Z
bit 153 C 0 A20
bit 152 O 1 A20 153 0 Z
bit 151 I 1 D21
bit 150 C 0 D21
bit 149 O 1 D21 150 0 Z
bit 148 C 0 A21
bit 147 O 1 A21 148 0 Z
bit 146 I 1 D22
bit 145 C 0 D22
bit 144 O 1 D22 145 0 Z
bit 143 C 0 A22
bit 142 O 1 A22 143 0 Z
bit 141 I 1 D23
bit 140 C 0 D23
bit 139 O 1 D23 140 0 Z
bit 138 C 0 A23
bit 137 O 1 A23 138 0 Z
bit 136 I 1 D24
bit 135 C 0 D24
bit 134 O 1 D24 135 0 Z
bit 133 C 0 A24
bit 132 O 1 A24 133 0 Z
bit 131 I 1 D25
bit 130 C 0 D25
bit 129 O 1 D25 130 0 Z
bit 128 I 1 nSCS0
bit 127 C 0 nSCS0
bit 126 O 1 nSCS0 127 0 Z
bit 125 I 1 D26
bit 124 C 0 D26
bit 123 O 1 D26 124 0 Z
bit 122 I 1 nSCS1
bit 121 C 0 nSCS1
bit 120 O 1 nSCS1 121 0 Z
bit 119 I 1 D27
bit 118 C 0 D27
bit 117 O 1 D27 118 0 Z
bit 116 I 1 nSCS2
bit 115 C 0 nSCS2
bit 114 O 1 nSCS2 115 0 Z
bit 113 I 1 D28
bit 112 C 0 D28
bit 111 O 1 D28 112 0 Z
bit 110 I 1 nSCS3
bit 109 C 0 nSCS3
bit 108 O 1 nSCS3 109 0 Z
bit 107 I 1 D29
bit 106 C 0 D29
bit 105 O 1 D29 106 0 Z
bit 104 C 0 nSWE
bit 103 O 1 nSWE 104 0 Z
bit 102 I 1 D30
bit 101 C 0 D30
bit 100 O 1 D30 101 0 Z
bit 99 I 1 nCAS
bit 98 C 0 nCAS
bit 97 O 1 nCAS 98 0 Z
bit 96 I 1 D31
bit 95 C 0 D31
bit 94 O 1 D31 95 0 Z
bit 93 I 1 nRAS
bit 92 C 0 nRAS
bit 91 O 1 nRAS 92 0 Z
bit 90 I 1 SCKEN3
bit 89 C 0 SCKEN3
bit 88 O 1 SCKEN3 89 0 Z
bit 87 I 1 SCLK
bit 86 C 0 SCLK
bit 85 O 1 SCLK 86 0 Z
bit 84 C 0 CS6
bit 83 O 1 CS6 84 0 Z
bit 82 C 0 CS7
bit 81 O 1 CS7 82 0 Z
bit 80 C 0 nWE3
bit 79 O 1 nWE3 80 0 Z
bit 78 I 1 DQM0
bit 77 C 0 DQM0
bit 76 O 1 DQM0 77 0 Z
bit 75 I 1 DQM1
bit 74 C 0 DQM1
bit 73 O 1 DQM1 74 0 Z
bit 72 I 1 DQM2
bit 71 C 0 DQM2
bit 70 O 1 DQM2 71 0 Z
bit 69 C 0 DQM3
bit 68 O 1 DQM3 69 0 Z
bit 67 C 0 nOE
bit 66 O 1 nOE 67 0 Z
bit 65 I 1 nWE0
bit 64 C 0 nWE0
bit 63 O 1 nWE0 64 0 Z
bit 62 I 1 A25
bit 61 C 0 A25
bit 60 O 1 A25 61 0 Z
bit 59 I 1 A26
bit 58 C 0 A26
bit 57 O 1 A26 58 0 Z
bit 56 C 0 A27
bit 55 O 1 A27 56 0 Z
bit 54 I 1 PWMEN0
bit 53 C 0 PWMEN0
bit 52 O 1 PWMEN0 53 0 Z
bit 51 I 1 PWMEN1
bit 50 C 0 PWMEN1
bit 49 O 1 PWMEN1 50 0 Z
bit 48 I 1 PWM0
bit 47 C 0 PWM0
bit 46 O 1 PWM0 47 0 Z
bit 45 I 1 PWM1
bit 44 C 0 PWM1
bit 43 O 1 PWM1 44 0 Z
bit 42 I 1 PF0
bit 41 C 0 PF0
bit 40 O 1 PF0 41 0 Z
bit 39 I 1 PF1
bit 38 C 0 PF1
bit 37 O 1 PF1 38 0 Z
bit 36 I 1 PF2
bit 35 C 0 PF2
bit 34 O 1 PF2 35 0 Z
bit 33 I 1 PF4
bit 32 C 0 PF4
bit 31 O 1 PF4 32 0 Z
bit 30 I 1 PF5
bit 29 C 0 PF5
bit 28 O 1 PF5 29 0 Z
bit 27 I 1 PF6
bit 26 C 0 PF6
bit 25 O 1 PF6 26 0 Z
bit 24 I 1 PF7
bit 23 C 0 PF7
bit 22 O 1 PF7 23 0 Z
bit 21 I 1 AC97CLK
bit 20 C 0 AC97CLK
bit 19 O 1 AC97CLK 20 0 Z
bit 18 I 1 PF3
bit 17 C 0 PF3
bit 16 O 1 PF3 17 0 Z
bit 15 C 0 AC97OUT
bit 14 O 1 AC97OUT 15 0 Z
bit 13 C 0 AC97SYNC
bit 12 O 1 AC97SYNC 13 0 Z
bit 11 I 1 AC97IN
bit 10 C 0 AC97IN
bit 9 O 1 AC97IN 10 0 Z
bit 8 I 1 MMCCLK
bit 7 C 0 MMCCLK
bit 6 O 1 MMCCLK 7 0 Z
bit 5 I 1 MMCCMD
bit 4 C 0 MMCCMD
bit 3 O 1 MMCCMD 4 0 Z
bit 2 I 1 MMCDATA
bit 1 C 0 MMCDATA
bit 0 O 1 MMCDATA 1 0 Z
