signal VCCO_3(1)
signal VCCO_3(2)
signal VCCO_2(1)
signal VCCO_2(2)
signal VCCO_1(1)
signal VCCO_1(2)
signal VCCO_0(1)
signal VCCO_0(2)
signal VCCINT(1)
signal VCCINT(2)
signal VCCINT(3)
signal VCCINT(4)
signal VCCAUX(1)
signal VCCAUX(2)
signal VCCAUX(3)
signal VCCAUX(4)
signal TMS
signal TDO
signal TDI
signal TCK
signal PUDC_B
signal PROG_B
signal P98
signal P95
signal P94
signal P92
signal P91
signal P90
signal P9
signal P86
signal P85
signal P84
signal P83
signal P79
signal P78
signal P71
signal P70
signal P68
signal P67
signal P66
signal P65
signal P63
signal P62
signal P61
signal P60
signal P58
signal P57
signal P54
signal P53
signal P50
signal P5
signal P49
signal P48
signal P47
signal P44
signal P43
signal P42
signal P41
signal P40
signal P4
signal P36
signal P35
signal P34
signal P33
signal P32
signal P3
signal P27
signal P26
signal P25
signal P24
signal P23
signal P22
signal P2
signal P18
signal P17
signal P16
signal P15
signal P12
signal P11
signal P10
signal IPAD83
signal IPAD29
signal IPAD28
signal IPAD204
signal IPAD151
signal IPAD145
signal IPAD144
signal GND(1)
signal GND(2)
signal GND(3)
signal GND(4)
signal GND(5)
signal GND(6)
signal GND(7)
signal GND(8)
signal GND(9)
signal GND(10)
signal GND(11)
signal GND(12)
signal DONE
instruction length 6
register DIR 32
register USERCODE 32
register BSR 588
register BYPASS 1
instruction BYPASS 111111 BYPASS
instruction HIGHZ 001010 BYPASS
instruction IDCODE 001001 DIR
instruction USERCODE 001000 DIR
instruction INTEST 000111 BSR
instruction PRELOAD 000001 BSR
instruction SAMPLE/PRELOAD 000001 BSR
instruction EXTEST 001111 BSR
bit 587 O ? *
bit 586 O ? *
bit 585 O ? *
bit 584 O 1 *
bit 583 O ? *
bit 582 O ? *
bit 581 O 1 *
bit 580 O ? *
bit 579 O ? *
bit 578 O 1 *
bit 577 O ? *
bit 576 O ? *
bit 575 O 1 *
bit 574 O ? *
bit 573 O ? *
bit 572 O ? *
bit 571 O 1 *
bit 570 O ? *
bit 569 O ? *
bit 568 O 1 *
bit 567 O ? *
bit 566 O ? *
bit 565 O 1 *
bit 564 O ? *
bit 563 O ? *
bit 562 O ? *
bit 561 O 1 *
bit 560 O ? *
bit 559 O ? *
bit 558 O 1 *
bit 557 O ? *
bit 556 O ? *
bit 555 O 1 *
bit 554 O ? *
bit 553 O ? *
bit 552 O 1 *
bit 551 O ? *
bit 550 O ? *
bit 549 O ? *
bit 548 O 1 *
bit 547 O ? *
bit 546 O ? *
bit 545 O 1 *
bit 544 O ? *
bit 543 O ? *
bit 542 O 1 *
bit 541 O ? *
bit 540 O ? *
bit 539 O 1 *
bit 538 O ? *
bit 537 O ? *
bit 536 O ? *
bit 535 O 1 *
bit 534 O ? *
bit 533 O ? *
bit 532 O 1 *
bit 531 I ? P71
bit 530 O ? P71 529 1 Z
bit 529 C 1 *
bit 528 I ? P70
bit 527 O ? P70 526 1 Z
bit 526 C 1 *
bit 525 I ? IPAD83
bit 524 I ? P68
bit 523 O ? P68 522 1 Z
bit 522 C 1 *
bit 521 I ? P67
bit 520 O ? P67 519 1 Z
bit 519 C 1 *
bit 518 I ? P66
bit 517 O ? P66 516 1 Z
bit 516 C 1 *
bit 515 I ? P65
bit 514 O ? P65 513 1 Z
bit 513 C 1 *
bit 512 O ? *
bit 511 I ? P63
bit 510 O ? P63 509 1 Z
bit 509 C 1 *
bit 508 I ? P62
bit 507 O ? P62 506 1 Z
bit 506 C 1 *
bit 505 I ? P61
bit 504 O ? P61 503 1 Z
bit 503 C 1 *
bit 502 I ? P60
bit 501 O ? P60 500 1 Z
bit 500 C 1 *
bit 499 O ? *
bit 498 O ? *
bit 497 O ? *
bit 496 O 1 *
bit 495 O ? *
bit 494 O ? *
bit 493 O 1 *
bit 492 I ? P58
bit 491 O ? P58 490 1 Z
bit 490 C 1 *
bit 489 I ? P57
bit 488 O ? P57 487 1 Z
bit 487 C 1 *
bit 486 O ? *
bit 485 O ? *
bit 484 O ? *
bit 483 O 1 *
bit 482 O ? *
bit 481 O ? *
bit 480 O 1 *
bit 479 O ? *
bit 478 O ? *
bit 477 O 1 *
bit 476 O ? *
bit 475 O ? *
bit 474 O 1 *
bit 473 O ? *
bit 472 O ? *
bit 471 O ? *
bit 470 O 1 *
bit 469 O ? *
bit 468 O ? *
bit 467 O 1 *
bit 466 O ? *
bit 465 O ? *
bit 464 O 1 *
bit 463 O ? *
bit 462 O ? *
bit 461 O 1 *
bit 460 O ? *
bit 459 O ? *
bit 458 O ? *
bit 457 O 1 *
bit 456 O ? *
bit 455 O ? *
bit 454 O 1 *
bit 453 O ? *
bit 452 O ? *
bit 451 O 1 *
bit 450 O ? *
bit 449 O ? *
bit 448 O ? *
bit 447 O 1 *
bit 446 O ? *
bit 445 O ? *
bit 444 O 1 *
bit 443 I ? P54
bit 442 O ? P54 441 1 Z
bit 441 C 1 *
bit 440 I ? P53
bit 439 O ? P53 438 1 Z
bit 438 C 1 *
bit 437 I ? DONE
bit 436 O ? DONE 435 1 Z
bit 435 C 1 *
bit 434 I ? P50
bit 433 O ? P50 432 1 Z
bit 432 C 1 *
bit 431 I ? P49
bit 430 O ? P49 429 1 Z
bit 429 C 1 *
bit 428 O ? *
bit 427 I ? P48
bit 426 O ? P48 425 1 Z
bit 425 C 1 *
bit 424 I ? P47
bit 423 O ? P47 422 1 Z
bit 422 C 1 *
bit 421 O ? *
bit 420 O ? *
bit 419 O 1 *
bit 418 O ? *
bit 417 O ? *
bit 416 O 1 *
bit 415 O ? *
bit 414 O ? *
bit 413 O 1 *
bit 412 O ? *
bit 411 O ? *
bit 410 O ? *
bit 409 O ? *
bit 408 O 1 *
bit 407 O ? *
bit 406 O ? *
bit 405 O 1 *
bit 404 O ? *
bit 403 O ? *
bit 402 O ? *
bit 401 O 1 *
bit 400 O ? *
bit 399 O ? *
bit 398 O 1 *
bit 397 O ? *
bit 396 O ? *
bit 395 O 1 *
bit 394 O ? *
bit 393 O ? *
bit 392 O 1 *
bit 391 O ? *
bit 390 O ? *
bit 389 O 1 *
bit 388 O ? *
bit 387 O ? *
bit 386 O 1 *
bit 385 O ? *
bit 384 O ? *
bit 383 O 1 *
bit 382 O ? *
bit 381 O ? *
bit 380 I ? P44
bit 379 O ? P44 378 1 Z
bit 378 C 1 *
bit 377 I ? P43
bit 376 O ? P43 375 1 Z
bit 375 C 1 *
bit 374 I ? P42
bit 373 O ? P42 372 1 Z
bit 372 C 1 *
bit 371 I ? P41
bit 370 O ? P41 369 1 Z
bit 369 C 1 *
bit 368 I ? P40
bit 367 O ? P40 366 1 Z
bit 366 C 1 *
bit 365 I ? IPAD144
bit 364 I ? IPAD145
bit 363 I ? P36
bit 362 O ? P36 361 1 Z
bit 361 C 1 *
bit 360 I ? P35
bit 359 O ? P35 358 1 Z
bit 358 C 1 *
bit 357 I ? P34
bit 356 O ? P34 355 1 Z
bit 355 C 1 *
bit 354 I ? P33
bit 353 O ? P33 352 1 Z
bit 352 C 1 *
bit 351 I ? P32
bit 350 O ? P32 349 1 Z
bit 349 C 1 *
bit 348 I ? IPAD151
bit 347 O ? *
bit 346 O ? *
bit 345 O ? *
bit 344 O 1 *
bit 343 O ? *
bit 342 O ? *
bit 341 O 1 *
bit 340 O ? *
bit 339 O ? *
bit 338 O 1 *
bit 337 O ? *
bit 336 O ? *
bit 335 O 1 *
bit 334 O ? *
bit 333 O ? *
bit 332 O 1 *
bit 331 O ? *
bit 330 O ? *
bit 329 O ? *
bit 328 O ? *
bit 327 O 1 *
bit 326 O ? *
bit 325 O ? *
bit 324 O 1 *
bit 323 O ? *
bit 322 O ? *
bit 321 O ? *
bit 320 O 1 *
bit 319 O ? *
bit 318 O ? *
bit 317 O 1 *
bit 316 O ? *
bit 315 O ? *
bit 314 O 1 *
bit 313 O ? *
bit 312 O ? *
bit 311 O 1 *
bit 310 O ? *
bit 309 O ? *
bit 308 O 1 *
bit 307 I ? P27
bit 306 O ? P27 305 1 Z
bit 305 C 1 *
bit 304 I ? P26
bit 303 O ? P26 302 1 Z
bit 302 C 1 *
bit 301 O ? *
bit 300 O ? *
bit 299 I ? P25
bit 298 O ? P25 297 1 Z
bit 297 C 1 *
bit 296 I ? P24
bit 295 O ? P24 294 1 Z
bit 294 C 1 *
bit 293 O ? *
bit 292 O ? *
bit 291 I ? P23
bit 290 O ? P23 289 1 Z
bit 289 C 1 *
bit 288 I ? P22
bit 287 O ? P22 286 1 Z
bit 286 C 1 *
bit 285 O ? *
bit 284 O ? *
bit 283 O 1 *
bit 282 O ? *
bit 281 O ? *
bit 280 O 1 *
bit 279 O ? *
bit 278 O ? *
bit 277 O ? *
bit 276 O 1 *
bit 275 O ? *
bit 274 O ? *
bit 273 O 1 *
bit 272 O ? *
bit 271 O ? *
bit 270 O 1 *
bit 269 O ? *
bit 268 O ? *
bit 267 O ? *
bit 266 O 1 *
bit 265 O ? *
bit 264 O ? *
bit 263 O 1 *
bit 262 O ? *
bit 261 O ? *
bit 260 O 1 *
bit 259 O ? *
bit 258 O ? *
bit 257 O 1 *
bit 256 O ? *
bit 255 O ? *
bit 254 O ? *
bit 253 O 1 *
bit 252 O ? *
bit 251 O ? *
bit 250 O 1 *
bit 249 O ? *
bit 248 O ? *
bit 247 O 1 *
bit 246 O ? *
bit 245 O ? *
bit 244 O 1 *
bit 243 O ? *
bit 242 O ? *
bit 241 O ? *
bit 240 O 1 *
bit 239 O ? *
bit 238 O ? *
bit 237 O 1 *
bit 236 O ? *
bit 235 O ? *
bit 234 O 1 *
bit 233 O ? *
bit 232 O ? *
bit 231 O 1 *
bit 230 O ? *
bit 229 I ? P18
bit 228 O ? P18 227 1 Z
bit 227 C 1 *
bit 226 I ? P17
bit 225 O ? P17 224 1 Z
bit 224 C 1 *
bit 223 I ? P16
bit 222 O ? P16 221 1 Z
bit 221 C 1 *
bit 220 I ? P15
bit 219 O ? P15 218 1 Z
bit 218 C 1 *
bit 217 I ? IPAD204
bit 216 I ? P12
bit 215 O ? P12 214 1 Z
bit 214 C 1 *
bit 213 I ? P11
bit 212 O ? P11 211 1 Z
bit 211 C 1 *
bit 210 I ? P10
bit 209 O ? P10 208 1 Z
bit 208 C 1 *
bit 207 I ? P9
bit 206 O ? P9 205 1 Z
bit 205 C 1 *
bit 204 O ? *
bit 203 O ? *
bit 202 O ? *
bit 201 O 1 *
bit 200 O ? *
bit 199 O ? *
bit 198 O 1 *
bit 197 O ? *
bit 196 O ? *
bit 195 O 1 *
bit 194 O ? *
bit 193 O ? *
bit 192 O 1 *
bit 191 O ? *
bit 190 O ? *
bit 189 O ? *
bit 188 O 1 *
bit 187 O ? *
bit 186 O ? *
bit 185 O 1 *
bit 184 O ? *
bit 183 O ? *
bit 182 O 1 *
bit 181 O ? *
bit 180 O ? *
bit 179 O 1 *
bit 178 O ? *
bit 177 O ? *
bit 176 O ? *
bit 175 O 1 *
bit 174 O ? *
bit 173 O ? *
bit 172 O 1 *
bit 171 O ? *
bit 170 O ? *
bit 169 O 1 *
bit 168 O ? *
bit 167 O ? *
bit 166 O 1 *
bit 165 O ? *
bit 164 O ? *
bit 163 O ? *
bit 162 O 1 *
bit 161 O ? *
bit 160 O ? *
bit 159 O 1 *
bit 158 O ? *
bit 157 O ? *
bit 156 O 1 *
bit 155 O ? *
bit 154 I ? P5
bit 153 O ? P5 152 1 Z
bit 152 C 1 *
bit 151 I ? P4
bit 150 O ? P4 149 1 Z
bit 149 C 1 *
bit 148 I ? P3
bit 147 O ? P3 146 1 Z
bit 146 C 1 *
bit 145 I ? P2
bit 144 O ? P2 143 1 Z
bit 143 C 1 *
bit 142 O 1 *
bit 141 O 1 *
bit 140 O 1 *
bit 139 O 1 *
bit 138 I ? P98
bit 137 O ? P98 136 1 Z
bit 136 C 1 *
bit 135 O ? *
bit 134 O ? *
bit 133 O ? *
bit 132 O 1 *
bit 131 O ? *
bit 130 O ? *
bit 129 O 1 *
bit 128 O ? *
bit 127 O ? *
bit 126 O 1 *
bit 125 O ? *
bit 124 O ? *
bit 123 O 1 *
bit 122 O ? *
bit 121 O ? *
bit 120 O 1 *
bit 119 O ? *
bit 118 O ? *
bit 117 O ? *
bit 116 O ? *
bit 115 O 1 *
bit 114 O ? *
bit 113 O ? *
bit 112 O 1 *
bit 111 O ? *
bit 110 O ? *
bit 109 O ? *
bit 108 O 1 *
bit 107 O ? *
bit 106 O ? *
bit 105 O 1 *
bit 104 I ? P95
bit 103 O ? P95 102 1 Z
bit 102 C 1 *
bit 101 I ? P94
bit 100 O ? P94 99 1 Z
bit 99 C 1 *
bit 98 O ? *
bit 97 O ? *
bit 96 O 1 *
bit 95 O ? *
bit 94 O ? *
bit 93 O 1 *
bit 92 O ? *
bit 91 O ? *
bit 90 O 1 *
bit 89 O ? *
bit 88 O ? *
bit 87 O ? *
bit 86 O ? *
bit 85 O 1 *
bit 84 O ? *
bit 83 O ? *
bit 82 O 1 *
bit 81 I ? P92
bit 80 O ? P92 79 1 Z
bit 79 C 1 *
bit 78 I ? P91
bit 77 O ? P91 76 1 Z
bit 76 C 1 *
bit 75 I ? P90
bit 74 O ? P90 73 1 Z
bit 73 C 1 *
bit 72 I ? IPAD28
bit 71 I ? IPAD29
bit 70 I ? P86
bit 69 O ? P86 68 1 Z
bit 68 C 1 *
bit 67 I ? P85
bit 66 O ? P85 65 1 Z
bit 65 C 1 *
bit 64 O ? *
bit 63 O ? *
bit 62 O 1 *
bit 61 I ? P84
bit 60 O ? P84 59 1 Z
bit 59 C 1 *
bit 58 I ? P83
bit 57 O ? P83 56 1 Z
bit 56 C 1 *
bit 55 O ? *
bit 54 O ? *
bit 53 O ? *
bit 52 O ? *
bit 51 O 1 *
bit 50 O ? *
bit 49 O ? *
bit 48 O 1 *
bit 47 O ? *
bit 46 O ? *
bit 45 O 1 *
bit 44 O ? *
bit 43 O ? *
bit 42 O 1 *
bit 41 O ? *
bit 40 O ? *
bit 39 O 1 *
bit 38 O ? *
bit 37 O ? *
bit 36 O ? *
bit 35 O ? *
bit 34 O 1 *
bit 33 O ? *
bit 32 O ? *
bit 31 O 1 *
bit 30 O ? *
bit 29 O ? *
bit 28 O ? *
bit 27 O 1 *
bit 26 O ? *
bit 25 O ? *
bit 24 O 1 *
bit 23 O ? *
bit 22 O ? *
bit 21 O 1 *
bit 20 O ? *
bit 19 O ? *
bit 18 O 1 *
bit 17 O ? *
bit 16 O ? *
bit 15 O 1 *
bit 14 O ? *
bit 13 O ? *
bit 12 O 1 *
bit 11 O ? *
bit 10 O ? *
bit 9 O 1 *
bit 8 O ? *
bit 7 O ? *
bit 6 I ? P79
bit 5 O ? P79 4 1 Z
bit 4 C 1 *
bit 3 I ? P78
bit 2 O ? P78 1 1 Z
bit 1 C 1 *
bit 0 O ? *
