signal GND1
signal GND2
signal GND3
signal GND4
signal GND5
signal GND6
signal GND7
signal GND8
signal GND9
signal GND10
signal GND11
signal GND12
signal GND13
signal GND14
signal GND15
signal GND16
signal CCLK_P72
signal DONE_P71
signal HSWAP_EN_P142
signal M0_P38
signal M1_P37
signal M2_P39
signal PROG_B
signal TCK
signal TDI
signal TDO
signal TMS
signal VCCAUX1
signal VCCAUX2
signal VCCAUX3
signal VCCAUX4
signal VCCINT1
signal VCCINT2
signal VCCINT3
signal VCCINT4
signal VCCO011
signal VCCO012
signal VCCO013
signal VCCO231
signal VCCO232
signal VCCO233
signal VCCO451
signal VCCO452
signal VCCO453
signal VCCO671
signal VCCO672
signal VCCO673
signal IO_P1
signal IO_P2
signal IO_P4
signal IO_P5
signal IO_P6
signal IO_P7
signal IO_P8
signal IO_P10
signal IO_P11
signal IO_P12
signal IO_P13
signal IO_P14
signal IO_P15
signal IO_P17
signal IO_P18
signal IO_P20
signal IO_P21
signal IO_P23
signal IO_P24
signal IO_P25
signal IO_P26
signal IO_P27
signal IO_P28
signal IO_P30
signal IO_P31
signal IO_P32
signal IO_P33
signal IO_P35
signal IO_P36
signal IO_P40
signal IO_P41
signal IO_P44
signal IO_P46
signal IO_P47
signal IO_P50
signal IO_P51
signal IO_P52
signal IO_P53
signal IO_P55
signal IO_P56
signal IO_P57
signal IO_P58
signal IO_P59
signal IO_P60
signal IO_P63
signal IO_P65
signal IO_P68
signal IO_P69
signal IO_P70
signal IO_P73
signal IO_P74
signal IO_P76
signal IO_P77
signal IO_P78
signal IO_P79
signal IO_P80
signal IO_P82
signal IO_P83
signal IO_P84
signal IO_P85
signal IO_P86
signal IO_P87
signal IO_P89
signal IO_P90
signal IO_P92
signal IO_P93
signal IO_P95
signal IO_P96
signal IO_P97
signal IO_P98
signal IO_P99
signal IO_P100
signal IO_P102
signal IO_P103
signal IO_P104
signal IO_P105
signal IO_P107
signal IO_P108
signal IO_P112
signal IO_P113
signal IO_P116
signal IO_P118
signal IO_P119
signal IO_P122
signal IO_P123
signal IO_P124
signal IO_P125
signal IO_P127
signal IO_P128
signal IO_P129
signal IO_P130
signal IO_P131
signal IO_P132
signal IO_P135
signal IO_P137
signal IO_P140

register	BSR	383
register	BR	1
register	DIR	32

instruction length 6

instruction EXTEST 000000 BSR
instruction SAMPLE/PRELOAD 000001 BSR
instruction IDCODE 001001 DIR
instruction BYPASS 111111 BR

bit 382 I 1 IO_P108
bit 381 O 1 IO_P108 380 1 Z
bit 380 C 1 *
bit 379 I 1 IO_P107
bit 378 O 1 IO_P107 377 1 Z
bit 377 C 1 *
bit 376 O 1 *
bit 375 O 1 *
bit 374 O 1 *
bit 373 O 1 *
bit 372 O 1 *
bit 371 O 1 *
bit 370 I 1 IO_P105
bit 369 O 1 IO_P105 368 1 Z
bit 368 C 1 *
bit 367 I 1 IO_P104
bit 366 O 1 IO_P104 365 1 Z
bit 365 C 1 *
bit 364 I 1 IO_P103
bit 363 O 1 IO_P103 362 1 Z
bit 362 C 1 *
bit 361 I 1 IO_P102
bit 360 O 1 IO_P102 359 1 Z
bit 359 C 1 *
bit 358 I 1 IO_P100
bit 357 O 1 IO_P100 356 1 Z
bit 356 C 1 *
bit 355 I 1 IO_P99
bit 354 O 1 IO_P99 353 1 Z
bit 353 C 1 *
bit 352 I 1 IO_P98
bit 351 O 1 IO_P98 350 1 Z
bit 350 C 1 *
bit 349 I 1 IO_P97
bit 348 O 1 IO_P97 347 1 Z
bit 347 C 1 *
bit 346 I 1 IO_P96
bit 345 O 1 IO_P96 344 1 Z
bit 344 C 1 *
bit 343 I 1 IO_P95
bit 342 O 1 IO_P95 341 1 Z
bit 341 C 1 *
bit 340 I 1 IO_P93
bit 339 O 1 IO_P93 338 1 Z
bit 338 C 1 *
bit 337 I 1 IO_P92
bit 336 O 1 IO_P92 335 1 Z
bit 335 C 1 *
bit 334 I 1 IO_P90
bit 333 O 1 IO_P90 332 1 Z
bit 332 C 1 *
bit 331 I 1 IO_P89
bit 330 O 1 IO_P89 329 1 Z
bit 329 C 1 *
bit 328 I 1 IO_P87
bit 327 O 1 IO_P87 326 1 Z
bit 326 C 1 *
bit 325 I 1 IO_P86
bit 324 O 1 IO_P86 323 1 Z
bit 323 C 1 *
bit 322 I 1 IO_P85
bit 321 O 1 IO_P85 320 1 Z
bit 320 C 1 *
bit 319 I 1 IO_P84
bit 318 O 1 IO_P84 317 1 Z
bit 317 C 1 *
bit 316 I 1 IO_P83
bit 315 O 1 IO_P83 314 1 Z
bit 314 C 1 *
bit 313 I 1 IO_P82
bit 312 O 1 IO_P82 311 1 Z
bit 311 C 1 *
bit 310 I 1 IO_P80
bit 309 O 1 IO_P80 308 1 Z
bit 308 C 1 *
bit 307 I 1 IO_P79
bit 306 O 1 IO_P79 305 1 Z
bit 305 C 1 *
bit 304 I 1 IO_P78
bit 303 O 1 IO_P78 302 1 Z
bit 302 C 1 *
bit 301 I 1 IO_P77
bit 300 O 1 IO_P77 299 1 Z
bit 299 C 1 *
bit 298 I 1 IO_P76
bit 297 O 1 IO_P76 296 1 Z
bit 296 C 1 *
bit 295 O 1 *
bit 294 O 1 *
bit 293 O 1 *
bit 292 I 1 IO_P74
bit 291 O 1 IO_P74 290 1 Z
bit 290 C 1 *
bit 289 I 1 IO_P73
bit 288 O 1 IO_P73 287 1 Z
bit 287 C 1 *
bit 286 I 1 CCLK_P72
bit 285 O 1 CCLK_P72 284 1 Z
bit 284 C 1 *
bit 283 I 1 DONE_P71
bit 282 O 1 DONE_P71 281 1 Z
bit 281 C 1 *
bit 280 I 1 IO_P70
bit 279 O 1 IO_P70 278 1 Z
bit 278 C 1 *
bit 277 I 1 IO_P69
bit 276 O 1 IO_P69 275 1 Z
bit 275 C 1 *
bit 274 I 1 IO_P68
bit 273 O 1 IO_P68 272 1 Z
bit 272 C 1 *
bit 271 O 1 *
bit 270 O 1 *
bit 269 O 1 *
bit 268 O 1 *
bit 267 O 1 *
bit 266 O 1 *
bit 265 O 1 *
bit 264 O 1 *
bit 263 O 1 *
bit 262 I 1 IO_P65
bit 261 O 1 IO_P65 260 1 Z
bit 260 C 1 *
bit 259 I 1 IO_P63
bit 258 O 1 IO_P63 257 1 Z
bit 257 C 1 *
bit 256 I 1 IO_P60
bit 255 O 1 IO_P60 254 1 Z
bit 254 C 1 *
bit 253 I 1 IO_P59
bit 252 O 1 IO_P59 251 1 Z
bit 251 C 1 *
bit 250 O 1 *
bit 249 O 1 *
bit 248 O 1 *
bit 247 I 1 IO_P58
bit 246 O 1 IO_P58 245 1 Z
bit 245 C 1 *
bit 244 I 1 IO_P57
bit 243 O 1 IO_P57 242 1 Z
bit 242 C 1 *
bit 241 I 1 IO_P56
bit 240 O 1 IO_P56 239 1 Z
bit 239 C 1 *
bit 238 I 1 IO_P55
bit 237 O 1 IO_P55 236 1 Z
bit 236 C 1 *
bit 235 O 1 *
bit 234 O 1 *
bit 233 O 1 *
bit 232 I 1 IO_P53
bit 231 O 1 IO_P53 230 1 Z
bit 230 C 1 *
bit 229 I 1 IO_P52
bit 228 O 1 IO_P52 227 1 Z
bit 227 C 1 *
bit 226 I 1 IO_P51
bit 225 O 1 IO_P51 224 1 Z
bit 224 C 1 *
bit 223 I 1 IO_P50
bit 222 O 1 IO_P50 221 1 Z
bit 221 C 1 *
bit 220 O 1 *
bit 219 O 1 *
bit 218 O 1 *
bit 217 I 1 IO_P47
bit 216 O 1 IO_P47 215 1 Z
bit 215 C 1 *
bit 214 I 1 IO_P46
bit 213 O 1 IO_P46 212 1 Z
bit 212 C 1 *
bit 211 I 1 IO_P44
bit 210 O 1 IO_P44 209 1 Z
bit 209 C 1 *
bit 208 O 1 *
bit 207 O 1 *
bit 206 O 1 *
bit 205 O 1 *
bit 204 O 1 *
bit 203 O 1 *
bit 202 O 1 *
bit 201 O 1 *
bit 200 O 1 *
bit 199 O 1 *
bit 198 O 1 *
bit 197 O 1 *
bit 196 I 1 IO_P41
bit 195 O 1 IO_P41 194 1 Z
bit 194 C 1 *
bit 193 I 1 IO_P40
bit 192 O 1 IO_P40 191 1 Z
bit 191 C 1 *
bit 190 I 1 M2_P39
bit 189 I 1 M0_P38
bit 188 I 1 M1_P37
bit 187 I 1 IO_P36
bit 186 O 1 IO_P36 185 1 Z
bit 185 C 1 *
bit 184 I 1 IO_P35
bit 183 O 1 IO_P35 182 1 Z
bit 182 C 1 *
bit 181 O 1 *
bit 180 O 1 *
bit 179 O 1 *
bit 178 O 1 *
bit 177 O 1 *
bit 176 O 1 *
bit 175 I 1 IO_P33
bit 174 O 1 IO_P33 173 1 Z
bit 173 C 1 *
bit 172 I 1 IO_P32
bit 171 O 1 IO_P32 170 1 Z
bit 170 C 1 *
bit 169 I 1 IO_P31
bit 168 O 1 IO_P31 167 1 Z
bit 167 C 1 *
bit 166 I 1 IO_P30
bit 165 O 1 IO_P30 164 1 Z
bit 164 C 1 *
bit 163 I 1 IO_P28
bit 162 O 1 IO_P28 161 1 Z
bit 161 C 1 *
bit 160 I 1 IO_P27
bit 159 O 1 IO_P27 158 1 Z
bit 158 C 1 *
bit 157 I 1 IO_P26
bit 156 O 1 IO_P26 155 1 Z
bit 155 C 1 *
bit 154 I 1 IO_P25
bit 153 O 1 IO_P25 152 1 Z
bit 152 C 1 *
bit 151 I 1 IO_P24
bit 150 O 1 IO_P24 149 1 Z
bit 149 C 1 *
bit 148 I 1 IO_P23
bit 147 O 1 IO_P23 146 1 Z
bit 146 C 1 *
bit 145 I 1 IO_P21
bit 144 O 1 IO_P21 143 1 Z
bit 143 C 1 *
bit 142 I 1 IO_P20
bit 141 O 1 IO_P20 140 1 Z
bit 140 C 1 *
bit 139 I 1 IO_P18
bit 138 O 1 IO_P18 137 1 Z
bit 137 C 1 *
bit 136 I 1 IO_P17
bit 135 O 1 IO_P17 134 1 Z
bit 134 C 1 *
bit 133 I 1 IO_P15
bit 132 O 1 IO_P15 131 1 Z
bit 131 C 1 *
bit 130 I 1 IO_P14
bit 129 O 1 IO_P14 128 1 Z
bit 128 C 1 *
bit 127 I 1 IO_P13
bit 126 O 1 IO_P13 125 1 Z
bit 125 C 1 *
bit 124 I 1 IO_P12
bit 123 O 1 IO_P12 122 1 Z
bit 122 C 1 *
bit 121 I 1 IO_P11
bit 120 O 1 IO_P11 119 1 Z
bit 119 C 1 *
bit 118 I 1 IO_P10
bit 117 O 1 IO_P10 116 1 Z
bit 116 C 1 *
bit 115 I 1 IO_P8
bit 114 O 1 IO_P8 113 1 Z
bit 113 C 1 *
bit 112 I 1 IO_P7
bit 111 O 1 IO_P7 110 1 Z
bit 110 C 1 *
bit 109 I 1 IO_P6
bit 108 O 1 IO_P6 107 1 Z
bit 107 C 1 *
bit 106 I 1 IO_P5
bit 105 O 1 IO_P5 104 1 Z
bit 104 C 1 *
bit 103 I 1 IO_P4
bit 102 O 1 IO_P4 101 1 Z
bit 101 C 1 *
bit 100 O 1 *
bit 99 O 1 *
bit 98 O 1 *
bit 97 I 1 IO_P2
bit 96 O 1 IO_P2 95 1 Z
bit 95 C 1 *
bit 94 I 1 IO_P1
bit 93 O 1 IO_P1 92 1 Z
bit 92 C 1 *
bit 91 O 1 *
bit 90 I 1 HSWAP_EN_P142
bit 89 O 1 *
bit 88 O 1 *
bit 87 O 1 *
bit 86 I 1 IO_P141
bit 85 O 1 IO_P141 84 1 Z
bit 84 C 1 *
bit 83 I 1 IO_P140
bit 82 O 1 IO_P140 81 1 Z
bit 81 C 1 *
bit 80 O 1 *
bit 79 O 1 *
bit 78 O 1 *
bit 77 O 1 *
bit 76 O 1 *
bit 75 O 1 *
bit 74 O 1 *
bit 73 O 1 *
bit 72 O 1 *
bit 71 I 1 IO_P137
bit 70 O 1 IO_P137 69 1 Z
bit 69 C 1 *
bit 68 I 1 IO_P135
bit 67 O 1 IO_P135 66 1 Z
bit 66 C 1 *
bit 65 I 1 IO_P132
bit 64 O 1 IO_P132 63 1 Z
bit 63 C 1 *
bit 62 I 1 IO_P131
bit 61 O 1 IO_P131 60 1 Z
bit 60 C 1 *
bit 59 O 1 *
bit 58 O 1 *
bit 57 O 1 *
bit 56 I 1 IO_P130
bit 55 O 1 IO_P130 54 1 Z
bit 54 C 1 *
bit 53 I 1 IO_P129
bit 52 O 1 IO_P129 51 1 Z
bit 51 C 1 *
bit 50 I 1 IO_P128
bit 49 O 1 IO_P128 48 1 Z
bit 48 C 1 *
bit 47 I 1 IO_P127
bit 46 O 1 IO_P127 45 1 Z
bit 45 C 1 *
bit 44 O 1 *
bit 43 O 1 *
bit 42 O 1 *
bit 41 I 1 IO_P125
bit 40 O 1 IO_P125 39 1 Z
bit 39 C 1 *
bit 38 I 1 IO_P124
bit 37 O 1 IO_P124 36 1 Z
bit 36 C 1 *
bit 35 I 1 IO_P123
bit 34 O 1 IO_P123 33 1 Z
bit 33 C 1 *
bit 32 I 1 IO_P122
bit 31 O 1 IO_P122 30 1 Z
bit 30 C 1 *
bit 29 O 1 *
bit 28 O 1 *
bit 27 O 1 *
bit 26 I 1 IO_P119
bit 25 O 1 IO_P119 24 1 Z
bit 24 C 1 *
bit 23 I 1 IO_P118
bit 22 O 1 IO_P118 21 1 Z
bit 21 C 1 *
bit 20 I 1 IO_P116
bit 19 O 1 IO_P116 18 1 Z
bit 18 C 1 *
bit 17 O 1 *
bit 16 O 1 *
bit 15 O 1 *
bit 14 O 1 *
bit 13 O 1 *
bit 12 O 1 *
bit 11 O 1 *
bit 10 O 1 *
bit 9 O 1 *
bit 8 O 1 *
bit 7 O 1 *
bit 6 O 1 *
bit 5 I 1 IO_P113
bit 4 O 1 IO_P113 3 1 Z
bit 3 C 1 *
bit 2 I 1 IO_P112
bit 1 O 1 IO_P112 0 1 Z
bit 0 C 1 *
