signal GND1
signal GND2
signal GND3
signal GND4
signal GND5
signal GND6
signal GND7
signal GND8
signal GND9
signal GND10
signal GND11
signal GND12
signal GND13
signal GND14
signal GND15
signal GND16
signal GND17
signal GND18
signal GND19
signal GND20
signal GND21
signal GND22
signal GND23
signal GND24
signal GND25
signal GND26
signal GND27
signal GND28
signal GND29
signal GND30
signal GND31
signal GND32
signal GND33
signal GND34
signal GND35
signal GND36
signal GND37
signal GND38
signal GND39
signal GND40
signal GND41
signal GND42
signal GND43
signal GND44
signal GND45
signal GND46
signal GND47
signal GND48
signal GND49
signal GND50
signal GND51
signal GND52
signal GND53
signal GND54
signal GND55
signal GND56
signal GND57
signal GND58
signal GND59
signal GND60
signal GND61
signal GND62
signal GND63
signal GND64
signal GND65
signal GND66
signal GND67
signal GND68
signal GND69
signal GND70
signal GND71
signal GND72
signal GND73
signal GND74
signal GND75
signal GND76
signal GND77
signal GND78
signal GND79
signal GND80
signal GND81
signal GND82
signal GND83
signal GND84
signal GND85
signal GND86
signal GND87
signal GND88
signal GND89
signal GND90
signal GND91
signal GND92
signal GND93
signal GND94
signal GND95
signal GND96
signal GND97
signal GND98
signal GND99
signal GND100
signal GND101
signal GND102
signal GND103
signal GND104
signal GND105
signal GND106
signal GND107
signal GND108
signal GND109
signal GND110
signal GND111
signal GND112
signal GND113
signal GND114
signal GND115
signal GND116
signal GND117
signal GND118
signal GND119
signal GND120
signal NOCONNECT1
signal NOCONNECT2
signal NOCONNECT3
signal NOCONNECT4
signal NOCONNECT5
signal NOCONNECT6
signal NOCONNECT7
signal NOCONNECT8
signal CCLK_AH28
signal DONE_AJ28
signal HSWAP_EN_A3
signal M0_AJ3
signal M1_AH3
signal M2_AK3
signal PROG_B
signal TCK
signal TDI
signal TDO
signal TMS
signal VCCAUX1
signal VCCAUX2
signal VCCAUX3
signal VCCAUX4
signal VCCAUX5
signal VCCAUX6
signal VCCAUX7
signal VCCAUX8
signal VCCAUX9
signal VCCAUX10
signal VCCAUX11
signal VCCAUX12
signal VCCAUX13
signal VCCAUX14
signal VCCAUX15
signal VCCAUX16
signal VCCAUX17
signal VCCAUX18
signal VCCAUX19
signal VCCAUX20
signal VCCAUX21
signal VCCAUX22
signal VCCAUX23
signal VCCAUX24
signal VCCINT1
signal VCCINT2
signal VCCINT3
signal VCCINT4
signal VCCINT5
signal VCCINT6
signal VCCINT7
signal VCCINT8
signal VCCINT9
signal VCCINT10
signal VCCINT11
signal VCCINT12
signal VCCINT13
signal VCCINT14
signal VCCINT15
signal VCCINT16
signal VCCINT17
signal VCCINT18
signal VCCINT19
signal VCCINT20
signal VCCINT21
signal VCCINT22
signal VCCINT23
signal VCCINT24
signal VCCINT25
signal VCCINT26
signal VCCINT27
signal VCCINT28
signal VCCINT29
signal VCCINT30
signal VCCINT31
signal VCCINT32
signal VCCO01
signal VCCO02
signal VCCO03
signal VCCO04
signal VCCO05
signal VCCO06
signal VCCO07
signal VCCO08
signal VCCO09
signal VCCO010
signal VCCO11
signal VCCO12
signal VCCO13
signal VCCO14
signal VCCO15
signal VCCO16
signal VCCO17
signal VCCO18
signal VCCO19
signal VCCO110
signal VCCO21
signal VCCO22
signal VCCO23
signal VCCO24
signal VCCO25
signal VCCO26
signal VCCO27
signal VCCO28
signal VCCO29
signal VCCO210
signal VCCO31
signal VCCO32
signal VCCO33
signal VCCO34
signal VCCO35
signal VCCO36
signal VCCO37
signal VCCO38
signal VCCO39
signal VCCO310
signal VCCO41
signal VCCO42
signal VCCO43
signal VCCO44
signal VCCO45
signal VCCO46
signal VCCO47
signal VCCO48
signal VCCO49
signal VCCO410
signal VCCO51
signal VCCO52
signal VCCO53
signal VCCO54
signal VCCO55
signal VCCO56
signal VCCO57
signal VCCO58
signal VCCO59
signal VCCO510
signal VCCO61
signal VCCO62
signal VCCO63
signal VCCO64
signal VCCO65
signal VCCO66
signal VCCO67
signal VCCO68
signal VCCO69
signal VCCO610
signal VCCO71
signal VCCO72
signal VCCO73
signal VCCO74
signal VCCO75
signal VCCO76
signal VCCO77
signal VCCO78
signal VCCO79
signal VCCO710
signal IO_A4
signal IO_A5
signal IO_A8
signal IO_A11
signal IO_A12
signal IO_A13
signal IO_A15
signal IO_A16
signal IO_A19
signal IO_A20
signal IO_A22
signal IO_A23
signal IO_A24
signal IO_A26
signal IO_A27
signal IO_B4
signal IO_B5
signal IO_B6
signal IO_B8
signal IO_B10
signal IO_B11
signal IO_B12
signal IO_B13
signal IO_B14
signal IO_B15
signal IO_B16
signal IO_B17
signal IO_B19
signal IO_B20
signal IO_B21
signal IO_B22
signal IO_B23
signal IO_B24
signal IO_B25
signal IO_B26
signal IO_B27
signal IO_C1
signal IO_C2
signal IO_C4
signal IO_C6
signal IO_C7
signal IO_C8
signal IO_C10
signal IO_C11
signal IO_C12
signal IO_C14
signal IO_C15
signal IO_C16
signal IO_C17
signal IO_C19
signal IO_C20
signal IO_C21
signal IO_C23
signal IO_C24
signal IO_C25
signal IO_C27
signal IO_C29
signal IO_C30
signal IO_D1
signal IO_D2
signal IO_D3
signal IO_D4
signal IO_D5
signal IO_D7
signal IO_D8
signal IO_D11
signal IO_D12
signal IO_D13
signal IO_D15
signal IO_D16
signal IO_D19
signal IO_D20
signal IO_D22
signal IO_D23
signal IO_D24
signal IO_D26
signal IO_D27
signal IO_D28
signal IO_D29
signal IO_D30
signal IO_E1
signal IO_E2
signal IO_E4
signal IO_E6
signal IO_E8
signal IO_E11
signal IO_E12
signal IO_E13
signal IO_E15
signal IO_E16
signal IO_E19
signal IO_E20
signal IO_E22
signal IO_E23
signal IO_E25
signal IO_E29
signal IO_E30
signal IO_F2
signal IO_F3
signal IO_F5
signal IO_F6
signal IO_F7
signal IO_F8
signal IO_F9
signal IO_F10
signal IO_F11
signal IO_F12
signal IO_F13
signal IO_F14
signal IO_F15
signal IO_F16
signal IO_F17
signal IO_F18
signal IO_F19
signal IO_F20
signal IO_F21
signal IO_F22
signal IO_F23
signal IO_F24
signal IO_F25
signal IO_F28
signal IO_F29
signal IO_G1
signal IO_G2
signal IO_G3
signal IO_G4
signal IO_G6
signal IO_G8
signal IO_G10
signal IO_G11
signal IO_G12
signal IO_G14
signal IO_G15
signal IO_G16
signal IO_G17
signal IO_G19
signal IO_G20
signal IO_G21
signal IO_G23
signal IO_G24
signal IO_G25
signal IO_G27
signal IO_G28
signal IO_G29
signal IO_G30
signal IO_H1
signal IO_H2
signal IO_H3
signal IO_H4
signal IO_H5
signal IO_H6
signal IO_H7
signal IO_H9
signal IO_H11
signal IO_H12
signal IO_H13
signal IO_H15
signal IO_H16
signal IO_H19
signal IO_H20
signal IO_H22
signal IO_H23
signal IO_H24
signal IO_H25
signal IO_H26
signal IO_H27
signal IO_H28
signal IO_H29
signal IO_H30
signal IO_J1
signal IO_J2
signal IO_J4
signal IO_J5
signal IO_J6
signal IO_J8
signal IO_J9
signal IO_J10
signal IO_J12
signal IO_J13
signal IO_J14
signal IO_J15
signal IO_J16
signal IO_J17
signal IO_J19
signal IO_J21
signal IO_J22
signal IO_J23
signal IO_J25
signal IO_J26
signal IO_J27
signal IO_J29
signal IO_J30
signal IO_K2
signal IO_K3
signal IO_K6
signal IO_K7
signal IO_K9
signal IO_K10
signal IO_K11
signal IO_K12
signal IO_K13
signal IO_K14
signal IO_K15
signal IO_K16
signal IO_K19
signal IO_K20
signal IO_K22
signal IO_K24
signal IO_K25
signal IO_L1
signal IO_L2
signal IO_L3
signal IO_L4
signal IO_L5
signal IO_L6
signal IO_L7
signal IO_L8
signal IO_L10
signal IO_L25
signal IO_L26
signal IO_L27
signal IO_L28
signal IO_L29
signal IO_L30
signal IO_M1
signal IO_M2
signal IO_M3
signal IO_M4
signal IO_M10
signal IO_M21
signal IO_M22
signal IO_M23
signal IO_M24
signal IO_M25
signal IO_M26
signal IO_M27
signal IO_M28
signal IO_N1
signal IO_N2
signal IO_N8
signal IO_N9
signal IO_N10
signal IO_N21
signal IO_N22
signal IO_N23
signal IO_N25
signal IO_N26
signal IO_N27
signal IO_N29
signal IO_N30
signal IO_P2
signal IO_P3
signal IO_P6
signal IO_P7
signal IO_P9
signal IO_P10
signal IO_P21
signal IO_P22
signal IO_P24
signal IO_P25
signal IO_P28
signal IO_P29
signal IO_R1
signal IO_R2
signal IO_R3
signal IO_R4
signal IO_R5
signal IO_R6
signal IO_R7
signal IO_R8
signal IO_R9
signal IO_R10
signal IO_R21
signal IO_R22
signal IO_R23
signal IO_R24
signal IO_R25
signal IO_R26
signal IO_R27
signal IO_R28
signal IO_R29
signal IO_R30
signal IO_T1
signal IO_T2
signal IO_T3
signal IO_T4
signal IO_T5
signal IO_T6
signal IO_T9
signal IO_T10
signal IO_T21
signal IO_T22
signal IO_T23
signal IO_T24
signal IO_T25
signal IO_T26
signal IO_T27
signal IO_T28
signal IO_T29
signal IO_T30
signal IO_U6
signal IO_U7
signal IO_U9
signal IO_U10
signal IO_U21
signal IO_U22
signal IO_U24
signal IO_U25
signal IO_U28
signal IO_U29
signal IO_V1
signal IO_V2
signal IO_V4
signal IO_V5
signal IO_V6
signal IO_V10
signal IO_V21
signal IO_V22
signal IO_V23
signal IO_V25
signal IO_V29
signal IO_V30
signal IO_W1
signal IO_W2
signal IO_W3
signal IO_W4
signal IO_W5
signal IO_W6
signal IO_W7
signal IO_W10
signal IO_W21
signal IO_W26
signal IO_W29
signal IO_W30
signal IO_Y1
signal IO_Y2
signal IO_Y5
signal IO_Y6
signal IO_Y7
signal IO_Y8
signal IO_Y10
signal IO_Y21
signal IO_Y23
signal IO_Y24
signal IO_Y25
signal IO_Y26
signal IO_Y27
signal IO_Y28
signal IO_Y29
signal IO_Y30
signal IO_AA2
signal IO_AA3
signal IO_AA6
signal IO_AA7
signal IO_AA9
signal IO_AA10
signal IO_AA11
signal IO_AA12
signal IO_AA13
signal IO_AA14
signal IO_AA15
signal IO_AA16
signal IO_AA17
signal IO_AA18
signal IO_AA19
signal IO_AA20
signal IO_AA21
signal IO_AA22
signal IO_AA24
signal IO_AA25
signal IO_AA28
signal IO_AA29
signal IO_AB1
signal IO_AB2
signal IO_AB4
signal IO_AB5
signal IO_AB6
signal IO_AB8
signal IO_AB9
signal IO_AB10
signal IO_AB12
signal IO_AB13
signal IO_AB14
signal IO_AB15
signal IO_AB16
signal IO_AB17
signal IO_AB18
signal IO_AB19
signal IO_AB21
signal IO_AB22
signal IO_AB23
signal IO_AB25
signal IO_AB26
signal IO_AB27
signal IO_AB29
signal IO_AB30
signal IO_AC1
signal IO_AC2
signal IO_AC3
signal IO_AC4
signal IO_AC5
signal IO_AC6
signal IO_AC7
signal IO_AC9
signal IO_AC11
signal IO_AC12
signal IO_AC13
signal IO_AC15
signal IO_AC16
signal IO_AC18
signal IO_AC19
signal IO_AC20
signal IO_AC22
signal IO_AC23
signal IO_AC24
signal IO_AC25
signal IO_AC26
signal IO_AC27
signal IO_AC28
signal IO_AC29
signal IO_AC30
signal IO_AD1
signal IO_AD2
signal IO_AD3
signal IO_AD4
signal IO_AD6
signal IO_AD7
signal IO_AD10
signal IO_AD11
signal IO_AD12
signal IO_AD14
signal IO_AD15
signal IO_AD16
signal IO_AD17
signal IO_AD19
signal IO_AD20
signal IO_AD21
signal IO_AD23
signal IO_AD24
signal IO_AD25
signal IO_AD27
signal IO_AD28
signal IO_AD29
signal IO_AD30
signal IO_AE2
signal IO_AE3
signal IO_AE5
signal IO_AE6
signal IO_AE7
signal IO_AE9
signal IO_AE10
signal IO_AE11
signal IO_AE12
signal IO_AE13
signal IO_AE14
signal IO_AE15
signal IO_AE16
signal IO_AE17
signal IO_AE18
signal IO_AE19
signal IO_AE20
signal IO_AE21
signal IO_AE22
signal IO_AE23
signal IO_AE26
signal IO_AE28
signal IO_AE29
signal IO_AF1
signal IO_AF2
signal IO_AF4
signal IO_AF6
signal IO_AF9
signal IO_AF11
signal IO_AF12
signal IO_AF13
signal IO_AF15
signal IO_AF16
signal IO_AF18
signal IO_AF19
signal IO_AF20
signal IO_AF22
signal IO_AF23
signal IO_AF25
signal IO_AF27
signal IO_AF29
signal IO_AF30
signal IO_AG1
signal IO_AG2
signal IO_AG3
signal IO_AG4
signal IO_AG5
signal IO_AG7
signal IO_AG9
signal IO_AG11
signal IO_AG12
signal IO_AG13
signal IO_AG15
signal IO_AG16
signal IO_AG18
signal IO_AG19
signal IO_AG20
signal IO_AG22
signal IO_AG23
signal IO_AG26
signal IO_AG27
signal IO_AG28
signal IO_AG29
signal IO_AG30
signal IO_AH1
signal IO_AH2
signal IO_AH4
signal IO_AH6
signal IO_AH7
signal IO_AH10
signal IO_AH11
signal IO_AH12
signal IO_AH14
signal IO_AH15
signal IO_AH16
signal IO_AH17
signal IO_AH19
signal IO_AH20
signal IO_AH21
signal IO_AH23
signal IO_AH27
signal IO_AH29
signal IO_AH30
signal IO_AJ4
signal IO_AJ5
signal IO_AJ6
signal IO_AJ8
signal IO_AJ9
signal IO_AJ10
signal IO_AJ11
signal IO_AJ12
signal IO_AJ13
signal IO_AJ14
signal IO_AJ15
signal IO_AJ16
signal IO_AJ17
signal IO_AJ18
signal IO_AJ19
signal IO_AJ20
signal IO_AJ21
signal IO_AJ22
signal IO_AJ23
signal IO_AJ26
signal IO_AJ27
signal IO_AK4
signal IO_AK5
signal IO_AK8
signal IO_AK9
signal IO_AK11
signal IO_AK12
signal IO_AK13
signal IO_AK15
signal IO_AK16
signal IO_AK18
signal IO_AK19
signal IO_AK20
signal IO_AK22
signal IO_AK23
signal IO_AK26
signal IO_AK27

register	BSR	1931
register	BR	1
register	DIR	32

instruction length 6

instruction EXTEST 000000 BSR
instruction SAMPLE/PRELOAD 000001 BSR
instruction IDCODE 001001 DIR
instruction BYPASS 111111 BR

bit 1930 I 1 IO_C29
bit 1929 O 1 IO_C29 1928 1 Z
bit 1928 C 1 *
bit 1927 I 1 IO_C30
bit 1926 O 1 IO_C30 1925 1 Z
bit 1925 C 1 *
bit 1924 I 1 IO_D27
bit 1923 O 1 IO_D27 1922 1 Z
bit 1922 C 1 *
bit 1921 I 1 IO_D28
bit 1920 O 1 IO_D28 1919 1 Z
bit 1919 C 1 *
bit 1918 I 1 IO_D29
bit 1917 O 1 IO_D29 1916 1 Z
bit 1916 C 1 *
bit 1915 I 1 IO_D30
bit 1914 O 1 IO_D30 1913 1 Z
bit 1913 C 1 *
bit 1912 I 1 IO_E29
bit 1911 O 1 IO_E29 1910 1 Z
bit 1910 C 1 *
bit 1909 I 1 IO_E30
bit 1908 O 1 IO_E30 1907 1 Z
bit 1907 C 1 *
bit 1906 I 1 IO_F28
bit 1905 O 1 IO_F28 1904 1 Z
bit 1904 C 1 *
bit 1903 I 1 IO_F29
bit 1902 O 1 IO_F29 1901 1 Z
bit 1901 C 1 *
bit 1900 I 1 IO_G27
bit 1899 O 1 IO_G27 1898 1 Z
bit 1898 C 1 *
bit 1897 I 1 IO_G28
bit 1896 O 1 IO_G28 1895 1 Z
bit 1895 C 1 *
bit 1894 I 1 IO_G29
bit 1893 O 1 IO_G29 1892 1 Z
bit 1892 C 1 *
bit 1891 I 1 IO_G30
bit 1890 O 1 IO_G30 1889 1 Z
bit 1889 C 1 *
bit 1888 I 1 IO_G25
bit 1887 O 1 IO_G25 1886 1 Z
bit 1886 C 1 *
bit 1885 I 1 IO_H24
bit 1884 O 1 IO_H24 1883 1 Z
bit 1883 C 1 *
bit 1882 I 1 IO_H25
bit 1881 O 1 IO_H25 1880 1 Z
bit 1880 C 1 *
bit 1879 I 1 IO_H26
bit 1878 O 1 IO_H26 1877 1 Z
bit 1877 C 1 *
bit 1876 I 1 IO_H27
bit 1875 O 1 IO_H27 1874 1 Z
bit 1874 C 1 *
bit 1873 I 1 IO_H28
bit 1872 O 1 IO_H28 1871 1 Z
bit 1871 C 1 *
bit 1870 O 1 *
bit 1869 O 1 *
bit 1868 O 1 *
bit 1867 I 1 IO_J25
bit 1866 O 1 IO_J25 1865 1 Z
bit 1865 C 1 *
bit 1864 I 1 IO_H29
bit 1863 O 1 IO_H29 1862 1 Z
bit 1862 C 1 *
bit 1861 I 1 IO_H30
bit 1860 O 1 IO_H30 1859 1 Z
bit 1859 C 1 *
bit 1858 I 1 IO_J26
bit 1857 O 1 IO_J26 1856 1 Z
bit 1856 C 1 *
bit 1855 I 1 IO_J27
bit 1854 O 1 IO_J27 1853 1 Z
bit 1853 C 1 *
bit 1852 I 1 IO_J29
bit 1851 O 1 IO_J29 1850 1 Z
bit 1850 C 1 *
bit 1849 I 1 IO_J30
bit 1848 O 1 IO_J30 1847 1 Z
bit 1847 C 1 *
bit 1846 I 1 IO_J23
bit 1845 O 1 IO_J23 1844 1 Z
bit 1844 C 1 *
bit 1843 I 1 IO_K22
bit 1842 O 1 IO_K22 1841 1 Z
bit 1841 C 1 *
bit 1840 I 1 IO_K24
bit 1839 O 1 IO_K24 1838 1 Z
bit 1838 C 1 *
bit 1837 I 1 IO_K25
bit 1836 O 1 IO_K25 1835 1 Z
bit 1835 C 1 *
bit 1834 O 1 *
bit 1833 O 1 *
bit 1832 O 1 *
bit 1831 O 1 *
bit 1830 O 1 *
bit 1829 O 1 *
bit 1828 O 1 *
bit 1827 O 1 *
bit 1826 O 1 *
bit 1825 O 1 *
bit 1824 O 1 *
bit 1823 O 1 *
bit 1822 I 1 IO_L25
bit 1821 O 1 IO_L25 1820 1 Z
bit 1820 C 1 *
bit 1819 I 1 IO_L26
bit 1818 O 1 IO_L26 1817 1 Z
bit 1817 C 1 *
bit 1816 I 1 IO_L27
bit 1815 O 1 IO_L27 1814 1 Z
bit 1814 C 1 *
bit 1813 I 1 IO_L28
bit 1812 O 1 IO_L28 1811 1 Z
bit 1811 C 1 *
bit 1810 I 1 IO_L29
bit 1809 O 1 IO_L29 1808 1 Z
bit 1808 C 1 *
bit 1807 I 1 IO_L30
bit 1806 O 1 IO_L30 1805 1 Z
bit 1805 C 1 *
bit 1804 I 1 IO_M22
bit 1803 O 1 IO_M22 1802 1 Z
bit 1802 C 1 *
bit 1801 I 1 IO_M23
bit 1800 O 1 IO_M23 1799 1 Z
bit 1799 C 1 *
bit 1798 I 1 IO_M24
bit 1797 O 1 IO_M24 1796 1 Z
bit 1796 C 1 *
bit 1795 I 1 IO_M25
bit 1794 O 1 IO_M25 1793 1 Z
bit 1793 C 1 *
bit 1792 I 1 IO_M27
bit 1791 O 1 IO_M27 1790 1 Z
bit 1790 C 1 *
bit 1789 I 1 IO_M28
bit 1788 O 1 IO_M28 1787 1 Z
bit 1787 C 1 *
bit 1786 O 1 *
bit 1785 O 1 *
bit 1784 O 1 *
bit 1783 O 1 *
bit 1782 O 1 *
bit 1781 O 1 *
bit 1780 I 1 IO_M21
bit 1779 O 1 IO_M21 1778 1 Z
bit 1778 C 1 *
bit 1777 I 1 IO_N21
bit 1776 O 1 IO_N21 1775 1 Z
bit 1775 C 1 *
bit 1774 I 1 IO_N22
bit 1773 O 1 IO_N22 1772 1 Z
bit 1772 C 1 *
bit 1771 I 1 IO_N23
bit 1770 O 1 IO_N23 1769 1 Z
bit 1769 C 1 *
bit 1768 I 1 IO_M26
bit 1767 O 1 IO_M26 1766 1 Z
bit 1766 C 1 *
bit 1765 I 1 IO_N25
bit 1764 O 1 IO_N25 1763 1 Z
bit 1763 C 1 *
bit 1762 I 1 IO_N26
bit 1761 O 1 IO_N26 1760 1 Z
bit 1760 C 1 *
bit 1759 I 1 IO_N27
bit 1758 O 1 IO_N27 1757 1 Z
bit 1757 C 1 *
bit 1756 O 1 *
bit 1755 O 1 *
bit 1754 O 1 *
bit 1753 O 1 *
bit 1752 O 1 *
bit 1751 O 1 *
bit 1750 I 1 IO_N29
bit 1749 O 1 IO_N29 1748 1 Z
bit 1748 C 1 *
bit 1747 I 1 IO_N30
bit 1746 O 1 IO_N30 1745 1 Z
bit 1745 C 1 *
bit 1744 I 1 IO_P21
bit 1743 O 1 IO_P21 1742 1 Z
bit 1742 C 1 *
bit 1741 I 1 IO_P22
bit 1740 O 1 IO_P22 1739 1 Z
bit 1739 C 1 *
bit 1738 I 1 IO_P24
bit 1737 O 1 IO_P24 1736 1 Z
bit 1736 C 1 *
bit 1735 I 1 IO_P25
bit 1734 O 1 IO_P25 1733 1 Z
bit 1733 C 1 *
bit 1732 I 1 IO_P28
bit 1731 O 1 IO_P28 1730 1 Z
bit 1730 C 1 *
bit 1729 I 1 IO_P29
bit 1728 O 1 IO_P29 1727 1 Z
bit 1727 C 1 *
bit 1726 I 1 IO_R21
bit 1725 O 1 IO_R21 1724 1 Z
bit 1724 C 1 *
bit 1723 I 1 IO_R22
bit 1722 O 1 IO_R22 1721 1 Z
bit 1721 C 1 *
bit 1720 O 1 *
bit 1719 O 1 *
bit 1718 O 1 *
bit 1717 O 1 *
bit 1716 O 1 *
bit 1715 O 1 *
bit 1714 I 1 IO_R23
bit 1713 O 1 IO_R23 1712 1 Z
bit 1712 C 1 *
bit 1711 I 1 IO_R24
bit 1710 O 1 IO_R24 1709 1 Z
bit 1709 C 1 *
bit 1708 I 1 IO_R25
bit 1707 O 1 IO_R25 1706 1 Z
bit 1706 C 1 *
bit 1705 I 1 IO_R26
bit 1704 O 1 IO_R26 1703 1 Z
bit 1703 C 1 *
bit 1702 I 1 IO_R27
bit 1701 O 1 IO_R27 1700 1 Z
bit 1700 C 1 *
bit 1699 I 1 IO_R28
bit 1698 O 1 IO_R28 1697 1 Z
bit 1697 C 1 *
bit 1696 I 1 IO_R29
bit 1695 O 1 IO_R29 1694 1 Z
bit 1694 C 1 *
bit 1693 I 1 IO_R30
bit 1692 O 1 IO_R30 1691 1 Z
bit 1691 C 1 *
bit 1690 I 1 IO_T30
bit 1689 O 1 IO_T30 1688 1 Z
bit 1688 C 1 *
bit 1687 I 1 IO_T29
bit 1686 O 1 IO_T29 1685 1 Z
bit 1685 C 1 *
bit 1684 I 1 IO_T28
bit 1683 O 1 IO_T28 1682 1 Z
bit 1682 C 1 *
bit 1681 I 1 IO_T27
bit 1680 O 1 IO_T27 1679 1 Z
bit 1679 C 1 *
bit 1678 I 1 IO_T26
bit 1677 O 1 IO_T26 1676 1 Z
bit 1676 C 1 *
bit 1675 I 1 IO_T25
bit 1674 O 1 IO_T25 1673 1 Z
bit 1673 C 1 *
bit 1672 I 1 IO_T24
bit 1671 O 1 IO_T24 1670 1 Z
bit 1670 C 1 *
bit 1669 I 1 IO_T23
bit 1668 O 1 IO_T23 1667 1 Z
bit 1667 C 1 *
bit 1666 O 1 *
bit 1665 O 1 *
bit 1664 O 1 *
bit 1663 O 1 *
bit 1662 O 1 *
bit 1661 O 1 *
bit 1660 I 1 IO_T22
bit 1659 O 1 IO_T22 1658 1 Z
bit 1658 C 1 *
bit 1657 I 1 IO_T21
bit 1656 O 1 IO_T21 1655 1 Z
bit 1655 C 1 *
bit 1654 I 1 IO_U29
bit 1653 O 1 IO_U29 1652 1 Z
bit 1652 C 1 *
bit 1651 I 1 IO_U28
bit 1650 O 1 IO_U28 1649 1 Z
bit 1649 C 1 *
bit 1648 I 1 IO_U25
bit 1647 O 1 IO_U25 1646 1 Z
bit 1646 C 1 *
bit 1645 I 1 IO_U24
bit 1644 O 1 IO_U24 1643 1 Z
bit 1643 C 1 *
bit 1642 I 1 IO_U22
bit 1641 O 1 IO_U22 1640 1 Z
bit 1640 C 1 *
bit 1639 I 1 IO_U21
bit 1638 O 1 IO_U21 1637 1 Z
bit 1637 C 1 *
bit 1636 I 1 IO_V30
bit 1635 O 1 IO_V30 1634 1 Z
bit 1634 C 1 *
bit 1633 I 1 IO_V29
bit 1632 O 1 IO_V29 1631 1 Z
bit 1631 C 1 *
bit 1630 O 1 *
bit 1629 O 1 *
bit 1628 O 1 *
bit 1627 O 1 *
bit 1626 O 1 *
bit 1625 O 1 *
bit 1624 I 1 IO_V25
bit 1623 O 1 IO_V25 1622 1 Z
bit 1622 C 1 *
bit 1621 I 1 IO_W26
bit 1620 O 1 IO_W26 1619 1 Z
bit 1619 C 1 *
bit 1618 I 1 IO_V23
bit 1617 O 1 IO_V23 1616 1 Z
bit 1616 C 1 *
bit 1615 I 1 IO_V22
bit 1614 O 1 IO_V22 1613 1 Z
bit 1613 C 1 *
bit 1612 I 1 IO_V21
bit 1611 O 1 IO_V21 1610 1 Z
bit 1610 C 1 *
bit 1609 I 1 IO_W21
bit 1608 O 1 IO_W21 1607 1 Z
bit 1607 C 1 *
bit 1606 I 1 IO_W30
bit 1605 O 1 IO_W30 1604 1 Z
bit 1604 C 1 *
bit 1603 I 1 IO_W29
bit 1602 O 1 IO_W29 1601 1 Z
bit 1601 C 1 *
bit 1600 O 1 *
bit 1599 O 1 *
bit 1598 O 1 *
bit 1597 O 1 *
bit 1596 O 1 *
bit 1595 O 1 *
bit 1594 I 1 IO_Y30
bit 1593 O 1 IO_Y30 1592 1 Z
bit 1592 C 1 *
bit 1591 I 1 IO_Y29
bit 1590 O 1 IO_Y29 1589 1 Z
bit 1589 C 1 *
bit 1588 I 1 IO_Y28
bit 1587 O 1 IO_Y28 1586 1 Z
bit 1586 C 1 *
bit 1585 I 1 IO_Y27
bit 1584 O 1 IO_Y27 1583 1 Z
bit 1583 C 1 *
bit 1582 I 1 IO_Y26
bit 1581 O 1 IO_Y26 1580 1 Z
bit 1580 C 1 *
bit 1579 I 1 IO_Y25
bit 1578 O 1 IO_Y25 1577 1 Z
bit 1577 C 1 *
bit 1576 I 1 IO_Y24
bit 1575 O 1 IO_Y24 1574 1 Z
bit 1574 C 1 *
bit 1573 I 1 IO_Y23
bit 1572 O 1 IO_Y23 1571 1 Z
bit 1571 C 1 *
bit 1570 I 1 IO_Y21
bit 1569 O 1 IO_Y21 1568 1 Z
bit 1568 C 1 *
bit 1567 I 1 IO_AA21
bit 1566 O 1 IO_AA21 1565 1 Z
bit 1565 C 1 *
bit 1564 I 1 IO_AA29
bit 1563 O 1 IO_AA29 1562 1 Z
bit 1562 C 1 *
bit 1561 I 1 IO_AA28
bit 1560 O 1 IO_AA28 1559 1 Z
bit 1559 C 1 *
bit 1558 O 1 *
bit 1557 O 1 *
bit 1556 O 1 *
bit 1555 O 1 *
bit 1554 O 1 *
bit 1553 O 1 *
bit 1552 I 1 IO_AA25
bit 1551 O 1 IO_AA25 1550 1 Z
bit 1550 C 1 *
bit 1549 I 1 IO_AA24
bit 1548 O 1 IO_AA24 1547 1 Z
bit 1547 C 1 *
bit 1546 I 1 IO_AA22
bit 1545 O 1 IO_AA22 1544 1 Z
bit 1544 C 1 *
bit 1543 I 1 IO_AB23
bit 1542 O 1 IO_AB23 1541 1 Z
bit 1541 C 1 *
bit 1540 I 1 IO_AB30
bit 1539 O 1 IO_AB30 1538 1 Z
bit 1538 C 1 *
bit 1537 I 1 IO_AB29
bit 1536 O 1 IO_AB29 1535 1 Z
bit 1535 C 1 *
bit 1534 I 1 IO_AB27
bit 1533 O 1 IO_AB27 1532 1 Z
bit 1532 C 1 *
bit 1531 I 1 IO_AB26
bit 1530 O 1 IO_AB26 1529 1 Z
bit 1529 C 1 *
bit 1528 I 1 IO_AC30
bit 1527 O 1 IO_AC30 1526 1 Z
bit 1526 C 1 *
bit 1525 I 1 IO_AC29
bit 1524 O 1 IO_AC29 1523 1 Z
bit 1523 C 1 *
bit 1522 I 1 IO_AB25
bit 1521 O 1 IO_AB25 1520 1 Z
bit 1520 C 1 *
bit 1519 O 1 *
bit 1518 O 1 *
bit 1517 O 1 *
bit 1516 I 1 IO_AC28
bit 1515 O 1 IO_AC28 1514 1 Z
bit 1514 C 1 *
bit 1513 I 1 IO_AC27
bit 1512 O 1 IO_AC27 1511 1 Z
bit 1511 C 1 *
bit 1510 I 1 IO_AC26
bit 1509 O 1 IO_AC26 1508 1 Z
bit 1508 C 1 *
bit 1507 I 1 IO_AC25
bit 1506 O 1 IO_AC25 1505 1 Z
bit 1505 C 1 *
bit 1504 I 1 IO_AC24
bit 1503 O 1 IO_AC24 1502 1 Z
bit 1502 C 1 *
bit 1501 I 1 IO_AD25
bit 1500 O 1 IO_AD25 1499 1 Z
bit 1499 C 1 *
bit 1498 I 1 IO_AD30
bit 1497 O 1 IO_AD30 1496 1 Z
bit 1496 C 1 *
bit 1495 I 1 IO_AD29
bit 1494 O 1 IO_AD29 1493 1 Z
bit 1493 C 1 *
bit 1492 I 1 IO_AD28
bit 1491 O 1 IO_AD28 1490 1 Z
bit 1490 C 1 *
bit 1489 I 1 IO_AD27
bit 1488 O 1 IO_AD27 1487 1 Z
bit 1487 C 1 *
bit 1486 I 1 IO_AE29
bit 1485 O 1 IO_AE29 1484 1 Z
bit 1484 C 1 *
bit 1483 I 1 IO_AE28
bit 1482 O 1 IO_AE28 1481 1 Z
bit 1481 C 1 *
bit 1480 I 1 IO_AE26
bit 1479 O 1 IO_AE26 1478 1 Z
bit 1478 C 1 *
bit 1477 I 1 IO_AF27
bit 1476 O 1 IO_AF27 1475 1 Z
bit 1475 C 1 *
bit 1474 I 1 IO_AF30
bit 1473 O 1 IO_AF30 1472 1 Z
bit 1472 C 1 *
bit 1471 I 1 IO_AF29
bit 1470 O 1 IO_AF29 1469 1 Z
bit 1469 C 1 *
bit 1468 I 1 IO_AG30
bit 1467 O 1 IO_AG30 1466 1 Z
bit 1466 C 1 *
bit 1465 I 1 IO_AG29
bit 1464 O 1 IO_AG29 1463 1 Z
bit 1463 C 1 *
bit 1462 I 1 IO_AG28
bit 1461 O 1 IO_AG28 1460 1 Z
bit 1460 C 1 *
bit 1459 I 1 IO_AG27
bit 1458 O 1 IO_AG27 1457 1 Z
bit 1457 C 1 *
bit 1456 I 1 IO_AH30
bit 1455 O 1 IO_AH30 1454 1 Z
bit 1454 C 1 *
bit 1453 I 1 IO_AH29
bit 1452 O 1 IO_AH29 1451 1 Z
bit 1451 C 1 *
bit 1450 I 1 CCLK_AH28
bit 1449 O 1 CCLK_AH28 1448 1 Z
bit 1448 C 1 *
bit 1447 I 1 DONE_AJ28
bit 1446 O 1 DONE_AJ28 1445 1 Z
bit 1445 C 1 *
bit 1444 I 1 IO_AK28
bit 1443 O 1 IO_AK28 1442 1 Z
bit 1442 C 1 *
bit 1441 I 1 IO_AJ27
bit 1440 O 1 IO_AJ27 1439 1 Z
bit 1439 C 1 *
bit 1438 I 1 IO_AK27
bit 1437 O 1 IO_AK27 1436 1 Z
bit 1436 C 1 *
bit 1435 I 1 IO_AJ26
bit 1434 O 1 IO_AJ26 1433 1 Z
bit 1433 C 1 *
bit 1432 I 1 IO_AK26
bit 1431 O 1 IO_AK26 1430 1 Z
bit 1430 C 1 *
bit 1429 I 1 IO_AH27
bit 1428 O 1 IO_AH27 1427 1 Z
bit 1427 C 1 *
bit 1426 I 1 IO_AG26
bit 1425 O 1 IO_AG26 1424 1 Z
bit 1424 C 1 *
bit 1423 I 1 IO_AF25
bit 1422 O 1 IO_AF25 1421 1 Z
bit 1421 C 1 *
bit 1420 I 1 IO_AD24
bit 1419 O 1 IO_AD24 1418 1 Z
bit 1418 C 1 *
bit 1417 I 1 IO_AC23
bit 1416 O 1 IO_AC23 1415 1 Z
bit 1415 C 1 *
bit 1414 I 1 IO_AD23
bit 1413 O 1 IO_AD23 1412 1 Z
bit 1412 C 1 *
bit 1411 I 1 IO_AE23
bit 1410 O 1 IO_AE23 1409 1 Z
bit 1409 C 1 *
bit 1408 I 1 IO_AF23
bit 1407 O 1 IO_AF23 1406 1 Z
bit 1406 C 1 *
bit 1405 I 1 IO_AG23
bit 1404 O 1 IO_AG23 1403 1 Z
bit 1403 C 1 *
bit 1402 I 1 IO_AH23
bit 1401 O 1 IO_AH23 1400 1 Z
bit 1400 C 1 *
bit 1399 O 1 *
bit 1398 O 1 *
bit 1397 O 1 *
bit 1396 I 1 IO_AJ23
bit 1395 O 1 IO_AJ23 1394 1 Z
bit 1394 C 1 *
bit 1393 I 1 IO_AK23
bit 1392 O 1 IO_AK23 1391 1 Z
bit 1391 C 1 *
bit 1390 I 1 IO_AB22
bit 1389 O 1 IO_AB22 1388 1 Z
bit 1388 C 1 *
bit 1387 I 1 IO_AC22
bit 1386 O 1 IO_AC22 1385 1 Z
bit 1385 C 1 *
bit 1384 I 1 IO_AE22
bit 1383 O 1 IO_AE22 1382 1 Z
bit 1382 C 1 *
bit 1381 I 1 IO_AF22
bit 1380 O 1 IO_AF22 1379 1 Z
bit 1379 C 1 *
bit 1378 I 1 IO_AG22
bit 1377 O 1 IO_AG22 1376 1 Z
bit 1376 C 1 *
bit 1375 I 1 IO_AJ22
bit 1374 O 1 IO_AJ22 1373 1 Z
bit 1373 C 1 *
bit 1372 I 1 IO_AK22
bit 1371 O 1 IO_AK22 1370 1 Z
bit 1370 C 1 *
bit 1369 O 1 *
bit 1368 O 1 *
bit 1367 O 1 *
bit 1366 I 1 IO_AD21
bit 1365 O 1 IO_AD21 1364 1 Z
bit 1364 C 1 *
bit 1363 I 1 IO_AE21
bit 1362 O 1 IO_AE21 1361 1 Z
bit 1361 C 1 *
bit 1360 I 1 IO_AH21
bit 1359 O 1 IO_AH21 1358 1 Z
bit 1358 C 1 *
bit 1357 I 1 IO_AJ21
bit 1356 O 1 IO_AJ21 1355 1 Z
bit 1355 C 1 *
bit 1354 O 1 *
bit 1353 O 1 *
bit 1352 O 1 *
bit 1351 I 1 IO_AB21
bit 1350 O 1 IO_AB21 1349 1 Z
bit 1349 C 1 *
bit 1348 I 1 IO_AA20
bit 1347 O 1 IO_AA20 1346 1 Z
bit 1346 C 1 *
bit 1345 I 1 IO_AC20
bit 1344 O 1 IO_AC20 1343 1 Z
bit 1343 C 1 *
bit 1342 I 1 IO_AD20
bit 1341 O 1 IO_AD20 1340 1 Z
bit 1340 C 1 *
bit 1339 O 1 *
bit 1338 O 1 *
bit 1337 O 1 *
bit 1336 I 1 IO_AE20
bit 1335 O 1 IO_AE20 1334 1 Z
bit 1334 C 1 *
bit 1333 I 1 IO_AF20
bit 1332 O 1 IO_AF20 1331 1 Z
bit 1331 C 1 *
bit 1330 I 1 IO_AG20
bit 1329 O 1 IO_AG20 1328 1 Z
bit 1328 C 1 *
bit 1327 I 1 IO_AH20
bit 1326 O 1 IO_AH20 1325 1 Z
bit 1325 C 1 *
bit 1324 O 1 *
bit 1323 O 1 *
bit 1322 O 1 *
bit 1321 I 1 IO_AJ20
bit 1320 O 1 IO_AJ20 1319 1 Z
bit 1319 C 1 *
bit 1318 I 1 IO_AK20
bit 1317 O 1 IO_AK20 1316 1 Z
bit 1316 C 1 *
bit 1315 I 1 IO_AA19
bit 1314 O 1 IO_AA19 1313 1 Z
bit 1313 C 1 *
bit 1312 I 1 IO_AB19
bit 1311 O 1 IO_AB19 1310 1 Z
bit 1310 C 1 *
bit 1309 O 1 *
bit 1308 O 1 *
bit 1307 O 1 *
bit 1306 I 1 IO_AC19
bit 1305 O 1 IO_AC19 1304 1 Z
bit 1304 C 1 *
bit 1303 I 1 IO_AD19
bit 1302 O 1 IO_AD19 1301 1 Z
bit 1301 C 1 *
bit 1300 I 1 IO_AE19
bit 1299 O 1 IO_AE19 1298 1 Z
bit 1298 C 1 *
bit 1297 I 1 IO_AF19
bit 1296 O 1 IO_AF19 1295 1 Z
bit 1295 C 1 *
bit 1294 O 1 *
bit 1293 O 1 *
bit 1292 O 1 *
bit 1291 I 1 IO_AG19
bit 1290 O 1 IO_AG19 1289 1 Z
bit 1289 C 1 *
bit 1288 I 1 IO_AH19
bit 1287 O 1 IO_AH19 1286 1 Z
bit 1286 C 1 *
bit 1285 I 1 IO_AJ19
bit 1284 O 1 IO_AJ19 1283 1 Z
bit 1283 C 1 *
bit 1282 I 1 IO_AK19
bit 1281 O 1 IO_AK19 1280 1 Z
bit 1280 C 1 *
bit 1279 I 1 IO_AA18
bit 1278 O 1 IO_AA18 1277 1 Z
bit 1277 C 1 *
bit 1276 I 1 IO_AB18
bit 1275 O 1 IO_AB18 1274 1 Z
bit 1274 C 1 *
bit 1273 I 1 IO_AC18
bit 1272 O 1 IO_AC18 1271 1 Z
bit 1271 C 1 *
bit 1270 I 1 IO_AE18
bit 1269 O 1 IO_AE18 1268 1 Z
bit 1268 C 1 *
bit 1267 I 1 IO_AF18
bit 1266 O 1 IO_AF18 1265 1 Z
bit 1265 C 1 *
bit 1264 I 1 IO_AG18
bit 1263 O 1 IO_AG18 1262 1 Z
bit 1262 C 1 *
bit 1261 I 1 IO_AJ18
bit 1260 O 1 IO_AJ18 1259 1 Z
bit 1259 C 1 *
bit 1258 I 1 IO_AK18
bit 1257 O 1 IO_AK18 1256 1 Z
bit 1256 C 1 *
bit 1255 I 1 IO_AA17
bit 1254 O 1 IO_AA17 1253 1 Z
bit 1253 C 1 *
bit 1252 I 1 IO_AB17
bit 1251 O 1 IO_AB17 1250 1 Z
bit 1250 C 1 *
bit 1249 I 1 IO_AA16
bit 1248 O 1 IO_AA16 1247 1 Z
bit 1247 C 1 *
bit 1246 I 1 IO_AD17
bit 1245 O 1 IO_AD17 1244 1 Z
bit 1244 C 1 *
bit 1243 I 1 IO_AE17
bit 1242 O 1 IO_AE17 1241 1 Z
bit 1241 C 1 *
bit 1240 I 1 IO_AH17
bit 1239 O 1 IO_AH17 1238 1 Z
bit 1238 C 1 *
bit 1237 I 1 IO_AJ17
bit 1236 O 1 IO_AJ17 1235 1 Z
bit 1235 C 1 *
bit 1234 O 1 *
bit 1233 O 1 *
bit 1232 O 1 *
bit 1231 I 1 IO_AB16
bit 1230 O 1 IO_AB16 1229 1 Z
bit 1229 C 1 *
bit 1228 I 1 IO_AC16
bit 1227 O 1 IO_AC16 1226 1 Z
bit 1226 C 1 *
bit 1225 I 1 IO_AD16
bit 1224 O 1 IO_AD16 1223 1 Z
bit 1223 C 1 *
bit 1222 I 1 IO_AE16
bit 1221 O 1 IO_AE16 1220 1 Z
bit 1220 C 1 *
bit 1219 I 1 IO_AF16
bit 1218 O 1 IO_AF16 1217 1 Z
bit 1217 C 1 *
bit 1216 I 1 IO_AG16
bit 1215 O 1 IO_AG16 1214 1 Z
bit 1214 C 1 *
bit 1213 I 1 IO_AH16
bit 1212 O 1 IO_AH16 1211 1 Z
bit 1211 C 1 *
bit 1210 I 1 IO_AJ16
bit 1209 O 1 IO_AJ16 1208 1 Z
bit 1208 C 1 *
bit 1207 I 1 IO_AK16
bit 1206 O 1 IO_AK16 1205 1 Z
bit 1205 C 1 *
bit 1204 I 1 IO_AK15
bit 1203 O 1 IO_AK15 1202 1 Z
bit 1202 C 1 *
bit 1201 I 1 IO_AJ15
bit 1200 O 1 IO_AJ15 1199 1 Z
bit 1199 C 1 *
bit 1198 I 1 IO_AH15
bit 1197 O 1 IO_AH15 1196 1 Z
bit 1196 C 1 *
bit 1195 I 1 IO_AG15
bit 1194 O 1 IO_AG15 1193 1 Z
bit 1193 C 1 *
bit 1192 I 1 IO_AF15
bit 1191 O 1 IO_AF15 1190 1 Z
bit 1190 C 1 *
bit 1189 I 1 IO_AE15
bit 1188 O 1 IO_AE15 1187 1 Z
bit 1187 C 1 *
bit 1186 I 1 IO_AD15
bit 1185 O 1 IO_AD15 1184 1 Z
bit 1184 C 1 *
bit 1183 I 1 IO_AD14
bit 1182 O 1 IO_AD14 1181 1 Z
bit 1181 C 1 *
bit 1180 I 1 IO_AC15
bit 1179 O 1 IO_AC15 1178 1 Z
bit 1178 C 1 *
bit 1177 I 1 IO_AB15
bit 1176 O 1 IO_AB15 1175 1 Z
bit 1175 C 1 *
bit 1174 I 1 IO_AA15
bit 1173 O 1 IO_AA15 1172 1 Z
bit 1172 C 1 *
bit 1171 I 1 IO_AJ14
bit 1170 O 1 IO_AJ14 1169 1 Z
bit 1169 C 1 *
bit 1168 I 1 IO_AH14
bit 1167 O 1 IO_AH14 1166 1 Z
bit 1166 C 1 *
bit 1165 I 1 IO_AE14
bit 1164 O 1 IO_AE14 1163 1 Z
bit 1163 C 1 *
bit 1162 I 1 IO_AE13
bit 1161 O 1 IO_AE13 1160 1 Z
bit 1160 C 1 *
bit 1159 O 1 *
bit 1158 O 1 *
bit 1157 O 1 *
bit 1156 I 1 IO_AB14
bit 1155 O 1 IO_AB14 1154 1 Z
bit 1154 C 1 *
bit 1153 I 1 IO_AA14
bit 1152 O 1 IO_AA14 1151 1 Z
bit 1151 C 1 *
bit 1150 I 1 IO_AK13
bit 1149 O 1 IO_AK13 1148 1 Z
bit 1148 C 1 *
bit 1147 I 1 IO_AJ13
bit 1146 O 1 IO_AJ13 1145 1 Z
bit 1145 C 1 *
bit 1144 O 1 *
bit 1143 O 1 *
bit 1142 O 1 *
bit 1141 I 1 IO_AG13
bit 1140 O 1 IO_AG13 1139 1 Z
bit 1139 C 1 *
bit 1138 I 1 IO_AF13
bit 1137 O 1 IO_AF13 1136 1 Z
bit 1136 C 1 *
bit 1135 I 1 IO_AC13
bit 1134 O 1 IO_AC13 1133 1 Z
bit 1133 C 1 *
bit 1132 I 1 IO_AB13
bit 1131 O 1 IO_AB13 1130 1 Z
bit 1130 C 1 *
bit 1129 O 1 *
bit 1128 O 1 *
bit 1127 O 1 *
bit 1126 I 1 IO_AA13
bit 1125 O 1 IO_AA13 1124 1 Z
bit 1124 C 1 *
bit 1123 I 1 IO_AA12
bit 1122 O 1 IO_AA12 1121 1 Z
bit 1121 C 1 *
bit 1120 I 1 IO_AK12
bit 1119 O 1 IO_AK12 1118 1 Z
bit 1118 C 1 *
bit 1117 I 1 IO_AJ12
bit 1116 O 1 IO_AJ12 1115 1 Z
bit 1115 C 1 *
bit 1114 O 1 *
bit 1113 O 1 *
bit 1112 O 1 *
bit 1111 I 1 IO_AH12
bit 1110 O 1 IO_AH12 1109 1 Z
bit 1109 C 1 *
bit 1108 I 1 IO_AG12
bit 1107 O 1 IO_AG12 1106 1 Z
bit 1106 C 1 *
bit 1105 I 1 IO_AF12
bit 1104 O 1 IO_AF12 1103 1 Z
bit 1103 C 1 *
bit 1102 I 1 IO_AE12
bit 1101 O 1 IO_AE12 1100 1 Z
bit 1100 C 1 *
bit 1099 O 1 *
bit 1098 O 1 *
bit 1097 O 1 *
bit 1096 I 1 IO_AD12
bit 1095 O 1 IO_AD12 1094 1 Z
bit 1094 C 1 *
bit 1093 I 1 IO_AC12
bit 1092 O 1 IO_AC12 1091 1 Z
bit 1091 C 1 *
bit 1090 I 1 IO_AB12
bit 1089 O 1 IO_AB12 1088 1 Z
bit 1088 C 1 *
bit 1087 I 1 IO_AC11
bit 1086 O 1 IO_AC11 1085 1 Z
bit 1085 C 1 *
bit 1084 O 1 *
bit 1083 O 1 *
bit 1082 O 1 *
bit 1081 I 1 IO_AK11
bit 1080 O 1 IO_AK11 1079 1 Z
bit 1079 C 1 *
bit 1078 I 1 IO_AJ11
bit 1077 O 1 IO_AJ11 1076 1 Z
bit 1076 C 1 *
bit 1075 I 1 IO_AH11
bit 1074 O 1 IO_AH11 1073 1 Z
bit 1073 C 1 *
bit 1072 I 1 IO_AG11
bit 1071 O 1 IO_AG11 1070 1 Z
bit 1070 C 1 *
bit 1069 O 1 *
bit 1068 O 1 *
bit 1067 O 1 *
bit 1066 I 1 IO_AF11
bit 1065 O 1 IO_AF11 1064 1 Z
bit 1064 C 1 *
bit 1063 I 1 IO_AE11
bit 1062 O 1 IO_AE11 1061 1 Z
bit 1061 C 1 *
bit 1060 I 1 IO_AD11
bit 1059 O 1 IO_AD11 1058 1 Z
bit 1058 C 1 *
bit 1057 I 1 IO_AD10
bit 1056 O 1 IO_AD10 1055 1 Z
bit 1055 C 1 *
bit 1054 I 1 IO_AA11
bit 1053 O 1 IO_AA11 1052 1 Z
bit 1052 C 1 *
bit 1051 I 1 IO_AJ10
bit 1050 O 1 IO_AJ10 1049 1 Z
bit 1049 C 1 *
bit 1048 I 1 IO_AH10
bit 1047 O 1 IO_AH10 1046 1 Z
bit 1046 C 1 *
bit 1045 I 1 IO_AE10
bit 1044 O 1 IO_AE10 1043 1 Z
bit 1043 C 1 *
bit 1042 I 1 IO_AE9
bit 1041 O 1 IO_AE9 1040 1 Z
bit 1040 C 1 *
bit 1039 I 1 IO_AB10
bit 1038 O 1 IO_AB10 1037 1 Z
bit 1037 C 1 *
bit 1036 I 1 IO_AK9
bit 1035 O 1 IO_AK9 1034 1 Z
bit 1034 C 1 *
bit 1033 I 1 IO_AJ9
bit 1032 O 1 IO_AJ9 1031 1 Z
bit 1031 C 1 *
bit 1030 I 1 IO_AG9
bit 1029 O 1 IO_AG9 1028 1 Z
bit 1028 C 1 *
bit 1027 I 1 IO_AF9
bit 1026 O 1 IO_AF9 1025 1 Z
bit 1025 C 1 *
bit 1024 O 1 *
bit 1023 O 1 *
bit 1022 O 1 *
bit 1021 I 1 IO_AC9
bit 1020 O 1 IO_AC9 1019 1 Z
bit 1019 C 1 *
bit 1018 I 1 IO_AB9
bit 1017 O 1 IO_AB9 1016 1 Z
bit 1016 C 1 *
bit 1015 I 1 IO_AK8
bit 1014 O 1 IO_AK8 1013 1 Z
bit 1013 C 1 *
bit 1012 I 1 IO_AJ8
bit 1011 O 1 IO_AJ8 1010 1 Z
bit 1010 C 1 *
bit 1009 O 1 *
bit 1008 O 1 *
bit 1007 O 1 *
bit 1006 I 1 IO_AH7
bit 1005 O 1 IO_AH7 1004 1 Z
bit 1004 C 1 *
bit 1003 I 1 IO_AG7
bit 1002 O 1 IO_AG7 1001 1 Z
bit 1001 C 1 *
bit 1000 I 1 IO_AE7
bit 999 O 1 IO_AE7 998 1 Z
bit 998 C 1 *
bit 997 I 1 IO_AD7
bit 996 O 1 IO_AD7 995 1 Z
bit 995 C 1 *
bit 994 I 1 IO_AE6
bit 993 O 1 IO_AE6 992 1 Z
bit 992 C 1 *
bit 991 I 1 IO_AJ6
bit 990 O 1 IO_AJ6 989 1 Z
bit 989 C 1 *
bit 988 I 1 IO_AH6
bit 987 O 1 IO_AH6 986 1 Z
bit 986 C 1 *
bit 985 I 1 IO_AF6
bit 984 O 1 IO_AF6 983 1 Z
bit 983 C 1 *
bit 982 I 1 IO_AG5
bit 981 O 1 IO_AG5 980 1 Z
bit 980 C 1 *
bit 979 I 1 IO_AH4
bit 978 O 1 IO_AH4 977 1 Z
bit 977 C 1 *
bit 976 I 1 IO_AK5
bit 975 O 1 IO_AK5 974 1 Z
bit 974 C 1 *
bit 973 I 1 IO_AJ5
bit 972 O 1 IO_AJ5 971 1 Z
bit 971 C 1 *
bit 970 I 1 IO_AK4
bit 969 O 1 IO_AK4 968 1 Z
bit 968 C 1 *
bit 967 I 1 IO_AJ4
bit 966 O 1 IO_AJ4 965 1 Z
bit 965 C 1 *
bit 964 I 1 M2_AK3
bit 963 I 1 M0_AJ3
bit 962 I 1 M1_AH3
bit 961 I 1 IO_AH2
bit 960 O 1 IO_AH2 959 1 Z
bit 959 C 1 *
bit 958 I 1 IO_AH1
bit 957 O 1 IO_AH1 956 1 Z
bit 956 C 1 *
bit 955 I 1 IO_AG4
bit 954 O 1 IO_AG4 953 1 Z
bit 953 C 1 *
bit 952 I 1 IO_AG3
bit 951 O 1 IO_AG3 950 1 Z
bit 950 C 1 *
bit 949 I 1 IO_AG2
bit 948 O 1 IO_AG2 947 1 Z
bit 947 C 1 *
bit 946 I 1 IO_AG1
bit 945 O 1 IO_AG1 944 1 Z
bit 944 C 1 *
bit 943 I 1 IO_AF2
bit 942 O 1 IO_AF2 941 1 Z
bit 941 C 1 *
bit 940 I 1 IO_AF1
bit 939 O 1 IO_AF1 938 1 Z
bit 938 C 1 *
bit 937 I 1 IO_AF4
bit 936 O 1 IO_AF4 935 1 Z
bit 935 C 1 *
bit 934 I 1 IO_AE5
bit 933 O 1 IO_AE5 932 1 Z
bit 932 C 1 *
bit 931 I 1 IO_AE3
bit 930 O 1 IO_AE3 929 1 Z
bit 929 C 1 *
bit 928 I 1 IO_AE2
bit 927 O 1 IO_AE2 926 1 Z
bit 926 C 1 *
bit 925 I 1 IO_AD4
bit 924 O 1 IO_AD4 923 1 Z
bit 923 C 1 *
bit 922 I 1 IO_AD3
bit 921 O 1 IO_AD3 920 1 Z
bit 920 C 1 *
bit 919 I 1 IO_AD2
bit 918 O 1 IO_AD2 917 1 Z
bit 917 C 1 *
bit 916 I 1 IO_AD1
bit 915 O 1 IO_AD1 914 1 Z
bit 914 C 1 *
bit 913 I 1 IO_AD6
bit 912 O 1 IO_AD6 911 1 Z
bit 911 C 1 *
bit 910 I 1 IO_AC7
bit 909 O 1 IO_AC7 908 1 Z
bit 908 C 1 *
bit 907 I 1 IO_AC6
bit 906 O 1 IO_AC6 905 1 Z
bit 905 C 1 *
bit 904 I 1 IO_AC5
bit 903 O 1 IO_AC5 902 1 Z
bit 902 C 1 *
bit 901 I 1 IO_AC4
bit 900 O 1 IO_AC4 899 1 Z
bit 899 C 1 *
bit 898 I 1 IO_AC3
bit 897 O 1 IO_AC3 896 1 Z
bit 896 C 1 *
bit 895 O 1 *
bit 894 O 1 *
bit 893 O 1 *
bit 892 I 1 IO_AB6
bit 891 O 1 IO_AB6 890 1 Z
bit 890 C 1 *
bit 889 I 1 IO_AC2
bit 888 O 1 IO_AC2 887 1 Z
bit 887 C 1 *
bit 886 I 1 IO_AC1
bit 885 O 1 IO_AC1 884 1 Z
bit 884 C 1 *
bit 883 I 1 IO_AB5
bit 882 O 1 IO_AB5 881 1 Z
bit 881 C 1 *
bit 880 I 1 IO_AB4
bit 879 O 1 IO_AB4 878 1 Z
bit 878 C 1 *
bit 877 I 1 IO_AB2
bit 876 O 1 IO_AB2 875 1 Z
bit 875 C 1 *
bit 874 I 1 IO_AB1
bit 873 O 1 IO_AB1 872 1 Z
bit 872 C 1 *
bit 871 I 1 IO_AB8
bit 870 O 1 IO_AB8 869 1 Z
bit 869 C 1 *
bit 868 I 1 IO_AA9
bit 867 O 1 IO_AA9 866 1 Z
bit 866 C 1 *
bit 865 I 1 IO_AA7
bit 864 O 1 IO_AA7 863 1 Z
bit 863 C 1 *
bit 862 I 1 IO_AA6
bit 861 O 1 IO_AA6 860 1 Z
bit 860 C 1 *
bit 859 O 1 *
bit 858 O 1 *
bit 857 O 1 *
bit 856 O 1 *
bit 855 O 1 *
bit 854 O 1 *
bit 853 I 1 IO_AA3
bit 852 O 1 IO_AA3 851 1 Z
bit 851 C 1 *
bit 850 I 1 IO_AA2
bit 849 O 1 IO_AA2 848 1 Z
bit 848 C 1 *
bit 847 I 1 IO_AA10
bit 846 O 1 IO_AA10 845 1 Z
bit 845 C 1 *
bit 844 I 1 IO_Y10
bit 843 O 1 IO_Y10 842 1 Z
bit 842 C 1 *
bit 841 I 1 IO_Y8
bit 840 O 1 IO_Y8 839 1 Z
bit 839 C 1 *
bit 838 I 1 IO_Y7
bit 837 O 1 IO_Y7 836 1 Z
bit 836 C 1 *
bit 835 I 1 IO_Y6
bit 834 O 1 IO_Y6 833 1 Z
bit 833 C 1 *
bit 832 I 1 IO_Y5
bit 831 O 1 IO_Y5 830 1 Z
bit 830 C 1 *
bit 829 O 1 *
bit 828 O 1 *
bit 827 O 1 *
bit 826 O 1 *
bit 825 O 1 *
bit 824 O 1 *
bit 823 I 1 IO_Y2
bit 822 O 1 IO_Y2 821 1 Z
bit 821 C 1 *
bit 820 I 1 IO_Y1
bit 819 O 1 IO_Y1 818 1 Z
bit 818 C 1 *
bit 817 O 1 *
bit 816 O 1 *
bit 815 O 1 *
bit 814 O 1 *
bit 813 O 1 *
bit 812 O 1 *
bit 811 I 1 IO_W7
bit 810 O 1 IO_W7 809 1 Z
bit 809 C 1 *
bit 808 I 1 IO_W6
bit 807 O 1 IO_W6 806 1 Z
bit 806 C 1 *
bit 805 I 1 IO_W4
bit 804 O 1 IO_W4 803 1 Z
bit 803 C 1 *
bit 802 I 1 IO_W3
bit 801 O 1 IO_W3 800 1 Z
bit 800 C 1 *
bit 799 I 1 IO_W2
bit 798 O 1 IO_W2 797 1 Z
bit 797 C 1 *
bit 796 I 1 IO_W1
bit 795 O 1 IO_W1 794 1 Z
bit 794 C 1 *
bit 793 I 1 IO_W10
bit 792 O 1 IO_W10 791 1 Z
bit 791 C 1 *
bit 790 I 1 IO_V10
bit 789 O 1 IO_V10 788 1 Z
bit 788 C 1 *
bit 787 O 1 *
bit 786 O 1 *
bit 785 O 1 *
bit 784 O 1 *
bit 783 O 1 *
bit 782 O 1 *
bit 781 I 1 IO_W5
bit 780 O 1 IO_W5 779 1 Z
bit 779 C 1 *
bit 778 I 1 IO_V6
bit 777 O 1 IO_V6 776 1 Z
bit 776 C 1 *
bit 775 I 1 IO_V5
bit 774 O 1 IO_V5 773 1 Z
bit 773 C 1 *
bit 772 I 1 IO_V4
bit 771 O 1 IO_V4 770 1 Z
bit 770 C 1 *
bit 769 I 1 IO_V2
bit 768 O 1 IO_V2 767 1 Z
bit 767 C 1 *
bit 766 I 1 IO_V1
bit 765 O 1 IO_V1 764 1 Z
bit 764 C 1 *
bit 763 I 1 IO_U10
bit 762 O 1 IO_U10 761 1 Z
bit 761 C 1 *
bit 760 I 1 IO_U9
bit 759 O 1 IO_U9 758 1 Z
bit 758 C 1 *
bit 757 I 1 IO_U7
bit 756 O 1 IO_U7 755 1 Z
bit 755 C 1 *
bit 754 I 1 IO_U6
bit 753 O 1 IO_U6 752 1 Z
bit 752 C 1 *
bit 751 O 1 *
bit 750 O 1 *
bit 749 O 1 *
bit 748 O 1 *
bit 747 O 1 *
bit 746 O 1 *
bit 745 I 1 IO_T10
bit 744 O 1 IO_T10 743 1 Z
bit 743 C 1 *
bit 742 I 1 IO_T9
bit 741 O 1 IO_T9 740 1 Z
bit 740 C 1 *
bit 739 I 1 IO_T6
bit 738 O 1 IO_T6 737 1 Z
bit 737 C 1 *
bit 736 I 1 IO_T5
bit 735 O 1 IO_T5 734 1 Z
bit 734 C 1 *
bit 733 I 1 IO_T4
bit 732 O 1 IO_T4 731 1 Z
bit 731 C 1 *
bit 730 I 1 IO_T3
bit 729 O 1 IO_T3 728 1 Z
bit 728 C 1 *
bit 727 I 1 IO_T2
bit 726 O 1 IO_T2 725 1 Z
bit 725 C 1 *
bit 724 I 1 IO_T1
bit 723 O 1 IO_T1 722 1 Z
bit 722 C 1 *
bit 721 I 1 IO_R1
bit 720 O 1 IO_R1 719 1 Z
bit 719 C 1 *
bit 718 I 1 IO_R2
bit 717 O 1 IO_R2 716 1 Z
bit 716 C 1 *
bit 715 I 1 IO_R3
bit 714 O 1 IO_R3 713 1 Z
bit 713 C 1 *
bit 712 I 1 IO_R4
bit 711 O 1 IO_R4 710 1 Z
bit 710 C 1 *
bit 709 I 1 IO_R5
bit 708 O 1 IO_R5 707 1 Z
bit 707 C 1 *
bit 706 I 1 IO_R6
bit 705 O 1 IO_R6 704 1 Z
bit 704 C 1 *
bit 703 I 1 IO_R7
bit 702 O 1 IO_R7 701 1 Z
bit 701 C 1 *
bit 700 I 1 IO_R8
bit 699 O 1 IO_R8 698 1 Z
bit 698 C 1 *
bit 697 O 1 *
bit 696 O 1 *
bit 695 O 1 *
bit 694 O 1 *
bit 693 O 1 *
bit 692 O 1 *
bit 691 I 1 IO_R9
bit 690 O 1 IO_R9 689 1 Z
bit 689 C 1 *
bit 688 I 1 IO_R10
bit 687 O 1 IO_R10 686 1 Z
bit 686 C 1 *
bit 685 I 1 IO_P2
bit 684 O 1 IO_P2 683 1 Z
bit 683 C 1 *
bit 682 I 1 IO_P3
bit 681 O 1 IO_P3 680 1 Z
bit 680 C 1 *
bit 679 I 1 IO_P6
bit 678 O 1 IO_P6 677 1 Z
bit 677 C 1 *
bit 676 I 1 IO_P7
bit 675 O 1 IO_P7 674 1 Z
bit 674 C 1 *
bit 673 I 1 IO_P9
bit 672 O 1 IO_P9 671 1 Z
bit 671 C 1 *
bit 670 I 1 IO_P10
bit 669 O 1 IO_P10 668 1 Z
bit 668 C 1 *
bit 667 I 1 IO_N1
bit 666 O 1 IO_N1 665 1 Z
bit 665 C 1 *
bit 664 I 1 IO_N2
bit 663 O 1 IO_N2 662 1 Z
bit 662 C 1 *
bit 661 O 1 *
bit 660 O 1 *
bit 659 O 1 *
bit 658 O 1 *
bit 657 O 1 *
bit 656 O 1 *
bit 655 I 1 IO_N8
bit 654 O 1 IO_N8 653 1 Z
bit 653 C 1 *
bit 652 I 1 IO_N9
bit 651 O 1 IO_N9 650 1 Z
bit 650 C 1 *
bit 649 I 1 IO_N10
bit 648 O 1 IO_N10 647 1 Z
bit 647 C 1 *
bit 646 I 1 IO_M10
bit 645 O 1 IO_M10 644 1 Z
bit 644 C 1 *
bit 643 I 1 IO_M1
bit 642 O 1 IO_M1 641 1 Z
bit 641 C 1 *
bit 640 I 1 IO_M2
bit 639 O 1 IO_M2 638 1 Z
bit 638 C 1 *
bit 637 I 1 IO_M3
bit 636 O 1 IO_M3 635 1 Z
bit 635 C 1 *
bit 634 I 1 IO_M4
bit 633 O 1 IO_M4 632 1 Z
bit 632 C 1 *
bit 631 O 1 *
bit 630 O 1 *
bit 629 O 1 *
bit 628 O 1 *
bit 627 O 1 *
bit 626 O 1 *
bit 625 I 1 IO_L1
bit 624 O 1 IO_L1 623 1 Z
bit 623 C 1 *
bit 622 I 1 IO_L2
bit 621 O 1 IO_L2 620 1 Z
bit 620 C 1 *
bit 619 I 1 IO_L3
bit 618 O 1 IO_L3 617 1 Z
bit 617 C 1 *
bit 616 I 1 IO_L4
bit 615 O 1 IO_L4 614 1 Z
bit 614 C 1 *
bit 613 I 1 IO_L5
bit 612 O 1 IO_L5 611 1 Z
bit 611 C 1 *
bit 610 I 1 IO_L6
bit 609 O 1 IO_L6 608 1 Z
bit 608 C 1 *
bit 607 I 1 IO_L7
bit 606 O 1 IO_L7 605 1 Z
bit 605 C 1 *
bit 604 I 1 IO_L8
bit 603 O 1 IO_L8 602 1 Z
bit 602 C 1 *
bit 601 I 1 IO_L10
bit 600 O 1 IO_L10 599 1 Z
bit 599 C 1 *
bit 598 I 1 IO_K10
bit 597 O 1 IO_K10 596 1 Z
bit 596 C 1 *
bit 595 I 1 IO_K2
bit 594 O 1 IO_K2 593 1 Z
bit 593 C 1 *
bit 592 I 1 IO_K3
bit 591 O 1 IO_K3 590 1 Z
bit 590 C 1 *
bit 589 O 1 *
bit 588 O 1 *
bit 587 O 1 *
bit 586 O 1 *
bit 585 O 1 *
bit 584 O 1 *
bit 583 I 1 IO_K6
bit 582 O 1 IO_K6 581 1 Z
bit 581 C 1 *
bit 580 I 1 IO_K7
bit 579 O 1 IO_K7 578 1 Z
bit 578 C 1 *
bit 577 I 1 IO_K9
bit 576 O 1 IO_K9 575 1 Z
bit 575 C 1 *
bit 574 I 1 IO_J8
bit 573 O 1 IO_J8 572 1 Z
bit 572 C 1 *
bit 571 I 1 IO_J1
bit 570 O 1 IO_J1 569 1 Z
bit 569 C 1 *
bit 568 I 1 IO_J2
bit 567 O 1 IO_J2 566 1 Z
bit 566 C 1 *
bit 565 I 1 IO_J4
bit 564 O 1 IO_J4 563 1 Z
bit 563 C 1 *
bit 562 I 1 IO_J5
bit 561 O 1 IO_J5 560 1 Z
bit 560 C 1 *
bit 559 I 1 IO_H1
bit 558 O 1 IO_H1 557 1 Z
bit 557 C 1 *
bit 556 I 1 IO_H2
bit 555 O 1 IO_H2 554 1 Z
bit 554 C 1 *
bit 553 I 1 IO_J6
bit 552 O 1 IO_J6 551 1 Z
bit 551 C 1 *
bit 550 O 1 *
bit 549 O 1 *
bit 548 O 1 *
bit 547 I 1 IO_H3
bit 546 O 1 IO_H3 545 1 Z
bit 545 C 1 *
bit 544 I 1 IO_H4
bit 543 O 1 IO_H4 542 1 Z
bit 542 C 1 *
bit 541 I 1 IO_H5
bit 540 O 1 IO_H5 539 1 Z
bit 539 C 1 *
bit 538 I 1 IO_H6
bit 537 O 1 IO_H6 536 1 Z
bit 536 C 1 *
bit 535 I 1 IO_H7
bit 534 O 1 IO_H7 533 1 Z
bit 533 C 1 *
bit 532 I 1 IO_G6
bit 531 O 1 IO_G6 530 1 Z
bit 530 C 1 *
bit 529 I 1 IO_G1
bit 528 O 1 IO_G1 527 1 Z
bit 527 C 1 *
bit 526 I 1 IO_G2
bit 525 O 1 IO_G2 524 1 Z
bit 524 C 1 *
bit 523 I 1 IO_G3
bit 522 O 1 IO_G3 521 1 Z
bit 521 C 1 *
bit 520 I 1 IO_G4
bit 519 O 1 IO_G4 518 1 Z
bit 518 C 1 *
bit 517 I 1 IO_F2
bit 516 O 1 IO_F2 515 1 Z
bit 515 C 1 *
bit 514 I 1 IO_F3
bit 513 O 1 IO_F3 512 1 Z
bit 512 C 1 *
bit 511 I 1 IO_F5
bit 510 O 1 IO_F5 509 1 Z
bit 509 C 1 *
bit 508 I 1 IO_E4
bit 507 O 1 IO_E4 506 1 Z
bit 506 C 1 *
bit 505 I 1 IO_E1
bit 504 O 1 IO_E1 503 1 Z
bit 503 C 1 *
bit 502 I 1 IO_E2
bit 501 O 1 IO_E2 500 1 Z
bit 500 C 1 *
bit 499 I 1 IO_D1
bit 498 O 1 IO_D1 497 1 Z
bit 497 C 1 *
bit 496 I 1 IO_D2
bit 495 O 1 IO_D2 494 1 Z
bit 494 C 1 *
bit 493 I 1 IO_D3
bit 492 O 1 IO_D3 491 1 Z
bit 491 C 1 *
bit 490 I 1 IO_D4
bit 489 O 1 IO_D4 488 1 Z
bit 488 C 1 *
bit 487 I 1 IO_C1
bit 486 O 1 IO_C1 485 1 Z
bit 485 C 1 *
bit 484 I 1 IO_C2
bit 483 O 1 IO_C2 482 1 Z
bit 482 C 1 *
bit 481 O 1 *
bit 480 I 1 HSWAP_EN_A3
bit 479 I 1 IO_C4
bit 478 O 1 IO_C4 477 1 Z
bit 477 C 1 *
bit 476 I 1 IO_B4
bit 475 O 1 IO_B4 474 1 Z
bit 474 C 1 *
bit 473 I 1 IO_A4
bit 472 O 1 IO_A4 471 1 Z
bit 471 C 1 *
bit 470 I 1 IO_B5
bit 469 O 1 IO_B5 468 1 Z
bit 468 C 1 *
bit 467 I 1 IO_A5
bit 466 O 1 IO_A5 465 1 Z
bit 465 C 1 *
bit 464 O 1 *
bit 463 O 1 *
bit 462 O 1 *
bit 461 I 1 IO_D5
bit 460 O 1 IO_D5 459 1 Z
bit 459 C 1 *
bit 458 I 1 IO_E6
bit 457 O 1 IO_E6 456 1 Z
bit 456 C 1 *
bit 455 I 1 IO_C6
bit 454 O 1 IO_C6 453 1 Z
bit 453 C 1 *
bit 452 I 1 IO_B6
bit 451 O 1 IO_B6 450 1 Z
bit 450 C 1 *
bit 449 O 1 *
bit 448 O 1 *
bit 447 O 1 *
bit 446 I 1 IO_F6
bit 445 O 1 IO_F6 444 1 Z
bit 444 C 1 *
bit 443 I 1 IO_F7
bit 442 O 1 IO_F7 441 1 Z
bit 441 C 1 *
bit 440 I 1 IO_D7
bit 439 O 1 IO_D7 438 1 Z
bit 438 C 1 *
bit 437 I 1 IO_C7
bit 436 O 1 IO_C7 435 1 Z
bit 435 C 1 *
bit 434 I 1 IO_G8
bit 433 O 1 IO_G8 432 1 Z
bit 432 C 1 *
bit 431 I 1 IO_F8
bit 430 O 1 IO_F8 429 1 Z
bit 429 C 1 *
bit 428 I 1 IO_E8
bit 427 O 1 IO_E8 426 1 Z
bit 426 C 1 *
bit 425 I 1 IO_D8
bit 424 O 1 IO_D8 423 1 Z
bit 423 C 1 *
bit 422 I 1 IO_C8
bit 421 O 1 IO_C8 420 1 Z
bit 420 C 1 *
bit 419 O 1 *
bit 418 O 1 *
bit 417 O 1 *
bit 416 I 1 IO_B8
bit 415 O 1 IO_B8 414 1 Z
bit 414 C 1 *
bit 413 I 1 IO_A8
bit 412 O 1 IO_A8 411 1 Z
bit 411 C 1 *
bit 410 I 1 IO_J9
bit 409 O 1 IO_J9 408 1 Z
bit 408 C 1 *
bit 407 I 1 IO_H9
bit 406 O 1 IO_H9 405 1 Z
bit 405 C 1 *
bit 404 I 1 IO_F9
bit 403 O 1 IO_F9 402 1 Z
bit 402 C 1 *
bit 401 I 1 IO_G10
bit 400 O 1 IO_G10 399 1 Z
bit 399 C 1 *
bit 398 I 1 IO_F10
bit 397 O 1 IO_F10 396 1 Z
bit 396 C 1 *
bit 395 I 1 IO_C10
bit 394 O 1 IO_C10 393 1 Z
bit 393 C 1 *
bit 392 I 1 IO_B10
bit 391 O 1 IO_B10 390 1 Z
bit 390 C 1 *
bit 389 O 1 *
bit 388 O 1 *
bit 387 O 1 *
bit 386 I 1 IO_J10
bit 385 O 1 IO_J10 384 1 Z
bit 384 C 1 *
bit 383 I 1 IO_K11
bit 382 O 1 IO_K11 381 1 Z
bit 381 C 1 *
bit 380 I 1 IO_H11
bit 379 O 1 IO_H11 378 1 Z
bit 378 C 1 *
bit 377 I 1 IO_G11
bit 376 O 1 IO_G11 375 1 Z
bit 375 C 1 *
bit 374 O 1 *
bit 373 O 1 *
bit 372 O 1 *
bit 371 I 1 IO_F11
bit 370 O 1 IO_F11 369 1 Z
bit 369 C 1 *
bit 368 I 1 IO_E11
bit 367 O 1 IO_E11 366 1 Z
bit 366 C 1 *
bit 365 I 1 IO_D11
bit 364 O 1 IO_D11 363 1 Z
bit 363 C 1 *
bit 362 I 1 IO_C11
bit 361 O 1 IO_C11 360 1 Z
bit 360 C 1 *
bit 359 O 1 *
bit 358 O 1 *
bit 357 O 1 *
bit 356 I 1 IO_B11
bit 355 O 1 IO_B11 354 1 Z
bit 354 C 1 *
bit 353 I 1 IO_A11
bit 352 O 1 IO_A11 351 1 Z
bit 351 C 1 *
bit 350 I 1 IO_K12
bit 349 O 1 IO_K12 348 1 Z
bit 348 C 1 *
bit 347 I 1 IO_J12
bit 346 O 1 IO_J12 345 1 Z
bit 345 C 1 *
bit 344 O 1 *
bit 343 O 1 *
bit 342 O 1 *
bit 341 I 1 IO_H12
bit 340 O 1 IO_H12 339 1 Z
bit 339 C 1 *
bit 338 I 1 IO_G12
bit 337 O 1 IO_G12 336 1 Z
bit 336 C 1 *
bit 335 I 1 IO_F12
bit 334 O 1 IO_F12 333 1 Z
bit 333 C 1 *
bit 332 I 1 IO_E12
bit 331 O 1 IO_E12 330 1 Z
bit 330 C 1 *
bit 329 O 1 *
bit 328 O 1 *
bit 327 O 1 *
bit 326 I 1 IO_D12
bit 325 O 1 IO_D12 324 1 Z
bit 324 C 1 *
bit 323 I 1 IO_C12
bit 322 O 1 IO_C12 321 1 Z
bit 321 C 1 *
bit 320 I 1 IO_B12
bit 319 O 1 IO_B12 318 1 Z
bit 318 C 1 *
bit 317 I 1 IO_A12
bit 316 O 1 IO_A12 315 1 Z
bit 315 C 1 *
bit 314 I 1 IO_K13
bit 313 O 1 IO_K13 312 1 Z
bit 312 C 1 *
bit 311 I 1 IO_J13
bit 310 O 1 IO_J13 309 1 Z
bit 309 C 1 *
bit 308 I 1 IO_H13
bit 307 O 1 IO_H13 306 1 Z
bit 306 C 1 *
bit 305 I 1 IO_F13
bit 304 O 1 IO_F13 303 1 Z
bit 303 C 1 *
bit 302 I 1 IO_E13
bit 301 O 1 IO_E13 300 1 Z
bit 300 C 1 *
bit 299 I 1 IO_D13
bit 298 O 1 IO_D13 297 1 Z
bit 297 C 1 *
bit 296 I 1 IO_B13
bit 295 O 1 IO_B13 294 1 Z
bit 294 C 1 *
bit 293 I 1 IO_A13
bit 292 O 1 IO_A13 291 1 Z
bit 291 C 1 *
bit 290 I 1 IO_K14
bit 289 O 1 IO_K14 288 1 Z
bit 288 C 1 *
bit 287 I 1 IO_J14
bit 286 O 1 IO_J14 285 1 Z
bit 285 C 1 *
bit 284 I 1 IO_K15
bit 283 O 1 IO_K15 282 1 Z
bit 282 C 1 *
bit 281 I 1 IO_G14
bit 280 O 1 IO_G14 279 1 Z
bit 279 C 1 *
bit 278 I 1 IO_F14
bit 277 O 1 IO_F14 276 1 Z
bit 276 C 1 *
bit 275 I 1 IO_C14
bit 274 O 1 IO_C14 273 1 Z
bit 273 C 1 *
bit 272 I 1 IO_B14
bit 271 O 1 IO_B14 270 1 Z
bit 270 C 1 *
bit 269 O 1 *
bit 268 O 1 *
bit 267 O 1 *
bit 266 I 1 IO_J15
bit 265 O 1 IO_J15 264 1 Z
bit 264 C 1 *
bit 263 I 1 IO_H15
bit 262 O 1 IO_H15 261 1 Z
bit 261 C 1 *
bit 260 I 1 IO_G15
bit 259 O 1 IO_G15 258 1 Z
bit 258 C 1 *
bit 257 I 1 IO_F15
bit 256 O 1 IO_F15 255 1 Z
bit 255 C 1 *
bit 254 I 1 IO_E15
bit 253 O 1 IO_E15 252 1 Z
bit 252 C 1 *
bit 251 I 1 IO_D15
bit 250 O 1 IO_D15 249 1 Z
bit 249 C 1 *
bit 248 I 1 IO_C15
bit 247 O 1 IO_C15 246 1 Z
bit 246 C 1 *
bit 245 I 1 IO_B15
bit 244 O 1 IO_B15 243 1 Z
bit 243 C 1 *
bit 242 I 1 IO_A15
bit 241 O 1 IO_A15 240 1 Z
bit 240 C 1 *
bit 239 I 1 IO_A16
bit 238 O 1 IO_A16 237 1 Z
bit 237 C 1 *
bit 236 I 1 IO_B16
bit 235 O 1 IO_B16 234 1 Z
bit 234 C 1 *
bit 233 I 1 IO_C16
bit 232 O 1 IO_C16 231 1 Z
bit 231 C 1 *
bit 230 I 1 IO_D16
bit 229 O 1 IO_D16 228 1 Z
bit 228 C 1 *
bit 227 I 1 IO_E16
bit 226 O 1 IO_E16 225 1 Z
bit 225 C 1 *
bit 224 I 1 IO_F16
bit 223 O 1 IO_F16 222 1 Z
bit 222 C 1 *
bit 221 I 1 IO_G16
bit 220 O 1 IO_G16 219 1 Z
bit 219 C 1 *
bit 218 I 1 IO_H16
bit 217 O 1 IO_H16 216 1 Z
bit 216 C 1 *
bit 215 I 1 IO_J16
bit 214 O 1 IO_J16 213 1 Z
bit 213 C 1 *
bit 212 I 1 IO_K16
bit 211 O 1 IO_K16 210 1 Z
bit 210 C 1 *
bit 209 I 1 IO_J17
bit 208 O 1 IO_J17 207 1 Z
bit 207 C 1 *
bit 206 I 1 IO_B17
bit 205 O 1 IO_B17 204 1 Z
bit 204 C 1 *
bit 203 I 1 IO_C17
bit 202 O 1 IO_C17 201 1 Z
bit 201 C 1 *
bit 200 I 1 IO_F17
bit 199 O 1 IO_F17 198 1 Z
bit 198 C 1 *
bit 197 I 1 IO_G17
bit 196 O 1 IO_G17 195 1 Z
bit 195 C 1 *
bit 194 I 1 IO_F18
bit 193 O 1 IO_F18 192 1 Z
bit 192 C 1 *
bit 191 I 1 IO_A19
bit 190 O 1 IO_A19 189 1 Z
bit 189 C 1 *
bit 188 I 1 IO_B19
bit 187 O 1 IO_B19 186 1 Z
bit 186 C 1 *
bit 185 I 1 IO_C19
bit 184 O 1 IO_C19 183 1 Z
bit 183 C 1 *
bit 182 I 1 IO_D19
bit 181 O 1 IO_D19 180 1 Z
bit 180 C 1 *
bit 179 O 1 *
bit 178 O 1 *
bit 177 O 1 *
bit 176 I 1 IO_E19
bit 175 O 1 IO_E19 174 1 Z
bit 174 C 1 *
bit 173 I 1 IO_F19
bit 172 O 1 IO_F19 171 1 Z
bit 171 C 1 *
bit 170 I 1 IO_G19
bit 169 O 1 IO_G19 168 1 Z
bit 168 C 1 *
bit 167 I 1 IO_H19
bit 166 O 1 IO_H19 165 1 Z
bit 165 C 1 *
bit 164 O 1 *
bit 163 O 1 *
bit 162 O 1 *
bit 161 I 1 IO_J19
bit 160 O 1 IO_J19 159 1 Z
bit 159 C 1 *
bit 158 I 1 IO_K19
bit 157 O 1 IO_K19 156 1 Z
bit 156 C 1 *
bit 155 I 1 IO_A20
bit 154 O 1 IO_A20 153 1 Z
bit 153 C 1 *
bit 152 I 1 IO_B20
bit 151 O 1 IO_B20 150 1 Z
bit 150 C 1 *
bit 149 O 1 *
bit 148 O 1 *
bit 147 O 1 *
bit 146 I 1 IO_C20
bit 145 O 1 IO_C20 144 1 Z
bit 144 C 1 *
bit 143 I 1 IO_D20
bit 142 O 1 IO_D20 141 1 Z
bit 141 C 1 *
bit 140 I 1 IO_E20
bit 139 O 1 IO_E20 138 1 Z
bit 138 C 1 *
bit 137 I 1 IO_F20
bit 136 O 1 IO_F20 135 1 Z
bit 135 C 1 *
bit 134 O 1 *
bit 133 O 1 *
bit 132 O 1 *
bit 131 I 1 IO_G20
bit 130 O 1 IO_G20 129 1 Z
bit 129 C 1 *
bit 128 I 1 IO_H20
bit 127 O 1 IO_H20 126 1 Z
bit 126 C 1 *
bit 125 I 1 IO_B21
bit 124 O 1 IO_B21 123 1 Z
bit 123 C 1 *
bit 122 I 1 IO_C21
bit 121 O 1 IO_C21 120 1 Z
bit 120 C 1 *
bit 119 I 1 IO_K20
bit 118 O 1 IO_K20 117 1 Z
bit 117 C 1 *
bit 116 I 1 IO_F21
bit 115 O 1 IO_F21 114 1 Z
bit 114 C 1 *
bit 113 I 1 IO_G21
bit 112 O 1 IO_G21 111 1 Z
bit 111 C 1 *
bit 110 I 1 IO_A22
bit 109 O 1 IO_A22 108 1 Z
bit 108 C 1 *
bit 107 I 1 IO_B22
bit 106 O 1 IO_B22 105 1 Z
bit 105 C 1 *
bit 104 I 1 IO_J21
bit 103 O 1 IO_J21 102 1 Z
bit 102 C 1 *
bit 101 I 1 IO_D22
bit 100 O 1 IO_D22 99 1 Z
bit 99 C 1 *
bit 98 I 1 IO_E22
bit 97 O 1 IO_E22 96 1 Z
bit 96 C 1 *
bit 95 I 1 IO_F22
bit 94 O 1 IO_F22 93 1 Z
bit 93 C 1 *
bit 92 I 1 IO_E23
bit 91 O 1 IO_E23 90 1 Z
bit 90 C 1 *
bit 89 O 1 *
bit 88 O 1 *
bit 87 O 1 *
bit 86 I 1 IO_H22
bit 85 O 1 IO_H22 84 1 Z
bit 84 C 1 *
bit 83 I 1 IO_J22
bit 82 O 1 IO_J22 81 1 Z
bit 81 C 1 *
bit 80 I 1 IO_A23
bit 79 O 1 IO_A23 78 1 Z
bit 78 C 1 *
bit 77 I 1 IO_B23
bit 76 O 1 IO_B23 75 1 Z
bit 75 C 1 *
bit 74 O 1 *
bit 73 O 1 *
bit 72 O 1 *
bit 71 I 1 IO_C23
bit 70 O 1 IO_C23 69 1 Z
bit 69 C 1 *
bit 68 I 1 IO_D23
bit 67 O 1 IO_D23 66 1 Z
bit 66 C 1 *
bit 65 I 1 IO_F23
bit 64 O 1 IO_F23 63 1 Z
bit 63 C 1 *
bit 62 I 1 IO_G23
bit 61 O 1 IO_G23 60 1 Z
bit 60 C 1 *
bit 59 O 1 *
bit 58 O 1 *
bit 57 O 1 *
bit 56 I 1 IO_H23
bit 55 O 1 IO_H23 54 1 Z
bit 54 C 1 *
bit 53 I 1 IO_G24
bit 52 O 1 IO_G24 51 1 Z
bit 51 C 1 *
bit 50 I 1 IO_A24
bit 49 O 1 IO_A24 48 1 Z
bit 48 C 1 *
bit 47 I 1 IO_B24
bit 46 O 1 IO_B24 45 1 Z
bit 45 C 1 *
bit 44 O 1 *
bit 43 O 1 *
bit 42 O 1 *
bit 41 I 1 IO_C24
bit 40 O 1 IO_C24 39 1 Z
bit 39 C 1 *
bit 38 I 1 IO_D24
bit 37 O 1 IO_D24 36 1 Z
bit 36 C 1 *
bit 35 I 1 IO_F24
bit 34 O 1 IO_F24 33 1 Z
bit 33 C 1 *
bit 32 I 1 IO_F25
bit 31 O 1 IO_F25 30 1 Z
bit 30 C 1 *
bit 29 I 1 IO_E25
bit 28 O 1 IO_E25 27 1 Z
bit 27 C 1 *
bit 26 I 1 IO_B25
bit 25 O 1 IO_B25 24 1 Z
bit 24 C 1 *
bit 23 I 1 IO_C25
bit 22 O 1 IO_C25 21 1 Z
bit 21 C 1 *
bit 20 I 1 IO_A26
bit 19 O 1 IO_A26 18 1 Z
bit 18 C 1 *
bit 17 I 1 IO_B26
bit 16 O 1 IO_B26 15 1 Z
bit 15 C 1 *
bit 14 O 1 *
bit 13 O 1 *
bit 12 O 1 *
bit 11 I 1 IO_D26
bit 10 O 1 IO_D26 9 1 Z
bit 9 C 1 *
bit 8 I 1 IO_C27
bit 7 O 1 IO_C27 6 1 Z
bit 6 C 1 *
bit 5 I 1 IO_A27
bit 4 O 1 IO_A27 3 1 Z
bit 3 C 1 *
bit 2 I 1 IO_B27
bit 1 O 1 IO_B27 0 1 Z
bit 0 C 1 *
