signal CCLK_P15
signal DONE_R14
signal GND1
signal GND2
signal GND3
signal GND4
signal GND5
signal GND6
signal GND7
signal GND8
signal GND9
signal GND10
signal GND11
signal GND12
signal GND13
signal GND14
signal GND15
signal GND16
signal GND17
signal GND18
signal GND19
signal GND20
signal GND21
signal GND22
signal GND23
signal GND24
signal GND25
signal GND26
signal GND27
signal GND28
signal GND29
signal GND30
signal GND31
signal GND32
signal HSWAP_EN_B3
signal M0_T2
signal M1_P2
signal M2_R3
signal PROG_B
signal PWRDWN_B
signal RSVD1
signal RSVD2
signal RSVD3
signal TCK
signal TDI
signal TDO
signal TMS
signal VBATT
signal VCCAUX1
signal VCCAUX2
signal VCCAUX3
signal VCCAUX4
signal VCCINT1
signal VCCINT2
signal VCCINT3
signal VCCINT4
signal VCCINT5
signal VCCINT6
signal VCCINT7
signal VCCINT8
signal VCCO01
signal VCCO02
signal VCCO03
signal VCCO11
signal VCCO12
signal VCCO13
signal VCCO21
signal VCCO22
signal VCCO23
signal VCCO31
signal VCCO32
signal VCCO33
signal VCCO41
signal VCCO42
signal VCCO43
signal VCCO51
signal VCCO52
signal VCCO53
signal VCCO61
signal VCCO62
signal VCCO63
signal VCCO71
signal VCCO72
signal VCCO73
signal IO_A5
signal IO_A6
signal IO_A7
signal IO_A8
signal IO_A9
signal IO_A10
signal IO_A11
signal IO_A12
signal IO_B4
signal IO_B5
signal IO_B6
signal IO_B7
signal IO_B8
signal IO_B9
signal IO_B10
signal IO_B11
signal IO_B12
signal IO_B13
signal IO_C1
signal IO_C4
signal IO_C5
signal IO_C6
signal IO_C7
signal IO_C8
signal IO_C9
signal IO_C10
signal IO_C11
signal IO_C12
signal IO_C13
signal IO_C16
signal IO_D1
signal IO_D2
signal IO_D3
signal IO_D5
signal IO_D6
signal IO_D7
signal IO_D8
signal IO_D9
signal IO_D10
signal IO_D11
signal IO_D12
signal IO_D14
signal IO_D15
signal IO_D16
signal IO_E1
signal IO_E2
signal IO_E3
signal IO_E4
signal IO_E6
signal IO_E7
signal IO_E10
signal IO_E11
signal IO_E13
signal IO_E14
signal IO_E15
signal IO_E16
signal IO_F1
signal IO_F2
signal IO_F3
signal IO_F4
signal IO_F5
signal IO_F12
signal IO_F13
signal IO_F14
signal IO_F15
signal IO_F16
signal IO_G1
signal IO_G2
signal IO_G3
signal IO_G4
signal IO_G5
signal IO_G12
signal IO_G13
signal IO_G14
signal IO_G15
signal IO_G16
signal IO_H1
signal IO_H2
signal IO_H3
signal IO_H4
signal IO_H13
signal IO_H14
signal IO_H15
signal IO_H16
signal IO_J1
signal IO_J2
signal IO_J3
signal IO_J4
signal IO_J13
signal IO_J14
signal IO_J15
signal IO_J16
signal IO_K1
signal IO_K2
signal IO_K3
signal IO_K4
signal IO_K5
signal IO_K12
signal IO_K13
signal IO_K14
signal IO_K15
signal IO_K16
signal IO_L1
signal IO_L2
signal IO_L3
signal IO_L4
signal IO_L5
signal IO_L12
signal IO_L13
signal IO_L14
signal IO_L15
signal IO_L16
signal IO_M1
signal IO_M2
signal IO_M3
signal IO_M4
signal IO_M6
signal IO_M7
signal IO_M10
signal IO_M11
signal IO_M13
signal IO_M14
signal IO_M15
signal IO_M16
signal IO_N1
signal IO_N2
signal IO_N3
signal IO_N5
signal IO_N6
signal IO_N7
signal IO_N8
signal IO_N9
signal IO_N10
signal IO_N11
signal IO_N12
signal IO_N14
signal IO_N15
signal IO_N16
signal IO_P1
signal IO_P4
signal IO_P5
signal IO_P6
signal IO_P7
signal IO_P8
signal IO_P9
signal IO_P10
signal IO_P11
signal IO_P12
signal IO_P13
signal IO_P16
signal IO_R4
signal IO_R5
signal IO_R6
signal IO_R7
signal IO_R8
signal IO_R9
signal IO_R10
signal IO_R11
signal IO_R12
signal IO_R13
signal IO_T3
signal IO_T4
signal IO_T5
signal IO_T6
signal IO_T7
signal IO_T8
signal IO_T9
signal IO_T10
signal IO_T11
signal IO_T12
signal IO_T13

register	BSR	1308
register	BR	1
register	DIR	32

instruction length 6

instruction EXTEST 000000 BSR
instruction SAMPLE/PRELOAD 000001 BSR
instruction IDCODE 001001 DIR
instruction BYPASS 111111 BR

bit 1307 I 1 IO_C16
bit 1306 O 1 IO_C16 1305 1 Z
bit 1305 C 1 *
bit 1304 I 1 IO_D16
bit 1303 O 1 IO_D16 1302 1 Z
bit 1302 C 1 *
bit 1301 I 1 IO_D14
bit 1300 O 1 IO_D14 1299 1 Z
bit 1299 C 1 *
bit 1298 I 1 IO_D15
bit 1297 O 1 IO_D15 1296 1 Z
bit 1296 C 1 *
bit 1295 I 1 IO_E13
bit 1294 O 1 IO_E13 1293 1 Z
bit 1293 C 1 *
bit 1292 I 1 IO_E14
bit 1291 O 1 IO_E14 1290 1 Z
bit 1290 C 1 *
bit 1289 I 1 IO_E15
bit 1288 O 1 IO_E15 1287 1 Z
bit 1287 C 1 *
bit 1286 I 1 IO_E16
bit 1285 O 1 IO_E16 1284 1 Z
bit 1284 C 1 *
bit 1283 O 1 *
bit 1282 O 1 *
bit 1281 O 1 *
bit 1280 O 1 *
bit 1279 O 1 *
bit 1278 O 1 *
bit 1277 I 1 IO_F13
bit 1276 O 1 IO_F13 1275 1 Z
bit 1275 C 1 *
bit 1274 I 1 IO_F14
bit 1273 O 1 IO_F14 1272 1 Z
bit 1272 C 1 *
bit 1271 O 1 *
bit 1270 O 1 *
bit 1269 O 1 *
bit 1268 O 1 *
bit 1267 O 1 *
bit 1266 O 1 *
bit 1265 O 1 *
bit 1264 O 1 *
bit 1263 O 1 *
bit 1262 O 1 *
bit 1261 O 1 *
bit 1260 O 1 *
bit 1259 O 1 *
bit 1258 O 1 *
bit 1257 O 1 *
bit 1256 O 1 *
bit 1255 O 1 *
bit 1254 O 1 *
bit 1253 O 1 *
bit 1252 O 1 *
bit 1251 O 1 *
bit 1250 O 1 *
bit 1249 O 1 *
bit 1248 O 1 *
bit 1247 O 1 *
bit 1246 O 1 *
bit 1245 O 1 *
bit 1244 O 1 *
bit 1243 O 1 *
bit 1242 O 1 *
bit 1241 O 1 *
bit 1240 O 1 *
bit 1239 O 1 *
bit 1238 O 1 *
bit 1237 O 1 *
bit 1236 O 1 *
bit 1235 I 1 IO_F15
bit 1234 O 1 IO_F15 1233 1 Z
bit 1233 C 1 *
bit 1232 I 1 IO_F16
bit 1231 O 1 IO_F16 1230 1 Z
bit 1230 C 1 *
bit 1229 O 1 *
bit 1228 O 1 *
bit 1227 O 1 *
bit 1226 O 1 *
bit 1225 O 1 *
bit 1224 O 1 *
bit 1223 I 1 IO_F12
bit 1222 O 1 IO_F12 1221 1 Z
bit 1221 C 1 *
bit 1220 I 1 IO_G12
bit 1219 O 1 IO_G12 1218 1 Z
bit 1218 C 1 *
bit 1217 O 1 *
bit 1216 O 1 *
bit 1215 O 1 *
bit 1214 O 1 *
bit 1213 O 1 *
bit 1212 O 1 *
bit 1211 O 1 *
bit 1210 O 1 *
bit 1209 O 1 *
bit 1208 O 1 *
bit 1207 O 1 *
bit 1206 O 1 *
bit 1205 O 1 *
bit 1204 O 1 *
bit 1203 O 1 *
bit 1202 O 1 *
bit 1201 O 1 *
bit 1200 O 1 *
bit 1199 O 1 *
bit 1198 O 1 *
bit 1197 O 1 *
bit 1196 O 1 *
bit 1195 O 1 *
bit 1194 O 1 *
bit 1193 O 1 *
bit 1192 O 1 *
bit 1191 O 1 *
bit 1190 O 1 *
bit 1189 O 1 *
bit 1188 O 1 *
bit 1187 O 1 *
bit 1186 O 1 *
bit 1185 O 1 *
bit 1184 O 1 *
bit 1183 O 1 *
bit 1182 O 1 *
bit 1181 O 1 *
bit 1180 O 1 *
bit 1179 O 1 *
bit 1178 O 1 *
bit 1177 O 1 *
bit 1176 O 1 *
bit 1175 O 1 *
bit 1174 O 1 *
bit 1173 O 1 *
bit 1172 O 1 *
bit 1171 O 1 *
bit 1170 O 1 *
bit 1169 O 1 *
bit 1168 O 1 *
bit 1167 O 1 *
bit 1166 O 1 *
bit 1165 O 1 *
bit 1164 O 1 *
bit 1163 I 1 IO_G13
bit 1162 O 1 IO_G13 1161 1 Z
bit 1161 C 1 *
bit 1160 I 1 IO_G14
bit 1159 O 1 IO_G14 1158 1 Z
bit 1158 C 1 *
bit 1157 O 1 *
bit 1156 O 1 *
bit 1155 O 1 *
bit 1154 O 1 *
bit 1153 O 1 *
bit 1152 O 1 *
bit 1151 I 1 IO_G15
bit 1150 O 1 IO_G15 1149 1 Z
bit 1149 C 1 *
bit 1148 I 1 IO_G16
bit 1147 O 1 IO_G16 1146 1 Z
bit 1146 C 1 *
bit 1145 I 1 IO_H13
bit 1144 O 1 IO_H13 1143 1 Z
bit 1143 C 1 *
bit 1142 I 1 IO_H14
bit 1141 O 1 IO_H14 1140 1 Z
bit 1140 C 1 *
bit 1139 O 1 *
bit 1138 O 1 *
bit 1137 O 1 *
bit 1136 O 1 *
bit 1135 O 1 *
bit 1134 O 1 *
bit 1133 I 1 IO_H15
bit 1132 O 1 IO_H15 1131 1 Z
bit 1131 C 1 *
bit 1130 I 1 IO_H16
bit 1129 O 1 IO_H16 1128 1 Z
bit 1128 C 1 *
bit 1127 I 1 IO_J16
bit 1126 O 1 IO_J16 1125 1 Z
bit 1125 C 1 *
bit 1124 I 1 IO_J15
bit 1123 O 1 IO_J15 1122 1 Z
bit 1122 C 1 *
bit 1121 O 1 *
bit 1120 O 1 *
bit 1119 O 1 *
bit 1118 O 1 *
bit 1117 O 1 *
bit 1116 O 1 *
bit 1115 I 1 IO_J14
bit 1114 O 1 IO_J14 1113 1 Z
bit 1113 C 1 *
bit 1112 I 1 IO_J13
bit 1111 O 1 IO_J13 1110 1 Z
bit 1110 C 1 *
bit 1109 I 1 IO_K16
bit 1108 O 1 IO_K16 1107 1 Z
bit 1107 C 1 *
bit 1106 I 1 IO_K15
bit 1105 O 1 IO_K15 1104 1 Z
bit 1104 C 1 *
bit 1103 O 1 *
bit 1102 O 1 *
bit 1101 O 1 *
bit 1100 O 1 *
bit 1099 O 1 *
bit 1098 O 1 *
bit 1097 I 1 IO_K14
bit 1096 O 1 IO_K14 1095 1 Z
bit 1095 C 1 *
bit 1094 I 1 IO_K13
bit 1093 O 1 IO_K13 1092 1 Z
bit 1092 C 1 *
bit 1091 O 1 *
bit 1090 O 1 *
bit 1089 O 1 *
bit 1088 O 1 *
bit 1087 O 1 *
bit 1086 O 1 *
bit 1085 O 1 *
bit 1084 O 1 *
bit 1083 O 1 *
bit 1082 O 1 *
bit 1081 O 1 *
bit 1080 O 1 *
bit 1079 O 1 *
bit 1078 O 1 *
bit 1077 O 1 *
bit 1076 O 1 *
bit 1075 O 1 *
bit 1074 O 1 *
bit 1073 O 1 *
bit 1072 O 1 *
bit 1071 O 1 *
bit 1070 O 1 *
bit 1069 O 1 *
bit 1068 O 1 *
bit 1067 O 1 *
bit 1066 O 1 *
bit 1065 O 1 *
bit 1064 O 1 *
bit 1063 O 1 *
bit 1062 O 1 *
bit 1061 O 1 *
bit 1060 O 1 *
bit 1059 O 1 *
bit 1058 O 1 *
bit 1057 O 1 *
bit 1056 O 1 *
bit 1055 O 1 *
bit 1054 O 1 *
bit 1053 O 1 *
bit 1052 O 1 *
bit 1051 O 1 *
bit 1050 O 1 *
bit 1049 O 1 *
bit 1048 O 1 *
bit 1047 O 1 *
bit 1046 O 1 *
bit 1045 O 1 *
bit 1044 O 1 *
bit 1043 O 1 *
bit 1042 O 1 *
bit 1041 O 1 *
bit 1040 O 1 *
bit 1039 O 1 *
bit 1038 O 1 *
bit 1037 I 1 IO_K12
bit 1036 O 1 IO_K12 1035 1 Z
bit 1035 C 1 *
bit 1034 I 1 IO_L12
bit 1033 O 1 IO_L12 1032 1 Z
bit 1032 C 1 *
bit 1031 O 1 *
bit 1030 O 1 *
bit 1029 O 1 *
bit 1028 O 1 *
bit 1027 O 1 *
bit 1026 O 1 *
bit 1025 I 1 IO_L16
bit 1024 O 1 IO_L16 1023 1 Z
bit 1023 C 1 *
bit 1022 I 1 IO_L15
bit 1021 O 1 IO_L15 1020 1 Z
bit 1020 C 1 *
bit 1019 O 1 *
bit 1018 O 1 *
bit 1017 O 1 *
bit 1016 O 1 *
bit 1015 O 1 *
bit 1014 O 1 *
bit 1013 O 1 *
bit 1012 O 1 *
bit 1011 O 1 *
bit 1010 O 1 *
bit 1009 O 1 *
bit 1008 O 1 *
bit 1007 O 1 *
bit 1006 O 1 *
bit 1005 O 1 *
bit 1004 O 1 *
bit 1003 O 1 *
bit 1002 O 1 *
bit 1001 O 1 *
bit 1000 O 1 *
bit 999 O 1 *
bit 998 O 1 *
bit 997 O 1 *
bit 996 O 1 *
bit 995 O 1 *
bit 994 O 1 *
bit 993 O 1 *
bit 992 O 1 *
bit 991 O 1 *
bit 990 O 1 *
bit 989 O 1 *
bit 988 O 1 *
bit 987 O 1 *
bit 986 O 1 *
bit 985 O 1 *
bit 984 O 1 *
bit 983 I 1 IO_L14
bit 982 O 1 IO_L14 981 1 Z
bit 981 C 1 *
bit 980 I 1 IO_L13
bit 979 O 1 IO_L13 978 1 Z
bit 978 C 1 *
bit 977 O 1 *
bit 976 O 1 *
bit 975 O 1 *
bit 974 O 1 *
bit 973 O 1 *
bit 972 O 1 *
bit 971 I 1 IO_M16
bit 970 O 1 IO_M16 969 1 Z
bit 969 C 1 *
bit 968 I 1 IO_M15
bit 967 O 1 IO_M15 966 1 Z
bit 966 C 1 *
bit 965 I 1 IO_M14
bit 964 O 1 IO_M14 963 1 Z
bit 963 C 1 *
bit 962 I 1 IO_M13
bit 961 O 1 IO_M13 960 1 Z
bit 960 C 1 *
bit 959 I 1 IO_N15
bit 958 O 1 IO_N15 957 1 Z
bit 957 C 1 *
bit 956 I 1 IO_N14
bit 955 O 1 IO_N14 954 1 Z
bit 954 C 1 *
bit 953 I 1 IO_N16
bit 952 O 1 IO_N16 951 1 Z
bit 951 C 1 *
bit 950 I 1 IO_P16
bit 949 O 1 IO_P16 948 1 Z
bit 948 C 1 *
bit 947 I 1 CCLK_P15
bit 946 O 1 CCLK_P15 945 1 Z
bit 945 C 1 *
bit 944 O 1 *
bit 943 I 1 DONE_R14
bit 942 O 1 DONE_R14 941 1 Z
bit 941 C 1 *
bit 940 I 1 IO_T14
bit 939 O 1 IO_T14 938 1 Z
bit 938 C 1 *
bit 937 I 1 IO_T13
bit 936 O 1 IO_T13 935 1 Z
bit 935 C 1 *
bit 934 I 1 IO_P13
bit 933 O 1 IO_P13 932 1 Z
bit 932 C 1 *
bit 931 I 1 IO_R13
bit 930 O 1 IO_R13 929 1 Z
bit 929 C 1 *
bit 928 I 1 IO_N12
bit 927 O 1 IO_N12 926 1 Z
bit 926 C 1 *
bit 925 I 1 IO_P12
bit 924 O 1 IO_P12 923 1 Z
bit 923 C 1 *
bit 922 I 1 IO_R12
bit 921 O 1 IO_R12 920 1 Z
bit 920 C 1 *
bit 919 I 1 IO_T12
bit 918 O 1 IO_T12 917 1 Z
bit 917 C 1 *
bit 916 I 1 IO_N11
bit 915 O 1 IO_N11 914 1 Z
bit 914 C 1 *
bit 913 I 1 IO_P11
bit 912 O 1 IO_P11 911 1 Z
bit 911 C 1 *
bit 910 O 1 *
bit 909 O 1 *
bit 908 O 1 *
bit 907 O 1 *
bit 906 O 1 *
bit 905 O 1 *
bit 904 O 1 *
bit 903 O 1 *
bit 902 O 1 *
bit 901 O 1 *
bit 900 O 1 *
bit 899 O 1 *
bit 898 O 1 *
bit 897 O 1 *
bit 896 O 1 *
bit 895 O 1 *
bit 894 O 1 *
bit 893 O 1 *
bit 892 O 1 *
bit 891 O 1 *
bit 890 O 1 *
bit 889 O 1 *
bit 888 O 1 *
bit 887 O 1 *
bit 886 O 1 *
bit 885 O 1 *
bit 884 O 1 *
bit 883 O 1 *
bit 882 O 1 *
bit 881 O 1 *
bit 880 O 1 *
bit 879 O 1 *
bit 878 O 1 *
bit 877 O 1 *
bit 876 O 1 *
bit 875 O 1 *
bit 874 O 1 *
bit 873 O 1 *
bit 872 O 1 *
bit 871 O 1 *
bit 870 O 1 *
bit 869 O 1 *
bit 868 O 1 *
bit 867 O 1 *
bit 866 O 1 *
bit 865 O 1 *
bit 864 O 1 *
bit 863 O 1 *
bit 862 O 1 *
bit 861 O 1 *
bit 860 O 1 *
bit 859 O 1 *
bit 858 O 1 *
bit 857 O 1 *
bit 856 O 1 *
bit 855 O 1 *
bit 854 O 1 *
bit 853 O 1 *
bit 852 O 1 *
bit 851 O 1 *
bit 850 O 1 *
bit 849 O 1 *
bit 848 O 1 *
bit 847 O 1 *
bit 846 O 1 *
bit 845 O 1 *
bit 844 O 1 *
bit 843 O 1 *
bit 842 O 1 *
bit 841 O 1 *
bit 840 O 1 *
bit 839 O 1 *
bit 838 O 1 *
bit 837 O 1 *
bit 836 O 1 *
bit 835 O 1 *
bit 834 O 1 *
bit 833 O 1 *
bit 832 I 1 IO_R11
bit 831 O 1 IO_R11 830 1 Z
bit 830 C 1 *
bit 829 I 1 IO_T11
bit 828 O 1 IO_T11 827 1 Z
bit 827 C 1 *
bit 826 I 1 IO_M11
bit 825 O 1 IO_M11 824 1 Z
bit 824 C 1 *
bit 823 I 1 IO_M10
bit 822 O 1 IO_M10 821 1 Z
bit 821 C 1 *
bit 820 I 1 IO_N10
bit 819 O 1 IO_N10 818 1 Z
bit 818 C 1 *
bit 817 I 1 IO_P10
bit 816 O 1 IO_P10 815 1 Z
bit 815 C 1 *
bit 814 I 1 IO_R10
bit 813 O 1 IO_R10 812 1 Z
bit 812 C 1 *
bit 811 I 1 IO_T10
bit 810 O 1 IO_T10 809 1 Z
bit 809 C 1 *
bit 808 I 1 IO_N9
bit 807 O 1 IO_N9 806 1 Z
bit 806 C 1 *
bit 805 I 1 IO_P9
bit 804 O 1 IO_P9 803 1 Z
bit 803 C 1 *
bit 802 I 1 IO_R9
bit 801 O 1 IO_R9 800 1 Z
bit 800 C 1 *
bit 799 I 1 IO_T9
bit 798 O 1 IO_T9 797 1 Z
bit 797 C 1 *
bit 796 I 1 IO_T8
bit 795 O 1 IO_T8 794 1 Z
bit 794 C 1 *
bit 793 I 1 IO_R8
bit 792 O 1 IO_R8 791 1 Z
bit 791 C 1 *
bit 790 I 1 IO_P8
bit 789 O 1 IO_P8 788 1 Z
bit 788 C 1 *
bit 787 I 1 IO_N8
bit 786 O 1 IO_N8 785 1 Z
bit 785 C 1 *
bit 784 I 1 IO_T7
bit 783 O 1 IO_T7 782 1 Z
bit 782 C 1 *
bit 781 I 1 IO_R7
bit 780 O 1 IO_R7 779 1 Z
bit 779 C 1 *
bit 778 I 1 IO_P7
bit 777 O 1 IO_P7 776 1 Z
bit 776 C 1 *
bit 775 I 1 IO_N7
bit 774 O 1 IO_N7 773 1 Z
bit 773 C 1 *
bit 772 I 1 IO_M7
bit 771 O 1 IO_M7 770 1 Z
bit 770 C 1 *
bit 769 I 1 IO_M6
bit 768 O 1 IO_M6 767 1 Z
bit 767 C 1 *
bit 766 I 1 IO_T6
bit 765 O 1 IO_T6 764 1 Z
bit 764 C 1 *
bit 763 I 1 IO_R6
bit 762 O 1 IO_R6 761 1 Z
bit 761 C 1 *
bit 760 O 1 *
bit 759 O 1 *
bit 758 O 1 *
bit 757 O 1 *
bit 756 O 1 *
bit 755 O 1 *
bit 754 O 1 *
bit 753 O 1 *
bit 752 O 1 *
bit 751 O 1 *
bit 750 O 1 *
bit 749 O 1 *
bit 748 O 1 *
bit 747 O 1 *
bit 746 O 1 *
bit 745 O 1 *
bit 744 O 1 *
bit 743 O 1 *
bit 742 O 1 *
bit 741 O 1 *
bit 740 O 1 *
bit 739 O 1 *
bit 738 O 1 *
bit 737 O 1 *
bit 736 O 1 *
bit 735 O 1 *
bit 734 O 1 *
bit 733 O 1 *
bit 732 O 1 *
bit 731 O 1 *
bit 730 O 1 *
bit 729 O 1 *
bit 728 O 1 *
bit 727 O 1 *
bit 726 O 1 *
bit 725 O 1 *
bit 724 O 1 *
bit 723 O 1 *
bit 722 O 1 *
bit 721 O 1 *
bit 720 O 1 *
bit 719 O 1 *
bit 718 O 1 *
bit 717 O 1 *
bit 716 O 1 *
bit 715 O 1 *
bit 714 O 1 *
bit 713 O 1 *
bit 712 O 1 *
bit 711 O 1 *
bit 710 O 1 *
bit 709 O 1 *
bit 708 O 1 *
bit 707 O 1 *
bit 706 O 1 *
bit 705 O 1 *
bit 704 O 1 *
bit 703 O 1 *
bit 702 O 1 *
bit 701 O 1 *
bit 700 O 1 *
bit 699 O 1 *
bit 698 O 1 *
bit 697 O 1 *
bit 696 O 1 *
bit 695 O 1 *
bit 694 O 1 *
bit 693 O 1 *
bit 692 O 1 *
bit 691 O 1 *
bit 690 O 1 *
bit 689 O 1 *
bit 688 O 1 *
bit 687 O 1 *
bit 686 O 1 *
bit 685 O 1 *
bit 684 O 1 *
bit 683 O 1 *
bit 682 I 1 IO_P6
bit 681 O 1 IO_P6 680 1 Z
bit 680 C 1 *
bit 679 I 1 IO_N6
bit 678 O 1 IO_N6 677 1 Z
bit 677 C 1 *
bit 676 I 1 IO_T5
bit 675 O 1 IO_T5 674 1 Z
bit 674 C 1 *
bit 673 I 1 IO_R5
bit 672 O 1 IO_R5 671 1 Z
bit 671 C 1 *
bit 670 I 1 IO_P5
bit 669 O 1 IO_P5 668 1 Z
bit 668 C 1 *
bit 667 I 1 IO_N5
bit 666 O 1 IO_N5 665 1 Z
bit 665 C 1 *
bit 664 I 1 IO_R4
bit 663 O 1 IO_R4 662 1 Z
bit 662 C 1 *
bit 661 I 1 IO_P4
bit 660 O 1 IO_P4 659 1 Z
bit 659 C 1 *
bit 658 I 1 IO_T4
bit 657 O 1 IO_T4 656 1 Z
bit 656 C 1 *
bit 655 I 1 IO_T3
bit 654 O 1 IO_T3 653 1 Z
bit 653 C 1 *
bit 652 I 1 M2_R3
bit 651 I 1 M0_T2
bit 650 I 1 M1_P2
bit 649 I 1 IO_P1
bit 648 O 1 IO_P1 647 1 Z
bit 647 C 1 *
bit 646 I 1 IO_N1
bit 645 O 1 IO_N1 644 1 Z
bit 644 C 1 *
bit 643 I 1 IO_N3
bit 642 O 1 IO_N3 641 1 Z
bit 641 C 1 *
bit 640 I 1 IO_N2
bit 639 O 1 IO_N2 638 1 Z
bit 638 C 1 *
bit 637 I 1 IO_M4
bit 636 O 1 IO_M4 635 1 Z
bit 635 C 1 *
bit 634 I 1 IO_M3
bit 633 O 1 IO_M3 632 1 Z
bit 632 C 1 *
bit 631 I 1 IO_M2
bit 630 O 1 IO_M2 629 1 Z
bit 629 C 1 *
bit 628 I 1 IO_M1
bit 627 O 1 IO_M1 626 1 Z
bit 626 C 1 *
bit 625 O 1 *
bit 624 O 1 *
bit 623 O 1 *
bit 622 O 1 *
bit 621 O 1 *
bit 620 O 1 *
bit 619 I 1 IO_L4
bit 618 O 1 IO_L4 617 1 Z
bit 617 C 1 *
bit 616 I 1 IO_L3
bit 615 O 1 IO_L3 614 1 Z
bit 614 C 1 *
bit 613 O 1 *
bit 612 O 1 *
bit 611 O 1 *
bit 610 O 1 *
bit 609 O 1 *
bit 608 O 1 *
bit 607 O 1 *
bit 606 O 1 *
bit 605 O 1 *
bit 604 O 1 *
bit 603 O 1 *
bit 602 O 1 *
bit 601 O 1 *
bit 600 O 1 *
bit 599 O 1 *
bit 598 O 1 *
bit 597 O 1 *
bit 596 O 1 *
bit 595 O 1 *
bit 594 O 1 *
bit 593 O 1 *
bit 592 O 1 *
bit 591 O 1 *
bit 590 O 1 *
bit 589 O 1 *
bit 588 O 1 *
bit 587 O 1 *
bit 586 O 1 *
bit 585 O 1 *
bit 584 O 1 *
bit 583 O 1 *
bit 582 O 1 *
bit 581 O 1 *
bit 580 O 1 *
bit 579 O 1 *
bit 578 O 1 *
bit 577 I 1 IO_L2
bit 576 O 1 IO_L2 575 1 Z
bit 575 C 1 *
bit 574 I 1 IO_L1
bit 573 O 1 IO_L1 572 1 Z
bit 572 C 1 *
bit 571 O 1 *
bit 570 O 1 *
bit 569 O 1 *
bit 568 O 1 *
bit 567 O 1 *
bit 566 O 1 *
bit 565 I 1 IO_L5
bit 564 O 1 IO_L5 563 1 Z
bit 563 C 1 *
bit 562 I 1 IO_K5
bit 561 O 1 IO_K5 560 1 Z
bit 560 C 1 *
bit 559 O 1 *
bit 558 O 1 *
bit 557 O 1 *
bit 556 O 1 *
bit 555 O 1 *
bit 554 O 1 *
bit 553 O 1 *
bit 552 O 1 *
bit 551 O 1 *
bit 550 O 1 *
bit 549 O 1 *
bit 548 O 1 *
bit 547 O 1 *
bit 546 O 1 *
bit 545 O 1 *
bit 544 O 1 *
bit 543 O 1 *
bit 542 O 1 *
bit 541 O 1 *
bit 540 O 1 *
bit 539 O 1 *
bit 538 O 1 *
bit 537 O 1 *
bit 536 O 1 *
bit 535 O 1 *
bit 534 O 1 *
bit 533 O 1 *
bit 532 O 1 *
bit 531 O 1 *
bit 530 O 1 *
bit 529 O 1 *
bit 528 O 1 *
bit 527 O 1 *
bit 526 O 1 *
bit 525 O 1 *
bit 524 O 1 *
bit 523 O 1 *
bit 522 O 1 *
bit 521 O 1 *
bit 520 O 1 *
bit 519 O 1 *
bit 518 O 1 *
bit 517 O 1 *
bit 516 O 1 *
bit 515 O 1 *
bit 514 O 1 *
bit 513 O 1 *
bit 512 O 1 *
bit 511 O 1 *
bit 510 O 1 *
bit 509 O 1 *
bit 508 O 1 *
bit 507 O 1 *
bit 506 O 1 *
bit 505 I 1 IO_K4
bit 504 O 1 IO_K4 503 1 Z
bit 503 C 1 *
bit 502 I 1 IO_K3
bit 501 O 1 IO_K3 500 1 Z
bit 500 C 1 *
bit 499 O 1 *
bit 498 O 1 *
bit 497 O 1 *
bit 496 O 1 *
bit 495 O 1 *
bit 494 O 1 *
bit 493 I 1 IO_K2
bit 492 O 1 IO_K2 491 1 Z
bit 491 C 1 *
bit 490 I 1 IO_K1
bit 489 O 1 IO_K1 488 1 Z
bit 488 C 1 *
bit 487 I 1 IO_J4
bit 486 O 1 IO_J4 485 1 Z
bit 485 C 1 *
bit 484 I 1 IO_J3
bit 483 O 1 IO_J3 482 1 Z
bit 482 C 1 *
bit 481 O 1 *
bit 480 O 1 *
bit 479 O 1 *
bit 478 O 1 *
bit 477 O 1 *
bit 476 O 1 *
bit 475 I 1 IO_J2
bit 474 O 1 IO_J2 473 1 Z
bit 473 C 1 *
bit 472 I 1 IO_J1
bit 471 O 1 IO_J1 470 1 Z
bit 470 C 1 *
bit 469 I 1 IO_H1
bit 468 O 1 IO_H1 467 1 Z
bit 467 C 1 *
bit 466 I 1 IO_H2
bit 465 O 1 IO_H2 464 1 Z
bit 464 C 1 *
bit 463 O 1 *
bit 462 O 1 *
bit 461 O 1 *
bit 460 O 1 *
bit 459 O 1 *
bit 458 O 1 *
bit 457 I 1 IO_H3
bit 456 O 1 IO_H3 455 1 Z
bit 455 C 1 *
bit 454 I 1 IO_H4
bit 453 O 1 IO_H4 452 1 Z
bit 452 C 1 *
bit 451 I 1 IO_G1
bit 450 O 1 IO_G1 449 1 Z
bit 449 C 1 *
bit 448 I 1 IO_G2
bit 447 O 1 IO_G2 446 1 Z
bit 446 C 1 *
bit 445 O 1 *
bit 444 O 1 *
bit 443 O 1 *
bit 442 O 1 *
bit 441 O 1 *
bit 440 O 1 *
bit 439 I 1 IO_G3
bit 438 O 1 IO_G3 437 1 Z
bit 437 C 1 *
bit 436 I 1 IO_G4
bit 435 O 1 IO_G4 434 1 Z
bit 434 C 1 *
bit 433 O 1 *
bit 432 O 1 *
bit 431 O 1 *
bit 430 O 1 *
bit 429 O 1 *
bit 428 O 1 *
bit 427 O 1 *
bit 426 O 1 *
bit 425 O 1 *
bit 424 O 1 *
bit 423 O 1 *
bit 422 O 1 *
bit 421 O 1 *
bit 420 O 1 *
bit 419 O 1 *
bit 418 O 1 *
bit 417 O 1 *
bit 416 O 1 *
bit 415 O 1 *
bit 414 O 1 *
bit 413 O 1 *
bit 412 O 1 *
bit 411 O 1 *
bit 410 O 1 *
bit 409 O 1 *
bit 408 O 1 *
bit 407 O 1 *
bit 406 O 1 *
bit 405 O 1 *
bit 404 O 1 *
bit 403 O 1 *
bit 402 O 1 *
bit 401 O 1 *
bit 400 O 1 *
bit 399 O 1 *
bit 398 O 1 *
bit 397 O 1 *
bit 396 O 1 *
bit 395 O 1 *
bit 394 O 1 *
bit 393 O 1 *
bit 392 O 1 *
bit 391 O 1 *
bit 390 O 1 *
bit 389 O 1 *
bit 388 O 1 *
bit 387 O 1 *
bit 386 O 1 *
bit 385 O 1 *
bit 384 O 1 *
bit 383 O 1 *
bit 382 O 1 *
bit 381 O 1 *
bit 380 O 1 *
bit 379 I 1 IO_G5
bit 378 O 1 IO_G5 377 1 Z
bit 377 C 1 *
bit 376 I 1 IO_F5
bit 375 O 1 IO_F5 374 1 Z
bit 374 C 1 *
bit 373 O 1 *
bit 372 O 1 *
bit 371 O 1 *
bit 370 O 1 *
bit 369 O 1 *
bit 368 O 1 *
bit 367 I 1 IO_F1
bit 366 O 1 IO_F1 365 1 Z
bit 365 C 1 *
bit 364 I 1 IO_F2
bit 363 O 1 IO_F2 362 1 Z
bit 362 C 1 *
bit 361 O 1 *
bit 360 O 1 *
bit 359 O 1 *
bit 358 O 1 *
bit 357 O 1 *
bit 356 O 1 *
bit 355 O 1 *
bit 354 O 1 *
bit 353 O 1 *
bit 352 O 1 *
bit 351 O 1 *
bit 350 O 1 *
bit 349 O 1 *
bit 348 O 1 *
bit 347 O 1 *
bit 346 O 1 *
bit 345 O 1 *
bit 344 O 1 *
bit 343 O 1 *
bit 342 O 1 *
bit 341 O 1 *
bit 340 O 1 *
bit 339 O 1 *
bit 338 O 1 *
bit 337 O 1 *
bit 336 O 1 *
bit 335 O 1 *
bit 334 O 1 *
bit 333 O 1 *
bit 332 O 1 *
bit 331 O 1 *
bit 330 O 1 *
bit 329 O 1 *
bit 328 O 1 *
bit 327 O 1 *
bit 326 O 1 *
bit 325 I 1 IO_F3
bit 324 O 1 IO_F3 323 1 Z
bit 323 C 1 *
bit 322 I 1 IO_F4
bit 321 O 1 IO_F4 320 1 Z
bit 320 C 1 *
bit 319 O 1 *
bit 318 O 1 *
bit 317 O 1 *
bit 316 O 1 *
bit 315 O 1 *
bit 314 O 1 *
bit 313 I 1 IO_E1
bit 312 O 1 IO_E1 311 1 Z
bit 311 C 1 *
bit 310 I 1 IO_E2
bit 309 O 1 IO_E2 308 1 Z
bit 308 C 1 *
bit 307 I 1 IO_E3
bit 306 O 1 IO_E3 305 1 Z
bit 305 C 1 *
bit 304 I 1 IO_E4
bit 303 O 1 IO_E4 302 1 Z
bit 302 C 1 *
bit 301 I 1 IO_D2
bit 300 O 1 IO_D2 299 1 Z
bit 299 C 1 *
bit 298 I 1 IO_D3
bit 297 O 1 IO_D3 296 1 Z
bit 296 C 1 *
bit 295 I 1 IO_D1
bit 294 O 1 IO_D1 293 1 Z
bit 293 C 1 *
bit 292 I 1 IO_C1
bit 291 O 1 IO_C1 290 1 Z
bit 290 C 1 *
bit 289 O 1 *
bit 288 I 1 HSWAP_EN_B3
bit 287 I 1 IO_C4
bit 286 O 1 IO_C4 285 1 Z
bit 285 C 1 *
bit 284 I 1 IO_B4
bit 283 O 1 IO_B4 282 1 Z
bit 282 C 1 *
bit 281 I 1 IO_D5
bit 280 O 1 IO_D5 279 1 Z
bit 279 C 1 *
bit 278 I 1 IO_C5
bit 277 O 1 IO_C5 276 1 Z
bit 276 C 1 *
bit 275 I 1 IO_B5
bit 274 O 1 IO_B5 273 1 Z
bit 273 C 1 *
bit 272 I 1 IO_A5
bit 271 O 1 IO_A5 270 1 Z
bit 270 C 1 *
bit 269 I 1 IO_D6
bit 268 O 1 IO_D6 267 1 Z
bit 267 C 1 *
bit 266 I 1 IO_C6
bit 265 O 1 IO_C6 264 1 Z
bit 264 C 1 *
bit 263 I 1 IO_B6
bit 262 O 1 IO_B6 261 1 Z
bit 261 C 1 *
bit 260 I 1 IO_A6
bit 259 O 1 IO_A6 258 1 Z
bit 258 C 1 *
bit 257 O 1 *
bit 256 O 1 *
bit 255 O 1 *
bit 254 O 1 *
bit 253 O 1 *
bit 252 O 1 *
bit 251 O 1 *
bit 250 O 1 *
bit 249 O 1 *
bit 248 O 1 *
bit 247 O 1 *
bit 246 O 1 *
bit 245 O 1 *
bit 244 O 1 *
bit 243 O 1 *
bit 242 O 1 *
bit 241 O 1 *
bit 240 O 1 *
bit 239 O 1 *
bit 238 O 1 *
bit 237 O 1 *
bit 236 O 1 *
bit 235 O 1 *
bit 234 O 1 *
bit 233 O 1 *
bit 232 O 1 *
bit 231 O 1 *
bit 230 O 1 *
bit 229 O 1 *
bit 228 O 1 *
bit 227 O 1 *
bit 226 O 1 *
bit 225 O 1 *
bit 224 O 1 *
bit 223 O 1 *
bit 222 O 1 *
bit 221 O 1 *
bit 220 O 1 *
bit 219 O 1 *
bit 218 O 1 *
bit 217 O 1 *
bit 216 O 1 *
bit 215 O 1 *
bit 214 O 1 *
bit 213 O 1 *
bit 212 O 1 *
bit 211 O 1 *
bit 210 O 1 *
bit 209 O 1 *
bit 208 O 1 *
bit 207 O 1 *
bit 206 O 1 *
bit 205 O 1 *
bit 204 O 1 *
bit 203 O 1 *
bit 202 O 1 *
bit 201 O 1 *
bit 200 O 1 *
bit 199 O 1 *
bit 198 O 1 *
bit 197 O 1 *
bit 196 O 1 *
bit 195 O 1 *
bit 194 O 1 *
bit 193 O 1 *
bit 192 O 1 *
bit 191 O 1 *
bit 190 O 1 *
bit 189 O 1 *
bit 188 O 1 *
bit 187 O 1 *
bit 186 O 1 *
bit 185 O 1 *
bit 184 O 1 *
bit 183 O 1 *
bit 182 O 1 *
bit 181 O 1 *
bit 180 O 1 *
bit 179 O 1 *
bit 178 O 1 *
bit 177 O 1 *
bit 176 O 1 *
bit 175 O 1 *
bit 174 O 1 *
bit 173 I 1 IO_E6
bit 172 O 1 IO_E6 171 1 Z
bit 171 C 1 *
bit 170 I 1 IO_E7
bit 169 O 1 IO_E7 168 1 Z
bit 168 C 1 *
bit 167 I 1 IO_D7
bit 166 O 1 IO_D7 165 1 Z
bit 165 C 1 *
bit 164 I 1 IO_C7
bit 163 O 1 IO_C7 162 1 Z
bit 162 C 1 *
bit 161 I 1 IO_B7
bit 160 O 1 IO_B7 159 1 Z
bit 159 C 1 *
bit 158 I 1 IO_A7
bit 157 O 1 IO_A7 156 1 Z
bit 156 C 1 *
bit 155 I 1 IO_D8
bit 154 O 1 IO_D8 153 1 Z
bit 153 C 1 *
bit 152 I 1 IO_C8
bit 151 O 1 IO_C8 150 1 Z
bit 150 C 1 *
bit 149 I 1 IO_B8
bit 148 O 1 IO_B8 147 1 Z
bit 147 C 1 *
bit 146 I 1 IO_A8
bit 145 O 1 IO_A8 144 1 Z
bit 144 C 1 *
bit 143 I 1 IO_A9
bit 142 O 1 IO_A9 141 1 Z
bit 141 C 1 *
bit 140 I 1 IO_B9
bit 139 O 1 IO_B9 138 1 Z
bit 138 C 1 *
bit 137 I 1 IO_C9
bit 136 O 1 IO_C9 135 1 Z
bit 135 C 1 *
bit 134 I 1 IO_D9
bit 133 O 1 IO_D9 132 1 Z
bit 132 C 1 *
bit 131 I 1 IO_A10
bit 130 O 1 IO_A10 129 1 Z
bit 129 C 1 *
bit 128 I 1 IO_B10
bit 127 O 1 IO_B10 126 1 Z
bit 126 C 1 *
bit 125 I 1 IO_C10
bit 124 O 1 IO_C10 123 1 Z
bit 123 C 1 *
bit 122 I 1 IO_D10
bit 121 O 1 IO_D10 120 1 Z
bit 120 C 1 *
bit 119 I 1 IO_E10
bit 118 O 1 IO_E10 117 1 Z
bit 117 C 1 *
bit 116 I 1 IO_E11
bit 115 O 1 IO_E11 114 1 Z
bit 114 C 1 *
bit 113 O 1 *
bit 112 O 1 *
bit 111 O 1 *
bit 110 O 1 *
bit 109 O 1 *
bit 108 O 1 *
bit 107 O 1 *
bit 106 O 1 *
bit 105 O 1 *
bit 104 O 1 *
bit 103 O 1 *
bit 102 O 1 *
bit 101 O 1 *
bit 100 O 1 *
bit 99 O 1 *
bit 98 O 1 *
bit 97 O 1 *
bit 96 O 1 *
bit 95 O 1 *
bit 94 O 1 *
bit 93 O 1 *
bit 92 O 1 *
bit 91 O 1 *
bit 90 O 1 *
bit 89 O 1 *
bit 88 O 1 *
bit 87 O 1 *
bit 86 O 1 *
bit 85 O 1 *
bit 84 O 1 *
bit 83 O 1 *
bit 82 O 1 *
bit 81 O 1 *
bit 80 O 1 *
bit 79 O 1 *
bit 78 O 1 *
bit 77 O 1 *
bit 76 O 1 *
bit 75 O 1 *
bit 74 O 1 *
bit 73 O 1 *
bit 72 O 1 *
bit 71 O 1 *
bit 70 O 1 *
bit 69 O 1 *
bit 68 O 1 *
bit 67 O 1 *
bit 66 O 1 *
bit 65 O 1 *
bit 64 O 1 *
bit 63 O 1 *
bit 62 O 1 *
bit 61 O 1 *
bit 60 O 1 *
bit 59 O 1 *
bit 58 O 1 *
bit 57 O 1 *
bit 56 O 1 *
bit 55 O 1 *
bit 54 O 1 *
bit 53 O 1 *
bit 52 O 1 *
bit 51 O 1 *
bit 50 O 1 *
bit 49 O 1 *
bit 48 O 1 *
bit 47 O 1 *
bit 46 O 1 *
bit 45 O 1 *
bit 44 O 1 *
bit 43 O 1 *
bit 42 O 1 *
bit 41 O 1 *
bit 40 O 1 *
bit 39 O 1 *
bit 38 O 1 *
bit 37 O 1 *
bit 36 O 1 *
bit 35 O 1 *
bit 34 O 1 *
bit 33 O 1 *
bit 32 O 1 *
bit 31 O 1 *
bit 30 O 1 *
bit 29 I 1 IO_A11
bit 28 O 1 IO_A11 27 1 Z
bit 27 C 1 *
bit 26 I 1 IO_B11
bit 25 O 1 IO_B11 24 1 Z
bit 24 C 1 *
bit 23 I 1 IO_C11
bit 22 O 1 IO_C11 21 1 Z
bit 21 C 1 *
bit 20 I 1 IO_D11
bit 19 O 1 IO_D11 18 1 Z
bit 18 C 1 *
bit 17 I 1 IO_A12
bit 16 O 1 IO_A12 15 1 Z
bit 15 C 1 *
bit 14 I 1 IO_B12
bit 13 O 1 IO_B12 12 1 Z
bit 12 C 1 *
bit 11 I 1 IO_C12
bit 10 O 1 IO_C12 9 1 Z
bit 9 C 1 *
bit 8 I 1 IO_D12
bit 7 O 1 IO_D12 6 1 Z
bit 6 C 1 *
bit 5 I 1 IO_B13
bit 4 O 1 IO_B13 3 1 Z
bit 3 C 1 *
bit 2 I 1 IO_C13
bit 1 O 1 IO_C13 0 1 Z
bit 0 C 1 *
