signal tdi
signal tck
signal tms
signal tdo
signal IO_0
signal IO_1
signal IO_2
signal IO_8
signal IO_9
signal IO_10
signal IO_11
signal IO_12
signal IO_16
signal IO_17
signal IO_20
signal IO_21
signal IO_22
signal IO_23
signal IO_25
signal IO_27
signal IO_28
signal IO_32
signal IO_33
signal IO_34
signal IO_37
signal IO_41
signal IO_42
signal IO_43
signal IO_45
signal IO_46
signal IO_48
signal IO_49
signal IO_54
signal IO_58
signal IO_60
signal IO_61
signal vdd1
signal vdd2
signal vdd3
signal gnd1
signal gnd2
signal gnd3

register	BSR	192
register	BR	1
register	DIR	32

instruction length 8

instruction BYPASS 11111111 BR
instruction SAMPLE/PRELOAD 00000011 BSR
instruction EXTEST 00000000 BSR
instruction IDCODE 00000001 DIR

bit 191 I 1 IO_0
bit 190 O 1 IO_0 189 0 Z
bit 189 C 0 *
bit 188 I 1 IO_1
bit 187 O 1 IO_1 186 0 Z
bit 186 C 0 *
bit 185 I 1 IO_2
bit 184 O 1 IO_2 183 0 Z
bit 183 C 0 *
bit 182 O 1 *
bit 181 O 1 *
bit 180 O 1 *
bit 179 O 1 *
bit 178 O 1 *
bit 177 O 1 *
bit 176 O 1 *
bit 175 O 1 *
bit 174 O 1 *
bit 173 O 1 *
bit 172 O 1 *
bit 171 O 1 *
bit 170 O 1 *
bit 169 O 1 *
bit 168 O 1 *
bit 167 I 1 IO_8
bit 166 O 1 IO_8 165 0 Z
bit 165 C 0 *
bit 164 I 1 IO_9
bit 163 O 1 IO_9 162 0 Z
bit 162 C 0 *
bit 161 I 1 IO_10
bit 160 O 1 IO_10 159 0 Z
bit 159 C 0 *
bit 158 I 1 IO_11
bit 157 O 1 IO_11 156 0 Z
bit 156 C 0 *
bit 155 I 1 IO_12
bit 154 O 1 IO_12 153 0 Z
bit 153 C 0 *
bit 152 O 1 *
bit 151 O 1 *
bit 150 O 1 *
bit 149 O 1 *
bit 148 O 1 *
bit 147 O 1 *
bit 146 O 1 *
bit 145 O 1 *
bit 144 O 1 *
bit 143 I 1 IO_32
bit 142 O 1 IO_32 141 0 Z
bit 141 C 0 *
bit 140 I 1 IO_33
bit 139 O 1 IO_33 138 0 Z
bit 138 C 0 *
bit 137 I 1 IO_34
bit 136 O 1 IO_34 135 0 Z
bit 135 C 0 *
bit 134 O 1 *
bit 133 O 1 *
bit 132 O 1 *
bit 131 O 1 *
bit 130 O 1 *
bit 129 O 1 *
bit 128 I 1 IO_37
bit 127 O 1 IO_37 126 0 Z
bit 126 C 0 *
bit 125 O 1 *
bit 124 O 1 *
bit 123 O 1 *
bit 122 O 1 *
bit 121 O 1 *
bit 120 O 1 *
bit 119 O 1 *
bit 118 O 1 *
bit 117 O 1 *
bit 116 I 1 IO_41
bit 115 O 1 IO_41 114 0 Z
bit 114 C 0 *
bit 113 I 1 IO_42
bit 112 O 1 IO_42 111 0 Z
bit 111 C 0 *
bit 110 I 1 IO_43
bit 109 O 1 IO_43 108 0 Z
bit 108 C 0 *
bit 107 O 1 *
bit 106 O 1 *
bit 105 O 1 *
bit 104 I 1 IO_45
bit 103 O 1 IO_45 102 0 Z
bit 102 C 0 *
bit 101 I 1 IO_46
bit 100 O 1 IO_46 99 0 Z
bit 99 C 0 *
bit 98 O 1 *
bit 97 O 1 *
bit 96 O 1 *
bit 95 I 1 IO_16
bit 94 O 1 IO_16 93 0 Z
bit 93 C 0 *
bit 92 I 1 IO_17
bit 91 O 1 IO_17 90 0 Z
bit 90 C 0 *
bit 89 O 1 *
bit 88 O 1 *
bit 87 O 1 *
bit 86 O 1 *
bit 85 O 1 *
bit 84 O 1 *
bit 83 I 1 IO_20
bit 82 O 1 IO_20 81 0 Z
bit 81 C 0 *
bit 80 I 1 IO_21
bit 79 O 1 IO_21 78 0 Z
bit 78 C 0 *
bit 77 I 1 IO_22
bit 76 O 1 IO_22 75 0 Z
bit 75 C 0 *
bit 74 I 1 IO_23
bit 73 O 1 IO_23 72 0 Z
bit 72 C 0 *
bit 71 O 1 *
bit 70 O 1 *
bit 69 O 1 *
bit 68 I 1 IO_25
bit 67 O 1 IO_25 66 0 Z
bit 66 C 0 *
bit 65 O 1 *
bit 64 O 1 *
bit 63 O 1 *
bit 62 I 1 IO_27
bit 61 O 1 IO_27 60 0 Z
bit 60 C 0 *
bit 59 I 1 IO_28
bit 58 O 1 IO_28 57 0 Z
bit 57 C 0 *
bit 56 O 1 *
bit 55 O 1 *
bit 54 O 1 *
bit 53 O 1 *
bit 52 O 1 *
bit 51 O 1 *
bit 50 O 1 *
bit 49 O 1 *
bit 48 O 1 *
bit 47 I 1 IO_48
bit 46 O 1 IO_48 45 0 Z
bit 45 C 0 *
bit 44 I 1 IO_49
bit 43 O 1 IO_49 42 0 Z
bit 42 C 0 *
bit 41 O 1 *
bit 40 O 1 *
bit 39 O 1 *
bit 38 O 1 *
bit 37 O 1 *
bit 36 O 1 *
bit 35 O 1 *
bit 34 O 1 *
bit 33 O 1 *
bit 32 O 1 *
bit 31 O 1 *
bit 30 O 1 *
bit 29 I 1 IO_54
bit 28 O 1 IO_54 27 0 Z
bit 27 C 0 *
bit 26 O 1 *
bit 25 O 1 *
bit 24 O 1 *
bit 23 O 1 *
bit 22 O 1 *
bit 21 O 1 *
bit 20 O 1 *
bit 19 O 1 *
bit 18 O 1 *
bit 17 I 1 IO_58
bit 16 O 1 IO_58 15 0 Z
bit 15 C 0 *
bit 14 O 1 *
bit 13 O 1 *
bit 12 O 1 *
bit 11 I 1 IO_60
bit 10 O 1 IO_60 9 0 Z
bit 9 C 0 *
bit 8 I 1 IO_61
bit 7 O 1 IO_61 6 0 Z
bit 6 C 0 *
bit 5 I 1 IO_62
bit 4 O 1 IO_62 3 0 Z
bit 3 C 0 *
bit 2 O 1 *
bit 1 O 1 *
bit 0 O 1 *
