signal CCLK_P155
signal DONE_P104
signal GCK0_P80
signal GCK1_P77
signal GCK2_P182
signal GCK3_P185
signal GND1
signal GND2
signal GND3
signal GND4
signal GND5
signal GND6
signal GND7
signal GND8
signal GND9
signal GND10
signal GND11
signal GND12
signal GND13
signal GND14
signal GND15
signal GND16
signal GND17
signal GND18
signal GND19
signal GND20
signal GND21
signal GND22
signal GND23
signal GND24
signal INIT_P107
signal M0_P52
signal M1_P50
signal M2_P54
signal PROGRAM
signal TCK
signal TDI
signal TDO
signal TMS
signal VCCINT1
signal VCCINT2
signal VCCINT3
signal VCCINT4
signal VCCINT5
signal VCCINT6
signal VCCINT7
signal VCCINT8
signal VCCINT9
signal VCCINT10
signal VCCINT11
signal VCCINT12
signal VCCO1
signal VCCO2
signal VCCO3
signal VCCO4
signal VCCO5
signal VCCO6
signal VCCO7
signal VCCO8
signal VCCO9
signal VCCO10
signal VCCO11
signal VCCO12
signal VCCO13
signal VCCO14
signal VCCO15
signal VCCO16
signal IO_P3
signal IO_P4
signal IO_P5
signal IO_P6
signal IO_P7
signal IO_P8
signal IO_P9
signal IO_P10
signal IO_P11
signal IO_P15
signal IO_P16
signal IO_P17
signal IO_P18
signal IO_P20
signal IO_P21
signal IO_P22
signal IO_P23
signal IO_P24
signal IO_P27
signal IO_P29
signal IO_P30
signal IO_P31
signal IO_P33
signal IO_P34
signal IO_P35
signal IO_P36
signal IO_P40
signal IO_P41
signal IO_P42
signal IO_P43
signal IO_P44
signal IO_P45
signal IO_P46
signal IO_P47
signal IO_P48
signal IO_P49
signal IO_P55
signal IO_P56
signal IO_P57
signal IO_P58
signal IO_P59
signal IO_P60
signal IO_P61
signal IO_P62
signal IO_P63
signal IO_P64
signal IO_P68
signal IO_P69
signal IO_P70
signal IO_P71
signal IO_P73
signal IO_P74
signal IO_P75
signal IO_P81
signal IO_P82
signal IO_P83
signal IO_P84
signal IO_P86
signal IO_P87
signal IO_P88
signal IO_P89
signal IO_P93
signal IO_P94
signal IO_P95
signal IO_P96
signal IO_P97
signal IO_P98
signal IO_P99
signal IO_P100
signal IO_P101
signal IO_P102
signal IO_P108
signal IO_P109
signal IO_P110
signal IO_P111
signal IO_P112
signal IO_P113
signal IO_P114
signal IO_P115
signal IO_P116
signal IO_P120
signal IO_P121
signal IO_P122
signal IO_P123
signal IO_P125
signal IO_P126
signal IO_P127
signal IO_P129
signal IO_P132
signal IO_P133
signal IO_P134
signal IO_P135
signal IO_P136
signal IO_P138
signal IO_P139
signal IO_P140
signal IO_P141
signal IO_P145
signal IO_P146
signal IO_P147
signal IO_P148
signal IO_P149
signal IO_P150
signal IO_P151
signal IO_P152
signal IO_P153
signal IO_P154
signal IO_P160
signal IO_P161
signal IO_P162
signal IO_P163
signal IO_P164
signal IO_P165
signal IO_P166
signal IO_P167
signal IO_P168
signal IO_P169
signal IO_P173
signal IO_P174
signal IO_P175
signal IO_P176
signal IO_P178
signal IO_P179
signal IO_P180
signal IO_P181
signal IO_P187
signal IO_P188
signal IO_P189
signal IO_P191
signal IO_P192
signal IO_P193
signal IO_P194
signal IO_P198
signal IO_P199
signal IO_P200
signal IO_P201
signal IO_P202
signal IO_P203
signal IO_P204
signal IO_P205

register	BSR	1022
register	BR	1
register	DIR	32

instruction length 5

instruction SAMPLE/PRELOAD 00001 BSR
instruction IDCODE 01001 DIR
instruction EXTEST 00000 BSR
instruction BYPASS 11111 BR

bit 1021 I 1 CCLK_P155
bit 1020 O 1 CCLK_P155 1019 1 Z
bit 1019 C 1 *
bit 1018 I 1 IO_P154
bit 1017 O 1 IO_P154 1016 1 Z
bit 1016 C 1 *
bit 1015 I 1 IO_P153
bit 1014 O 1 IO_P153 1013 1 Z
bit 1013 C 1 *
bit 1012 O 1 *
bit 1011 O 1 *
bit 1010 O 1 *
bit 1009 O 1 *
bit 1008 O 1 *
bit 1007 O 1 *
bit 1006 O 1 *
bit 1005 O 1 *
bit 1004 O 1 *
bit 1003 O 1 *
bit 1002 O 1 *
bit 1001 O 1 *
bit 1000 I 1 IO_P152
bit 999 O 1 IO_P152 998 1 Z
bit 998 C 1 *
bit 997 O 1 *
bit 996 O 1 *
bit 995 O 1 *
bit 994 O 1 *
bit 993 O 1 *
bit 992 O 1 *
bit 991 O 1 *
bit 990 O 1 *
bit 989 O 1 *
bit 988 O 1 *
bit 987 O 1 *
bit 986 O 1 *
bit 985 I 1 IO_P151
bit 984 O 1 IO_P151 983 1 Z
bit 983 C 1 *
bit 982 I 1 IO_P150
bit 981 O 1 IO_P150 980 1 Z
bit 980 C 1 *
bit 979 I 1 IO_P149
bit 978 O 1 IO_P149 977 1 Z
bit 977 C 1 *
bit 976 O 1 *
bit 975 O 1 *
bit 974 O 1 *
bit 973 O 1 *
bit 972 O 1 *
bit 971 O 1 *
bit 970 O 1 *
bit 969 O 1 *
bit 968 O 1 *
bit 967 I 1 IO_P148
bit 966 O 1 IO_P148 965 1 Z
bit 965 C 1 *
bit 964 I 1 IO_P147
bit 963 O 1 IO_P147 962 1 Z
bit 962 C 1 *
bit 961 O 1 *
bit 960 O 1 *
bit 959 O 1 *
bit 958 I 1 IO_P146
bit 957 O 1 IO_P146 956 1 Z
bit 956 C 1 *
bit 955 I 1 IO_P145
bit 954 O 1 IO_P145 953 1 Z
bit 953 C 1 *
bit 952 I 1 IO_P141
bit 951 O 1 IO_P141 950 1 Z
bit 950 C 1 *
bit 949 I 1 IO_P140
bit 948 O 1 IO_P140 947 1 Z
bit 947 C 1 *
bit 946 O 1 *
bit 945 O 1 *
bit 944 O 1 *
bit 943 O 1 *
bit 942 O 1 *
bit 941 O 1 *
bit 940 O 1 *
bit 939 O 1 *
bit 938 O 1 *
bit 937 O 1 *
bit 936 O 1 *
bit 935 O 1 *
bit 934 O 1 *
bit 933 O 1 *
bit 932 O 1 *
bit 931 O 1 *
bit 930 O 1 *
bit 929 O 1 *
bit 928 I 1 IO_P139
bit 927 O 1 IO_P139 926 1 Z
bit 926 C 1 *
bit 925 I 1 IO_P138
bit 924 O 1 IO_P138 923 1 Z
bit 923 C 1 *
bit 922 I 1 IO_P136
bit 921 O 1 IO_P136 920 1 Z
bit 920 C 1 *
bit 919 I 1 IO_P135
bit 918 O 1 IO_P135 917 1 Z
bit 917 C 1 *
bit 916 O 1 *
bit 915 O 1 *
bit 914 O 1 *
bit 913 O 1 *
bit 912 O 1 *
bit 911 O 1 *
bit 910 O 1 *
bit 909 O 1 *
bit 908 O 1 *
bit 907 I 1 IO_P134
bit 906 O 1 IO_P134 905 1 Z
bit 905 C 1 *
bit 904 O 1 *
bit 903 O 1 *
bit 902 O 1 *
bit 901 O 1 *
bit 900 O 1 *
bit 899 O 1 *
bit 898 I 1 IO_P133
bit 897 O 1 IO_P133 896 1 Z
bit 896 C 1 *
bit 895 I 1 IO_P132
bit 894 O 1 IO_P132 893 1 Z
bit 893 C 1 *
bit 892 I 1 IO_P129
bit 891 O 1 IO_P129 890 1 Z
bit 890 C 1 *
bit 889 O 1 *
bit 888 O 1 *
bit 887 O 1 *
bit 886 O 1 *
bit 885 O 1 *
bit 884 O 1 *
bit 883 O 1 *
bit 882 O 1 *
bit 881 O 1 *
bit 880 I 1 IO_P127
bit 879 O 1 IO_P127 878 1 Z
bit 878 C 1 *
bit 877 O 1 *
bit 876 O 1 *
bit 875 O 1 *
bit 874 O 1 *
bit 873 O 1 *
bit 872 O 1 *
bit 871 O 1 *
bit 870 O 1 *
bit 869 O 1 *
bit 868 I 1 IO_P126
bit 867 O 1 IO_P126 866 1 Z
bit 866 C 1 *
bit 865 I 1 IO_P125
bit 864 O 1 IO_P125 863 1 Z
bit 863 C 1 *
bit 862 I 1 IO_P123
bit 861 O 1 IO_P123 860 1 Z
bit 860 C 1 *
bit 859 I 1 IO_P122
bit 858 O 1 IO_P122 857 1 Z
bit 857 C 1 *
bit 856 O 1 *
bit 855 O 1 *
bit 854 O 1 *
bit 853 O 1 *
bit 852 O 1 *
bit 851 O 1 *
bit 850 O 1 *
bit 849 O 1 *
bit 848 O 1 *
bit 847 O 1 *
bit 846 O 1 *
bit 845 O 1 *
bit 844 O 1 *
bit 843 O 1 *
bit 842 O 1 *
bit 841 O 1 *
bit 840 O 1 *
bit 839 O 1 *
bit 838 I 1 IO_P121
bit 837 O 1 IO_P121 836 1 Z
bit 836 C 1 *
bit 835 I 1 IO_P120
bit 834 O 1 IO_P120 833 1 Z
bit 833 C 1 *
bit 832 I 1 IO_P116
bit 831 O 1 IO_P116 830 1 Z
bit 830 C 1 *
bit 829 I 1 IO_P115
bit 828 O 1 IO_P115 827 1 Z
bit 827 C 1 *
bit 826 O 1 *
bit 825 O 1 *
bit 824 O 1 *
bit 823 I 1 IO_P114
bit 822 O 1 IO_P114 821 1 Z
bit 821 C 1 *
bit 820 I 1 IO_P113
bit 819 O 1 IO_P113 818 1 Z
bit 818 C 1 *
bit 817 O 1 *
bit 816 O 1 *
bit 815 O 1 *
bit 814 O 1 *
bit 813 O 1 *
bit 812 O 1 *
bit 811 O 1 *
bit 810 O 1 *
bit 809 O 1 *
bit 808 I 1 IO_P112
bit 807 O 1 IO_P112 806 1 Z
bit 806 C 1 *
bit 805 I 1 IO_P111
bit 804 O 1 IO_P111 803 1 Z
bit 803 C 1 *
bit 802 I 1 IO_P110
bit 801 O 1 IO_P110 800 1 Z
bit 800 C 1 *
bit 799 O 1 *
bit 798 O 1 *
bit 797 O 1 *
bit 796 O 1 *
bit 795 O 1 *
bit 794 O 1 *
bit 793 O 1 *
bit 792 O 1 *
bit 791 O 1 *
bit 790 O 1 *
bit 789 O 1 *
bit 788 O 1 *
bit 787 I 1 IO_P109
bit 786 O 1 IO_P109 785 1 Z
bit 785 C 1 *
bit 784 O 1 *
bit 783 O 1 *
bit 782 O 1 *
bit 781 O 1 *
bit 780 O 1 *
bit 779 O 1 *
bit 778 O 1 *
bit 777 O 1 *
bit 776 O 1 *
bit 775 O 1 *
bit 774 O 1 *
bit 773 O 1 *
bit 772 I 1 IO_P108
bit 771 O 1 IO_P108 770 1 Z
bit 770 C 1 *
bit 769 I 1 INIT_P107
bit 768 O 1 INIT_P107 767 1 Z
bit 767 C 1 *
bit 766 O 1 *
bit 765 I 1 DONE_P104
bit 764 O 1 DONE_P104 763 1 Z
bit 763 C 1 *
bit 762 I 1 IO_P102
bit 761 O 1 IO_P102 760 1 Z
bit 760 C 1 *
bit 759 I 1 IO_P101
bit 758 O 1 IO_P101 757 1 Z
bit 757 C 1 *
bit 756 O 1 *
bit 755 O 1 *
bit 754 O 1 *
bit 753 O 1 *
bit 752 O 1 *
bit 751 O 1 *
bit 750 O 1 *
bit 749 O 1 *
bit 748 O 1 *
bit 747 O 1 *
bit 746 O 1 *
bit 745 O 1 *
bit 744 I 1 IO_P100
bit 743 O 1 IO_P100 742 1 Z
bit 742 C 1 *
bit 741 O 1 *
bit 740 O 1 *
bit 739 O 1 *
bit 738 O 1 *
bit 737 O 1 *
bit 736 O 1 *
bit 735 O 1 *
bit 734 O 1 *
bit 733 O 1 *
bit 732 O 1 *
bit 731 O 1 *
bit 730 O 1 *
bit 729 I 1 IO_P99
bit 728 O 1 IO_P99 727 1 Z
bit 727 C 1 *
bit 726 I 1 IO_P98
bit 725 O 1 IO_P98 724 1 Z
bit 724 C 1 *
bit 723 I 1 IO_P97
bit 722 O 1 IO_P97 721 1 Z
bit 721 C 1 *
bit 720 O 1 *
bit 719 O 1 *
bit 718 O 1 *
bit 717 O 1 *
bit 716 O 1 *
bit 715 O 1 *
bit 714 O 1 *
bit 713 O 1 *
bit 712 O 1 *
bit 711 I 1 IO_P96
bit 710 O 1 IO_P96 709 1 Z
bit 709 C 1 *
bit 708 I 1 IO_P95
bit 707 O 1 IO_P95 706 1 Z
bit 706 C 1 *
bit 705 O 1 *
bit 704 O 1 *
bit 703 O 1 *
bit 702 I 1 IO_P94
bit 701 O 1 IO_P94 700 1 Z
bit 700 C 1 *
bit 699 I 1 IO_P93
bit 698 O 1 IO_P93 697 1 Z
bit 697 C 1 *
bit 696 I 1 IO_P89
bit 695 O 1 IO_P89 694 1 Z
bit 694 C 1 *
bit 693 I 1 IO_P88
bit 692 O 1 IO_P88 691 1 Z
bit 691 C 1 *
bit 690 O 1 *
bit 689 O 1 *
bit 688 O 1 *
bit 687 O 1 *
bit 686 O 1 *
bit 685 O 1 *
bit 684 O 1 *
bit 683 O 1 *
bit 682 O 1 *
bit 681 O 1 *
bit 680 O 1 *
bit 679 O 1 *
bit 678 O 1 *
bit 677 O 1 *
bit 676 O 1 *
bit 675 O 1 *
bit 674 O 1 *
bit 673 O 1 *
bit 672 I 1 IO_P87
bit 671 O 1 IO_P87 670 1 Z
bit 670 C 1 *
bit 669 I 1 IO_P86
bit 668 O 1 IO_P86 667 1 Z
bit 667 C 1 *
bit 666 I 1 IO_P84
bit 665 O 1 IO_P84 664 1 Z
bit 664 C 1 *
bit 663 I 1 IO_P83
bit 662 O 1 IO_P83 661 1 Z
bit 661 C 1 *
bit 660 O 1 *
bit 659 O 1 *
bit 658 O 1 *
bit 657 O 1 *
bit 656 O 1 *
bit 655 O 1 *
bit 654 O 1 *
bit 653 O 1 *
bit 652 O 1 *
bit 651 I 1 IO_P82
bit 650 O 1 IO_P82 649 1 Z
bit 649 C 1 *
bit 648 O 1 *
bit 647 O 1 *
bit 646 O 1 *
bit 645 O 1 *
bit 644 O 1 *
bit 643 O 1 *
bit 642 O 1 *
bit 641 O 1 *
bit 640 O 1 *
bit 639 I 1 IO_P81
bit 638 O 1 IO_P81 637 1 Z
bit 637 C 1 *
bit 636 I 1 GCK0_P80
bit 635 I 1 GCK1_P77
bit 634 I 1 IO_P75
bit 633 O 1 IO_P75 632 1 Z
bit 632 C 1 *
bit 631 O 1 *
bit 630 O 1 *
bit 629 O 1 *
bit 628 O 1 *
bit 627 O 1 *
bit 626 O 1 *
bit 625 O 1 *
bit 624 O 1 *
bit 623 O 1 *
bit 622 O 1 *
bit 621 O 1 *
bit 620 O 1 *
bit 619 O 1 *
bit 618 O 1 *
bit 617 O 1 *
bit 616 O 1 *
bit 615 O 1 *
bit 614 O 1 *
bit 613 O 1 *
bit 612 O 1 *
bit 611 O 1 *
bit 610 I 1 IO_P74
bit 609 O 1 IO_P74 608 1 Z
bit 608 C 1 *
bit 607 I 1 IO_P73
bit 606 O 1 IO_P73 605 1 Z
bit 605 C 1 *
bit 604 I 1 IO_P71
bit 603 O 1 IO_P71 602 1 Z
bit 602 C 1 *
bit 601 I 1 IO_P70
bit 600 O 1 IO_P70 599 1 Z
bit 599 C 1 *
bit 598 O 1 *
bit 597 O 1 *
bit 596 O 1 *
bit 595 O 1 *
bit 594 O 1 *
bit 593 O 1 *
bit 592 O 1 *
bit 591 O 1 *
bit 590 O 1 *
bit 589 O 1 *
bit 588 O 1 *
bit 587 O 1 *
bit 586 O 1 *
bit 585 O 1 *
bit 584 O 1 *
bit 583 O 1 *
bit 582 O 1 *
bit 581 O 1 *
bit 580 I 1 IO_P69
bit 579 O 1 IO_P69 578 1 Z
bit 578 C 1 *
bit 577 I 1 IO_P68
bit 576 O 1 IO_P68 575 1 Z
bit 575 C 1 *
bit 574 I 1 IO_P64
bit 573 O 1 IO_P64 572 1 Z
bit 572 C 1 *
bit 571 I 1 IO_P63
bit 570 O 1 IO_P63 569 1 Z
bit 569 C 1 *
bit 568 O 1 *
bit 567 O 1 *
bit 566 O 1 *
bit 565 I 1 IO_P62
bit 564 O 1 IO_P62 563 1 Z
bit 563 C 1 *
bit 562 I 1 IO_P61
bit 561 O 1 IO_P61 560 1 Z
bit 560 C 1 *
bit 559 O 1 *
bit 558 O 1 *
bit 557 O 1 *
bit 556 O 1 *
bit 555 O 1 *
bit 554 O 1 *
bit 553 O 1 *
bit 552 O 1 *
bit 551 O 1 *
bit 550 I 1 IO_P60
bit 549 O 1 IO_P60 548 1 Z
bit 548 C 1 *
bit 547 I 1 IO_P59
bit 546 O 1 IO_P59 545 1 Z
bit 545 C 1 *
bit 544 I 1 IO_P58
bit 543 O 1 IO_P58 542 1 Z
bit 542 C 1 *
bit 541 O 1 *
bit 540 O 1 *
bit 539 O 1 *
bit 538 O 1 *
bit 537 O 1 *
bit 536 O 1 *
bit 535 O 1 *
bit 534 O 1 *
bit 533 O 1 *
bit 532 O 1 *
bit 531 O 1 *
bit 530 O 1 *
bit 529 I 1 IO_P57
bit 528 O 1 IO_P57 527 1 Z
bit 527 C 1 *
bit 526 O 1 *
bit 525 O 1 *
bit 524 O 1 *
bit 523 O 1 *
bit 522 O 1 *
bit 521 O 1 *
bit 520 O 1 *
bit 519 O 1 *
bit 518 O 1 *
bit 517 O 1 *
bit 516 O 1 *
bit 515 O 1 *
bit 514 I 1 IO_P56
bit 513 O 1 IO_P56 512 1 Z
bit 512 C 1 *
bit 511 I 1 IO_P55
bit 510 O 1 IO_P55 509 1 Z
bit 509 C 1 *
bit 508 I 1 M2_P54
bit 507 I 1 M0_P52
bit 506 I 1 M1_P50
bit 505 I 1 IO_P49
bit 504 O 1 IO_P49 503 1 Z
bit 503 C 1 *
bit 502 I 1 IO_P48
bit 501 O 1 IO_P48 500 1 Z
bit 500 C 1 *
bit 499 O 1 *
bit 498 O 1 *
bit 497 O 1 *
bit 496 O 1 *
bit 495 O 1 *
bit 494 O 1 *
bit 493 O 1 *
bit 492 O 1 *
bit 491 O 1 *
bit 490 O 1 *
bit 489 O 1 *
bit 488 O 1 *
bit 487 I 1 IO_P47
bit 486 O 1 IO_P47 485 1 Z
bit 485 C 1 *
bit 484 O 1 *
bit 483 O 1 *
bit 482 O 1 *
bit 481 O 1 *
bit 480 O 1 *
bit 479 O 1 *
bit 478 O 1 *
bit 477 O 1 *
bit 476 O 1 *
bit 475 O 1 *
bit 474 O 1 *
bit 473 O 1 *
bit 472 I 1 IO_P46
bit 471 O 1 IO_P46 470 1 Z
bit 470 C 1 *
bit 469 I 1 IO_P45
bit 468 O 1 IO_P45 467 1 Z
bit 467 C 1 *
bit 466 I 1 IO_P44
bit 465 O 1 IO_P44 464 1 Z
bit 464 C 1 *
bit 463 O 1 *
bit 462 O 1 *
bit 461 O 1 *
bit 460 O 1 *
bit 459 O 1 *
bit 458 O 1 *
bit 457 O 1 *
bit 456 O 1 *
bit 455 O 1 *
bit 454 I 1 IO_P43
bit 453 O 1 IO_P43 452 1 Z
bit 452 C 1 *
bit 451 I 1 IO_P42
bit 450 O 1 IO_P42 449 1 Z
bit 449 C 1 *
bit 448 O 1 *
bit 447 O 1 *
bit 446 O 1 *
bit 445 I 1 IO_P41
bit 444 O 1 IO_P41 443 1 Z
bit 443 C 1 *
bit 442 I 1 IO_P40
bit 441 O 1 IO_P40 440 1 Z
bit 440 C 1 *
bit 439 I 1 IO_P36
bit 438 O 1 IO_P36 437 1 Z
bit 437 C 1 *
bit 436 I 1 IO_P35
bit 435 O 1 IO_P35 434 1 Z
bit 434 C 1 *
bit 433 O 1 *
bit 432 O 1 *
bit 431 O 1 *
bit 430 O 1 *
bit 429 O 1 *
bit 428 O 1 *
bit 427 O 1 *
bit 426 O 1 *
bit 425 O 1 *
bit 424 O 1 *
bit 423 O 1 *
bit 422 O 1 *
bit 421 O 1 *
bit 420 O 1 *
bit 419 O 1 *
bit 418 O 1 *
bit 417 O 1 *
bit 416 O 1 *
bit 415 I 1 IO_P34
bit 414 O 1 IO_P34 413 1 Z
bit 413 C 1 *
bit 412 I 1 IO_P33
bit 411 O 1 IO_P33 410 1 Z
bit 410 C 1 *
bit 409 I 1 IO_P31
bit 408 O 1 IO_P31 407 1 Z
bit 407 C 1 *
bit 406 I 1 IO_P30
bit 405 O 1 IO_P30 404 1 Z
bit 404 C 1 *
bit 403 O 1 *
bit 402 O 1 *
bit 401 O 1 *
bit 400 O 1 *
bit 399 O 1 *
bit 398 O 1 *
bit 397 O 1 *
bit 396 O 1 *
bit 395 O 1 *
bit 394 I 1 IO_P29
bit 393 O 1 IO_P29 392 1 Z
bit 392 C 1 *
bit 391 O 1 *
bit 390 O 1 *
bit 389 O 1 *
bit 388 O 1 *
bit 387 O 1 *
bit 386 O 1 *
bit 385 O 1 *
bit 384 O 1 *
bit 383 O 1 *
bit 382 I 1 IO_P27
bit 381 O 1 IO_P27 380 1 Z
bit 380 C 1 *
bit 379 I 1 IO_P24
bit 378 O 1 IO_P24 377 1 Z
bit 377 C 1 *
bit 376 I 1 IO_P23
bit 375 O 1 IO_P23 374 1 Z
bit 374 C 1 *
bit 373 O 1 *
bit 372 O 1 *
bit 371 O 1 *
bit 370 O 1 *
bit 369 O 1 *
bit 368 O 1 *
bit 367 I 1 IO_P22
bit 366 O 1 IO_P22 365 1 Z
bit 365 C 1 *
bit 364 O 1 *
bit 363 O 1 *
bit 362 O 1 *
bit 361 O 1 *
bit 360 O 1 *
bit 359 O 1 *
bit 358 O 1 *
bit 357 O 1 *
bit 356 O 1 *
bit 355 I 1 IO_P21
bit 354 O 1 IO_P21 353 1 Z
bit 353 C 1 *
bit 352 I 1 IO_P20
bit 351 O 1 IO_P20 350 1 Z
bit 350 C 1 *
bit 349 I 1 IO_P18
bit 348 O 1 IO_P18 347 1 Z
bit 347 C 1 *
bit 346 I 1 IO_P17
bit 345 O 1 IO_P17 344 1 Z
bit 344 C 1 *
bit 343 O 1 *
bit 342 O 1 *
bit 341 O 1 *
bit 340 O 1 *
bit 339 O 1 *
bit 338 O 1 *
bit 337 O 1 *
bit 336 O 1 *
bit 335 O 1 *
bit 334 O 1 *
bit 333 O 1 *
bit 332 O 1 *
bit 331 O 1 *
bit 330 O 1 *
bit 329 O 1 *
bit 328 O 1 *
bit 327 O 1 *
bit 326 O 1 *
bit 325 I 1 IO_P16
bit 324 O 1 IO_P16 323 1 Z
bit 323 C 1 *
bit 322 I 1 IO_P15
bit 321 O 1 IO_P15 320 1 Z
bit 320 C 1 *
bit 319 I 1 IO_P11
bit 318 O 1 IO_P11 317 1 Z
bit 317 C 1 *
bit 316 I 1 IO_P10
bit 315 O 1 IO_P10 314 1 Z
bit 314 C 1 *
bit 313 O 1 *
bit 312 O 1 *
bit 311 O 1 *
bit 310 I 1 IO_P9
bit 309 O 1 IO_P9 308 1 Z
bit 308 C 1 *
bit 307 I 1 IO_P8
bit 306 O 1 IO_P8 305 1 Z
bit 305 C 1 *
bit 304 O 1 *
bit 303 O 1 *
bit 302 O 1 *
bit 301 O 1 *
bit 300 O 1 *
bit 299 O 1 *
bit 298 O 1 *
bit 297 O 1 *
bit 296 O 1 *
bit 295 I 1 IO_P7
bit 294 O 1 IO_P7 293 1 Z
bit 293 C 1 *
bit 292 I 1 IO_P6
bit 291 O 1 IO_P6 290 1 Z
bit 290 C 1 *
bit 289 I 1 IO_P5
bit 288 O 1 IO_P5 287 1 Z
bit 287 C 1 *
bit 286 O 1 *
bit 285 O 1 *
bit 284 O 1 *
bit 283 O 1 *
bit 282 O 1 *
bit 281 O 1 *
bit 280 O 1 *
bit 279 O 1 *
bit 278 O 1 *
bit 277 O 1 *
bit 276 O 1 *
bit 275 O 1 *
bit 274 I 1 IO_P4
bit 273 O 1 IO_P4 272 1 Z
bit 272 C 1 *
bit 271 O 1 *
bit 270 O 1 *
bit 269 O 1 *
bit 268 O 1 *
bit 267 O 1 *
bit 266 O 1 *
bit 265 O 1 *
bit 264 O 1 *
bit 263 O 1 *
bit 262 O 1 *
bit 261 O 1 *
bit 260 O 1 *
bit 259 I 1 IO_P3
bit 258 O 1 IO_P3 257 1 Z
bit 257 C 1 *
bit 256 O 1 *
bit 255 O 1 *
bit 254 O 1 *
bit 253 O 1 *
bit 252 O 1 *
bit 251 O 1 *
bit 250 I 1 IO_P206
bit 249 O 1 IO_P206 248 1 Z
bit 248 C 1 *
bit 247 O 1 *
bit 246 O 1 *
bit 245 O 1 *
bit 244 O 1 *
bit 243 O 1 *
bit 242 O 1 *
bit 241 O 1 *
bit 240 O 1 *
bit 239 O 1 *
bit 238 O 1 *
bit 237 O 1 *
bit 236 O 1 *
bit 235 I 1 IO_P205
bit 234 O 1 IO_P205 233 1 Z
bit 233 C 1 *
bit 232 O 1 *
bit 231 O 1 *
bit 230 O 1 *
bit 229 O 1 *
bit 228 O 1 *
bit 227 O 1 *
bit 226 O 1 *
bit 225 O 1 *
bit 224 O 1 *
bit 223 O 1 *
bit 222 O 1 *
bit 221 O 1 *
bit 220 I 1 IO_P204
bit 219 O 1 IO_P204 218 1 Z
bit 218 C 1 *
bit 217 I 1 IO_P203
bit 216 O 1 IO_P203 215 1 Z
bit 215 C 1 *
bit 214 I 1 IO_P202
bit 213 O 1 IO_P202 212 1 Z
bit 212 C 1 *
bit 211 O 1 *
bit 210 O 1 *
bit 209 O 1 *
bit 208 O 1 *
bit 207 O 1 *
bit 206 O 1 *
bit 205 O 1 *
bit 204 O 1 *
bit 203 O 1 *
bit 202 I 1 IO_P201
bit 201 O 1 IO_P201 200 1 Z
bit 200 C 1 *
bit 199 I 1 IO_P200
bit 198 O 1 IO_P200 197 1 Z
bit 197 C 1 *
bit 196 O 1 *
bit 195 O 1 *
bit 194 O 1 *
bit 193 I 1 IO_P199
bit 192 O 1 IO_P199 191 1 Z
bit 191 C 1 *
bit 190 I 1 IO_P198
bit 189 O 1 IO_P198 188 1 Z
bit 188 C 1 *
bit 187 I 1 IO_P194
bit 186 O 1 IO_P194 185 1 Z
bit 185 C 1 *
bit 184 I 1 IO_P193
bit 183 O 1 IO_P193 182 1 Z
bit 182 C 1 *
bit 181 O 1 *
bit 180 O 1 *
bit 179 O 1 *
bit 178 O 1 *
bit 177 O 1 *
bit 176 O 1 *
bit 175 O 1 *
bit 174 O 1 *
bit 173 O 1 *
bit 172 O 1 *
bit 171 O 1 *
bit 170 O 1 *
bit 169 O 1 *
bit 168 O 1 *
bit 167 O 1 *
bit 166 O 1 *
bit 165 O 1 *
bit 164 O 1 *
bit 163 I 1 IO_P192
bit 162 O 1 IO_P192 161 1 Z
bit 161 C 1 *
bit 160 I 1 IO_P191
bit 159 O 1 IO_P191 158 1 Z
bit 158 C 1 *
bit 157 I 1 IO_P189
bit 156 O 1 IO_P189 155 1 Z
bit 155 C 1 *
bit 154 I 1 IO_P188
bit 153 O 1 IO_P188 152 1 Z
bit 152 C 1 *
bit 151 O 1 *
bit 150 O 1 *
bit 149 O 1 *
bit 148 O 1 *
bit 147 O 1 *
bit 146 O 1 *
bit 145 O 1 *
bit 144 O 1 *
bit 143 O 1 *
bit 142 O 1 *
bit 141 O 1 *
bit 140 O 1 *
bit 139 O 1 *
bit 138 O 1 *
bit 137 O 1 *
bit 136 O 1 *
bit 135 O 1 *
bit 134 O 1 *
bit 133 O 1 *
bit 132 O 1 *
bit 131 O 1 *
bit 130 I 1 IO_P187
bit 129 O 1 IO_P187 128 1 Z
bit 128 C 1 *
bit 127 I 1 GCK3_P185
bit 126 I 1 GCK2_P182
bit 125 I 1 IO_P181
bit 124 O 1 IO_P181 123 1 Z
bit 123 C 1 *
bit 122 O 1 *
bit 121 O 1 *
bit 120 O 1 *
bit 119 O 1 *
bit 118 O 1 *
bit 117 O 1 *
bit 116 O 1 *
bit 115 O 1 *
bit 114 O 1 *
bit 113 I 1 IO_P180
bit 112 O 1 IO_P180 111 1 Z
bit 111 C 1 *
bit 110 O 1 *
bit 109 O 1 *
bit 108 O 1 *
bit 107 O 1 *
bit 106 O 1 *
bit 105 O 1 *
bit 104 O 1 *
bit 103 O 1 *
bit 102 O 1 *
bit 101 I 1 IO_P179
bit 100 O 1 IO_P179 99 1 Z
bit 99 C 1 *
bit 98 I 1 IO_P178
bit 97 O 1 IO_P178 96 1 Z
bit 96 C 1 *
bit 95 I 1 IO_P176
bit 94 O 1 IO_P176 93 1 Z
bit 93 C 1 *
bit 92 I 1 IO_P175
bit 91 O 1 IO_P175 90 1 Z
bit 90 C 1 *
bit 89 O 1 *
bit 88 O 1 *
bit 87 O 1 *
bit 86 O 1 *
bit 85 O 1 *
bit 84 O 1 *
bit 83 O 1 *
bit 82 O 1 *
bit 81 O 1 *
bit 80 O 1 *
bit 79 O 1 *
bit 78 O 1 *
bit 77 O 1 *
bit 76 O 1 *
bit 75 O 1 *
bit 74 O 1 *
bit 73 O 1 *
bit 72 O 1 *
bit 71 I 1 IO_P174
bit 70 O 1 IO_P174 69 1 Z
bit 69 C 1 *
bit 68 I 1 IO_P173
bit 67 O 1 IO_P173 66 1 Z
bit 66 C 1 *
bit 65 I 1 IO_P169
bit 64 O 1 IO_P169 63 1 Z
bit 63 C 1 *
bit 62 I 1 IO_P168
bit 61 O 1 IO_P168 60 1 Z
bit 60 C 1 *
bit 59 O 1 *
bit 58 O 1 *
bit 57 O 1 *
bit 56 I 1 IO_P167
bit 55 O 1 IO_P167 54 1 Z
bit 54 C 1 *
bit 53 I 1 IO_P166
bit 52 O 1 IO_P166 51 1 Z
bit 51 C 1 *
bit 50 O 1 *
bit 49 O 1 *
bit 48 O 1 *
bit 47 O 1 *
bit 46 O 1 *
bit 45 O 1 *
bit 44 O 1 *
bit 43 O 1 *
bit 42 O 1 *
bit 41 I 1 IO_P165
bit 40 O 1 IO_P165 39 1 Z
bit 39 C 1 *
bit 38 I 1 IO_P164
bit 37 O 1 IO_P164 36 1 Z
bit 36 C 1 *
bit 35 I 1 IO_P163
bit 34 O 1 IO_P163 33 1 Z
bit 33 C 1 *
bit 32 O 1 *
bit 31 O 1 *
bit 30 O 1 *
bit 29 O 1 *
bit 28 O 1 *
bit 27 O 1 *
bit 26 O 1 *
bit 25 O 1 *
bit 24 O 1 *
bit 23 O 1 *
bit 22 O 1 *
bit 21 O 1 *
bit 20 I 1 IO_P162
bit 19 O 1 IO_P162 18 1 Z
bit 18 C 1 *
bit 17 O 1 *
bit 16 O 1 *
bit 15 O 1 *
bit 14 O 1 *
bit 13 O 1 *
bit 12 O 1 *
bit 11 O 1 *
bit 10 O 1 *
bit 9 O 1 *
bit 8 O 1 *
bit 7 O 1 *
bit 6 O 1 *
bit 5 I 1 IO_P161
bit 4 O 1 IO_P161 3 1 Z
bit 3 C 1 *
bit 2 I 1 IO_P160
bit 1 O 1 IO_P160 0 1 Z
bit 0 C 1 *
