#
# $Id: hd64465 581 2003-10-20 11:11:06Z telka $
#
# JTAG declarations for Hitachi HD64465BP/HD64465BQ
# Copyright (C) 2003 Elcom s.r.o.
#
# This program is free software; you can redistribute it and/or
# modify it under the terms of the GNU General Public License
# as published by the Free Software Foundation; either version 2
# of the License, or (at your option) any later version.
#
# This program is distributed in the hope that it will be useful,
# but WITHOUT ANY WARRANTY; without even the implied warranty of
# MERCHANTABILITY or FITNESS FOR A PARTICULAR PURPOSE.  See the
# GNU General Public License for more details.
#
# You should have received a copy of the GNU General Public License
# along with this program; if not, write to the Free Software
# Foundation, Inc., 59 Temple Place - Suite 330, Boston, MA
# 02111-1307, USA.
#
# Written by Marcel Telka <marcel@telka.sk>, 2003.
#
# Documentation:
# [1] Hitachi Ltd., "Windows CE Intelligent Peripheral Controller
#     HD64465 User's Manual", 03/08/01, Rev. 3.0, ADE-602-168B
#

# Test Mode (see Table 4.3 in [1])
signal	TST
signal	TDI
signal	TDO
signal	TMS
signal	TCK
signal	TRST

# CPU interface (see Table 4.4 in [1])
signal	CKIO
signal	A0
signal	A1
signal	A2
signal	A3
signal	A4
signal	A5
signal	A6
signal	A7
signal	A8
signal	A9
signal	A10
signal	A11
signal	A12
signal	A13
signal	A14
signal	A15
signal	A16
signal	A17
signal	A18
signal	A19
signal	A20
signal	A21
signal	A22
signal	A23
signal	A24
signal	A25
signal	D0
signal	D1
signal	D2
signal	D3
signal	D4
signal	D5
signal	D6
signal	D7
signal	D8
signal	D9
signal	D10
signal	D11
signal	D12
signal	D13
signal	D14
signal	D15
signal	D16
signal	D17
signal	D18
signal	D19
signal	D20
signal	D21
signal	D22
signal	D23
signal	D24
signal	D25
signal	D26
signal	D27
signal	D28
signal	D29
signal	D30
signal	D31
signal	nCS4
signal	nWE0
signal	nWE1
signal	nWE2
signal	nWE3
signal	nRDWR
signal	nRD
signal	nRDY
signal	nBS
signal	nDREQ0
signal	nDREQ1
signal	DRAK0
signal	DRAK1
signal	nIRQ0
signal	SH_MODE
signal	nCE1B
signal	nCE2B
signal	nCE1A
signal	nCE2A
signal	nIOIS16

# PCMCIA 0 (see Table 4.5 in [1])
signal	PCC0A0
signal	PCC0A1
signal	PCC0A2
signal	PCC0A3
signal	PCC0A4
signal	PCC0A5
signal	PCC0A6
signal	PCC0A7
signal	PCC0A8
signal	PCC0A9
signal	PCC0A10
signal	PCC0A11
signal	PCC0A12
signal	PCC0A13
signal	PCC0A14
signal	PCC0A15
signal	PCC0A16
signal	PCC0A17
signal	PCC0A18
signal	PCC0A19
signal	PCC0A20
signal	PCC0A21
signal	PCC0A22
signal	PCC0A23
signal	PCC0A24
signal	PCC0A25
signal	PCC0D0
signal	PCC0D1
signal	PCC0D2
signal	PCC0D3
signal	PCC0D4
signal	PCC0D5
signal	PCC0D6
signal	PCC0D7
signal	PCC0D8
signal	PCC0D9
signal	PCC0D10
signal	PCC0D11
signal	PCC0D12
signal	PCC0D13
signal	PCC0D14
signal	PCC0D15
signal	nPCC0CE1B
signal	nPCC0CE2B
signal	nRDB
signal	nWEB
signal	nPCC0ICIORDB
signal	nPCC0ICIOWRB
signal	PCC0RESET
signal	nPCC0WAIT
signal	nPCC0WP
signal	PCC0RDY
signal	PCC0BVD1
signal	PCC0BVD2
signal	nPCC0CD1
signal	nPCC0CD2
signal	nPCC0VS1
signal	nPCC0VS2
signal	nPCC0REG
signal	VCC0SEL1
signal	VCC0SEL0
signal	VCC0VPP1
signal	VCC0VPP0

# PCMCIA 1 (see Table 4.6 in [1])
signal	PCC1A0
signal	PCC1A1
signal	PCC1A2
signal	PCC1A3
signal	PCC1A4
signal	PCC1A5
signal	PCC1A6
signal	PCC1A7
signal	PCC1A8
signal	PCC1A9
signal	PCC1A10
signal	PCC1A11
signal	PCC1A12
signal	PCC1A13
signal	PCC1A14
signal	PCC1A15
signal	PCC1A16
signal	PCC1A17
signal	PCC1A18
signal	PCC1A19
signal	PCC1A20
signal	PCC1A21
signal	PCC1A22
signal	PCC1A23
signal	PCC1A24
signal	PCC1A25
signal	PCC1D0
signal	PCC1D1
signal	PCC1D2
signal	PCC1D3
signal	PCC1D4
signal	PCC1D5
signal	PCC1D6
signal	PCC1D7
signal	PCC1D8
signal	PCC1D9
signal	PCC1D10
signal	PCC1D11
signal	PCC1D12
signal	PCC1D13
signal	PCC1D14
signal	PCC1D15
signal	nPCC1CE1A
signal	nPCC1CE2A
signal	nRDA
signal	nWEA
signal	nPCC1ICIORDA
signal	nPCC1ICIOWRA
signal	PCC1RESET
signal	nPCC1WAIT
signal	nPCC1WP
signal	PCC1RDY
signal	PCC1BVD1
signal	PCC1BVD2
signal	nPCC1CD1
signal	nPCC1CD2
signal	nPCC1VS1
signal	nPCC1VS2
signal	nPCC1REG
signal	VCC1SEL1
signal	VCC1SEL0
signal	VCC1VPP1
signal	VCC1VPP0

# UART 0 (see Table 4.7 in [1])
signal	TXD0
signal	RXD0
signal	nRTS0
signal	nCTS0
signal	nDTR0
signal	nDSR0
signal	nDCD0
signal	nRI0

# IrDA (see Table 4.8 in [1])
signal	MODSEL
signal	TXD
signal	nRX

# Printer Interface (see Table 4.9 in [1])
signal	nSTB
signal	nAFD
signal	nERR
signal	nINIT
signal	nSLIN
signal	nACK
signal	BUSY
signal	PE
signal	SLCT
signal	PPD0
signal	PPD1
signal	PPD2
signal	PPD3
signal	PPD4
signal	PPD5
signal	PPD6
signal	PPD7

# AFE Interface (see Table 4.10 in [1])
signal	DOUT
signal	DIN
signal	SCLK
signal	HC1
signal	FS
signal	nAFERST
signal	nAFEPDN
signal	MCLKO
signal	OFFHOOK
signal	RING

# CODEC Interface (see Table 4.11 in [1])
signal	ACCLK
signal	nACRST
signal	nACPD
signal	SIBDIN
signal	SIBCLK
signal	SIBDOUT
signal	SIBSYNC

# USB Interface (see Table 4.12 in [1])
signal	nUSBPEN
signal	nUSBOVR
signal	USBD1P
signal	USBD1M
signal	USBD2P
signal	USBD2M

# Keyboard Interface (see Table 4.13 in [1])
signal	nKBCS
signal	nXIOW
signal	nXIOR
signal	KBIRQ0
signal	KBIRQ1

# IO Port A (see Table 4.14 in [1])
signal	PA0
signal	PA1
signal	PA2
signal	PA3
signal	PA4
signal	PA5
signal	PA6
signal	PA7

# IO Port B (see Table 4.15 in [1])
signal	PB0
signal	PB1
signal	PB2
signal	PB3
signal	PB4
signal	PB5
signal	PB6
signal	PB7

# IO Port C (see Table 4.16 in [1])
signal	PC0
signal	PC1
signal	PC2
signal	PC3
signal	PC4
signal	PC5
signal	PC6
signal	PC7

# IO Port D (see Table 4.17 in [1])
signal	PD0
signal	PD1
signal	PD2
signal	PD3
signal	PD4
signal	PD5
signal	PD6
signal	PD7

# IO Port E (see Table 4.18 in [1])
signal	PE0
signal	PE1
signal	PE2
signal	PE3
signal	PE4
signal	PE5
signal	PE6
signal	PE7

# 10-bit ADC Interface (see Table 4.19 in [1])
signal	TSMX
signal	TSMY
signal	TSPX
signal	TSPY

# PS/2 Interface (see Table 4.20 in [1])
signal	KBCK
signal	KBDATA
signal	MSCK
signal	MSDATA

# System Reset Interface (see Table 4.21 in [1])
signal	nRESETPI
signal	nRESETMI
signal	nRESETPO
signal	nRESETMO

# Crystal Interface (see Table 4.22 in [1])
signal	AFECK
signal	AFECKE
signal	UCK
signal	UCKE

# Miscellaneous Interface (see Table 4.23 in [1])
signal	PWM0
signal	PWM1
signal	P80LE

# No Connected Pins (see Table 4.24 in [1])
signal	NC(1)
signal	NC(2)
signal	NC(3)
signal	NC(4)
signal	NC(5)
signal	NC(6)
signal	NC(7)
signal	NC(8)
signal	NC(9)
signal	NC(10)
signal	NC(11)
signal	NC(12)
signal	NC(13)
signal	NC(14)

# Power/Ground (see Tabe 4.25 in [1])
signal	VSS
signal	VCC
signal	VCC5
signal	VCCA
signal	VCCB
signal	AVCC1
signal	AVSS1
signal	AVCC2
signal	AVSS2
signal	AVCC3
signal	AVSS3
signal	AVCC4
signal	AVSS4
signal	AVCC5
signal	AVCC6
signal	AVSS6

# mandatory data registers
register	BSR	550
register	BR	1

# instructions
instruction length 3
# mandatory instructions
instruction BYPASS		111	BR
instruction EXTEST		000	BSR
instruction SAMPLE/PRELOAD	001	BSR

# boundary scan register
bit 549 I ? nBS
bit 548 I ? RING
bit 547 I ? FS
bit 546 I ? SCLK
bit 545 I ? DIN
bit 544 O ? nAFERST
bit 543 O ? nAFEPDN
bit 542 O ? HC1 541 0 Z
bit 541 C 0 .
bit 540 O ? OFFHOOK 541 0 Z
bit 539 O ? MCLKO 541 0 Z
bit 538 O ? DOUT 541 0 Z
bit 537 O ? PA0 535 0 Z
bit 536 I ? PA0
bit 535 C 0 .
bit 534 O ? PA1 532 0 Z
bit 533 I ? PA1
bit 532 C 0 .
bit 531 O ? PA2 529 0 Z
bit 530 I ? PA2
bit 529 C 0 .
bit 528 O ? PA3 526 0 Z
bit 527 I ? PA3
bit 526 C 0 .
bit 525 O ? PA4 523 0 Z
bit 524 I ? PA4
bit 523 C 0 .
bit 522 O ? PA5 520 0 Z
bit 521 I ? PA5
bit 520 C 0 .
bit 519 O ? PA6 517 0 Z
bit 518 I ? PA6
bit 517 C 0 .
bit 516 O ? PA7 514 0 Z
bit 515 I ? PA7
bit 514 C 0 .
bit 513 O ? nXIOW
bit 512 O ? nXIOR
bit 511 O ? nKBCS
bit 510 I ? KBIRQ0
bit 509 I ? KBIRQ1
bit 508 O ? P80LE
bit 507 I ? CKIO
bit 506 I ? nRESETPI
bit 505 I ? SH_MODE
bit 504 I ? A12
bit 503 I ? A11
bit 502 I ? A10
bit 501 I ? A9
bit 500 I ? A8
bit 499 I ? A7
bit 498 I ? A6
bit 497 I ? A5
bit 496 I ? A4
bit 495 I ? A3
bit 494 I ? A2
bit 493 I ? A1
bit 492 I ? A0
bit 491 O ? D31 489 0 Z
bit 490 I ? D31
bit 489 C 0 .
bit 488 O ? D30 489 0 Z
bit 487 I ? D30
bit 486 O ? D29 489 0 Z
bit 485 I ? D29
bit 484 O ? D28 489 0 Z
bit 483 I ? D28
bit 482 O ? D27 489 0 Z
bit 481 I ? D27
bit 480 O ? D26 489 0 Z
bit 479 I ? D26
bit 478 O ? D25 489 0 Z
bit 477 I ? D25
bit 476 O ? D24 489 0 Z
bit 475 I ? D24
bit 474 O ? D15 472 0 Z
bit 473 I ? D15
bit 472 C 0 .
bit 471 O ? D14 472 0 Z
bit 470 I ? D14
bit 469 O ? D13 472 0 Z
bit 468 I ? D13
bit 467 O ? D12 472 0 Z
bit 466 I ? D12
bit 465 O ? D11 472 0 Z
bit 464 I ? D11
bit 463 O ? D10 472 0 Z
bit 462 I ? D10
bit 461 O ? D9 472 0 Z
bit 460 I ? D9
bit 459 O ? D8 472 0 Z
bit 458 I ? D8
bit 457 O ? D23 455 0 Z
bit 456 I ? D23
bit 455 C 0 .
bit 454 O ? D22 455 0 Z
bit 453 I ? D22
bit 452 O ? D21 455 0 Z
bit 451 I ? D21
bit 450 O ? D20 455 0 Z
bit 449 I ? D20
bit 448 O ? D19 455 0 Z
bit 447 I ? D19
bit 446 O ? D18 455 0 Z
bit 445 I ? D18
bit 444 O ? D17 455 0 Z
bit 443 I ? D17
bit 442 O ? D16 455 0 Z
bit 441 I ? D16
bit 440 O ? D7 438 0 Z
bit 439 I ? D7
bit 438 C 0 .
bit 437 O ? D6 438 0 Z
bit 436 I ? D6
bit 435 O ? D5 438 0 Z
bit 434 I ? D5
bit 433 O ? D4 438 0 Z
bit 432 I ? D4
bit 431 O ? D3 438 0 Z
bit 430 I ? D3
bit 429 O ? D2 438 0 Z
bit 428 I ? D2
bit 427 O ? D1 438 0 Z
bit 426 I ? D1
bit 425 O ? D0 438 0 Z
bit 424 I ? D0
bit 423 O ? nIRQ0
bit 422 O ? nRDY 421 0 Z
bit 421 C 0 .
bit 420 I ? DRAK1
bit 419 O ? nDREQ1
bit 418 I ? DRAK0
bit 417 O ? nDREQ0
bit 416 I ? A13
bit 415 I ? A14
bit 414 I ? A15
bit 413 I ? A16
bit 412 I ? A17
bit 411 I ? A18
bit 410 I ? A19
bit 409 I ? A20
bit 408 I ? A21
bit 407 I ? A22
bit 406 I ? A23
bit 405 I ? A24
bit 404 I ? A25
bit 403 I ? nCS4
bit 402 I ? nRDWR
bit 401 I ? nRD
bit 400 I ? nWE0
bit 399 I ? nWE1
bit 398 I ? nWE2
bit 397 I ? nWE3
bit 396 I ? nCE2A
bit 395 I ? nCE1A
bit 394 I ? nCE2B
bit 393 I ? nCE1B
bit 392 O ? nIOIS16 391 0 Z
bit 391 C 0 .
bit 390 O ? VCC0SEL1
bit 389 O ? VCC0SEL0
bit 388 O ? VCC0VPP1
bit 387 O ? VCC0VPP0
bit 386 I ? nPCC0CD2
bit 385 I ? nPCC0CD1
bit 384 I ? nPCC0VS2
bit 383 I ? nPCC0VS1
bit 382 I ? PCC0BVD2
bit 381 I ? PCC0BVD1
bit 380 I ? PCC0RDY
bit 379 I ? nPCC0WP
bit 378 I ? nPCC0WAIT
bit 377 O ? PCC0D0 375 0 Z
bit 376 I ? PCC0D0
bit 375 C 0 .
bit 374 O ? PCC0D8 372 0 Z
bit 373 I ? PCC0D8
bit 372 C 0 .
bit 371 O ? PCC0D1 375 0 Z
bit 370 I ? PCC0D1
bit 369 O ? PCC0D9 372 0 Z
bit 368 I ? PCC0D9
bit 367 O ? PCC0D2 375 0 Z
bit 366 I ? PCC0D2
bit 365 O ? PCC0D10 372 0 Z
bit 364 I ? PCC0D10
bit 363 O ? PCC0D3 375 0 Z
bit 362 I ? PCC0D3
bit 361 O ? PCC0D11 372 0 Z
bit 360 I ? PCC0D11
bit 359 O ? PCC0A25 358 0 Z
bit 358 C 0 .
bit 357 O ? PCC0A24 358 0 Z
bit 356 O ? PCC0A23 358 0 Z
bit 355 O ? PCC0A22 358 0 Z
bit 354 O ? PCC0A21 358 0 Z
bit 353 O ? PCC0A20 358 0 Z
bit 352 O ? PCC0A19 358 0 Z
bit 351 O ? PCC0A18 358 0 Z
bit 350 O ? PCC0A17 358 0 Z
bit 349 O ? PCC0A16 358 0 Z
bit 348 O ? PCC0A15 358 0 Z
bit 347 O ? PCC0A14 358 0 Z
bit 346 O ? PCC0A13 358 0 Z
bit 345 O ? PCC0RESET 358 0 Z
bit 344 O ? nPCC0ICIORDB 358 0 Z
bit 343 O ? nPCC0ICIOWRB 358 0 Z
bit 342 O ? nWEB 358 0 Z
bit 341 O ? nRDB 358 0 Z
bit 340 O ? nPCC0CE1B 358 0 Z
bit 339 O ? nPCC0CE2B 358 0 Z
bit 338 O ? nPCC0REG 358 0 Z
bit 337 O ? PCC0A12 358 0 Z
bit 336 O ? PCC0A11 358 0 Z
bit 335 O ? PCC0A10 358 0 Z
bit 334 O ? PCC0A9 358 0 Z
bit 333 O ? PCC0A8 358 0 Z
bit 332 O ? PCC0A7 358 0 Z
bit 331 O ? PCC0A6 358 0 Z
bit 330 O ? PCC0A5 358 0 Z
bit 329 O ? PCC0A4 358 0 Z
bit 328 O ? PCC0A3 358 0 Z
bit 327 O ? PCC0A2 358 0 Z
bit 326 O ? PCC0A1 358 0 Z
bit 325 O ? PCC0A0 358 0 Z
bit 324 O ? PCC0D12 372 0 Z
bit 323 I ? PCC0D12
bit 322 O ? PCC0D4 375 0 Z
bit 321 I ? PCC0D4
bit 320 O ? PCC0D13 372 0 Z
bit 319 I ? PCC0D13
bit 318 O ? PCC0D5 375 0 Z
bit 317 I ? PCC0D5
bit 316 O ? PCC0D14 372 0 Z
bit 315 I ? PCC0D14
bit 314 O ? PCC0D6 375 0 Z
bit 313 I ? PCC0D6
bit 312 O ? PCC0D15 372 0 Z
bit 311 I ? PCC0D15
bit 310 O ? PCC0D7 375 0 Z
bit 309 I ? PCC0D7
bit 308 O ? PCC1A15 307 0 Z
bit 307 C 0 .
bit 306 O ? PCC1A14 307 0 Z
bit 305 O ? PCC1A13 307 0 Z
bit 304 O ? PCC1A12 307 0 Z
bit 303 O ? PCC1A11 307 0 Z
bit 302 O ? PCC1A10 307 0 Z
bit 301 O ? PCC1A9 307 0 Z
bit 300 O ? PCC1A8 307 0 Z
bit 299 O ? PCC1A7 307 0 Z
bit 298 O ? PCC1A6 307 0 Z
bit 297 O ? PCC1A5 307 0 Z
bit 296 O ? PCC1A4 307 0 Z
bit 295 O ? PCC1A3 307 0 Z
bit 294 O ? PCC1A2 307 0 Z
bit 293 O ? PCC1A1 307 0 Z
bit 292 O ? PCC1A0 307 0 Z
bit 291 O ? PCC1D7 289 0 Z
bit 290 I ? PCC1D7
bit 289 C 0 .
bit 288 O ? PCC1D15 286 0 Z
bit 287 I ? PCC1D15
bit 286 C 0 .
bit 285 O ? PCC1D6 289 0 Z
bit 284 I ? PCC1D6
bit 283 O ? PCC1D14 286 0 Z
bit 282 I ? PCC1D14
bit 281 O ? PCC1D5 289 0 Z
bit 280 I ? PCC1D5
bit 279 O ? PCC1D13 286 0 Z
bit 278 I ? PCC1D13
bit 277 O ? PCC1D4 289 0 Z
bit 276 I ? PCC1D4
bit 275 O ? PCC1D12 286 0 Z
bit 274 I ? PCC1D12
bit 273 O ? PCC1D3 289 0 Z
bit 272 I ? PCC1D3
bit 271 O ? PCC1D11 286 0 Z
bit 270 I ? PCC1D11
bit 269 O ? PCC1D2 289 0 Z
bit 268 I ? PCC1D2
bit 267 O ? PCC1D10 286 0 Z
bit 266 I ? PCC1D10
bit 265 O ? PCC1D1 289 0 Z
bit 264 I ? PCC1D1
bit 263 O ? PCC1D9 286 0 Z
bit 262 I ? PCC1D9
bit 261 O ? PCC1D0 289 0 Z
bit 260 I ? PCC1D0
bit 259 O ? PCC1D8 286 0 Z
bit 258 I ? PCC1D8
bit 257 O ? PCC1A16 307 0 Z
bit 256 O ? PCC1A17 307 0 Z
bit 255 O ? PCC1A18 307 0 Z
bit 254 O ? PCC1A19 307 0 Z
bit 253 O ? PCC1A20 307 0 Z
bit 252 O ? PCC1A21 307 0 Z
bit 251 O ? PCC1A22 307 0 Z
bit 250 O ? PCC1A23 307 0 Z
bit 249 O ? PCC1A24 307 0 Z
bit 248 O ? PCC1A25 307 0 Z
bit 247 O ? nPCC1REG 307 0 Z
bit 246 O ? nPCC1CE2A 307 0 Z
bit 245 O ? nPCC1CE1A 307 0 Z
bit 244 O ? nRDA 307 0 Z
bit 243 O ? nWEA 307 0 Z
bit 242 O ? nPCC1ICIORDA 307 0 Z
bit 241 O ? nPCC1ICIOWRA 307 0 Z
bit 240 O ? PCC1RESET 307 0 Z
bit 239 I ? nPCC1WAIT
bit 238 I ? nPCC1WP
bit 237 I ? PCC1RDY
bit 236 I ? PCC1BVD1
bit 235 I ? PCC1BVD2
bit 234 I ? nPCC1VS1
bit 233 I ? nPCC1VS2
bit 232 I ? nPCC1CD1
bit 231 I ? nPCC1CD2
bit 230 O ? VCC1VPP0
bit 229 O ? VCC1VPP1
bit 228 O ? VCC1SEL0
bit 227 O ? VCC1SEL1
bit 226 O ? NC(14) 224 0 Z
bit 225 I ? NC(14)
bit 224 C 0 .
bit 223 O ? NC(13) 221 0 Z
bit 222 I ? NC(13)
bit 221 C 0 .
bit 220 O ? NC(12) 218 0 Z
bit 219 I ? NC(12)
bit 218 C 0 .
bit 217 O ? NC(11) 215 0 Z
bit 216 I ? NC(11)
bit 215 C 0 .
bit 214 O ? NC(10) 212 0 Z
bit 213 I ? NC(10)
bit 212 C 0 .
bit 211 O ? NC(9) 209 0 Z
bit 210 I ? NC(9)
bit 209 C 0 .
bit 208 O ? NC(8) 206 0 Z
bit 207 I ? NC(8)
bit 206 C 0 .
bit 205 O ? NC(7) 203 0 Z
bit 204 I ? NC(7)
bit 203 C 0 .
bit 202 O ? NC(6) 200 0 Z
bit 201 I ? NC(6)
bit 200 C 0 .
bit 199 O ? NC(5) 197 0 Z
bit 198 I ? NC(5)
bit 197 C 0 .
bit 196 O ? NC(4) 194 0 Z
bit 195 I ? NC(4)
bit 194 C 0 .
bit 193 O ? NC(3) 191 0 Z
bit 192 I ? NC(3)
bit 191 C 0 .
bit 190 O ? NC(2) 188 0 Z
bit 189 I ? NC(2)
bit 188 C 0 .
bit 187 O ? NC(1) 185 0 Z
bit 186 I ? NC(1)
bit 185 C 0 .
bit 184 O ? PWM0 182 0 Z
bit 183 I ? PWM0
bit 182 C 0 .
bit 181 O ? nRESETMI 179 0 Z
bit 180 I ? nRESETMI
bit 179 C 0 .
bit 178 O ? nRESETPO 176 0 Z
bit 177 I ? nRESETPO
bit 176 C 0 .
bit 175 O ? nRESETMO 173 0 Z
bit 174 I ? nRESETMO
bit 173 C 0 .
bit 172 O ? PWM1 170 0 Z
bit 171 I ? PWM1
bit 170 C 0 .
bit 169 O ? KBCK 167 0 Z
bit 168 I ? KBCK
bit 167 C 0 .
bit 166 O ? KBDATA 164 0 Z
bit 165 I ? KBDATA
bit 164 C 0 .
bit 163 O ? MSCK 161 0 Z
bit 162 I ? MSCK
bit 161 C 0 .
bit 160 O ? MSDATA 158 0 Z
bit 159 I ? MSDATA
bit 158 C 0 .
bit 157 O ? PE7 155 0 Z
bit 156 I ? PE7
bit 155 C 0 .
bit 154 O ? PE6 152 0 Z
bit 153 I ? PE6
bit 152 C 0 .
bit 151 O ? PE5 149 0 Z
bit 150 I ? PE5
bit 149 C 0 .
bit 148 O ? PE4 146 0 Z
bit 147 I ? PE4
bit 146 C 0 .
bit 145 O ? PE3 143 0 Z
bit 144 I ? PE3
bit 143 C 0 .
bit 142 O ? PE2 140 0 Z
bit 141 I ? PE2
bit 140 C 0 .
bit 139 O ? PE1 137 0 Z
bit 138 I ? PE1
bit 137 C 0 .
bit 136 O ? PE0 134 0 Z
bit 135 I ? PE0
bit 134 C 0 .
bit 133 O ? PD7 131 0 Z
bit 132 I ? PD7
bit 131 C 0 .
bit 130 O ? PD6 128 0 Z
bit 129 I ? PD6
bit 128 C 0 .
bit 127 O ? PD5 125 0 Z
bit 126 I ? PD5
bit 125 C 0 .
bit 124 O ? PD4 122 0 Z
bit 123 I ? PD4
bit 122 C 0 .
bit 121 O ? PD3 119 0 Z
bit 120 I ? PD3
bit 119 C 0 .
bit 118 O ? PD2 116 0 Z
bit 117 I ? PD2
bit 116 C 0 .
bit 115 O ? PD1 113 0 Z
bit 114 I ? PD1
bit 113 C 0 .
bit 112 O ? PD0 110 0 Z
bit 111 I ? PD0
bit 110 C 0 .
bit 109 O ? PC7 107 0 Z
bit 108 I ? PC7
bit 107 C 0 .
bit 106 O ? PC6 104 0 Z
bit 105 I ? PC6
bit 104 C 0 .
bit 103 O ? PC5 101 0 Z
bit 102 I ? PC5
bit 101 C 0 .
bit 100 O ? PC4 98 0 Z
bit 99 I ? PC4
bit 98 C 0 .
bit 97 I ? RXD0
bit 96 I ? nCTS0
bit 95 I ? nDSR0
bit 94 I ? nDCD0
bit 93 I ? nRI0
bit 92 O ? TXD0
bit 91 O ? nRTS0
bit 90 O ? nDTR0
bit 89 O ? PC3 87 0 Z
bit 88 I ? PC3
bit 87 C 0 .
bit 86 O ? PC2 84 0 Z
bit 85 I ? PC2
bit 84 C 0 .
bit 83 O ? PC1 81 0 Z
bit 82 I ? PC1
bit 81 C 0 .
bit 80 O ? PC0 78 0 Z
bit 79 I ? PC0
bit 78 C 0 .
bit 77 O ? nUSBPEN 75 0 Z
bit 76 I ? nUSBPEN
bit 75 C 0 .
bit 74 I ? nUSBOVR
bit 73 O ? MODSEL 71 0 Z
bit 72 I ? MODSEL
bit 71 C 0 .
bit 70 O ? TXD
bit 69 O ? nRX 67 0 Z
bit 68 I ? nRX
bit 67 C 0 .
bit 66 O ? PPD0 64 0 Z
bit 65 I ? PPD0
bit 64 C 0 .
bit 63 O ? PPD1 64 0 Z
bit 62 I ? PPD1
bit 61 O ? PPD2 64 0 Z
bit 60 I ? PPD2
bit 59 O ? PPD3 64 0 Z
bit 58 I ? PPD3
bit 57 O ? nINIT 56 0 Z
bit 56 C 0 .
bit 55 I ? nERR
bit 54 O ? nAFD 56 0 Z
bit 53 O ? nSTB 56 0 Z
bit 52 I ? SLCT
bit 51 I ? PE
bit 50 I ? BUSY
bit 49 I ? nACK
bit 48 O ? nSLIN 56 0 Z
bit 47 O ? PPD4 64 0 Z
bit 46 I ? PPD4
bit 45 O ? PPD5 64 0 Z
bit 44 I ? PPD5
bit 43 O ? PPD6 64 0 Z
bit 42 I ? PPD6
bit 41 O ? PPD7 64 0 Z
bit 40 I ? PPD7
bit 39 O ? PB0 37 0 Z
bit 38 I ? PB0
bit 37 C 0 .
bit 36 O ? PB1 34 0 Z
bit 35 I ? PB1
bit 34 C 0 .
bit 33 O ? PB2 31 0 Z
bit 32 I ? PB2
bit 31 C 0 .
bit 30 O ? PB3 28 0 Z
bit 29 I ? PB3
bit 28 C 0 .
bit 27 O ? PB4 25 0 Z
bit 26 I ? PB4
bit 25 C 0 .
bit 24 O ? PB5 22 0 Z
bit 23 I ? PB5
bit 22 C 0 .
bit 21 O ? PB6 19 0 Z
bit 20 I ? PB6
bit 19 C 0 .
bit 18 O ? PB7 16 0 Z
bit 17 I ? PB7
bit 16 C 0 .
bit 15 O ? nACPD 13 0 Z
bit 14 I ? nACPD
bit 13 C 0 .
bit 12 O ? ACCLK 11 0 Z
bit 11 C 0 .
bit 10 I ? SIBDIN
bit 9 O ? SIBCLK 7 0 Z
bit 8 I ? SIBCLK
bit 7 C 0 .
bit 6 O ? SIBDOUT 5 0 Z
bit 5 C 0 .
bit 4 O ? SIBSYNC 2 0 Z
bit 3 I ? SIBSYNC
bit 2 C 0 .
bit 1 O ? nACRST 0 0 Z
bit 0 C 0 .
