signal TCK
signal TDI
signal TDO
signal TMS
signal PAD101
signal PAD102
signal PAD60
signal PAD61
signal PAD104
signal IPAD93
signal PAD62
signal PAD105
signal PAD63
signal PAD106
signal PAD107
signal IPAD204
signal PAD109
signal IPAD98
signal PAD66
signal PAD67
signal IPAD209
signal PAD181
signal PAD185
signal PAD186
signal PAD187
signal PAD188
signal IPAD28
signal IPAD29
signal PAD110
signal PAD111
signal PAD71
signal PAD113
signal PAD72
signal PAD114
signal PAD115
signal PAD116
signal PAD74
signal PAD117
signal PAD75
signal PAD118
signal IPAD214
signal IPAD144
signal IPAD145
signal PAD79
signal PAD190
signal PAD191
signal PAD192
signal PAD193
signal PAD195
signal PAD196
signal PAD197
signal PAD198
signal IPAD35
signal IPAD36
signal DONE
signal PAD120
signal PAD121
signal PAD80
signal PAD122
signal PAD81
signal PAD123
signal PAD82
signal PAD124
signal PAD84
signal PAD127
signal PAD85
signal PAD128
signal IPAD151
signal PAD86
signal IPAD152
signal PAD87
signal IPAD228
signal PAD89
signal IPAD3
signal IPAD9
signal PAD11
signal PAD12
signal IPAD46
signal PAD16
signal PAD17
signal PAD19
signal PAD200
signal PAD201
signal PAD202
signal PAD203
signal PAD130
signal PAD131
signal PAD205
signal PAD132
signal PAD90
signal PAD206
signal PAD133
signal PAD91
signal PAD207
signal PAD208
signal PAD92
signal PAD94
signal PAD95
signal IPAD162
signal PAD139
signal PAD96
signal PAD97
signal PAD20
signal PAD23
signal IPAD54
signal PAD24
signal IPAD55
signal PAD25
signal PAD26
signal PAD27
signal IPAD58
signal IPAD59
signal PAD210
signal PAD211
signal PAD212
signal PAD213
signal PAD140
signal PAD141
signal PAD142
signal PAD143
signal PAD217
signal PAD218
signal PAD146
signal IPAD170
signal PAD147
signal IPAD171
signal PAD148
signal PAD149
signal IPAD174
signal IPAD175
signal PAD30
signal PAD31
signal PAD32
signal IPAD64
signal PAD33
signal PAD34
signal PAD1
signal PAD2
signal IPAD68
signal PAD4
signal PAD5
signal PAD6
signal PAD220
signal PAD7
signal PAD221
signal PAD8
signal PAD222
signal PAD150
signal PAD223
signal PAD225
signal PAD153
signal PAD154
signal PAD156
signal PAD229
signal PAD157
signal IPAD184
signal PAD40
signal PAD41
signal IPAD112
signal IPAD78
signal PAD47
signal PAD48
signal PAD49
signal PAD230
signal PAD231
signal PAD232
signal IPAD119
signal PAD163
signal PAD164
signal PAD165
signal PAD166
signal PAD167
signal PAD168
signal PAD169
signal PROG_B
signal IPAD194
signal IPAD199
signal PAD50
signal PAD51
signal IPAD83
signal PAD52
signal PAD53
signal IPAD88
signal PAD56
signal PAD57
signal IPAD125
signal IPAD126
signal IPAD129
signal PAD172
signal IPAD10
signal PAD173
signal PAD176
signal IPAD13
signal PAD177
signal PAD178
signal PAD179
signal GND0
signal GND1
signal GND2
signal GND3
signal GND4
signal GND5
signal GND6
signal GND7
signal GND8
signal GND9
signal GND10
signal GND11
signal GND12
signal GND13
signal GND14
signal GND15
signal GND16
signal GND17
signal GND18
signal GND19
signal GND20
signal GND21
signal GND22
signal GND23
signal GND24
signal GND25
signal GND26
signal VDD0
signal VDD1
signal VDD2
signal VDD3
signal VDD4
signal VDD5
signal VDD6
signal VDD7
signal VDD8
signal VDD9
signal VDD10
signal VDD11
signal VDD12
signal VDD13
signal VDD14
signal VDD15
signal VDD16
signal VDD17
signal VDD18
signal VDD19
signal VDD20
signal VDD21
signal VDD22
signal VDD23
signal Vaux0
signal Vaux1
signal Vaux2
signal Vaux3
signal Vaux4
signal Vaux5

register	BSR	588
register	BR	1
register	DIR	32

instruction length 6

instruction SAMPLE/PRELOAD 100000 BSR
instruction IDCODE 100100 DIR
instruction EXTEST 111100 BSR
instruction BYPASS 111111 BR

bit 587 I 1 IPAD59
bit 586 I 1 PAD60
bit 585 O 1 PAD60 584 0 Z
bit 584 C 0 *
bit 583 I 1 PAD61
bit 582 O 1 PAD61 581 0 Z
bit 581 C 0 *
bit 580 I 1 PAD62
bit 579 O 1 PAD62 578 0 Z
bit 578 C 0 *
bit 577 I 1 PAD63
bit 576 O 1 PAD63 575 0 Z
bit 575 C 0 *
bit 574 I 1 IPAD64
bit 573 O 1 *
bit 572 O 1 *
bit 571 O 1 *
bit 570 I 1 PAD66
bit 569 O 1 PAD66 568 0 Z
bit 568 C 0 *
bit 567 I 1 PAD67
bit 566 O 1 PAD67 565 0 Z
bit 565 C 0 *
bit 564 I 1 IPAD68
bit 563 O 1 *
bit 562 O 1 *
bit 561 O 1 *
bit 560 O 1 *
bit 559 O 1 *
bit 558 O 1 *
bit 557 I 1 PAD71
bit 556 O 1 PAD71 555 0 Z
bit 555 C 0 *
bit 554 I 1 PAD72
bit 553 O 1 PAD72 552 0 Z
bit 552 C 0 *
bit 551 O 1 *
bit 550 I 1 PAD74
bit 549 O 1 PAD74 548 0 Z
bit 548 C 0 *
bit 547 I 1 PAD75
bit 546 O 1 PAD75 545 0 Z
bit 545 C 0 *
bit 544 O 1 *
bit 543 O 1 *
bit 542 O 1 *
bit 541 O 1 *
bit 540 O 1 *
bit 539 O 1 *
bit 538 I 1 IPAD78
bit 537 I 1 PAD79
bit 536 O 1 PAD79 535 0 Z
bit 535 C 0 *
bit 534 I 1 PAD80
bit 533 O 1 PAD80 532 0 Z
bit 532 C 0 *
bit 531 I 1 PAD81
bit 530 O 1 PAD81 529 0 Z
bit 529 C 0 *
bit 528 I 1 PAD82
bit 527 O 1 PAD82 526 0 Z
bit 526 C 0 *
bit 525 I 1 IPAD83
bit 524 I 1 PAD84
bit 523 O 1 PAD84 522 0 Z
bit 522 C 0 *
bit 521 I 1 PAD85
bit 520 O 1 PAD85 519 0 Z
bit 519 C 0 *
bit 518 I 1 PAD86
bit 517 O 1 PAD86 516 0 Z
bit 516 C 0 *
bit 515 I 1 PAD87
bit 514 O 1 PAD87 513 0 Z
bit 513 C 0 *
bit 512 I 1 IPAD88
bit 511 I 1 PAD89
bit 510 O 1 PAD89 509 0 Z
bit 509 C 0 *
bit 508 I 1 PAD90
bit 507 O 1 PAD90 506 0 Z
bit 506 C 0 *
bit 505 I 1 PAD91
bit 504 O 1 PAD91 503 0 Z
bit 503 C 0 *
bit 502 I 1 PAD92
bit 501 O 1 PAD92 500 0 Z
bit 500 C 0 *
bit 499 I 1 IPAD93
bit 498 I 1 PAD94
bit 497 O 1 PAD94 496 0 Z
bit 496 C 0 *
bit 495 I 1 PAD95
bit 494 O 1 PAD95 493 0 Z
bit 493 C 0 *
bit 492 I 1 PAD96
bit 491 O 1 PAD96 490 0 Z
bit 490 C 0 *
bit 489 I 1 PAD97
bit 488 O 1 PAD97 487 0 Z
bit 487 C 0 *
bit 486 I 1 IPAD98
bit 485 O 1 *
bit 484 O 1 *
bit 483 O 1 *
bit 482 O 1 *
bit 481 O 1 *
bit 480 O 1 *
bit 479 I 1 PAD101
bit 478 O 1 PAD101 477 0 Z
bit 477 C 0 *
bit 476 I 1 PAD102
bit 475 O 1 PAD102 474 0 Z
bit 474 C 0 *
bit 473 O 1 *
bit 472 I 1 PAD104
bit 471 O 1 PAD104 470 0 Z
bit 470 C 0 *
bit 469 I 1 PAD105
bit 468 O 1 PAD105 467 0 Z
bit 467 C 0 *
bit 466 I 1 PAD106
bit 465 O 1 PAD106 464 0 Z
bit 464 C 0 *
bit 463 I 1 PAD107
bit 462 O 1 PAD107 461 0 Z
bit 461 C 0 *
bit 460 O 1 *
bit 459 I 1 PAD109
bit 458 O 1 *
bit 457 O 1 *
bit 456 I 1 PAD110
bit 455 O 1 *
bit 454 O 1 *
bit 453 I 1 PAD111
bit 452 O 1 *
bit 451 O 1 *
bit 450 I 1 IPAD112
bit 449 I 1 PAD113
bit 448 O 1 *
bit 447 O 1 *
bit 446 I 1 PAD114
bit 445 O 1 *
bit 444 O 1 *
bit 443 I 1 PAD115
bit 442 O 1 *
bit 441 O 1 *
bit 440 I 1 PAD116
bit 439 O 1 *
bit 438 O 1 *
bit 437 I 1 DONE
bit 436 O 1 PAD109 435 0 Z
bit 435 C 0 *
bit 434 I 1 PAD117
bit 433 O 1 PAD110 432 0 Z
bit 432 C 0 *
bit 431 I 1 PAD118
bit 430 O 1 *
bit 429 O 1 *
bit 428 I 1 IPAD119
bit 427 I 1 PAD120
bit 426 O 1 *
bit 425 O 1 *
bit 424 I 1 PAD121
bit 423 O 1 *
bit 422 O 1 *
bit 421 I 1 PAD122
bit 420 O 1 *
bit 419 O 1 *
bit 418 I 1 PAD123
bit 417 O 1 *
bit 416 O 1 *
bit 415 I 1 PAD124
bit 414 O 1 *
bit 413 O 1 *
bit 412 I 1 IPAD125
bit 411 I 1 IPAD126
bit 410 I 1 PAD127
bit 409 O 1 *
bit 408 O 1 *
bit 407 I 1 PAD128
bit 406 O 1 *
bit 405 O 1 *
bit 404 I 1 IPAD129
bit 403 I 1 PAD130
bit 402 O 1 *
bit 401 O 1 *
bit 400 I 1 PAD131
bit 399 O 1 *
bit 398 O 1 *
bit 397 I 1 PAD132
bit 396 O 1 *
bit 395 O 1 *
bit 394 I 1 PAD133
bit 393 O 1 *
bit 392 O 1 *
bit 391 O 1 *
bit 390 O 1 *
bit 389 O 1 *
bit 388 O 1 *
bit 387 O 1 *
bit 386 O 1 *
bit 385 O 1 *
bit 384 O 1 *
bit 383 O 1 *
bit 382 O 1 *
bit 381 O 1 *
bit 380 I 1 PAD139
bit 379 O 1 *
bit 378 O 1 *
bit 377 I 1 PAD140
bit 376 O 1 *
bit 375 O 1 *
bit 374 I 1 PAD141
bit 373 O 1 *
bit 372 O 1 *
bit 371 I 1 PAD142
bit 370 O 1 PAD113 369 0 Z
bit 369 C 0 *
bit 368 I 1 PAD143
bit 367 O 1 IPAD112 366 0 Z
bit 366 C 0 *
bit 365 I 1 IPAD144
bit 364 I 1 IPAD145
bit 363 I 1 PAD146
bit 362 O 1 *
bit 361 O 1 *
bit 360 I 1 PAD147
bit 359 O 1 *
bit 358 O 1 *
bit 357 I 1 PAD148
bit 356 O 1 *
bit 355 O 1 *
bit 354 I 1 PAD149
bit 353 O 1 *
bit 352 O 1 *
bit 351 I 1 PAD150
bit 350 O 1 *
bit 349 O 1 *
bit 348 I 1 IPAD151
bit 347 I 1 IPAD152
bit 346 I 1 PAD153
bit 345 O 1 *
bit 344 O 1 *
bit 343 I 1 PAD154
bit 342 O 1 *
bit 341 O 1 *
bit 340 O 1 *
bit 339 O 1 *
bit 338 O 1 *
bit 337 I 1 PAD156
bit 336 O 1 *
bit 335 O 1 *
bit 334 I 1 PAD157
bit 333 O 1 *
bit 332 O 1 *
bit 331 O 1 *
bit 330 O 1 *
bit 329 O 1 *
bit 328 O 1 *
bit 327 O 1 *
bit 326 O 1 *
bit 325 O 1 *
bit 324 O 1 *
bit 323 I 1 IPAD162
bit 322 I 1 PAD163
bit 321 O 1 *
bit 320 O 1 *
bit 319 I 1 PAD164
bit 318 O 1 *
bit 317 O 1 *
bit 316 I 1 PAD165
bit 315 O 1 *
bit 314 O 1 *
bit 313 I 1 PAD166
bit 312 O 1 *
bit 311 O 1 *
bit 310 I 1 PAD167
bit 309 O 1 *
bit 308 O 1 *
bit 307 I 1 PAD168
bit 306 O 1 *
bit 305 O 1 *
bit 304 I 1 PAD169
bit 303 O 1 *
bit 302 O 1 *
bit 301 I 1 IPAD170
bit 300 I 1 IPAD171
bit 299 I 1 PAD172
bit 298 O 1 *
bit 297 O 1 *
bit 296 I 1 PAD173
bit 295 O 1 *
bit 294 O 1 *
bit 293 I 1 IPAD174
bit 292 I 1 IPAD175
bit 291 I 1 PAD176
bit 290 O 1 *
bit 289 O 1 *
bit 288 I 1 PAD177
bit 287 O 1 *
bit 286 O 1 *
bit 285 I 1 PAD178
bit 284 O 1 *
bit 283 O 1 *
bit 282 I 1 PAD179
bit 281 O 1 *
bit 280 O 1 *
bit 279 O 1 *
bit 278 I 1 PAD181
bit 277 O 1 *
bit 276 O 1 *
bit 275 O 1 *
bit 274 O 1 *
bit 273 O 1 *
bit 272 O 1 *
bit 271 O 1 *
bit 270 O 1 *
bit 269 I 1 IPAD184
bit 268 I 1 PAD185
bit 267 O 1 *
bit 266 O 1 *
bit 265 I 1 PAD186
bit 264 O 1 *
bit 263 O 1 *
bit 262 I 1 PAD187
bit 261 O 1 *
bit 260 O 1 *
bit 259 I 1 PAD188
bit 258 O 1 *
bit 257 O 1 *
bit 256 O 1 *
bit 255 I 1 PAD190
bit 254 O 1 *
bit 253 O 1 *
bit 252 I 1 PAD191
bit 251 O 1 *
bit 250 O 1 *
bit 249 I 1 PAD192
bit 248 O 1 *
bit 247 O 1 *
bit 246 I 1 PAD193
bit 245 O 1 *
bit 244 O 1 *
bit 243 I 1 IPAD194
bit 242 I 1 PAD195
bit 241 O 1 *
bit 240 O 1 *
bit 239 I 1 PAD196
bit 238 O 1 *
bit 237 O 1 *
bit 236 I 1 PAD197
bit 235 O 1 *
bit 234 O 1 *
bit 233 I 1 PAD198
bit 232 O 1 *
bit 231 O 1 *
bit 230 I 1 IPAD199
bit 229 I 1 PAD200
bit 228 O 1 *
bit 227 O 1 *
bit 226 I 1 PAD201
bit 225 O 1 *
bit 224 O 1 *
bit 223 I 1 PAD202
bit 222 O 1 *
bit 221 O 1 *
bit 220 I 1 PAD203
bit 219 O 1 *
bit 218 O 1 *
bit 217 I 1 IPAD204
bit 216 I 1 PAD205
bit 215 O 1 *
bit 214 O 1 *
bit 213 I 1 PAD206
bit 212 O 1 *
bit 211 O 1 *
bit 210 I 1 PAD207
bit 209 O 1 *
bit 208 O 1 *
bit 207 I 1 PAD208
bit 206 O 1 *
bit 205 O 1 *
bit 204 I 1 IPAD209
bit 203 I 1 PAD210
bit 202 O 1 *
bit 201 O 1 *
bit 200 I 1 PAD211
bit 199 O 1 *
bit 198 O 1 *
bit 197 I 1 PAD212
bit 196 O 1 *
bit 195 O 1 *
bit 194 I 1 PAD213
bit 193 O 1 *
bit 192 O 1 *
bit 191 I 1 IPAD214
bit 190 O 1 *
bit 189 O 1 *
bit 188 O 1 *
bit 187 O 1 *
bit 186 O 1 *
bit 185 O 1 *
bit 184 I 1 PAD217
bit 183 O 1 *
bit 182 O 1 *
bit 181 I 1 PAD218
bit 180 O 1 *
bit 179 O 1 *
bit 178 O 1 *
bit 177 I 1 PAD220
bit 176 O 1 *
bit 175 O 1 *
bit 174 I 1 PAD221
bit 173 O 1 *
bit 172 O 1 *
bit 171 I 1 PAD222
bit 170 O 1 *
bit 169 O 1 *
bit 168 I 1 PAD223
bit 167 O 1 *
bit 166 O 1 *
bit 165 O 1 *
bit 164 I 1 PAD225
bit 163 O 1 *
bit 162 O 1 *
bit 161 O 1 *
bit 160 O 1 *
bit 159 O 1 *
bit 158 O 1 *
bit 157 O 1 *
bit 156 O 1 *
bit 155 I 1 IPAD228
bit 154 I 1 PAD229
bit 153 O 1 *
bit 152 O 1 *
bit 151 I 1 PAD230
bit 150 O 1 *
bit 149 O 1 *
bit 148 I 1 PAD231
bit 147 O 1 *
bit 146 O 1 *
bit 145 I 1 PAD232
bit 144 O 1 *
bit 143 O 1 *
bit 142 I 1 PROG_B
bit 141 I 1 PAD1
bit 140 O 1 PAD1 139 0 Z
bit 139 C 0 *
bit 138 I 1 PAD2
bit 137 O 1 PAD2 136 0 Z
bit 136 C 0 *
bit 135 I 1 IPAD3
bit 134 I 1 PAD4
bit 133 O 1 PAD4 132 0 Z
bit 132 C 0 *
bit 131 I 1 PAD5
bit 130 O 1 PAD5 129 0 Z
bit 129 C 0 *
bit 128 I 1 PAD6
bit 127 O 1 PAD6 126 0 Z
bit 126 C 0 *
bit 125 I 1 PAD7
bit 124 O 1 PAD7 123 0 Z
bit 123 C 0 *
bit 122 I 1 PAD8
bit 121 O 1 PAD8 120 0 Z
bit 120 C 0 *
bit 119 I 1 IPAD9
bit 118 I 1 IPAD10
bit 117 I 1 PAD11
bit 116 O 1 PAD11 115 0 Z
bit 115 C 0 *
bit 114 I 1 PAD12
bit 113 O 1 PAD12 112 0 Z
bit 112 C 0 *
bit 111 I 1 IPAD13
bit 110 O 1 *
bit 109 O 1 *
bit 108 O 1 *
bit 107 O 1 *
bit 106 O 1 *
bit 105 O 1 *
bit 104 I 1 PAD16
bit 103 O 1 PAD16 102 0 Z
bit 102 C 0 *
bit 101 I 1 PAD17
bit 100 O 1 PAD17 99 0 Z
bit 99 C 0 *
bit 98 O 1 *
bit 97 O 1 *
bit 96 O 1 *
bit 95 I 1 PAD19
bit 94 O 1 PAD19 93 0 Z
bit 93 C 0 *
bit 92 I 1 PAD20
bit 91 O 1 PAD20 90 0 Z
bit 90 C 0 *
bit 89 O 1 *
bit 88 O 1 *
bit 87 I 1 PAD23
bit 86 O 1 PAD23 85 0 Z
bit 85 C 0 *
bit 84 I 1 PAD24
bit 83 O 1 PAD24 82 0 Z
bit 82 C 0 *
bit 81 I 1 PAD25
bit 80 O 1 PAD25 79 0 Z
bit 79 C 0 *
bit 78 I 1 PAD26
bit 77 O 1 PAD26 76 0 Z
bit 76 C 0 *
bit 75 I 1 PAD27
bit 74 O 1 PAD27 73 0 Z
bit 73 C 0 *
bit 72 I 1 IPAD28
bit 71 I 1 IPAD29
bit 70 I 1 PAD30
bit 69 O 1 PAD30 68 0 Z
bit 68 C 0 *
bit 67 I 1 PAD31
bit 66 O 1 PAD31 65 0 Z
bit 65 C 0 *
bit 64 I 1 PAD32
bit 63 O 1 PAD32 62 0 Z
bit 62 C 0 *
bit 61 I 1 PAD33
bit 60 O 1 PAD33 59 0 Z
bit 59 C 0 *
bit 58 I 1 PAD34
bit 57 O 1 PAD34 56 0 Z
bit 56 C 0 *
bit 55 I 1 IPAD35
bit 54 I 1 IPAD36
bit 53 O 1 *
bit 52 O 1 *
bit 51 O 1 *
bit 50 O 1 *
bit 49 O 1 *
bit 48 O 1 *
bit 47 O 1 *
bit 46 O 1 *
bit 45 O 1 *
bit 44 I 1 PAD40
bit 43 O 1 PAD40 42 0 Z
bit 42 C 0 *
bit 41 I 1 PAD41
bit 40 O 1 PAD41 39 0 Z
bit 39 C 0 *
bit 38 O 1 *
bit 37 O 1 *
bit 36 O 1 *
bit 35 O 1 *
bit 34 O 1 *
bit 33 O 1 *
bit 32 O 1 *
bit 31 O 1 *
bit 30 I 1 IPAD46
bit 29 I 1 PAD47
bit 28 O 1 PAD47 27 0 Z
bit 27 C 0 *
bit 26 I 1 PAD48
bit 25 O 1 PAD48 24 0 Z
bit 24 C 0 *
bit 23 I 1 PAD49
bit 22 O 1 PAD49 21 0 Z
bit 21 C 0 *
bit 20 I 1 PAD50
bit 19 O 1 PAD50 18 0 Z
bit 18 C 0 *
bit 17 I 1 PAD51
bit 16 O 1 PAD51 15 0 Z
bit 15 C 0 *
bit 14 I 1 PAD52
bit 13 O 1 PAD52 12 0 Z
bit 12 C 0 *
bit 11 I 1 PAD53
bit 10 O 1 PAD53 9 0 Z
bit 9 C 0 *
bit 8 I 1 IPAD54
bit 7 I 1 IPAD55
bit 6 I 1 PAD56
bit 5 O 1 PAD56 4 0 Z
bit 4 C 0 *
bit 3 I 1 PAD57
bit 2 O 1 PAD57 1 0 Z
bit 1 C 0 *
bit 0 I 1 IPAD58
