signal ABE_B0
signal ABE_B1
signal ADDR1
signal ADDR2
signal ADDR3
signal ADDR4
signal ADDR5
signal ADDR6
signal ADDR7
signal ADDR8
signal ADDR9
signal ADDR10
signal ADDR11
signal ADDR12
signal ADDR13
signal ADDR14
signal ADDR15
signal ADDR16
signal ADDR17
signal ADDR18
signal ADDR19
signal AMS_B0
signal AMS_B1
signal AMS_B2
signal AMS_B3
signal AOE_B
signal ARDY
signal ARE_B
signal AWE_B
signal BG_B
signal BGH_B
signal BMODE0
signal BMODE1
signal BR_B
signal CANRX
signal CANTX
signal CLKIN
signal CLKOUT
signal DATA0
signal DATA1
signal DATA2
signal DATA3
signal DATA4
signal DATA5
signal DATA6
signal DATA7
signal DATA8
signal DATA9
signal DATA10
signal DATA11
signal DATA12
signal DATA13
signal DATA14
signal DATA15
signal DR0PRI
signal DR0SEC
signal DR1PRI
signal DR1SEC
signal DR2PRI
signal DR2SEC
signal DR3PRI
signal DR3SEC
signal DT0PRI
signal DT0SEC
signal DT1PRI
signal DT1SEC
signal DT2PRI
signal DT2SEC
signal DT3PRI
signal DT3SEC
signal EMU_B
signal FCE_B
signal FRESET_B
signal GND0
signal GND1
signal GND2
signal GND3
signal GND4
signal GND5
signal GND6
signal GND7
signal GND8
signal GND9
signal GND10
signal GND11
signal GND12
signal GND13
signal GND14
signal GND15
signal GND16
signal GND17
signal GND18
signal GND19
signal GND20
signal GND21
signal GND22
signal GND23
signal GND24
signal GND25
signal GND26
signal GND27
signal GND28
signal GND29
signal GND30
signal GND31
signal GND32
signal GND33
signal GND34
signal GND35
signal GND36
signal GND37
signal GND38
signal GND39
signal GND40
signal GND41
signal GND42
signal GND43
signal GND44
signal GND45
signal GND46
signal GND47
signal GND48
signal GND49
signal GND50
signal GND51
signal GND52
signal GND53
signal GND54
signal GND55
signal GND56
signal GND57
signal GND58
signal GND59
signal GND60
signal GND61
signal GND62
signal GND63
signal GND64
signal GND65
signal GND66
signal GND67
signal GND68
signal GND69
signal GND70
signal GND71
signal GND72
signal GND73
signal GND74
signal GND75
signal GND76
signal GND77
signal GND78
signal GND79
signal GND80
signal GND81
signal GND82
signal GND83
signal GND84
signal GND85
signal GND86
signal GND87
signal GND88
signal GND89
signal GND90
signal GND91
signal GND92
signal GND93
signal GND94
signal GND95
signal GND96
signal GND97
signal GND98
signal GND99
signal GND100
signal GND101
signal GND102
signal GND103
signal GND104
signal GND105
signal GND106
signal GND107
signal GND108
signal GND109
signal GND110
signal GND111
signal GND112
signal GND113
signal GND114
signal GND115
signal GND116
signal GND117
signal GND118
signal GP
signal GPW_B
signal MISO0
signal MISO1
signal MISO2
signal MOSI0
signal MOSI1
signal MOSI2
signal PC4
signal PC6
signal PC7
signal PC8
signal PC5
signal NC
signal NMI_B
signal PC9
signal PF0
signal PF1
signal PF2
signal PF3
signal PF4
signal PF5
signal PF6
signal PF7
signal PF8
signal PF9
signal PF10
signal PF11
signal PF12
signal PF13
signal PF14
signal PF15
signal PPI_CLK
signal PPI0
signal PPI1
signal PPI2
signal PPI3
signal RESET_B
signal RFS0
signal RFS1
signal RFS2
signal RFS3
signal RSCLK0
signal RSCLK1
signal RSCLK2
signal RSCLK3
signal RTXI
signal RTXO
signal RX0
signal RX1
signal RX2
signal SA10
signal SCAS_B
signal SCK0
signal SCK1
signal SCK2
signal SCKE
signal SCL0
signal SCL1
signal SDA0
signal SDA1
signal SMS_B
signal SPI1SS_B
signal SPI1SEL1_B
signal SPI2SS_B
signal SPI2SEL1_B
signal SRAS_B
signal SWE_B
signal TCK
signal TDI
signal TDO
signal TFS0
signal TFS1
signal TFS2
signal TFS3
signal TMR0
signal TMR1
signal TMR2
signal TMS
signal TRST_B
signal TSCLK0
signal TSCLK1
signal TSCLK2
signal TSCLK3
signal TX0
signal TX1
signal TX2
signal VDDEXT0
signal VDDEXT1
signal VDDEXT2
signal VDDEXT3
signal VDDEXT4
signal VDDEXT5
signal VDDEXT6
signal VDDEXT7
signal VDDEXT8
signal VDDEXT9
signal VDDEXT10
signal VDDEXT11
signal VDDEXT12
signal VDDEXT13
signal VDDEXT14
signal VDDEXT15
signal VDDEXT16
signal VDDEXT17
signal VDDEXT18
signal VDDEXT19
signal VDDINT0
signal VDDINT1
signal VDDINT2
signal VDDINT3
signal VDDINT4
signal VDDINT5
signal VDDINT6
signal VDDINT7
signal VDDINT8
signal VDDINT9
signal VDDINT10
signal VDDINT11
signal VDDRTC
signal VROUT0
signal VROUT1

register	BSR	325
register	BR	1
register	DIR	32
register	DBGSTAT	16
register	DBGCTL	16
register	EMUIR	32
register	EMUDAT	32
register	EMUPC	32

instruction length 5

instruction BYPASS 11111 BR
instruction EXTEST 00000 BSR
instruction SAMPLE/PRELOAD 10000 BSR
instruction IDCODE 00010 DIR
instruction DBGSTAT_SCAN 01100 DBGSTAT
instruction DBGCTL_SCAN 00100 DBGCTL
instruction EMUIR_SCAN 01000 EMUIR
instruction EMUDAT_SCAN 10100 EMUDAT
instruction EMUPC_SCAN 11110 EMUPC

bit 324 C 0 *
bit 323 O 1 DATA0 324 0 Z
bit 322 I 1 DATA0
bit 321 O 1 DATA1 324 0 Z
bit 320 I 1 DATA1
bit 319 O 1 DATA2 324 0 Z
bit 318 I 1 DATA2
bit 317 C 0 *
bit 316 O 1 TSCLK2 317 0 Z
bit 315 I 1 TSCLK2
bit 314 C 0 *
bit 313 O 1 DR2SEC 314 0 Z
bit 312 I 1 DR2SEC
bit 311 C 0 *
bit 310 O 1 DR2PRI 311 0 Z
bit 309 I 1 DR2PRI
bit 308 O 1 DATA3 324 0 Z
bit 307 I 1 DATA3
bit 306 O 1 DATA4 324 0 Z
bit 305 I 1 DATA4
bit 304 O 1 DATA5 324 0 Z
bit 303 I 1 DATA5
bit 302 O 1 DATA6 324 0 Z
bit 301 I 1 DATA6
bit 300 C 0 *
bit 299 O 1 RFS2 300 0 Z
bit 298 I 1 RFS2
bit 297 O 1 DATA7 324 0 Z
bit 296 I 1 DATA7
bit 295 O 1 DATA8 324 0 Z
bit 294 I 1 DATA8
bit 293 O 1 DATA9 324 0 Z
bit 292 I 1 DATA9
bit 291 O 1 DATA10 324 0 Z
bit 290 I 1 DATA10
bit 289 O 1 DATA11 324 0 Z
bit 288 I 1 DATA11
bit 287 C 0 *
bit 286 O 1 RSCLK2 287 0 Z
bit 285 I 1 RSCLK2
bit 284 C 0 *
bit 283 O 1 RX2 284 0 Z
bit 282 I 1 RX2
bit 281 O 1 DATA12 324 0 Z
bit 280 I 1 DATA12
bit 279 O 1 DATA13 324 0 Z
bit 278 I 1 DATA13
bit 277 O 1 DATA14 324 0 Z
bit 276 I 1 DATA14
bit 275 O 1 DATA15 324 0 Z
bit 274 I 1 DATA15
bit 273 I 1 BMODE0
bit 272 I 1 BMODE1
bit 271 I 1 RX0
bit 270 O 1 TX0
bit 269 C 0 *
bit 268 O 1 RSCLK1 269 0 Z
bit 267 I 1 RSCLK1
bit 266 C 0 *
bit 265 O 1 TMR0 266 0 Z
bit 264 I 1 TMR0
bit 263 C 0 *
bit 262 O 1 TMR1 263 0 Z
bit 261 I 1 TMR1
bit 260 C 0 *
bit 259 O 1 TMR2 260 0 Z
bit 258 I 1 TMR2
bit 257 C 0 *
bit 256 O 1 RSCLK0 257 0 Z
bit 255 I 1 RSCLK0
bit 254 C 0 *
bit 253 O 1 RFS0 254 0 Z
bit 252 I 1 RFS0
bit 251 I 1 DR0PRI
bit 250 I 1 DR0SEC
bit 249 C 0 *
bit 248 O 1 RFS1 249 0 Z
bit 247 I 1 RFS1
bit 246 I 1 DR1PRI
bit 245 I 1 DR1SEC
bit 244 C 0 *
bit 243 O 1 TSCLK0 244 0 Z
bit 242 I 1 TSCLK0
bit 241 C 0 *
bit 240 O 1 TFS0 241 0 Z
bit 239 I 1 TFS0
bit 238 C 0 *
bit 237 O 1 DT0PRI 238 0 Z
bit 236 C 0 *
bit 235 O 1 DT0SEC 236 0 Z
bit 234 C 0 *
bit 233 O 1 PF0 234 0 Z
bit 232 I 1 PF0
bit 231 C 0 *
bit 230 O 1 PF1 231 0 Z
bit 229 I 1 PF1
bit 228 C 0 *
bit 227 O 1 PF2 228 0 Z
bit 226 I 1 PF2
bit 225 C 0 *
bit 224 O 1 PF3 225 0 Z
bit 223 I 1 PF3
bit 222 C 0 *
bit 221 O 1 PF4 222 0 Z
bit 220 I 1 PF4
bit 219 C 0 *
bit 218 O 1 PF5 219 0 Z
bit 217 I 1 PF5
bit 216 C 0 *
bit 215 O 1 TSCLK1 216 0 Z
bit 214 I 1 TSCLK1
bit 213 C 0 *
bit 212 O 1 TFS1 213 0 Z
bit 211 I 1 TFS1
bit 210 C 0 *
bit 209 O 1 DT1PRI 210 0 Z
bit 208 C 0 *
bit 207 O 1 PF6 208 0 Z
bit 206 I 1 PF6
bit 205 C 0 *
bit 204 O 1 MOSI0 205 0 Z
bit 203 I 1 MOSI0
bit 202 C 0 *
bit 201 O 1 MISO0 202 0 Z
bit 200 I 1 MISO0
bit 199 C 0 *
bit 198 O 1 DT1SEC 199 0 Z
bit 197 C 0 *
bit 196 O 1 SCK0 197 0 Z
bit 195 I 1 SCK0
bit 194 C 0 *
bit 193 O 1 PF7 194 0 Z
bit 192 I 1 PF7
bit 191 C 0 *
bit 190 O 1 PF8 191 0 Z
bit 189 I 1 PF8
bit 188 C 0 *
bit 187 O 1 PF9 188 0 Z
bit 186 I 1 PF9
bit 185 C 0 *
bit 184 O 1 PF10 185 0 Z
bit 183 I 1 PF10
bit 182 C 0 *
bit 181 O 1 PF11 182 0 Z
bit 180 I 1 PF11
bit 179 C 0 *
bit 178 O 1 PF12 179 0 Z
bit 177 I 1 PF12
bit 176 C 0 *
bit 175 O 1 PF13 176 0 Z
bit 174 I 1 PF13
bit 173 C 0 *
bit 172 O 1 PF14 173 0 Z
bit 171 I 1 PF14
bit 170 C 0 *
bit 169 O 1 PF15 170 0 Z
bit 168 I 1 PF15
bit 167 C 0 *
bit 166 O 1 PPI3 167 0 Z
bit 165 I 1 PPI3
bit 164 C 0 *
bit 163 O 1 PPI2 164 0 Z
bit 162 I 1 PPI2
bit 161 C 0 *
bit 160 O 1 PPI1 161 0 Z
bit 159 I 1 PPI1
bit 158 C 0 *
bit 157 O 1 PPI0 158 0 Z
bit 156 I 1 PPI0
bit 155 C 0 *
bit 154 O 1 RX1 155 0 Z
bit 153 I 1 RX1
bit 152 C 0 *
bit 151 O 1 TX1 152 0 Z
bit 150 I 1 TX1
bit 149 I 1 PPI_CLK
bit 148 C 0 *
bit 147 O 1 SCL0 148 0 Z
bit 146 I 1 SCL0
bit 145 C 0 *
bit 144 O 1 SDA0 145 0 Z
bit 143 I 1 SDA0
bit 142 O 0 *
bit 141 O 0 *
bit 140 I 1 CANRX
bit 139 C 0 *
bit 138 O 1 CANTX 139 0 Z
bit 137 I 1 CANTX
bit 136 C 0 *
bit 135 O 1 SPI2SEL1_B 136 0 Z
bit 134 I 1 SPI2SEL1_B
bit 133 C 0 *
bit 132 O 1 SPI2SS_B 133 0 Z
bit 131 I 1 SPI2SS_B
bit 130 C 0 *
bit 129 O 1 MOSI2 130 0 Z
bit 128 I 1 MOSI2
bit 127 C 0 *
bit 126 O 1 MISO2 127 0 Z
bit 125 I 1 MISO2
bit 124 I 1 NMI_B
bit 123 I 1 RESET_B
bit 122 C 0 *
bit 121 O 1 SCK2 122 0 Z
bit 120 I 1 SCK2
bit 119 C 0 *
bit 118 O 1 SPI1SEL1_B 119 0 Z
bit 117 I 1 SPI1SEL1_B
bit 116 C 0 *
bit 115 O 1 SPI1SS_B 116 0 Z
bit 114 I 1 SPI1SS_B
bit 113 C 0 *
bit 112 O 1 MOSI1 113 0 Z
bit 111 I 1 MOSI1
bit 110 C 0 *
bit 109 O 1 MISO1 110 0 Z
bit 108 I 1 MISO1
bit 107 C 0 *
bit 106 O 1 SCK1 107 0 Z
bit 105 I 1 SCK1
bit 104 C 0 *
bit 103 O 1 SCL1 104 0 Z
bit 102 I 1 SCL1
bit 101 C 0 *
bit 100 O 1 SDA1 101 0 Z
bit 99 I 1 SDA1
bit 98 C 0 *
bit 97 O 1 PC9 98 0 Z
bit 96 I 1 PC9
bit 95 O 0 *
bit 94 O 0 *
bit 93 I 1 GPW_B
bit 92 O 1 SCKE 84 0 Z
bit 91 O 1 SMS_B 84 0 Z
bit 90 C 0 *
bit 89 O 1 PC6 90 0 Z
bit 88 I 1 PC6
bit 87 C 0 *
bit 86 O 1 PC7 87 0 Z
bit 85 I 1 PC7
bit 84 C 0 *
bit 83 O 1 CLKOUT 84 0 Z
bit 82 I 1 ARDY
bit 81 I 1 BR_B
bit 80 C 0 *
bit 79 O 1 DT3SEC 80 0 Z
bit 78 I 1 DT3SEC
bit 77 C 0 *
bit 76 O 1 DT3PRI 77 0 Z
bit 75 I 1 DT3PRI
bit 74 C 0 *
bit 73 O 1 TFS3 74 0 Z
bit 72 I 1 TFS3
bit 71 O 1 SRAS_B 84 0 Z
bit 70 O 1 SCAS_B 84 0 Z
bit 69 O 1 SWE_B 84 0 Z
bit 68 O 1 SA10 84 0 Z
bit 67 C 0 *
bit 66 O 1 PC8 67 0 Z
bit 65 I 1 PC8
bit 64 C 0 *
bit 63 O 1 PC5 64 0 Z
bit 62 I 1 PC5
bit 61 O 0 *
bit 60 O 0 *
bit 59 I 1 PC4
bit 58 O 1 AMS_B0 45 0 Z
bit 57 C 0 *
bit 56 O 1 TSCLK3 57 0 Z
bit 55 I 1 TSCLK3
bit 54 C 0 *
bit 53 O 1 DR3SEC 54 0 Z
bit 52 I 1 DR3SEC
bit 51 C 0 *
bit 50 O 1 DR3PRI 51 0 Z
bit 49 I 1 DR3PRI
bit 48 O 1 AMS_B1 45 0 Z
bit 47 O 1 AMS_B2 45 0 Z
bit 46 O 1 AMS_B3 45 0 Z
bit 45 C 0 *
bit 44 O 1 AOE_B 45 0 Z
bit 43 O 1 ARE_B 45 0 Z
bit 42 O 1 AWE_B 45 0 Z
bit 41 O 1 ABE_B0 26 0 Z
bit 40 O 1 ABE_B1 26 0 Z
bit 39 C 0 *
bit 38 O 1 RFS3 39 0 Z
bit 37 I 1 RFS3
bit 36 C 0 *
bit 35 O 1 RSCLK3 36 0 Z
bit 34 I 1 RSCLK3
bit 33 C 0 *
bit 32 O 1 TX2 33 0 Z
bit 31 I 1 TX2
bit 30 O 1 ADDR1 26 0 Z
bit 29 O 1 ADDR2 26 0 Z
bit 28 O 1 ADDR3 26 0 Z
bit 27 O 1 ADDR4 26 0 Z
bit 26 C 0 *
bit 25 O 1 ADDR5 26 0 Z
bit 24 O 1 ADDR6 26 0 Z
bit 23 O 1 ADDR7 26 0 Z
bit 22 O 1 ADDR8 26 0 Z
bit 21 O 1 ADDR9 26 0 Z
bit 20 O 1 ADDR10 26 0 Z
bit 19 O 1 ADDR11 26 0 Z
bit 18 O 1 ADDR12 26 0 Z
bit 17 O 1 ADDR13 26 0 Z
bit 16 O 1 ADDR14 26 0 Z
bit 15 C 0 *
bit 14 O 1 DT2SEC 15 0 Z
bit 13 I 1 DT2SEC
bit 12 C 0 *
bit 11 O 1 DT2PRI 12 0 Z
bit 10 I 1 DT2PRI
bit 9 O 1 ADDR15 26 0 Z
bit 8 O 1 ADDR16 26 0 Z
bit 7 O 1 ADDR17 26 0 Z
bit 6 O 1 ADDR18 26 0 Z
bit 5 O 1 ADDR19 26 0 Z
bit 4 C 0 *
bit 3 O 1 TFS2 4 0 Z
bit 2 I 1 TFS2
bit 1 O 1 BGH_B
bit 0 O 1 BG_B
