#
# $Id: xcr3256xl-ft256 504 2003-08-13 09:24:36Z telka $
#
# Copyright (C) 2003 Jachym Holecek <freza@psi.cz>
#
# This program is free software; you can redistribute it and/or
# modify it under the terms of the GNU General Public License
# as published by the Free Software Foundation; either version 2
# of the License, or (at your option) any later version.
#
# This program is distributed in the hope that it will be useful,
# but WITHOUT ANY WARRANTY; without even the implied warranty of
# MERCHANTABILITY or FITNESS FOR A PARTICULAR PURPOSE.  See the
# GNU General Public License for more details.
#
# You should have received a copy of the GNU General Public License
# along with this program; if not, write to the Free Software
# Foundation, Inc., 59 Temple Place - Suite 330, Boston, MA
# 02111-1307, USA.
#

signal tdi
signal tck
signal tms
signal tdo
signal CLK0
signal CLK1
signal CLK2
signal CLK3
signal IO_0
signal IO_1
signal IO_2
signal IO_3
signal IO_4
signal IO_5
signal IO_6
signal IO_7
signal IO_8
signal IO_9
signal IO_10
signal IO_11
signal IO_12
signal IO_13
signal IO_14
signal IO_15
signal IO_16
signal IO_17
signal IO_18
signal IO_19
signal IO_20
signal IO_21
signal IO_22
signal IO_23
signal IO_24
signal IO_25
signal IO_26
signal IO_27
signal IO_28
signal IO_29
signal IO_30
signal IO_31
signal IO_32
signal IO_33
signal IO_34
signal IO_35
signal IO_36
signal IO_38
signal IO_39
signal IO_40
signal IO_41
signal IO_43
signal IO_44
signal IO_45
signal IO_46
signal IO_47
signal IO_48
signal IO_49
signal IO_50
signal IO_51
signal IO_52
signal IO_53
signal IO_54
signal IO_55
signal IO_56
signal IO_57
signal IO_58
signal IO_59
signal IO_60
signal IO_61
signal IO_62
signal IO_63
signal IO_64
signal IO_65
signal IO_66
signal IO_67
signal IO_68
signal IO_69
signal IO_70
signal IO_71
signal IO_72
signal IO_73
signal IO_74
signal IO_75
signal IO_76
signal IO_77
signal IO_78
signal IO_79
signal IO_80
signal IO_81
signal IO_82
signal IO_83
signal IO_84
signal IO_85
signal IO_86
signal IO_87
signal IO_88
signal IO_89
signal IO_90
signal IO_91
signal IO_92
signal IO_93
signal IO_94
signal IO_95
signal IO_96
signal IO_97
signal IO_98
signal IO_99
signal IO_100
signal IO_101
signal IO_102
signal IO_103
signal IO_104
signal IO_105
signal IO_106
signal IO_108
signal IO_109
signal IO_110
signal IO_111
signal IO_112
signal IO_113
signal IO_114
signal IO_115
signal IO_116
signal IO_117
signal IO_118
signal IO_119
signal IO_120
signal IO_121
signal IO_122
signal IO_123
signal IO_124
signal IO_125
signal IO_126
signal IO_127
signal IO_128
signal IO_129
signal IO_130
signal IO_131
signal IO_133
signal IO_134
signal IO_135
signal IO_136
signal IO_137
signal IO_138
signal IO_139
signal IO_140
signal IO_141
signal IO_142
signal IO_143
signal IO_144
signal IO_145
signal IO_146
signal IO_147
signal IO_148
signal IO_149
signal IO_150
signal IO_151
signal IO_152
signal IO_153
signal IO_154
signal IO_155
signal IO_156
signal IO_157
signal IO_158

# Boundary Scan (mandatory regs)
register    BSR            740 		# Boundary Scan Register
register    BR             1		# Bypass Register

# Optional data reg
register    DIR            32           # ID Code Register

# In-System Programming (user defined regs)
register    ISPSR          313          # ISP Shift Register

instruction length 5

# Mandatory cmds
instruction BYPASS         11111 BR
instruction SAMPLE/PRELOAD 00010 BSR
instruction EXTEST         00000 BSR

# Optional cmds
instruction IDCODE         00001 DIR
instruction INTEST         00011 BSR
instruction HIGHZ          00101 BR

# Mysterious cmds
#instruction STRTEST        00100
#instruction CLAMP          00110 BR

# User defined regs
instruction ENABLE         01001 ISPSR
instruction ERASE          01010 ISPSR
instruction PROGRAM        01011 ISPSR
instruction DISABLE        10000 ISPSR
instruction VERIFY         01100 ISPSR

# Another mysterious cmds
#instruction ISP_EOTF       01000 ISPSR
#instruction ISP_INIT       01101 BR
#instruction ISP_WRITE      00111 ISPSR
#instruction ISP_READ       01110 ISPSR
#instruction TEST_MODE      10001 BR

bit 739 O 1 *
bit 738 I 1 IO_0
bit 737 O 1 IO_0 736 0 Z
bit 736 C 1 *
bit 735 O 1 *
bit 734 I 1 IO_1
bit 733 O 1 IO_1 732 0 Z
bit 732 C 1 *
bit 731 O 1 *
bit 730 I 1 IO_2
bit 729 O 1 IO_2 728 0 Z
bit 728 C 1 *
bit 727 O 1 *
bit 726 I 1 IO_3
bit 725 O 1 IO_3 724 0 Z
bit 724 C 1 *
bit 723 O 1 *
bit 722 I 1 IO_4
bit 721 O 1 IO_4 720 0 Z
bit 720 C 1 *
bit 719 O 1 *
bit 718 O 1 *
bit 717 O 1 *
bit 716 O 1 *
bit 715 O 1 *
bit 714 O 1 *
bit 713 O 1 *
bit 712 I 1 IO_5
bit 711 O 1 IO_5 710 0 Z
bit 710 C 1 *
bit 709 O 1 *
bit 708 I 1 IO_6
bit 707 O 1 IO_6 706 0 Z
bit 706 C 1 *
bit 705 O 1 *
bit 704 I 1 IO_7
bit 703 O 1 IO_7 702 0 Z
bit 702 C 1 *
bit 701 O 1 *
bit 700 I 1 IO_8
bit 699 O 1 IO_8 698 0 Z
bit 698 C 1 *
bit 697 O 1 *
bit 696 I 1 IO_9
bit 695 O 1 IO_9 694 0 Z
bit 694 C 1 *
bit 693 O 1 *
bit 692 I 1 IO_10
bit 691 O 1 IO_10 690 0 Z
bit 690 C 1 *
bit 689 O 1 *
bit 688 I 1 IO_11
bit 687 O 1 IO_11 686 0 Z
bit 686 C 1 *
bit 685 O 1 *
bit 684 I 1 IO_12
bit 683 O 1 IO_12 682 0 Z
bit 682 C 1 *
bit 681 O 1 *
bit 680 I 1 IO_13
bit 679 O 1 IO_13 678 0 Z
bit 678 C 1 *
bit 677 O 1 *
bit 676 I 1 IO_14
bit 675 O 1 IO_14 674 0 Z
bit 674 C 1 *
bit 673 O 1 *
bit 672 O 1 *
bit 671 O 1 *
bit 670 O 1 *
bit 669 O 1 *
bit 668 O 1 *
bit 667 O 1 *
bit 666 I 1 IO_15
bit 665 O 1 IO_15 664 0 Z
bit 664 C 1 *
bit 663 O 1 *
bit 662 I 1 IO_16
bit 661 O 1 IO_16 660 0 Z
bit 660 C 1 *
bit 659 O 1 *
bit 658 I 1 IO_17
bit 657 O 1 IO_17 656 0 Z
bit 656 C 1 *
bit 655 O 1 *
bit 654 I 1 IO_18
bit 653 O 1 IO_18 652 0 Z
bit 652 C 1 *
bit 651 O 1 *
bit 650 I 1 IO_19
bit 649 O 1 IO_19 648 0 Z
bit 648 C 1 *
bit 647 O 1 *
bit 646 I 1 IO_20
bit 645 O 1 IO_20 644 0 Z
bit 644 C 1 *
bit 643 O 1 *
bit 642 I 1 IO_21
bit 641 O 1 IO_21 640 0 Z
bit 640 C 1 *
bit 639 O 1 *
bit 638 I 1 IO_22
bit 637 O 1 IO_22 636 0 Z
bit 636 C 1 *
bit 635 O 1 *
bit 634 I 1 IO_23
bit 633 O 1 IO_23 632 0 Z
bit 632 C 1 *
bit 631 O 1 *
bit 630 I 1 IO_24
bit 629 O 1 IO_24 628 0 Z
bit 628 C 1 *
bit 627 O 1 *
bit 626 O 1 *
bit 625 O 1 *
bit 624 O 1 *
bit 623 O 1 *
bit 622 O 1 *
bit 621 O 1 *
bit 620 I 1 IO_25
bit 619 O 1 IO_25 618 0 Z
bit 618 C 1 *
bit 617 O 1 *
bit 616 I 1 IO_26
bit 615 O 1 IO_26 614 0 Z
bit 614 C 1 *
bit 613 O 1 *
bit 612 I 1 IO_27
bit 611 O 1 IO_27 610 0 Z
bit 610 C 1 *
bit 609 O 1 *
bit 608 I 1 IO_28
bit 607 O 1 IO_28 606 0 Z
bit 606 C 1 *
bit 605 O 1 *
bit 604 I 1 IO_29
bit 603 O 1 IO_29 602 0 Z
bit 602 C 1 *
bit 601 O 1 *
bit 600 I 1 IO_30
bit 599 O 1 IO_30 598 0 Z
bit 598 C 1 *
bit 597 O 1 *
bit 596 I 1 IO_31
bit 595 O 1 IO_31 594 0 Z
bit 594 C 1 *
bit 593 O 1 *
bit 592 I 1 IO_32
bit 591 O 1 IO_32 590 0 Z
bit 590 C 1 *
bit 589 O 1 *
bit 588 I 1 IO_33
bit 587 O 1 IO_33 586 0 Z
bit 586 C 1 *
bit 585 O 1 *
bit 584 I 1 IO_34
bit 583 O 1 IO_34 582 0 Z
bit 582 C 1 *
bit 581 O 1 *
bit 580 O 1 *
bit 579 O 1 *
bit 578 O 1 *
bit 577 O 1 *
bit 576 O 1 *
bit 575 O 1 *
bit 574 I 1 IO_35
bit 573 O 1 IO_35 572 0 Z
bit 572 C 1 *
bit 571 O 1 *
bit 570 I 1 IO_36
bit 569 O 1 IO_36 568 0 Z
bit 568 C 1 *
bit 567 O 1 *
bit 566 O 1 *
bit 565 O 1 *
bit 564 O 1 *
bit 563 O 1 *
bit 562 I 1 IO_38
bit 561 O 1 IO_38 560 0 Z
bit 560 C 1 *
bit 559 O 1 *
bit 558 I 1 IO_39
bit 557 O 1 IO_39 556 0 Z
bit 556 C 1 *
bit 555 O 1 *
bit 554 I 1 IO_40
bit 553 O 1 IO_40 552 0 Z
bit 552 C 1 *
bit 551 O 1 *
bit 550 I 1 IO_41
bit 549 O 1 IO_41 548 0 Z
bit 548 C 1 *
bit 547 O 1 *
bit 546 O 1 *
bit 545 O 1 *
bit 544 O 1 *
bit 543 O 1 *
bit 542 I 1 IO_43
bit 541 O 1 IO_43 540 0 Z
bit 540 C 1 *
bit 539 O 1 *
bit 538 I 1 IO_44
bit 537 O 1 IO_44 536 0 Z
bit 536 C 1 *
bit 535 O 1 *
bit 534 O 1 *
bit 533 O 1 *
bit 532 O 1 *
bit 531 O 1 *
bit 530 O 1 *
bit 529 O 1 *
bit 528 I 1 IO_45
bit 527 O 1 IO_45 526 0 Z
bit 526 C 1 *
bit 525 O 1 *
bit 524 I 1 IO_46
bit 523 O 1 IO_46 522 0 Z
bit 522 C 1 *
bit 521 O 1 *
bit 520 I 1 IO_47
bit 519 O 1 IO_47 518 0 Z
bit 518 C 1 *
bit 517 O 1 *
bit 516 I 1 IO_48
bit 515 O 1 IO_48 514 0 Z
bit 514 C 1 *
bit 513 O 1 *
bit 512 I 1 IO_49
bit 511 O 1 IO_49 510 0 Z
bit 510 C 1 *
bit 509 O 1 *
bit 508 I 1 IO_50
bit 507 O 1 IO_50 506 0 Z
bit 506 C 1 *
bit 505 O 1 *
bit 504 I 1 IO_51
bit 503 O 1 IO_51 502 0 Z
bit 502 C 1 *
bit 501 O 1 *
bit 500 I 1 IO_52
bit 499 O 1 IO_52 498 0 Z
bit 498 C 1 *
bit 497 O 1 *
bit 496 I 1 IO_53
bit 495 O 1 IO_53 494 0 Z
bit 494 C 1 *
bit 493 O 1 *
bit 492 I 1 IO_54
bit 491 O 1 IO_54 490 0 Z
bit 490 C 1 *
bit 489 O 1 *
bit 488 O 1 *
bit 487 O 1 *
bit 486 O 1 *
bit 485 O 1 *
bit 484 O 1 *
bit 483 O 1 *
bit 482 I 1 IO_55
bit 481 O 1 IO_55 480 0 Z
bit 480 C 1 *
bit 479 O 1 *
bit 478 I 1 IO_56
bit 477 O 1 IO_56 476 0 Z
bit 476 C 1 *
bit 475 O 1 *
bit 474 I 1 IO_57
bit 473 O 1 IO_57 472 0 Z
bit 472 C 1 *
bit 471 O 1 *
bit 470 I 1 IO_58
bit 469 O 1 IO_58 468 0 Z
bit 468 C 1 *
bit 467 O 1 *
bit 466 I 1 IO_59
bit 465 O 1 IO_59 464 0 Z
bit 464 C 1 *
bit 463 O 1 *
bit 462 I 1 IO_60
bit 461 O 1 IO_60 460 0 Z
bit 460 C 1 *
bit 459 O 1 *
bit 458 I 1 IO_61
bit 457 O 1 IO_61 456 0 Z
bit 456 C 1 *
bit 455 O 1 *
bit 454 I 1 IO_62
bit 453 O 1 IO_62 452 0 Z
bit 452 C 1 *
bit 451 O 1 *
bit 450 I 1 IO_63
bit 449 O 1 IO_63 448 0 Z
bit 448 C 1 *
bit 447 O 1 *
bit 446 I 1 IO_64
bit 445 O 1 IO_64 444 0 Z
bit 444 C 1 *
bit 443 O 1 *
bit 442 O 1 *
bit 441 O 1 *
bit 440 O 1 *
bit 439 O 1 *
bit 438 O 1 *
bit 437 O 1 *
bit 436 I 1 IO_65
bit 435 O 1 IO_65 434 0 Z
bit 434 C 1 *
bit 433 O 1 *
bit 432 I 1 IO_66
bit 431 O 1 IO_66 430 0 Z
bit 430 C 1 *
bit 429 O 1 *
bit 428 I 1 IO_67
bit 427 O 1 IO_67 426 0 Z
bit 426 C 1 *
bit 425 O 1 *
bit 424 I 1 IO_68
bit 423 O 1 IO_68 422 0 Z
bit 422 C 1 *
bit 421 O 1 *
bit 420 I 1 IO_69
bit 419 O 1 IO_69 418 0 Z
bit 418 C 1 *
bit 417 O 1 *
bit 416 I 1 IO_70
bit 415 O 1 IO_70 414 0 Z
bit 414 C 1 *
bit 413 O 1 *
bit 412 I 1 IO_71
bit 411 O 1 IO_71 410 0 Z
bit 410 C 1 *
bit 409 O 1 *
bit 408 I 1 IO_72
bit 407 O 1 IO_72 406 0 Z
bit 406 C 1 *
bit 405 O 1 *
bit 404 I 1 IO_73
bit 403 O 1 IO_73 402 0 Z
bit 402 C 1 *
bit 401 O 1 *
bit 400 I 1 IO_74
bit 399 O 1 IO_74 398 0 Z
bit 398 C 1 *
bit 397 O 1 *
bit 396 O 1 *
bit 395 O 1 *
bit 394 O 1 *
bit 393 O 1 *
bit 392 O 1 *
bit 391 O 1 *
bit 390 I 1 IO_75
bit 389 O 1 IO_75 388 0 Z
bit 388 C 1 *
bit 387 O 1 *
bit 386 I 1 IO_76
bit 385 O 1 IO_76 384 0 Z
bit 384 C 1 *
bit 383 O 1 *
bit 382 I 1 IO_77
bit 381 O 1 IO_77 380 0 Z
bit 380 C 1 *
bit 379 O 1 *
bit 378 I 1 IO_78
bit 377 O 1 IO_78 376 0 Z
bit 376 C 1 *
bit 375 O 1 *
bit 374 I 1 IO_79
bit 373 O 1 IO_79 372 0 Z
bit 372 C 1 *
bit 371 O 1 *
bit 370 I 1 IO_80
bit 369 O 1 IO_80 368 0 Z
bit 368 C 1 *
bit 367 O 1 *
bit 366 I 1 IO_81
bit 365 O 1 IO_81 364 0 Z
bit 364 C 1 *
bit 363 O 1 *
bit 362 I 1 IO_82
bit 361 O 1 IO_82 360 0 Z
bit 360 C 1 *
bit 359 O 1 *
bit 358 I 1 IO_83
bit 357 O 1 IO_83 356 0 Z
bit 356 C 1 *
bit 355 O 1 *
bit 354 I 1 IO_84
bit 353 O 1 IO_84 352 0 Z
bit 352 C 1 *
bit 351 O 1 *
bit 350 O 1 *
bit 349 O 1 *
bit 348 O 1 *
bit 347 O 1 *
bit 346 O 1 *
bit 345 O 1 *
bit 344 I 1 IO_85
bit 343 O 1 IO_85 342 0 Z
bit 342 C 1 *
bit 341 O 1 *
bit 340 I 1 IO_86
bit 339 O 1 IO_86 338 0 Z
bit 338 C 1 *
bit 337 O 1 *
bit 336 I 1 IO_87
bit 335 O 1 IO_87 334 0 Z
bit 334 C 1 *
bit 333 O 1 *
bit 332 I 1 IO_88
bit 331 O 1 IO_88 330 0 Z
bit 330 C 1 *
bit 329 O 1 *
bit 328 I 1 IO_89
bit 327 O 1 IO_89 326 0 Z
bit 326 C 1 *
bit 325 O 1 *
bit 324 I 1 IO_90
bit 323 O 1 IO_90 322 0 Z
bit 322 C 1 *
bit 321 O 1 *
bit 320 I 1 IO_91
bit 319 O 1 IO_91 318 0 Z
bit 318 C 1 *
bit 317 O 1 *
bit 316 I 1 IO_92
bit 315 O 1 IO_92 314 0 Z
bit 314 C 1 *
bit 313 O 1 *
bit 312 I 1 IO_93
bit 311 O 1 IO_93 310 0 Z
bit 310 C 1 *
bit 309 O 1 *
bit 308 I 1 IO_94
bit 307 O 1 IO_94 306 0 Z
bit 306 C 1 *
bit 305 O 1 *
bit 304 O 1 *
bit 303 O 1 *
bit 302 O 1 *
bit 301 O 1 *
bit 300 O 1 *
bit 299 O 1 *
bit 298 I 1 IO_95
bit 297 O 1 IO_95 296 0 Z
bit 296 C 1 *
bit 295 O 1 *
bit 294 I 1 IO_96
bit 293 O 1 IO_96 292 0 Z
bit 292 C 1 *
bit 291 O 1 *
bit 290 I 1 IO_97
bit 289 O 1 IO_97 288 0 Z
bit 288 C 1 *
bit 287 O 1 *
bit 286 I 1 IO_98
bit 285 O 1 IO_98 284 0 Z
bit 284 C 1 *
bit 283 O 1 *
bit 282 I 1 IO_99
bit 281 O 1 IO_99 280 0 Z
bit 280 C 1 *
bit 279 O 1 *
bit 278 I 1 IO_100
bit 277 O 1 IO_100 276 0 Z
bit 276 C 1 *
bit 275 O 1 *
bit 274 I 1 IO_101
bit 273 O 1 IO_101 272 0 Z
bit 272 C 1 *
bit 271 O 1 *
bit 270 I 1 IO_102
bit 269 O 1 IO_102 268 0 Z
bit 268 C 1 *
bit 267 O 1 *
bit 266 I 1 IO_103
bit 265 O 1 IO_103 264 0 Z
bit 264 C 1 *
bit 263 O 1 *
bit 262 I 1 IO_104
bit 261 O 1 IO_104 260 0 Z
bit 260 C 1 *
bit 259 O 1 *
bit 258 O 1 *
bit 257 O 1 *
bit 256 O 1 *
bit 255 O 1 *
bit 254 O 1 *
bit 253 O 1 *
bit 252 I 1 IO_105
bit 251 O 1 IO_105 250 0 Z
bit 250 C 1 *
bit 249 O 1 *
bit 248 I 1 IO_106
bit 247 O 1 IO_106 246 0 Z
bit 246 C 1 *
bit 245 O 1 *
bit 244 O 1 *
bit 243 O 1 *
bit 242 O 1 *
bit 241 O 1 *
bit 240 I 1 IO_108
bit 239 O 1 IO_108 238 0 Z
bit 238 C 1 *
bit 237 O 1 *
bit 236 I 1 IO_109
bit 235 O 1 IO_109 234 0 Z
bit 234 C 1 *
bit 233 O 1 *
bit 232 I 1 IO_110
bit 231 O 1 IO_110 230 0 Z
bit 230 C 1 *
bit 229 O 1 *
bit 228 I 1 IO_111
bit 227 O 1 IO_111 226 0 Z
bit 226 C 1 *
bit 225 O 1 *
bit 224 I 1 IO_112
bit 223 O 1 IO_112 222 0 Z
bit 222 C 1 *
bit 221 O 1 *
bit 220 I 1 IO_113
bit 219 O 1 IO_113 218 0 Z
bit 218 C 1 *
bit 217 O 1 *
bit 216 I 1 IO_114
bit 215 O 1 IO_114 214 0 Z
bit 214 C 1 *
bit 213 O 1 *
bit 212 O 1 *
bit 211 O 1 *
bit 210 O 1 *
bit 209 O 1 *
bit 208 O 1 *
bit 207 O 1 *
bit 206 I 1 IO_115
bit 205 O 1 IO_115 204 0 Z
bit 204 C 1 *
bit 203 O 1 *
bit 202 I 1 IO_116
bit 201 O 1 IO_116 200 0 Z
bit 200 C 1 *
bit 199 O 1 *
bit 198 I 1 IO_117
bit 197 O 1 IO_117 196 0 Z
bit 196 C 1 *
bit 195 O 1 *
bit 194 I 1 IO_118
bit 193 O 1 IO_118 192 0 Z
bit 192 C 1 *
bit 191 O 1 *
bit 190 I 1 IO_119
bit 189 O 1 IO_119 188 0 Z
bit 188 C 1 *
bit 187 O 1 *
bit 186 I 1 IO_120
bit 185 O 1 IO_120 184 0 Z
bit 184 C 1 *
bit 183 O 1 *
bit 182 I 1 IO_121
bit 181 O 1 IO_121 180 0 Z
bit 180 C 1 *
bit 179 O 1 *
bit 178 I 1 IO_122
bit 177 O 1 IO_122 176 0 Z
bit 176 C 1 *
bit 175 O 1 *
bit 174 I 1 IO_123
bit 173 O 1 IO_123 172 0 Z
bit 172 C 1 *
bit 171 O 1 *
bit 170 I 1 IO_124
bit 169 O 1 IO_124 168 0 Z
bit 168 C 1 *
bit 167 O 1 *
bit 166 O 1 *
bit 165 O 1 *
bit 164 O 1 *
bit 163 O 1 *
bit 162 O 1 *
bit 161 O 1 *
bit 160 I 1 IO_125
bit 159 O 1 IO_125 158 0 Z
bit 158 C 1 *
bit 157 O 1 *
bit 156 I 1 IO_126
bit 155 O 1 IO_126 154 0 Z
bit 154 C 1 *
bit 153 O 1 *
bit 152 I 1 IO_127
bit 151 O 1 IO_127 150 0 Z
bit 150 C 1 *
bit 149 O 1 *
bit 148 I 1 IO_128
bit 147 O 1 IO_128 146 0 Z
bit 146 C 1 *
bit 145 O 1 *
bit 144 I 1 IO_129
bit 143 O 1 IO_129 142 0 Z
bit 142 C 1 *
bit 141 O 1 *
bit 140 I 1 IO_130
bit 139 O 1 IO_130 138 0 Z
bit 138 C 1 *
bit 137 O 1 *
bit 136 I 1 IO_131
bit 135 O 1 IO_131 134 0 Z
bit 134 C 1 *
bit 133 O 1 *
bit 132 O 1 *
bit 131 O 1 *
bit 130 O 1 *
bit 129 O 1 *
bit 128 I 1 IO_133
bit 127 O 1 IO_133 126 0 Z
bit 126 C 1 *
bit 125 O 1 *
bit 124 I 1 IO_134
bit 123 O 1 IO_134 122 0 Z
bit 122 C 1 *
bit 121 O 1 *
bit 120 O 1 *
bit 119 O 1 *
bit 118 O 1 *
bit 117 O 1 *
bit 116 O 1 *
bit 115 O 1 *
bit 114 I 1 IO_135
bit 113 O 1 IO_135 112 0 Z
bit 112 C 1 *
bit 111 O 1 *
bit 110 I 1 IO_136
bit 109 O 1 IO_136 108 0 Z
bit 108 C 1 *
bit 107 O 1 *
bit 106 I 1 IO_137
bit 105 O 1 IO_137 104 0 Z
bit 104 C 1 *
bit 103 O 1 *
bit 102 I 1 IO_138
bit 101 O 1 IO_138 100 0 Z
bit 100 C 1 *
bit 99 O 1 *
bit 98 I 1 IO_139
bit 97 O 1 IO_139 96 0 Z
bit 96 C 1 *
bit 95 O 1 *
bit 94 I 1 IO_140
bit 93 O 1 IO_140 92 0 Z
bit 92 C 1 *
bit 91 O 1 *
bit 90 I 1 IO_141
bit 89 O 1 IO_141 88 0 Z
bit 88 C 1 *
bit 87 O 1 *
bit 86 I 1 IO_142
bit 85 O 1 IO_142 84 0 Z
bit 84 C 1 *
bit 83 O 1 *
bit 82 I 1 IO_143
bit 81 O 1 IO_143 80 0 Z
bit 80 C 1 *
bit 79 O 1 *
bit 78 I 1 IO_144
bit 77 O 1 IO_144 76 0 Z
bit 76 C 1 *
bit 75 O 1 *
bit 74 O 1 *
bit 73 O 1 *
bit 72 O 1 *
bit 71 O 1 *
bit 70 O 1 *
bit 69 O 1 *
bit 68 I 1 IO_145
bit 67 O 1 IO_145 66 0 Z
bit 66 C 1 *
bit 65 O 1 *
bit 64 I 1 IO_146
bit 63 O 1 IO_146 62 0 Z
bit 62 C 1 *
bit 61 O 1 *
bit 60 I 1 IO_147
bit 59 O 1 IO_147 58 0 Z
bit 58 C 1 *
bit 57 O 1 *
bit 56 I 1 IO_148
bit 55 O 1 IO_148 54 0 Z
bit 54 C 1 *
bit 53 O 1 *
bit 52 I 1 IO_149
bit 51 O 1 IO_149 50 0 Z
bit 50 C 1 *
bit 49 O 1 *
bit 48 I 1 IO_150
bit 47 O 1 IO_150 46 0 Z
bit 46 C 1 *
bit 45 O 1 *
bit 44 I 1 IO_151
bit 43 O 1 IO_151 42 0 Z
bit 42 C 1 *
bit 41 O 1 *
bit 40 I 1 IO_152
bit 39 O 1 IO_152 38 0 Z
bit 38 C 1 *
bit 37 O 1 *
bit 36 I 1 IO_153
bit 35 O 1 IO_153 34 0 Z
bit 34 C 1 *
bit 33 O 1 *
bit 32 I 1 IO_154
bit 31 O 1 IO_154 30 0 Z
bit 30 C 1 *
bit 29 O 1 *
bit 28 O 1 *
bit 27 O 1 *
bit 26 O 1 *
bit 25 O 1 *
bit 24 O 1 *
bit 23 O 1 *
bit 22 I 1 IO_155
bit 21 O 1 IO_155 20 0 Z
bit 20 C 1 *
bit 19 O 1 *
bit 18 I 1 IO_156
bit 17 O 1 IO_156 16 0 Z
bit 16 C 1 *
bit 15 O 1 *
bit 14 I 1 IO_157
bit 13 O 1 IO_157 12 0 Z
bit 12 C 1 *
bit 11 O 1 *
bit 10 I 1 IO_158
bit 9 O 1 IO_158 8 0 Z
bit 8 C 1 *
bit 7 O 1 *
bit 6 I 1 IO_159
bit 5 O 1 IO_159 4 0 Z
bit 4 C 1 *
bit 3 I 1 CLK0
bit 2 I 1 CLK1
bit 1 I 1 CLK2
bit 0 I 1 CLK3
