signal ADDR[1]
signal ADDR[2]
signal ADDR[3]
signal ADDR[4]
signal ADDR[5]
signal ADDR[6]
signal ADDR[7]
signal ADDR[8]
signal ADDR[9]
signal ADDR[10]
signal ADDR[11]
signal ADDR[12]
signal ADDR[13]
signal ADDR[14]
signal ADDR[15]
signal ADDR[16]
signal ADDR[17]
signal ADDR[18]
signal ADDR[19]
signal AMS_B0
signal AMS_B1
signal AMS_B2
signal AMS_B3
signal AOE_B
signal ARDY
signal ARE_B
signal AWE_B
signal ABE_B0
signal ABE_B1
signal BG_B
signal BGH_B
signal BMODE0
signal BMODE1
signal BR_B
signal DATA[0]
signal DATA[1]
signal DATA[2]
signal DATA[3]
signal DATA[4]
signal DATA[5]
signal DATA[6]
signal DATA[7]
signal DATA[8]
signal DATA[9]
signal DATA[10]
signal DATA[11]
signal DATA[12]
signal DATA[13]
signal DATA[14]
signal DATA[15]
signal DR0PRI
signal DR0SEC
signal DR1PRI
signal DR1SEC
signal DT0PRI
signal DT0SEC
signal DT1PRI
signal DT1SEC
signal MISO
signal MOSI
signal NMI
signal PF0
signal PF1
signal PF2
signal PF3
signal PF4
signal PF5
signal PF6
signal PF7
signal PF8
signal PF9
signal PF10
signal PF11
signal PF12
signal PF13
signal PF14
signal PF15
signal PP_CLK
signal PP0
signal PP1
signal PP2
signal PP3
signal RESET_B
signal RFS0
signal RFS1
signal RSCLK0
signal RSCLK1
signal TSCLK0
signal TSCLK1
signal CLKOUT
signal RX
signal TX
signal SA10
signal SCAS_B
signal SCK
signal SCKE
signal SMS_B
signal SRAS_B
signal SWE_B
signal TCK
signal TDI
signal TDO
signal TMS
signal TRST_B
signal EMU_B
signal TEST
signal TFS0
signal TFS1
signal TMR0
signal TMR1
signal TMR2
signal RTXI
signal RTXO
signal VDD_INT0
signal VDD_INT1
signal VDD_INT2
signal VDD_INT3
signal VDD_INT4
signal VDD_INT5
signal VDD_EXT0
signal VDD_EXT1
signal VDD_EXT2
signal VDD_EXT3
signal VDD_EXT4
signal VDD_EXT5
signal VDD_EXT6
signal VDD_EXT7
signal VDD_EXT8
signal VDD_EXT9
signal VDD_EXT10
signal VDD_EXT11
signal GND0
signal GND1
signal GND2
signal GND3
signal GND4
signal GND5
signal GND6
signal GND7
signal GND8
signal GND9
signal GND10
signal GND11
signal GND12
signal GND13
signal GND14
signal GND15
signal GND16
signal GND17
signal GND18
signal GND19
signal GND20
signal GND21
signal GND22
signal GND23
signal VDD_RTC
signal CLKIN
signal XTAL
signal VROUT0

register	BSR	197
register	BR	1
register	DIR	32
register	DBGSTAT	16
register	DBGCTL	16
register	EMUIR	32
register	EMUDAT	32
register	EMUPC	32

instruction length 5

instruction EXTEST 00000 BSR
instruction SAMPLE/PRELOAD 10000 BSR
instruction IDCODE 00010 DIR
instruction BYPASS 11111 BR
instruction DBGSTAT_SCAN 01100 DBGSTAT
instruction DBGCTL_SCAN 00100 DBGCTL
instruction EMUIR_SCAN 01000 EMUIR
instruction EMUDAT_SCAN 10100 EMUDAT
instruction EMUPC_SCAN 11110 EMUPC

bit 196 C 0 *
bit 195 O 1 DATA[0] 196 0 Z
bit 194 I 1 DATA[0]
bit 193 O 1 DATA[1] 196 0 Z
bit 192 I 1 DATA[1]
bit 191 O 1 DATA[2] 196 0 Z
bit 190 I 1 DATA[2]
bit 189 O 1 DATA[3] 196 0 Z
bit 188 I 1 DATA[3]
bit 187 O 1 DATA[4] 196 0 Z
bit 186 I 1 DATA[4]
bit 185 O 1 DATA[5] 196 0 Z
bit 184 I 1 DATA[5]
bit 183 O 1 DATA[6] 196 0 Z
bit 182 I 1 DATA[6]
bit 181 O 1 DATA[7] 196 0 Z
bit 180 I 1 DATA[7]
bit 179 O 1 DATA[8] 196 0 Z
bit 178 I 1 DATA[8]
bit 177 O 1 DATA[9] 196 0 Z
bit 176 I 1 DATA[9]
bit 175 O 1 DATA[10] 196 0 Z
bit 174 I 1 DATA[10]
bit 173 O 1 DATA[11] 196 0 Z
bit 172 I 1 DATA[11]
bit 171 O 1 DATA[12] 196 0 Z
bit 170 I 1 DATA[12]
bit 169 O 1 DATA[13] 196 0 Z
bit 168 I 1 DATA[13]
bit 167 O 1 DATA[14] 196 0 Z
bit 166 I 1 DATA[14]
bit 165 O 1 DATA[15] 196 0 Z
bit 164 I 1 DATA[15]
bit 163 I 1 TEST
bit 162 I 1 BMODE0
bit 161 I 1 BMODE1
bit 160 I 1 RX
bit 159 O 1 TX
bit 158 C 0 *
bit 157 O 1 TMR0 158 0 Z
bit 156 I 1 TMR0
bit 155 C 0 *
bit 154 O 1 TMR1 155 0 Z
bit 153 I 1 TMR1
bit 152 C 0 *
bit 151 O 1 TMR2 152 0 Z
bit 150 I 1 TMR2
bit 149 C 0 *
bit 148 O 1 RSCLK0 149 0 Z
bit 147 I 1 RSCLK0
bit 146 C 0 *
bit 145 O 1 RFS0 146 0 Z
bit 144 I 1 RFS0
bit 143 I 1 DR0PRI
bit 142 I 1 DR0SEC
bit 141 C 0 *
bit 140 O 1 TSCLK0 141 0 Z
bit 139 I 1 TSCLK0
bit 138 C 0 *
bit 137 O 1 TFS0 138 0 Z
bit 136 I 1 TFS0
bit 135 C 0 *
bit 134 O 1 DT0PRI 135 0 Z
bit 133 C 0 *
bit 132 O 1 DT0SEC 133 0 Z
bit 131 C 0 *
bit 130 O 1 RSCLK1 131 0 Z
bit 129 I 1 RSCLK1
bit 128 C 0 *
bit 127 O 1 RFS1 128 0 Z
bit 126 I 1 RFS1
bit 125 I 1 DR1PRI
bit 124 I 1 DR1SEC
bit 123 C 0 *
bit 122 O 1 TSCLK1 123 0 Z
bit 121 I 1 TSCLK1
bit 120 C 0 *
bit 119 O 1 TFS1 120 0 Z
bit 118 I 1 TFS1
bit 117 C 0 *
bit 116 O 1 DT1PRI 117 0 Z
bit 115 C 0 *
bit 114 O 1 DT1SEC 115 0 Z
bit 113 C 0 *
bit 112 O 1 MOSI 113 0 Z
bit 111 I 1 MOSI
bit 110 C 0 *
bit 109 O 1 MISO 110 0 Z
bit 108 I 1 MISO
bit 107 C 0 *
bit 106 O 1 SCK 107 0 Z
bit 105 I 1 SCK
bit 104 C 0 *
bit 103 O 1 PF0 104 0 Z
bit 102 I 1 PF0
bit 101 C 0 *
bit 100 O 1 PF1 101 0 Z
bit 99 I 1 PF1
bit 98 C 0 *
bit 97 O 1 PF2 98 0 Z
bit 96 I 1 PF2
bit 95 C 0 *
bit 94 O 1 PF3 95 0 Z
bit 93 I 1 PF3
bit 92 C 0 *
bit 91 O 1 PF4 92 0 Z
bit 90 I 1 PF4
bit 89 C 0 *
bit 88 O 1 PF5 89 0 Z
bit 87 I 1 PF5
bit 86 C 0 *
bit 85 O 1 PF6 86 0 Z
bit 84 I 1 PF6
bit 83 C 0 *
bit 82 O 1 PF7 83 0 Z
bit 81 I 1 PF7
bit 80 C 0 *
bit 79 O 1 PF8 80 0 Z
bit 78 I 1 PF8
bit 77 C 0 *
bit 76 O 1 PF9 77 0 Z
bit 75 I 1 PF9
bit 74 C 0 *
bit 73 O 1 PF10 74 0 Z
bit 72 I 1 PF10
bit 71 C 0 *
bit 70 O 1 PF11 71 0 Z
bit 69 I 1 PF11
bit 68 C 0 *
bit 67 O 1 PF12 68 0 Z
bit 66 I 1 PF12
bit 65 C 0 *
bit 64 O 1 PF13 65 0 Z
bit 63 I 1 PF13
bit 62 C 0 *
bit 61 O 1 PF14 62 0 Z
bit 60 I 1 PF14
bit 59 C 0 *
bit 58 O 1 PF15 59 0 Z
bit 57 I 1 PF15
bit 56 C 0 *
bit 55 O 1 PP3 56 0 Z
bit 54 I 1 PP3
bit 53 C 0 *
bit 52 O 1 PP2 53 0 Z
bit 51 I 1 PP2
bit 50 C 0 *
bit 49 O 1 PP1 50 0 Z
bit 48 I 1 PP1
bit 47 C 0 *
bit 46 O 1 PP0 47 0 Z
bit 45 I 1 PP0
bit 44 I 1 PP_CLK
bit 43 I 1 NMI
bit 42 I 1 RESET_B
bit 41 O 1 SCKE 39 0 Z
bit 40 O 1 SMS_B 39 0 Z
bit 39 C 0 *
bit 38 O 1 CLKOUT 39 0 Z
bit 37 O 1 SRAS_B 39 0 Z
bit 36 O 1 SCAS_B 39 0 Z
bit 35 O 1 SWE_B 39 0 Z
bit 34 O 1 SA10 39 0 Z
bit 33 I 1 BR_B
bit 32 I 1 ARDY
bit 31 O 1 AMS_B0 27 0 Z
bit 30 O 1 AMS_B1 27 0 Z
bit 29 O 1 AMS_B2 27 0 Z
bit 28 O 1 AMS_B3 27 0 Z
bit 27 C 0 *
bit 26 O 1 AOE_B 27 0 Z
bit 25 O 1 ARE_B 27 0 Z
bit 24 O 1 AWE_B 27 0 Z
bit 23 O 1 ABE_B0 17 0 Z
bit 22 O 1 ABE_B1 17 0 Z
bit 21 O 1 ADDR[1] 17 0 Z
bit 20 O 1 ADDR[2] 17 0 Z
bit 19 O 1 ADDR[3] 17 0 Z
bit 18 O 1 ADDR[4] 17 0 Z
bit 17 C 0 *
bit 16 O 1 ADDR[5] 17 0 Z
bit 15 O 1 ADDR[6] 17 0 Z
bit 14 O 1 ADDR[7] 17 0 Z
bit 13 O 1 ADDR[8] 17 0 Z
bit 12 O 1 ADDR[9] 17 0 Z
bit 11 O 1 ADDR[10] 17 0 Z
bit 10 O 1 ADDR[11] 17 0 Z
bit 9 O 1 ADDR[12] 17 0 Z
bit 8 O 1 ADDR[13] 17 0 Z
bit 7 O 1 ADDR[14] 17 0 Z
bit 6 O 1 ADDR[15] 17 0 Z
bit 5 O 1 ADDR[16] 17 0 Z
bit 4 O 1 ADDR[17] 17 0 Z
bit 3 O 1 ADDR[18] 17 0 Z
bit 2 O 1 ADDR[19] 17 0 Z
bit 1 O 1 BGH_B
bit 0 O 1 BG_B
