#
# $Id: bcm1250 558 2003-09-05 21:09:14Z telka $
#
# JTAG declarations for BCM1250
# Copyright (C) 2003 ETC s.r.o.
#
# This program is free software; you can redistribute it and/or
# modify it under the terms of the GNU General Public License
# as published by the Free Software Foundation; either version 2
# of the License, or (at your option) any later version.
#
# This program is distributed in the hope that it will be useful,
# but WITHOUT ANY WARRANTY; without even the implied warranty of
# MERCHANTABILITY or FITNESS FOR A PARTICULAR PURPOSE.  See the
# GNU General Public License for more details.
#
# You should have received a copy of the GNU General Public License
# along with this program; if not, write to the Free Software
# Foundation, Inc., 59 Temple Place - Suite 330, Boston, MA
# 02111-1307, USA.
#
# Written by Matan Ziv-Av <matan@svgalib.org>, 2003.
#

signal TRST_L
signal TMS
signal TDO
signal TDI
signal TCK
signal SPARE2
signal SPARE3
signal SPARE4
signal SPARE5
signal SDA0
signal SDA1
signal SCL0
signal SCL1
signal S1_TIN
signal S1_RTS_TSTROBE
signal S1_RIN
signal S1_DOUT
signal S1_DIN
signal S1_CTS_TCLKIN
signal S1_COUT
signal S1_CIN_RCLKIN
signal S0_TIN
signal S0_RTS_TSTROBE
signal S0_RIN
signal S0_DOUT
signal S0_DIN
signal S0_CTS_TCLKIN
signal S0_COUT
signal S0_CIN_RCLKIN
signal RESET_L
signal RESETOUT_L
signal REFCLK2
signal REFCLK01
signal P_TRDY_L
signal P_STOP_L
signal P_SERR_L
signal P_RST_L
signal P_REQ_l0
signal P_REQ_L1
signal P_REQ_L2
signal P_REQ_L3
signal P_PERR_L
signal P_PAR
signal P_IRDY_L
signal P_INTD_L
signal P_INTC_L
signal P_INTB_L
signal P_INTA_L
signal P_GNT_l0
signal P_GNT_L1
signal P_GNT_L2
signal P_GNT_L3
signal P_FRAME_L
signal P_DEVSEL_L
signal P_CLK
signal P_CBE_L0
signal P_CBE_L1
signal P_CBE_L2
signal P_CBE_L3
signal P_AD0
signal P_AD1
signal P_AD2
signal P_AD3
signal P_AD4
signal P_AD5
signal P_AD6
signal P_AD7
signal P_AD8
signal P_AD9
signal P_AD10
signal P_AD11
signal P_AD12
signal P_AD13
signal P_AD14
signal P_AD15
signal P_AD16
signal P_AD17
signal P_AD18
signal P_AD19
signal P_AD20
signal P_AD21
signal P_AD22
signal P_AD23
signal P_AD24
signal P_AD25
signal P_AD26
signal P_AD27
signal P_AD28
signal P_AD29
signal P_AD30
signal P_AD31
signal PLLBYP
signal PC_ENVPP
signal PC_ENV5V
signal PC_ENV3V
signal M1_WE_L
signal M1_RAS_L
signal M1_ECC0
signal M1_ECC1
signal M1_ECC2
signal M1_ECC3
signal M1_ECC4
signal M1_ECC5
signal M1_ECC6
signal M1_ECC7
signal M1_DQS0
signal M1_DQS1
signal M1_DQS2
signal M1_DQS3
signal M1_DQS4
signal M1_DQS5
signal M1_DQS6
signal M1_DQS7
signal M1_DQS8
signal M1_DQ0
signal M1_DQ1
signal M1_DQ2
signal M1_DQ3
signal M1_DQ4
signal M1_DQ5
signal M1_DQ6
signal M1_DQ7
signal M1_DQ8
signal M1_DQ9
signal M1_DQ10
signal M1_DQ11
signal M1_DQ12
signal M1_DQ13
signal M1_DQ14
signal M1_DQ15
signal M1_DQ16
signal M1_DQ17
signal M1_DQ18
signal M1_DQ19
signal M1_DQ20
signal M1_DQ21
signal M1_DQ22
signal M1_DQ23
signal M1_DQ24
signal M1_DQ25
signal M1_DQ26
signal M1_DQ27
signal M1_DQ28
signal M1_DQ29
signal M1_DQ30
signal M1_DQ31
signal M1_DQ32
signal M1_DQ33
signal M1_DQ34
signal M1_DQ35
signal M1_DQ36
signal M1_DQ37
signal M1_DQ38
signal M1_DQ39
signal M1_DQ40
signal M1_DQ41
signal M1_DQ42
signal M1_DQ43
signal M1_DQ44
signal M1_DQ45
signal M1_DQ46
signal M1_DQ47
signal M1_DQ48
signal M1_DQ49
signal M1_DQ50
signal M1_DQ51
signal M1_DQ52
signal M1_DQ53
signal M1_DQ54
signal M1_DQ55
signal M1_DQ56
signal M1_DQ57
signal M1_DQ58
signal M1_DQ59
signal M1_DQ60
signal M1_DQ61
signal M1_DQ62
signal M1_DQ63
signal M1_CS_L0
signal M1_CS_L1
signal M1_CS_L2
signal M1_CS_L3
signal M1_CLK_L
signal M1_CLK
signal M1_CKE
signal M1_CAS_L
signal M1_BA0
signal M1_BA1
signal M1_A0
signal M1_A1
signal M1_A2
signal M1_A3
signal M1_A4
signal M1_A5
signal M1_A6
signal M1_A7
signal M1_A8
signal M1_A9
signal M1_A10
signal M1_A11
signal M1_A12
signal M0_WE_L
signal M0_RAS_L
signal M0_ECC0
signal M0_ECC1
signal M0_ECC2
signal M0_ECC3
signal M0_ECC4
signal M0_ECC5
signal M0_ECC6
signal M0_ECC7
signal M0_DQS0
signal M0_DQS1
signal M0_DQS2
signal M0_DQS3
signal M0_DQS4
signal M0_DQS5
signal M0_DQS6
signal M0_DQS7
signal M0_DQS8
signal M0_DQ0
signal M0_DQ1
signal M0_DQ2
signal M0_DQ3
signal M0_DQ4
signal M0_DQ5
signal M0_DQ6
signal M0_DQ7
signal M0_DQ8
signal M0_DQ9
signal M0_DQ10
signal M0_DQ11
signal M0_DQ12
signal M0_DQ13
signal M0_DQ14
signal M0_DQ15
signal M0_DQ16
signal M0_DQ17
signal M0_DQ18
signal M0_DQ19
signal M0_DQ20
signal M0_DQ21
signal M0_DQ22
signal M0_DQ23
signal M0_DQ24
signal M0_DQ25
signal M0_DQ26
signal M0_DQ27
signal M0_DQ28
signal M0_DQ29
signal M0_DQ30
signal M0_DQ31
signal M0_DQ32
signal M0_DQ33
signal M0_DQ34
signal M0_DQ35
signal M0_DQ36
signal M0_DQ37
signal M0_DQ38
signal M0_DQ39
signal M0_DQ40
signal M0_DQ41
signal M0_DQ42
signal M0_DQ43
signal M0_DQ44
signal M0_DQ45
signal M0_DQ46
signal M0_DQ47
signal M0_DQ48
signal M0_DQ49
signal M0_DQ50
signal M0_DQ51
signal M0_DQ52
signal M0_DQ53
signal M0_DQ54
signal M0_DQ55
signal M0_DQ56
signal M0_DQ57
signal M0_DQ58
signal M0_DQ59
signal M0_DQ60
signal M0_DQ61
signal M0_DQ62
signal M0_DQ63
signal M0_CS_L0
signal M0_CS_L1
signal M0_CS_L2
signal M0_CS_L3
signal M0_CLK_L
signal M0_CLK
signal M0_CKE
signal M0_CAS_L
signal M0_BA0
signal M0_BA1
signal M0_A0
signal M0_A1
signal M0_A2
signal M0_A3
signal M0_A4
signal M0_A5
signal M0_A6
signal M0_A7
signal M0_A8
signal M0_A9
signal M0_A10
signal M0_A11
signal M0_A12
signal LDT_TX_CTLP
signal LDT_TX_CTLN
signal LDT_TX_CLKP
signal LDT_TX_CLKN
signal LDT_TX_CADP0
signal LDT_TX_CADP1
signal LDT_TX_CADP2
signal LDT_TX_CADP3
signal LDT_TX_CADP4
signal LDT_TX_CADP5
signal LDT_TX_CADP6
signal LDT_TX_CADP7
signal LDT_TX_CADN0
signal LDT_TX_CADN1
signal LDT_TX_CADN2
signal LDT_TX_CADN3
signal LDT_TX_CADN4
signal LDT_TX_CADN5
signal LDT_TX_CADN6
signal LDT_TX_CADN7
signal LDT_RX_CTLP
signal LDT_RX_CTLN
signal LDT_RX_CADP0
signal LDT_RX_CADP1
signal LDT_RX_CADP2
signal LDT_RX_CADP3
signal LDT_RX_CADP4
signal LDT_RX_CADP5
signal LDT_RX_CADP6
signal LDT_RX_CADP7
signal LDT_RX_CADN0
signal LDT_RX_CADN1
signal LDT_RX_CADN2
signal LDT_RX_CADN3
signal LDT_RX_CADN4
signal LDT_RX_CADN5
signal LDT_RX_CADN6
signal LDT_RX_CADN7
signal LDT_RESET_L
signal LDT_PWROK
signal IO_WR_L
signal IO_RW
signal IO_RDY
signal IO_OE_L
signal IO_CS_L0
signal IO_CS_L1
signal IO_CS_L2
signal IO_CS_L3
signal IO_CS_L4
signal IO_CS_L5
signal IO_CS_L6
signal IO_CS_L7
signal IO_CLK100
signal IO_ALE
signal IO_AD0
signal IO_AD1
signal IO_AD2
signal IO_AD3
signal IO_AD4
signal IO_AD5
signal IO_AD6
signal IO_AD7
signal IO_AD8
signal IO_AD9
signal IO_AD10
signal IO_AD11
signal IO_AD12
signal IO_AD13
signal IO_AD14
signal IO_AD15
signal IO_AD16
signal IO_AD17
signal IO_AD18
signal IO_AD19
signal IO_AD20
signal IO_AD21
signal IO_AD22
signal IO_AD23
signal IO_AD24
signal IO_AD25
signal IO_AD26
signal IO_AD27
signal IO_AD28
signal IO_AD29
signal IO_AD30
signal IO_AD31
signal GPIO0
signal GPIO1
signal GPIO2
signal GPIO3
signal GPIO4
signal GPIO5
signal GPIO6
signal GPIO7
signal GPIO8
signal GPIO9
signal GPIO10
signal GPIO11
signal GPIO12
signal GPIO13
signal GPIO14
signal GPIO15
signal E2_TXER
signal E2_TXEN
signal E2_TXD0
signal E2_TXD1
signal E2_TXD2
signal E2_TXD3
signal E2_TXD4
signal E2_TXD5
signal E2_TXD6
signal E2_TXD7
signal E2_TCLKO
signal E2_TCLKI
signal E2_RXER
signal E2_RXDV
signal E2_RXD0
signal E2_RXD1
signal E2_RXD2
signal E2_RXD3
signal E2_RXD4
signal E2_RXD5
signal E2_RXD6
signal E2_RXD7
signal E2_RCLK
signal E2_MDIO
signal E2_MDC
signal E2_GENO
signal E2_CRS
signal E2_COL
signal E1_TXER
signal E1_TXEN
signal E1_TXD0
signal E1_TXD1
signal E1_TXD2
signal E1_TXD3
signal E1_TXD4
signal E1_TXD5
signal E1_TXD6
signal E1_TXD7
signal E1_TCLKO
signal E1_TCLKI
signal E1_RXER
signal E1_RXDV
signal E1_RXD0
signal E1_RXD1
signal E1_RXD2
signal E1_RXD3
signal E1_RXD4
signal E1_RXD5
signal E1_RXD6
signal E1_RXD7
signal E1_RCLK
signal E1_MDIO
signal E1_MDC
signal E1_GENO
signal E1_CRS
signal E1_COL
signal E0_TXER
signal E0_TXEN
signal E0_TXD0
signal E0_TXD1
signal E0_TXD2
signal E0_TXD3
signal E0_TXD4
signal E0_TXD5
signal E0_TXD6
signal E0_TXD7
signal E0_TCLKO
signal E0_TCLKI
signal E0_RXER
signal E0_RXDV
signal E0_RXD0
signal E0_RXD1
signal E0_RXD2
signal E0_RXD3
signal E0_RXD4
signal E0_RXD5
signal E0_RXD6
signal E0_RXD7
signal E0_RCLK
signal E0_MDIO
signal E0_MDC
signal E0_GENO
signal E0_CRS
signal E0_COL
signal DEBUG_L
signal COLDRES_L
signal CLK100P
signal CLK100N
signal GND0
signal GND1
signal GND2
signal GND3
signal GND4
signal GND5
signal GND6
signal GND7
signal GND8
signal GND9
signal GND10
signal GND11
signal GND12
signal GND13
signal GND14
signal GND15
signal GND16
signal GND17
signal GND18
signal GND19
signal GND20
signal GND21
signal GND22
signal GND23
signal GND24
signal GND25
signal GND26
signal GND27
signal GND28
signal GND29
signal GND30
signal GND31
signal GND32
signal GND33
signal GND34
signal GND35
signal GND36
signal GND37
signal GND38
signal GND39
signal GND40
signal GND41
signal GND42
signal GND43
signal GND44
signal GND45
signal GND46
signal GND47
signal GND48
signal GND49
signal GND50
signal GND51
signal GND52
signal GND53
signal GND54
signal GND55
signal GND56
signal GND57
signal GND58
signal GND59
signal GND60
signal GND61
signal GND62
signal GND63
signal GND64
signal GND65
signal GND66
signal GND67
signal GND68
signal GND69
signal GND70
signal GND71
signal GND72
signal GND73
signal GND74
signal GND75
signal GND76
signal GND77
signal GND78
signal GND79
signal GND80
signal GND81
signal GND82
signal GND83
signal GND84
signal GND85
signal GND86
signal GND87
signal GND88
signal GND89
signal GND90
signal GND91
signal GND92
signal GND93
signal GND94
signal GND95
signal GND96
signal GND97
signal GND98
signal GND99
signal GND100
signal GND101
signal GND102
signal GND103
signal GND104
signal GND105
signal GND106
signal GND107
signal GND108
signal GND109
signal GND110
signal GND111
signal GND112
signal GND113
signal GND114
signal GND115
signal GND116
signal GND117
signal GND118
signal GND119
signal GND120
signal GND121
signal GND122
signal GND123
signal GND124
signal GND125
signal GND126
signal GND127
signal GND128
signal GND129
signal GND130
signal GND131
signal GND132
signal GND133
signal GND134
signal GND135
signal GND136
signal GND137
signal GND138
signal GND139
signal GND140
signal GND141
signal GND142
signal GND143
signal GND144
signal GND145
signal GND146
signal GND147
signal GND148
signal GND149
signal GND150
signal GND151
signal GND152
signal GND153
signal GND154
signal GND155
signal GND156
signal GND157
signal GND158
signal GND159
signal GND160
signal GND161
signal GND162
signal GND163
signal GND164
signal GND165
signal GND166
signal GND167
signal GND168
signal GND169
signal GND170
signal GND171
signal GND172
signal GND173
signal GND174
signal GND175
signal GND176
signal GND177
signal GND178
signal GND179
signal GND180
signal LDT_RX_CAL0
signal LDT_RX_CAL1
signal LDT_RX_CLKN
signal LDT_RX_CLKP
signal LDT_TX_CAL0
signal LDT_TX_CAL1
signal M0_VREF
signal M1_VREF
signal TEMPN
signal TEMPP
signal VDDCORE0
signal VDDCORE1
signal VDDCORE2
signal VDDCORE3
signal VDDCORE4
signal VDDCORE5
signal VDDCORE6
signal VDDCORE7
signal VDDCORE8
signal VDDCORE9
signal VDDCORE10
signal VDDCORE11
signal VDDCORE12
signal VDDCORE13
signal VDDCORE14
signal VDDCORE15
signal VDDCORE16
signal VDDCORE17
signal VDDCORE18
signal VDDCORE19
signal VDDCORE20
signal VDDCORE21
signal VDDCORE22
signal VDDCORE23
signal VDDCORE24
signal VDDCORE25
signal VDDCORE26
signal VDDCORE27
signal VDDCORE28
signal VDDCORE29
signal VDDCORE30
signal VDDCORE31
signal VDDCORE32
signal VDDCORE33
signal VDDCORE34
signal VDDCORE35
signal VDDCORE36
signal VDDCORE37
signal VDDCORE38
signal VDDCORE39
signal VDDCORE40
signal VDDCORE41
signal VDDCORE42
signal VDDCORE43
signal VDDCORE44
signal VDDCORE45
signal VDDCORE46
signal VDDIO0
signal VDDIO1
signal VDDIO2
signal VDDIO3
signal VDDIO4
signal VDDIO5
signal VDDIO6
signal VDDIO7
signal VDDIO8
signal VDDIO9
signal VDDIO10
signal VDDIO11
signal VDDIO12
signal VDDIO13
signal VDDIO14
signal VDDIO15
signal VDDIO16
signal VDDIO17
signal VDDIO18
signal VDDIO19
signal VDDIO20
signal VDDIO21
signal VDDIO22
signal VDDIO23
signal VDDIO24
signal VDDIO25
signal VDDIO26
signal VDDIO27
signal VDDIO28
signal VDDIO29
signal VDDIO30
signal VDDIO31
signal VDDIO32
signal VDDIO33
signal VDDIO34
signal VDDIO35
signal VDDIO36
signal VDDIO37
signal VDDIO38
signal VDDIO39
signal VDDIO40
signal VDDIO41
signal VDDIO42
signal VDDIO43
signal VDDIO44
signal VDDIO45
signal VDDIO46
signal VDDIO47
signal VDDIO48
signal VDDIO49
signal VDDIO50
signal VDDIO51
signal VDDIO52
signal VDDIO53
signal VDDIO54
signal VDDIO55
signal VDDLDT0
signal VDDLDT1
signal VDDLDT2
signal VDDLDT3
signal VDDLDT4
signal VDDLDT5
signal VDDLDT6
signal VDDLDT7
signal VDDLDT8
signal VDDLDT9
signal VDDLDT10
signal VDDLDT11
signal VDDLDT12
signal VDDLDT13
signal VDDLDT14
signal VDDLDT15
signal VDDLDT16
signal VDDLDT17
signal VDDLDT18
signal VDDMEM0
signal VDDMEM1
signal VDDMEM2
signal VDDMEM3
signal VDDMEM4
signal VDDMEM5
signal VDDMEM6
signal VDDMEM7
signal VDDMEM8
signal VDDMEM9
signal VDDMEM10
signal VDDMEM11
signal VDDMEM12
signal VDDMEM13
signal VDDMEM14
signal VDDMEM15
signal VDDMEM16
signal VDDMEM17
signal VDDMEM18
signal VDDMEM19
signal VDDMEM20
signal VDDMEM21
signal VDDMEM22
signal VDDMEM23
signal VDDMEM24
signal VDDMEM25
signal VDDMEM26
signal VDDMEM27
signal VDDMEM28
signal VDDMEM29
signal VDDMEM30
signal VDDMEM31
signal VDDMEM32
signal VDDMEM33
signal VDDMEM34
signal VDDMEM35
signal VDDMEM36
signal VDDMEM37
signal VDDMEM38
signal VDDMEM39
signal VDDMEM40
signal VDDMEM41
signal VDDMEM42
signal VDDMEM43
signal VDDMEM44
signal VDDMEM45
signal VDDMEM46
signal VDDMEM47
signal VDDMEM48

register	BSR	1434
register	BR	1
register	DIR	32
register	CTRL	12
register	DATAR	277
register	ADDRR	77
register	SCD	64
register	IMP	32


instruction length 6

instruction	EXTEST		000000	BSR
instruction	IDCODE		000001	DIR
instruction	SAMPLE/PRELOAD	111101	BSR
instruction	BYPASS		111111	BR
instruction	CONTROLL	001010	CTRL
instruction	DATA		001001	DATAR
instruction	ADDR		001000	ADDRR
instruction	SCANSCD		110110	SCD
instruction	IMPCODE		000011	IMP

bit 1433 O 0 *
bit 1432 O 0 *
bit 1431 O 0 *
bit 1430 O 0 *
bit 1429 O 0 *
bit 1428 O 0 *
bit 1427 O 0 *
bit 1426 O 0 *
bit 1425 O 0 *
bit 1424 O 0 *
bit 1423 O 0 *
bit 1422 O 0 *
bit 1421 O 0 *
bit 1420 O 0 *
bit 1419 O 0 *
bit 1418 O 0 *
bit 1417 C 0 *
bit 1416 O 0 *
bit 1415 O 0 *
bit 1414 I 1 LDT_RX_CTLP
bit 1413 I 1 LDT_RX_CTLN
bit 1412 O 1 LDT_TX_CADP0 1417 0 Z
bit 1411 O 1 LDT_TX_CADN0 1417 0 Z
bit 1410 I 1 LDT_RX_CADP7
bit 1409 I 1 LDT_RX_CADN7
bit 1408 O 1 LDT_TX_CADP1 1417 0 Z
bit 1407 O 1 LDT_TX_CADN1 1417 0 Z
bit 1406 I 1 LDT_RX_CADP6
bit 1405 I 1 LDT_RX_CADN6
bit 1404 O 1 LDT_TX_CADP2 1417 0 Z
bit 1403 O 1 LDT_TX_CADN2 1417 0 Z
bit 1402 I 1 LDT_RX_CADP5
bit 1401 I 1 LDT_RX_CADN5
bit 1400 O 1 LDT_TX_CADP3 1417 0 Z
bit 1399 O 1 LDT_TX_CADN3 1417 0 Z
bit 1398 I 1 LDT_RX_CADP4
bit 1397 I 1 LDT_RX_CADN4
bit 1396 O 1 LDT_TX_CLKP 1417 0 Z
bit 1395 O 1 LDT_TX_CLKN 1417 0 Z
bit 1394 O 1 LDT_TX_CADP4 1417 0 Z
bit 1393 O 1 LDT_TX_CADN4 1417 0 Z
bit 1392 I 1 LDT_RX_CADP3
bit 1391 I 1 LDT_RX_CADN3
bit 1390 O 1 LDT_TX_CADP5 1417 0 Z
bit 1389 O 1 LDT_TX_CADN5 1417 0 Z
bit 1388 I 1 LDT_RX_CADP2
bit 1387 I 1 LDT_RX_CADN2
bit 1386 O 1 LDT_TX_CADP6 1417 0 Z
bit 1385 O 1 LDT_TX_CADN6 1417 0 Z
bit 1384 I 1 LDT_RX_CADP1
bit 1383 I 1 LDT_RX_CADN1
bit 1382 O 1 LDT_TX_CADP7 1417 0 Z
bit 1381 O 1 LDT_TX_CADN7 1417 0 Z
bit 1380 I 1 LDT_RX_CADP0
bit 1379 I 1 LDT_RX_CADN0
bit 1378 O 1 LDT_TX_CTLP 1417 0 Z
bit 1377 O 1 LDT_TX_CTLN 1417 0 Z
bit 1376 O 1 LDT_PWROK 1375 0 Z
bit 1375 C 0 *
bit 1374 I 1 LDT_PWROK
bit 1373 O 1 LDT_RESET_L 1372 0 Z
bit 1372 C 0 *
bit 1371 I 1 LDT_RESET_L
bit 1370 O 1 M1_DQ0 1369 0 Z
bit 1369 C 0 *
bit 1368 I 1 M1_DQ0
bit 1367 O 1 M1_DQ1 1366 0 Z
bit 1366 C 0 *
bit 1365 I 1 M1_DQ1
bit 1364 O 1 M1_DQ2 1363 0 Z
bit 1363 C 0 *
bit 1362 I 1 M1_DQ2
bit 1361 O 1 M1_DQ3 1360 0 Z
bit 1360 C 0 *
bit 1359 I 1 M1_DQ3
bit 1358 O 1 M1_DQS0 1357 0 Z
bit 1357 C 0 *
bit 1356 I 1 M1_DQS0
bit 1355 O 1 M1_DQ4 1354 0 Z
bit 1354 C 0 *
bit 1353 I 1 M1_DQ4
bit 1352 O 1 M1_DQ5 1351 0 Z
bit 1351 C 0 *
bit 1350 I 1 M1_DQ5
bit 1349 O 1 M1_DQ6 1348 0 Z
bit 1348 C 0 *
bit 1347 I 1 M1_DQ6
bit 1346 O 1 M1_DQ7 1345 0 Z
bit 1345 C 0 *
bit 1344 I 1 M1_DQ7
bit 1343 O 1 M1_DQ8 1342 0 Z
bit 1342 C 0 *
bit 1341 I 1 M1_DQ8
bit 1340 O 1 M1_DQ9 1339 0 Z
bit 1339 C 0 *
bit 1338 I 1 M1_DQ9
bit 1337 O 1 M1_DQ10 1336 0 Z
bit 1336 C 0 *
bit 1335 I 1 M1_DQ10
bit 1334 O 1 M1_DQ11 1333 0 Z
bit 1333 C 0 *
bit 1332 I 1 M1_DQ11
bit 1331 O 1 M1_DQS1 1330 0 Z
bit 1330 C 0 *
bit 1329 I 1 M1_DQS1
bit 1328 O 1 M1_DQ12 1327 0 Z
bit 1327 C 0 *
bit 1326 I 1 M1_DQ12
bit 1325 O 1 M1_DQ13 1324 0 Z
bit 1324 C 0 *
bit 1323 I 1 M1_DQ13
bit 1322 O 1 M1_DQ14 1321 0 Z
bit 1321 C 0 *
bit 1320 I 1 M1_DQ14
bit 1319 O 1 M1_DQ15 1318 0 Z
bit 1318 C 0 *
bit 1317 I 1 M1_DQ15
bit 1316 O 1 M1_DQ16 1315 0 Z
bit 1315 C 0 *
bit 1314 I 1 M1_DQ16
bit 1313 O 1 M1_DQ17 1312 0 Z
bit 1312 C 0 *
bit 1311 I 1 M1_DQ17
bit 1310 O 1 M1_DQ18 1309 0 Z
bit 1309 C 0 *
bit 1308 I 1 M1_DQ18
bit 1307 O 1 M1_DQ19 1306 0 Z
bit 1306 C 0 *
bit 1305 I 1 M1_DQ19
bit 1304 O 1 M1_DQS2 1303 0 Z
bit 1303 C 0 *
bit 1302 I 1 M1_DQS2
bit 1301 O 1 M1_DQ20 1300 0 Z
bit 1300 C 0 *
bit 1299 I 1 M1_DQ20
bit 1298 O 1 M1_DQ21 1297 0 Z
bit 1297 C 0 *
bit 1296 I 1 M1_DQ21
bit 1295 O 1 M1_DQ22 1294 0 Z
bit 1294 C 0 *
bit 1293 I 1 M1_DQ22
bit 1292 O 1 M1_DQ23 1291 0 Z
bit 1291 C 0 *
bit 1290 I 1 M1_DQ23
bit 1289 O 1 M1_DQ24 1288 0 Z
bit 1288 C 0 *
bit 1287 I 1 M1_DQ24
bit 1286 O 1 M1_DQ25 1285 0 Z
bit 1285 C 0 *
bit 1284 I 1 M1_DQ25
bit 1283 O 1 M1_DQ26 1282 0 Z
bit 1282 C 0 *
bit 1281 I 1 M1_DQ26
bit 1280 O 1 M1_DQ27 1279 0 Z
bit 1279 C 0 *
bit 1278 I 1 M1_DQ27
bit 1277 O 1 M1_DQS3 1276 0 Z
bit 1276 C 0 *
bit 1275 I 1 M1_DQS3
bit 1274 O 1 M1_DQ28 1273 0 Z
bit 1273 C 0 *
bit 1272 I 1 M1_DQ28
bit 1271 O 1 M1_DQ29 1270 0 Z
bit 1270 C 0 *
bit 1269 I 1 M1_DQ29
bit 1268 O 1 M1_DQ30 1267 0 Z
bit 1267 C 0 *
bit 1266 I 1 M1_DQ30
bit 1265 O 1 M1_DQ31 1264 0 Z
bit 1264 C 0 *
bit 1263 I 1 M1_DQ31
bit 1262 O 1 M1_A12 1261 0 Z
bit 1261 C 0 *
bit 1260 O 0 *
bit 1259 O 1 M1_A8 1258 0 Z
bit 1258 C 0 *
bit 1257 O 0 *
bit 1256 O 1 M1_A11 1255 0 Z
bit 1255 C 0 *
bit 1254 O 0 *
bit 1253 O 1 M1_A5 1252 0 Z
bit 1252 C 0 *
bit 1251 O 0 *
bit 1250 O 1 M1_A9 1249 0 Z
bit 1249 C 0 *
bit 1248 O 0 *
bit 1247 O 1 M1_A6 1246 0 Z
bit 1246 C 0 *
bit 1245 O 0 *
bit 1244 O 1 M1_A7 1243 0 Z
bit 1243 C 0 *
bit 1242 O 0 *
bit 1241 O 1 M1_A2 1240 0 Z
bit 1240 C 0 *
bit 1239 O 0 *
bit 1238 O 1 M1_A4 1237 0 Z
bit 1237 C 0 *
bit 1236 O 0 *
bit 1235 O 1 M1_A1 1234 0 Z
bit 1234 C 0 *
bit 1233 O 0 *
bit 1232 O 1 M1_A3 1231 0 Z
bit 1231 C 0 *
bit 1230 O 0 *
bit 1229 O 1 M1_BA1 1228 0 Z
bit 1228 C 0 *
bit 1227 O 0 *
bit 1226 O 1 M1_A0 1225 0 Z
bit 1225 C 0 *
bit 1224 O 0 *
bit 1223 O 1 M1_WE_L 1222 0 Z
bit 1222 C 0 *
bit 1221 O 0 *
bit 1220 O 1 M1_A10 1219 0 Z
bit 1219 C 0 *
bit 1218 O 0 *
bit 1217 O 1 M1_CAS_L 1216 0 Z
bit 1216 C 0 *
bit 1215 O 0 *
bit 1214 O 1 M1_BA0 1213 0 Z
bit 1213 C 0 *
bit 1212 O 0 *
bit 1211 O 1 M1_CS_L1 1210 0 Z
bit 1210 C 0 *
bit 1209 O 0 *
bit 1208 O 1 M1_CS_L0 1207 0 Z
bit 1207 C 0 *
bit 1206 O 0 *
bit 1205 O 1 M1_CS_L2 1204 0 Z
bit 1204 C 0 *
bit 1203 O 0 *
bit 1202 O 1 M1_RAS_L 1201 0 Z
bit 1201 C 0 *
bit 1200 O 0 *
bit 1199 O 1 M1_CS_L3 1198 0 Z
bit 1198 C 0 *
bit 1197 O 0 *
bit 1196 O 1 M1_CLK 1195 0 Z
bit 1195 C 0 *
bit 1194 O 0 *
bit 1193 O 1 M1_CKE 1192 0 Z
bit 1192 C 0 *
bit 1191 O 0 *
bit 1190 O 1 M1_CLK_L 1189 0 Z
bit 1189 C 0 *
bit 1188 O 0 *
bit 1187 O 1 M1_ECC0 1186 0 Z
bit 1186 C 0 *
bit 1185 I 1 M1_ECC0
bit 1184 O 1 M1_ECC1 1183 0 Z
bit 1183 C 0 *
bit 1182 I 1 M1_ECC1
bit 1181 O 1 M1_ECC2 1180 0 Z
bit 1180 C 0 *
bit 1179 I 1 M1_ECC2
bit 1178 O 1 M1_ECC3 1177 0 Z
bit 1177 C 0 *
bit 1176 I 1 M1_ECC3
bit 1175 O 1 M1_DQS8 1174 0 Z
bit 1174 C 0 *
bit 1173 I 1 M1_DQS8
bit 1172 O 1 M1_ECC4 1171 0 Z
bit 1171 C 0 *
bit 1170 I 1 M1_ECC4
bit 1169 O 1 M1_ECC5 1168 0 Z
bit 1168 C 0 *
bit 1167 I 1 M1_ECC5
bit 1166 O 1 M1_ECC6 1165 0 Z
bit 1165 C 0 *
bit 1164 I 1 M1_ECC6
bit 1163 O 1 M1_ECC7 1162 0 Z
bit 1162 C 0 *
bit 1161 I 1 M1_ECC7
bit 1160 O 1 M1_DQ32 1159 0 Z
bit 1159 C 0 *
bit 1158 I 1 M1_DQ32
bit 1157 O 1 M1_DQ33 1156 0 Z
bit 1156 C 0 *
bit 1155 I 1 M1_DQ33
bit 1154 O 1 M1_DQ34 1153 0 Z
bit 1153 C 0 *
bit 1152 I 1 M1_DQ34
bit 1151 O 1 M1_DQ35 1150 0 Z
bit 1150 C 0 *
bit 1149 I 1 M1_DQ35
bit 1148 O 1 M1_DQS4 1147 0 Z
bit 1147 C 0 *
bit 1146 I 1 M1_DQS4
bit 1145 O 1 M1_DQ36 1144 0 Z
bit 1144 C 0 *
bit 1143 I 1 M1_DQ36
bit 1142 O 1 M1_DQ37 1141 0 Z
bit 1141 C 0 *
bit 1140 I 1 M1_DQ37
bit 1139 O 1 M1_DQ38 1138 0 Z
bit 1138 C 0 *
bit 1137 I 1 M1_DQ38
bit 1136 O 1 M1_DQ39 1135 0 Z
bit 1135 C 0 *
bit 1134 I 1 M1_DQ39
bit 1133 O 1 M1_DQ40 1132 0 Z
bit 1132 C 0 *
bit 1131 I 1 M1_DQ40
bit 1130 O 1 M1_DQ41 1129 0 Z
bit 1129 C 0 *
bit 1128 I 1 M1_DQ41
bit 1127 O 1 M1_DQ42 1126 0 Z
bit 1126 C 0 *
bit 1125 I 1 M1_DQ42
bit 1124 O 1 M1_DQ43 1123 0 Z
bit 1123 C 0 *
bit 1122 I 1 M1_DQ43
bit 1121 O 1 M1_DQS5 1120 0 Z
bit 1120 C 0 *
bit 1119 I 1 M1_DQS5
bit 1118 O 1 M1_DQ44 1117 0 Z
bit 1117 C 0 *
bit 1116 I 1 M1_DQ44
bit 1115 O 1 M1_DQ45 1114 0 Z
bit 1114 C 0 *
bit 1113 I 1 M1_DQ45
bit 1112 O 1 M1_DQ46 1111 0 Z
bit 1111 C 0 *
bit 1110 I 1 M1_DQ46
bit 1109 O 1 M1_DQ47 1108 0 Z
bit 1108 C 0 *
bit 1107 I 1 M1_DQ47
bit 1106 O 1 M1_DQ48 1105 0 Z
bit 1105 C 0 *
bit 1104 I 1 M1_DQ48
bit 1103 O 1 M1_DQ49 1102 0 Z
bit 1102 C 0 *
bit 1101 I 1 M1_DQ49
bit 1100 O 1 M1_DQ50 1099 0 Z
bit 1099 C 0 *
bit 1098 I 1 M1_DQ50
bit 1097 O 1 M1_DQ51 1096 0 Z
bit 1096 C 0 *
bit 1095 I 1 M1_DQ51
bit 1094 O 1 M1_DQS6 1093 0 Z
bit 1093 C 0 *
bit 1092 I 1 M1_DQS6
bit 1091 O 1 M1_DQ52 1090 0 Z
bit 1090 C 0 *
bit 1089 I 1 M1_DQ52
bit 1088 O 1 M1_DQ53 1087 0 Z
bit 1087 C 0 *
bit 1086 I 1 M1_DQ53
bit 1085 O 1 M1_DQ54 1084 0 Z
bit 1084 C 0 *
bit 1083 I 1 M1_DQ54
bit 1082 O 1 M1_DQ55 1081 0 Z
bit 1081 C 0 *
bit 1080 I 1 M1_DQ55
bit 1079 O 1 M1_DQ56 1078 0 Z
bit 1078 C 0 *
bit 1077 I 1 M1_DQ56
bit 1076 O 1 M1_DQ57 1075 0 Z
bit 1075 C 0 *
bit 1074 I 1 M1_DQ57
bit 1073 O 1 M1_DQ58 1072 0 Z
bit 1072 C 0 *
bit 1071 I 1 M1_DQ58
bit 1070 O 1 M1_DQ59 1069 0 Z
bit 1069 C 0 *
bit 1068 I 1 M1_DQ59
bit 1067 O 1 M1_DQS7 1066 0 Z
bit 1066 C 0 *
bit 1065 I 1 M1_DQS7
bit 1064 O 1 M1_DQ60 1063 0 Z
bit 1063 C 0 *
bit 1062 I 1 M1_DQ60
bit 1061 O 1 M1_DQ61 1060 0 Z
bit 1060 C 0 *
bit 1059 I 1 M1_DQ61
bit 1058 O 1 M1_DQ62 1057 0 Z
bit 1057 C 0 *
bit 1056 I 1 M1_DQ62
bit 1055 O 1 M1_DQ63 1054 0 Z
bit 1054 C 0 *
bit 1053 I 1 M1_DQ63
bit 1052 O 1 M0_DQ63 1051 0 Z
bit 1051 C 0 *
bit 1050 I 1 M0_DQ63
bit 1049 O 1 M0_DQ62 1048 0 Z
bit 1048 C 0 *
bit 1047 I 1 M0_DQ62
bit 1046 O 1 M0_DQ61 1045 0 Z
bit 1045 C 0 *
bit 1044 I 1 M0_DQ61
bit 1043 O 1 M0_DQ60 1042 0 Z
bit 1042 C 0 *
bit 1041 I 1 M0_DQ60
bit 1040 O 1 M0_DQS7 1039 0 Z
bit 1039 C 0 *
bit 1038 I 1 M0_DQS7
bit 1037 O 1 M0_DQ59 1036 0 Z
bit 1036 C 0 *
bit 1035 I 1 M0_DQ59
bit 1034 O 1 M0_DQ58 1033 0 Z
bit 1033 C 0 *
bit 1032 I 1 M0_DQ58
bit 1031 O 1 M0_DQ57 1030 0 Z
bit 1030 C 0 *
bit 1029 I 1 M0_DQ57
bit 1028 O 1 M0_DQ56 1027 0 Z
bit 1027 C 0 *
bit 1026 I 1 M0_DQ56
bit 1025 O 1 M0_DQ55 1024 0 Z
bit 1024 C 0 *
bit 1023 I 1 M0_DQ55
bit 1022 O 1 M0_DQ54 1021 0 Z
bit 1021 C 0 *
bit 1020 I 1 M0_DQ54
bit 1019 O 1 M0_DQ53 1018 0 Z
bit 1018 C 0 *
bit 1017 I 1 M0_DQ53
bit 1016 O 1 M0_DQ52 1015 0 Z
bit 1015 C 0 *
bit 1014 I 1 M0_DQ52
bit 1013 O 1 M0_DQS6 1012 0 Z
bit 1012 C 0 *
bit 1011 I 1 M0_DQS6
bit 1010 O 1 M0_DQ51 1009 0 Z
bit 1009 C 0 *
bit 1008 I 1 M0_DQ51
bit 1007 O 1 M0_DQ50 1006 0 Z
bit 1006 C 0 *
bit 1005 I 1 M0_DQ50
bit 1004 O 1 M0_DQ49 1003 0 Z
bit 1003 C 0 *
bit 1002 I 1 M0_DQ49
bit 1001 O 1 M0_DQ48 1000 0 Z
bit 1000 C 0 *
bit 999 I 1 M0_DQ48
bit 998 O 1 M0_DQ47 997 0 Z
bit 997 C 0 *
bit 996 I 1 M0_DQ47
bit 995 O 1 M0_DQ46 994 0 Z
bit 994 C 0 *
bit 993 I 1 M0_DQ46
bit 992 O 1 M0_DQ45 991 0 Z
bit 991 C 0 *
bit 990 I 1 M0_DQ45
bit 989 O 1 M0_DQ44 988 0 Z
bit 988 C 0 *
bit 987 I 1 M0_DQ44
bit 986 O 1 M0_DQS5 985 0 Z
bit 985 C 0 *
bit 984 I 1 M0_DQS5
bit 983 O 1 M0_DQ43 982 0 Z
bit 982 C 0 *
bit 981 I 1 M0_DQ43
bit 980 O 1 M0_DQ42 979 0 Z
bit 979 C 0 *
bit 978 I 1 M0_DQ42
bit 977 O 1 M0_DQ41 976 0 Z
bit 976 C 0 *
bit 975 I 1 M0_DQ41
bit 974 O 1 M0_DQ40 973 0 Z
bit 973 C 0 *
bit 972 I 1 M0_DQ40
bit 971 O 1 M0_DQ39 970 0 Z
bit 970 C 0 *
bit 969 I 1 M0_DQ39
bit 968 O 1 M0_DQ38 967 0 Z
bit 967 C 0 *
bit 966 I 1 M0_DQ38
bit 965 O 1 M0_DQ37 964 0 Z
bit 964 C 0 *
bit 963 I 1 M0_DQ37
bit 962 O 1 M0_DQ36 961 0 Z
bit 961 C 0 *
bit 960 I 1 M0_DQ36
bit 959 O 1 M0_DQS4 958 0 Z
bit 958 C 0 *
bit 957 I 1 M0_DQS4
bit 956 O 1 M0_DQ35 955 0 Z
bit 955 C 0 *
bit 954 I 1 M0_DQ35
bit 953 O 1 M0_DQ34 952 0 Z
bit 952 C 0 *
bit 951 I 1 M0_DQ34
bit 950 O 1 M0_DQ33 949 0 Z
bit 949 C 0 *
bit 948 I 1 M0_DQ33
bit 947 O 1 M0_DQ32 946 0 Z
bit 946 C 0 *
bit 945 I 1 M0_DQ32
bit 944 O 1 M0_ECC7 943 0 Z
bit 943 C 0 *
bit 942 I 1 M0_ECC7
bit 941 O 1 M0_ECC6 940 0 Z
bit 940 C 0 *
bit 939 I 1 M0_ECC6
bit 938 O 1 M0_ECC5 937 0 Z
bit 937 C 0 *
bit 936 I 1 M0_ECC5
bit 935 O 1 M0_ECC4 934 0 Z
bit 934 C 0 *
bit 933 I 1 M0_ECC4
bit 932 O 1 M0_DQS8 931 0 Z
bit 931 C 0 *
bit 930 I 1 M0_DQS8
bit 929 O 1 M0_ECC3 928 0 Z
bit 928 C 0 *
bit 927 I 1 M0_ECC3
bit 926 O 1 M0_ECC2 925 0 Z
bit 925 C 0 *
bit 924 I 1 M0_ECC2
bit 923 O 1 M0_ECC1 922 0 Z
bit 922 C 0 *
bit 921 I 1 M0_ECC1
bit 920 O 1 M0_ECC0 919 0 Z
bit 919 C 0 *
bit 918 I 1 M0_ECC0
bit 917 O 1 M0_CS_L3 916 0 Z
bit 916 C 0 *
bit 915 O 0 *
bit 914 O 1 M0_CLK_L 913 0 Z
bit 913 C 0 *
bit 912 O 0 *
bit 911 O 1 M0_CKE 910 0 Z
bit 910 C 0 *
bit 909 O 0 *
bit 908 O 1 M0_CLK 907 0 Z
bit 907 C 0 *
bit 906 O 0 *
bit 905 O 1 M0_CS_L2 904 0 Z
bit 904 C 0 *
bit 903 O 0 *
bit 902 O 1 M0_RAS_L 901 0 Z
bit 901 C 0 *
bit 900 O 0 *
bit 899 O 1 M0_CS_L1 898 0 Z
bit 898 C 0 *
bit 897 O 0 *
bit 896 O 1 M0_CS_L0 895 0 Z
bit 895 C 0 *
bit 894 O 0 *
bit 893 O 1 M0_CAS_L 892 0 Z
bit 892 C 0 *
bit 891 O 0 *
bit 890 O 1 M0_BA0 889 0 Z
bit 889 C 0 *
bit 888 O 0 *
bit 887 O 1 M0_WE_L 886 0 Z
bit 886 C 0 *
bit 885 O 0 *
bit 884 O 1 M0_A10 883 0 Z
bit 883 C 0 *
bit 882 O 0 *
bit 881 O 1 M0_BA1 880 0 Z
bit 880 C 0 *
bit 879 O 0 *
bit 878 O 1 M0_A2 877 0 Z
bit 877 C 0 *
bit 876 O 0 *
bit 875 O 1 M0_A0 874 0 Z
bit 874 C 0 *
bit 873 O 0 *
bit 872 O 1 M0_A4 871 0 Z
bit 871 C 0 *
bit 870 O 0 *
bit 869 O 1 M0_A1 868 0 Z
bit 868 C 0 *
bit 867 O 0 *
bit 866 O 1 M0_A3 865 0 Z
bit 865 C 0 *
bit 864 O 0 *
bit 863 O 1 M0_A9 862 0 Z
bit 862 C 0 *
bit 861 O 0 *
bit 860 O 1 M0_A6 859 0 Z
bit 859 C 0 *
bit 858 O 0 *
bit 857 O 1 M0_A11 856 0 Z
bit 856 C 0 *
bit 855 O 0 *
bit 854 O 1 M0_A5 853 0 Z
bit 853 C 0 *
bit 852 O 0 *
bit 851 O 1 M0_A7 850 0 Z
bit 850 C 0 *
bit 849 O 0 *
bit 848 O 1 M0_A12 847 0 Z
bit 847 C 0 *
bit 846 O 0 *
bit 845 O 1 M0_A8 844 0 Z
bit 844 C 0 *
bit 843 O 0 *
bit 842 O 1 M0_DQ31 841 0 Z
bit 841 C 0 *
bit 840 I 1 M0_DQ31
bit 839 O 1 M0_DQ30 838 0 Z
bit 838 C 0 *
bit 837 I 1 M0_DQ30
bit 836 O 1 M0_DQ29 835 0 Z
bit 835 C 0 *
bit 834 I 1 M0_DQ29
bit 833 O 1 M0_DQ28 832 0 Z
bit 832 C 0 *
bit 831 I 1 M0_DQ28
bit 830 O 1 M0_DQS3 829 0 Z
bit 829 C 0 *
bit 828 I 1 M0_DQS3
bit 827 O 1 M0_DQ27 826 0 Z
bit 826 C 0 *
bit 825 I 1 M0_DQ27
bit 824 O 1 M0_DQ26 823 0 Z
bit 823 C 0 *
bit 822 I 1 M0_DQ26
bit 821 O 1 M0_DQ25 820 0 Z
bit 820 C 0 *
bit 819 I 1 M0_DQ25
bit 818 O 1 M0_DQ24 817 0 Z
bit 817 C 0 *
bit 816 I 1 M0_DQ24
bit 815 O 1 M0_DQ23 814 0 Z
bit 814 C 0 *
bit 813 I 1 M0_DQ23
bit 812 O 1 M0_DQ22 811 0 Z
bit 811 C 0 *
bit 810 I 1 M0_DQ22
bit 809 O 1 M0_DQ21 808 0 Z
bit 808 C 0 *
bit 807 I 1 M0_DQ21
bit 806 O 1 M0_DQ20 805 0 Z
bit 805 C 0 *
bit 804 I 1 M0_DQ20
bit 803 O 1 M0_DQS2 802 0 Z
bit 802 C 0 *
bit 801 I 1 M0_DQS2
bit 800 O 1 M0_DQ19 799 0 Z
bit 799 C 0 *
bit 798 I 1 M0_DQ19
bit 797 O 1 M0_DQ18 796 0 Z
bit 796 C 0 *
bit 795 I 1 M0_DQ18
bit 794 O 1 M0_DQ17 793 0 Z
bit 793 C 0 *
bit 792 I 1 M0_DQ17
bit 791 O 1 M0_DQ16 790 0 Z
bit 790 C 0 *
bit 789 I 1 M0_DQ16
bit 788 O 1 M0_DQ15 787 0 Z
bit 787 C 0 *
bit 786 I 1 M0_DQ15
bit 785 O 1 M0_DQ14 784 0 Z
bit 784 C 0 *
bit 783 I 1 M0_DQ14
bit 782 O 1 M0_DQ13 781 0 Z
bit 781 C 0 *
bit 780 I 1 M0_DQ13
bit 779 O 1 M0_DQ12 778 0 Z
bit 778 C 0 *
bit 777 I 1 M0_DQ12
bit 776 O 1 M0_DQS1 775 0 Z
bit 775 C 0 *
bit 774 I 1 M0_DQS1
bit 773 O 1 M0_DQ11 772 0 Z
bit 772 C 0 *
bit 771 I 1 M0_DQ11
bit 770 O 1 M0_DQ10 769 0 Z
bit 769 C 0 *
bit 768 I 1 M0_DQ10
bit 767 O 1 M0_DQ9 766 0 Z
bit 766 C 0 *
bit 765 I 1 M0_DQ9
bit 764 O 1 M0_DQ8 763 0 Z
bit 763 C 0 *
bit 762 I 1 M0_DQ8
bit 761 O 1 M0_DQ7 760 0 Z
bit 760 C 0 *
bit 759 I 1 M0_DQ7
bit 758 O 1 M0_DQ6 757 0 Z
bit 757 C 0 *
bit 756 I 1 M0_DQ6
bit 755 O 1 M0_DQ5 754 0 Z
bit 754 C 0 *
bit 753 I 1 M0_DQ5
bit 752 O 1 M0_DQ4 751 0 Z
bit 751 C 0 *
bit 750 I 1 M0_DQ4
bit 749 O 1 M0_DQS0 748 0 Z
bit 748 C 0 *
bit 747 I 1 M0_DQS0
bit 746 O 1 M0_DQ3 745 0 Z
bit 745 C 0 *
bit 744 I 1 M0_DQ3
bit 743 O 1 M0_DQ2 742 0 Z
bit 742 C 0 *
bit 741 I 1 M0_DQ2
bit 740 O 1 M0_DQ1 739 0 Z
bit 739 C 0 *
bit 738 I 1 M0_DQ1
bit 737 O 1 M0_DQ0 736 0 Z
bit 736 C 0 *
bit 735 I 1 M0_DQ0
bit 734 O 0 *
bit 733 O 0 *
bit 732 I 1 E0_RXDV
bit 731 O 1 E0_MDIO 730 0 Z
bit 730 C 0 *
bit 729 I 1 E0_MDIO
bit 728 O 0 *
bit 727 O 0 *
bit 726 I 1 E0_RXER
bit 725 O 1 E0_MDC 724 0 Z
bit 724 C 0 *
bit 723 O 0 *
bit 722 O 0 *
bit 721 O 0 *
bit 720 I 1 E0_TCLKI
bit 719 O 1 E0_TXD0 718 0 Z
bit 718 C 0 *
bit 717 O 0 *
bit 716 O 0 *
bit 715 O 0 *
bit 714 I 1 E0_RXD7
bit 713 O 1 E0_TXD1 712 0 Z
bit 712 C 0 *
bit 711 O 0 *
bit 710 O 0 *
bit 709 O 0 *
bit 708 I 1 E0_RXD6
bit 707 O 1 E0_TXD2 706 0 Z
bit 706 C 0 *
bit 705 O 0 *
bit 704 O 0 *
bit 703 O 0 *
bit 702 I 1 E0_RXD5
bit 701 O 1 E0_TXD3 700 0 Z
bit 700 C 0 *
bit 699 O 0 *
bit 698 O 0 *
bit 697 O 0 *
bit 696 I 1 E0_RXD4
bit 695 O 1 E0_TCLKO 694 0 Z
bit 694 C 0 *
bit 693 O 0 *
bit 692 O 0 *
bit 691 O 0 *
bit 690 I 1 E0_RXD3
bit 689 O 1 E0_TXD4 688 0 Z
bit 688 C 0 *
bit 687 O 0 *
bit 686 O 0 *
bit 685 O 0 *
bit 684 I 1 E0_RXD2
bit 683 O 1 E0_TXD5 682 0 Z
bit 682 C 0 *
bit 681 O 0 *
bit 680 O 0 *
bit 679 O 0 *
bit 678 I 1 E0_RXD1
bit 677 O 1 E0_TXD6 676 0 Z
bit 676 C 0 *
bit 675 O 0 *
bit 674 O 0 *
bit 673 O 0 *
bit 672 I 1 E0_RXD0
bit 671 O 1 E0_TXD7 670 0 Z
bit 670 C 0 *
bit 669 O 0 *
bit 668 O 0 *
bit 667 O 0 *
bit 666 I 1 E0_RCLK
bit 665 O 1 E0_TXER 664 0 Z
bit 664 C 0 *
bit 663 O 0 *
bit 662 O 0 *
bit 661 O 0 *
bit 660 I 1 E0_CRS
bit 659 O 1 E0_GENO 658 0 Z
bit 658 C 0 *
bit 657 O 0 *
bit 656 O 0 *
bit 655 O 0 *
bit 654 I 1 E0_COL
bit 653 O 1 E0_TXEN 652 0 Z
bit 652 C 0 *
bit 651 O 0 *
bit 650 O 0 *
bit 649 O 0 *
bit 648 I 1 REFCLK01
bit 647 O 1 E1_MDC 646 0 Z
bit 646 C 0 *
bit 645 O 0 *
bit 644 O 0 *
bit 643 O 0 *
bit 642 I 1 E1_RCLK
bit 641 O 1 E1_MDIO 640 0 Z
bit 640 C 0 *
bit 639 I 1 E1_MDIO
bit 638 O 0 *
bit 637 O 0 *
bit 636 I 1 E1_RXER
bit 635 O 1 E1_TXD0 634 0 Z
bit 634 C 0 *
bit 633 O 0 *
bit 632 O 0 *
bit 631 O 0 *
bit 630 I 1 E1_RXDV
bit 629 O 1 E1_TXD1 628 0 Z
bit 628 C 0 *
bit 627 O 0 *
bit 626 O 0 *
bit 625 O 0 *
bit 624 I 1 E1_RXD7
bit 623 O 1 E1_TXD2 622 0 Z
bit 622 C 0 *
bit 621 O 0 *
bit 620 O 0 *
bit 619 O 0 *
bit 618 I 1 E1_RXD6
bit 617 O 1 E1_TXD3 616 0 Z
bit 616 C 0 *
bit 615 O 0 *
bit 614 O 0 *
bit 613 O 0 *
bit 612 I 1 E1_RXD5
bit 611 O 1 E1_TCLKO 610 0 Z
bit 610 C 0 *
bit 609 O 0 *
bit 608 O 0 *
bit 607 O 0 *
bit 606 I 1 E1_RXD4
bit 605 O 1 E1_TXD4 604 0 Z
bit 604 C 0 *
bit 603 O 0 *
bit 602 O 0 *
bit 601 O 0 *
bit 600 I 1 E1_RXD3
bit 599 O 1 E1_TXD5 598 0 Z
bit 598 C 0 *
bit 597 O 0 *
bit 596 O 0 *
bit 595 O 0 *
bit 594 I 1 E1_RXD2
bit 593 O 1 E1_TXD6 592 0 Z
bit 592 C 0 *
bit 591 O 0 *
bit 590 O 0 *
bit 589 O 0 *
bit 588 I 1 E1_RXD1
bit 587 O 1 E1_TXD7 586 0 Z
bit 586 C 0 *
bit 585 O 0 *
bit 584 O 0 *
bit 583 O 0 *
bit 582 I 1 E1_RXD0
bit 581 O 1 E1_TXEN 580 0 Z
bit 580 C 0 *
bit 579 O 0 *
bit 578 O 0 *
bit 577 O 0 *
bit 576 I 1 E1_TCLKI
bit 575 O 1 E1_TXER 574 0 Z
bit 574 C 0 *
bit 573 O 0 *
bit 572 O 0 *
bit 571 O 0 *
bit 570 I 1 E1_CRS
bit 569 O 1 E1_GENO 568 0 Z
bit 568 C 0 *
bit 567 O 0 *
bit 566 O 0 *
bit 565 O 0 *
bit 564 I 1 E1_COL
bit 563 O 1 E2_MDC 562 0 Z
bit 562 C 0 *
bit 561 O 0 *
bit 560 O 0 *
bit 559 O 0 *
bit 558 I 1 E2_RCLK
bit 557 O 1 E2_MDIO 556 0 Z
bit 556 C 0 *
bit 555 I 1 E2_MDIO
bit 554 O 0 *
bit 553 O 0 *
bit 552 I 1 REFCLK2
bit 551 O 1 E2_TXD0 550 0 Z
bit 550 C 0 *
bit 549 O 0 *
bit 548 O 0 *
bit 547 O 0 *
bit 546 I 1 E2_RXDV
bit 545 O 1 E2_TXD1 544 0 Z
bit 544 C 0 *
bit 543 O 0 *
bit 542 O 0 *
bit 541 O 0 *
bit 540 I 1 E2_RXER
bit 539 O 1 E2_TXD2 538 0 Z
bit 538 C 0 *
bit 537 O 0 *
bit 536 O 0 *
bit 535 O 0 *
bit 534 I 1 E2_RXD7
bit 533 O 1 E2_TXD3 532 0 Z
bit 532 C 0 *
bit 531 O 0 *
bit 530 O 0 *
bit 529 O 0 *
bit 528 I 1 E2_RXD6
bit 527 O 1 E2_TCLKO 526 0 Z
bit 526 C 0 *
bit 525 O 0 *
bit 524 O 0 *
bit 523 O 0 *
bit 522 I 1 E2_RXD5
bit 521 O 1 E2_TXD4 520 0 Z
bit 520 C 0 *
bit 519 O 0 *
bit 518 O 0 *
bit 517 O 0 *
bit 516 I 1 E2_RXD4
bit 515 O 1 E2_TXD5 514 0 Z
bit 514 C 0 *
bit 513 O 0 *
bit 512 O 0 *
bit 511 O 0 *
bit 510 I 1 E2_RXD3
bit 509 O 1 E2_TXD6 508 0 Z
bit 508 C 0 *
bit 507 O 0 *
bit 506 O 0 *
bit 505 O 0 *
bit 504 I 1 E2_RXD2
bit 503 O 1 E2_TXD7 502 0 Z
bit 502 C 0 *
bit 501 O 0 *
bit 500 O 0 *
bit 499 O 0 *
bit 498 I 1 E2_RXD1
bit 497 O 1 E2_TXER 496 0 Z
bit 496 C 0 *
bit 495 O 0 *
bit 494 O 0 *
bit 493 O 0 *
bit 492 I 1 E2_RXD0
bit 491 O 1 E2_TXEN 490 0 Z
bit 490 C 0 *
bit 489 O 0 *
bit 488 O 0 *
bit 487 O 0 *
bit 486 I 1 E2_TCLKI
bit 485 O 1 E2_GENO 484 0 Z
bit 484 C 0 *
bit 483 O 0 *
bit 482 O 0 *
bit 481 O 0 *
bit 480 I 1 E2_CRS
bit 479 O 0 *
bit 478 O 0 *
bit 477 I 1 E2_COL
bit 476 O 1 IO_RW 475 0 Z
bit 475 C 0 *
bit 474 O 0 *
bit 473 O 0 *
bit 472 O 0 *
bit 471 I 1 SPARE2
bit 470 O 0 *
bit 469 O 0 *
bit 468 I 1 SPARE4
bit 467 O 0 *
bit 466 O 0 *
bit 465 I 1 SPARE3
bit 464 O 1 S1_COUT 463 0 Z
bit 463 C 0 *
bit 462 O 0 *
bit 461 O 0 *
bit 460 O 0 *
bit 459 I 1 S1_DIN
bit 458 O 0 *
bit 457 O 0 *
bit 456 I 1 S1_RIN
bit 455 O 0 *
bit 454 O 0 *
bit 453 I 1 S1_CIN_RCLKIN
bit 452 O 1 S1_RTS_TSTROBE 451 0 Z
bit 451 C 0 *
bit 450 O 0 *
bit 449 O 0 *
bit 448 O 0 *
bit 447 I 1 S1_TIN
bit 446 O 0 *
bit 445 O 0 *
bit 444 I 1 S1_CTS_TCLKIN
bit 443 O 1 GPIO1 442 0 Z
bit 442 C 0 *
bit 441 I 1 GPIO1
bit 440 O 1 S1_DOUT 439 0 Z
bit 439 C 0 *
bit 438 O 0 *
bit 437 O 0 *
bit 436 O 0 *
bit 435 I 1 S0_DIN
bit 434 O 1 S0_RTS_TSTROBE 433 0 Z
bit 433 C 0 *
bit 432 O 0 *
bit 431 O 0 *
bit 430 O 0 *
bit 429 I 1 S0_RIN
bit 428 O 1 S0_COUT 427 0 Z
bit 427 C 0 *
bit 426 O 0 *
bit 425 O 0 *
bit 424 O 0 *
bit 423 I 1 S0_CIN_RCLKIN
bit 422 O 0 *
bit 421 O 0 *
bit 420 I 1 S0_CTS_TCLKIN
bit 419 O 0 *
bit 418 O 0 *
bit 417 I 1 S0_TIN
bit 416 O 1 S0_DOUT 415 0 Z
bit 415 C 0 *
bit 414 O 0 *
bit 413 O 1 GPIO5 412 0 Z
bit 412 C 0 *
bit 411 I 1 GPIO5
bit 410 O 1 GPIO0 409 0 Z
bit 409 C 0 *
bit 408 I 1 GPIO0
bit 407 O 1 GPIO4 406 0 Z
bit 406 C 0 *
bit 405 I 1 GPIO4
bit 404 O 1 GPIO3 403 0 Z
bit 403 C 0 *
bit 402 I 1 GPIO3
bit 401 O 1 GPIO2 400 0 Z
bit 400 C 0 *
bit 399 I 1 GPIO2
bit 398 O 0 *
bit 397 O 0 *
bit 396 I 1 IO_RDY
bit 395 O 1 IO_OE_L 394 0 Z
bit 394 C 0 *
bit 393 O 0 *
bit 392 O 1 IO_WR_L 391 0 Z
bit 391 C 0 *
bit 390 O 0 *
bit 389 O 1 IO_ALE 388 0 Z
bit 388 C 0 *
bit 387 O 0 *
bit 386 O 1 IO_CS_L7 385 0 Z
bit 385 C 0 *
bit 384 O 0 *
bit 383 O 1 IO_CS_L6 382 0 Z
bit 382 C 0 *
bit 381 O 0 *
bit 380 O 1 IO_CS_L5 379 0 Z
bit 379 C 0 *
bit 378 O 0 *
bit 377 O 1 IO_CS_L4 376 0 Z
bit 376 C 0 *
bit 375 O 0 *
bit 374 O 1 IO_CS_L3 373 0 Z
bit 373 C 0 *
bit 372 O 0 *
bit 371 O 1 IO_CS_L2 370 0 Z
bit 370 C 0 *
bit 369 O 0 *
bit 368 O 1 IO_CS_L1 367 0 Z
bit 367 C 0 *
bit 366 O 0 *
bit 365 O 1 IO_CS_L0 364 0 Z
bit 364 C 0 *
bit 363 O 0 *
bit 362 O 1 IO_AD31 361 0 Z
bit 361 C 0 *
bit 360 I 1 IO_AD31
bit 359 O 1 IO_AD30 358 0 Z
bit 358 C 0 *
bit 357 I 1 IO_AD30
bit 356 O 1 IO_AD28 355 0 Z
bit 355 C 0 *
bit 354 I 1 IO_AD28
bit 353 O 1 IO_AD29 352 0 Z
bit 352 C 0 *
bit 351 I 1 IO_AD29
bit 350 O 1 IO_AD27 349 0 Z
bit 349 C 0 *
bit 348 I 1 IO_AD27
bit 347 O 1 IO_AD26 346 0 Z
bit 346 C 0 *
bit 345 I 1 IO_AD26
bit 344 O 1 IO_AD25 343 0 Z
bit 343 C 0 *
bit 342 I 1 IO_AD25
bit 341 O 1 IO_AD24 340 0 Z
bit 340 C 0 *
bit 339 I 1 IO_AD24
bit 338 O 1 IO_AD23 337 0 Z
bit 337 C 0 *
bit 336 I 1 IO_AD23
bit 335 O 1 IO_AD22 334 0 Z
bit 334 C 0 *
bit 333 I 1 IO_AD22
bit 332 O 1 IO_AD21 331 0 Z
bit 331 C 0 *
bit 330 I 1 IO_AD21
bit 329 O 1 IO_AD20 328 0 Z
bit 328 C 0 *
bit 327 I 1 IO_AD20
bit 326 O 1 IO_AD19 325 0 Z
bit 325 C 0 *
bit 324 I 1 IO_AD19
bit 323 O 1 IO_AD18 322 0 Z
bit 322 C 0 *
bit 321 I 1 IO_AD18
bit 320 O 1 IO_AD17 319 0 Z
bit 319 C 0 *
bit 318 I 1 IO_AD17
bit 317 O 1 IO_AD15 316 0 Z
bit 316 C 0 *
bit 315 I 1 IO_AD15
bit 314 O 1 IO_AD16 313 0 Z
bit 313 C 0 *
bit 312 I 1 IO_AD16
bit 311 O 1 IO_AD11 310 0 Z
bit 310 C 0 *
bit 309 I 1 IO_AD11
bit 308 O 1 IO_AD14 307 0 Z
bit 307 C 0 *
bit 306 I 1 IO_AD14
bit 305 O 1 IO_AD12 304 0 Z
bit 304 C 0 *
bit 303 I 1 IO_AD12
bit 302 O 1 IO_AD13 301 0 Z
bit 301 C 0 *
bit 300 I 1 IO_AD13
bit 299 O 1 IO_AD10 298 0 Z
bit 298 C 0 *
bit 297 I 1 IO_AD10
bit 296 O 1 IO_AD9 295 0 Z
bit 295 C 0 *
bit 294 I 1 IO_AD9
bit 293 O 0 *
bit 292 O 0 *
bit 291 I 1 SPARE5
bit 290 O 0 *
bit 289 O 0 *
bit 288 O 0 *
bit 287 O 0 *
bit 286 O 0 *
bit 285 I 1 CLK100N
bit 284 O 0 *
bit 283 O 0 *
bit 282 I 1 PLLBYP
bit 281 O 0 *
bit 280 O 0 *
bit 279 I 1 CLK100P
bit 278 O 0 *
bit 277 O 0 *
bit 276 O 0 *
bit 275 O 1 RESETOUT_L 274 0 Z
bit 274 C 0 *
bit 273 O 0 *
bit 272 O 1 IO_AD8 271 0 Z
bit 271 C 0 *
bit 270 I 1 IO_AD8
bit 269 O 1 IO_AD7 268 0 Z
bit 268 C 0 *
bit 267 I 1 IO_AD7
bit 266 O 1 DEBUG_L 265 0 Z
bit 265 C 0 *
bit 264 I 1 DEBUG_L
bit 263 O 1 IO_AD6 262 0 Z
bit 262 C 0 *
bit 261 I 1 IO_AD6
bit 260 O 1 IO_AD5 259 0 Z
bit 259 C 0 *
bit 258 I 1 IO_AD5
bit 257 O 1 IO_AD3 256 0 Z
bit 256 C 0 *
bit 255 I 1 IO_AD3
bit 254 O 1 IO_AD4 253 0 Z
bit 253 C 0 *
bit 252 I 1 IO_AD4
bit 251 O 1 IO_AD2 250 0 Z
bit 250 C 0 *
bit 249 I 1 IO_AD2
bit 248 O 1 IO_AD1 247 0 Z
bit 247 C 0 *
bit 246 I 1 IO_AD1
bit 245 O 1 IO_AD0 244 0 Z
bit 244 C 0 *
bit 243 I 1 IO_AD0
bit 242 O 1 GPIO6 241 0 Z
bit 241 C 0 *
bit 240 I 1 GPIO6
bit 239 O 1 GPIO7 238 0 Z
bit 238 C 0 *
bit 237 I 1 GPIO7
bit 236 O 1 GPIO8 235 0 Z
bit 235 C 0 *
bit 234 I 1 GPIO8
bit 233 O 1 GPIO9 232 0 Z
bit 232 C 0 *
bit 231 I 1 GPIO9
bit 230 O 1 GPIO10 229 0 Z
bit 229 C 0 *
bit 228 I 1 GPIO10
bit 227 O 1 IO_CLK100 226 0 Z
bit 226 C 0 *
bit 225 O 0 *
bit 224 O 1 GPIO11 223 0 Z
bit 223 C 0 *
bit 222 I 1 GPIO11
bit 221 O 1 GPIO12 220 0 Z
bit 220 C 0 *
bit 219 I 1 GPIO12
bit 218 O 1 GPIO13 217 0 Z
bit 217 C 0 *
bit 216 I 1 GPIO13
bit 215 O 1 PC_ENVPP 214 0 Z
bit 214 C 0 *
bit 213 O 0 *
bit 212 O 1 GPIO14 211 0 Z
bit 211 C 0 *
bit 210 I 1 GPIO14
bit 209 O 1 PC_ENV5V 208 0 Z
bit 208 C 0 *
bit 207 O 0 *
bit 206 O 1 GPIO15 205 0 Z
bit 205 C 0 *
bit 204 I 1 GPIO15
bit 203 O 1 SCL1 202 0 Z
bit 202 C 0 *
bit 201 I 1 SCL1
bit 200 O 1 PC_ENV3V 199 0 Z
bit 199 C 0 *
bit 198 O 0 *
bit 197 O 1 P_GNT_L3 196 0 Z
bit 196 C 0 *
bit 195 O 0 *
bit 194 O 1 SDA1 193 0 Z
bit 193 C 0 *
bit 192 I 1 SDA1
bit 191 O 1 SCL0 190 0 Z
bit 190 C 0 *
bit 189 I 1 SCL0
bit 188 O 1 SDA0 187 0 Z
bit 187 C 0 *
bit 186 I 1 SDA0
bit 185 O 1 P_GNT_L2 184 0 Z
bit 184 C 0 *
bit 183 O 0 *
bit 182 O 0 *
bit 181 O 0 *
bit 180 I 1 P_CLK
bit 179 O 1 P_REQ_l0 178 0 Z
bit 178 C 0 *
bit 177 I 1 P_REQ_l0
bit 176 O 0 *
bit 175 O 0 *
bit 174 I 1 P_REQ_L3
bit 173 O 1 P_GNT_L1 172 0 Z
bit 172 C 0 *
bit 171 O 0 *
bit 170 O 0 *
bit 169 O 0 *
bit 168 I 1 P_REQ_L1
bit 167 O 1 P_GNT_l0 166 0 Z
bit 166 C 0 *
bit 165 I 1 P_GNT_l0
bit 164 O 0 *
bit 163 O 0 *
bit 162 I 1 P_REQ_L2
bit 161 O 1 P_IRDY_L 160 0 Z
bit 160 C 0 *
bit 159 I 1 P_IRDY_L
bit 158 O 1 P_FRAME_L 157 0 Z
bit 157 C 0 *
bit 156 I 1 P_FRAME_L
bit 155 O 1 P_TRDY_L 154 0 Z
bit 154 C 0 *
bit 153 I 1 P_TRDY_L
bit 152 O 1 P_DEVSEL_L 151 0 Z
bit 151 C 0 *
bit 150 I 1 P_DEVSEL_L
bit 149 O 1 P_PERR_L 148 0 Z
bit 148 C 0 *
bit 147 I 1 P_PERR_L
bit 146 O 1 P_STOP_L 145 0 Z
bit 145 C 0 *
bit 144 I 1 P_STOP_L
bit 143 O 1 P_PAR 142 0 Z
bit 142 C 0 *
bit 141 I 1 P_PAR
bit 140 O 1 P_SERR_L 139 0 Z
bit 139 C 0 *
bit 138 I 1 P_SERR_L
bit 137 O 1 P_INTA_L 136 0 Z
bit 136 C 0 *
bit 135 I 1 P_INTA_L
bit 134 O 1 P_CBE_L3 133 0 Z
bit 133 C 0 *
bit 132 I 1 P_CBE_L3
bit 131 O 0 *
bit 130 O 0 *
bit 129 I 1 P_INTB_L
bit 128 O 1 P_CBE_L2 127 0 Z
bit 127 C 0 *
bit 126 I 1 P_CBE_L2
bit 125 O 0 *
bit 124 O 0 *
bit 123 I 1 P_INTC_L
bit 122 O 1 P_CBE_L1 121 0 Z
bit 121 C 0 *
bit 120 I 1 P_CBE_L1
bit 119 O 0 *
bit 118 O 0 *
bit 117 I 1 P_INTD_L
bit 116 O 1 P_CBE_L0 115 0 Z
bit 115 C 0 *
bit 114 I 1 P_CBE_L0
bit 113 O 1 P_RST_L 112 0 Z
bit 112 C 0 *
bit 111 O 0 *
bit 110 O 0 *
bit 109 O 0 *
bit 108 O 0 *
bit 107 O 0 *
bit 106 O 0 *
bit 105 O 0 *
bit 104 O 0 *
bit 103 O 0 *
bit 102 O 0 *
bit 101 O 0 *
bit 100 O 0 *
bit 99 O 0 *
bit 98 O 1 P_AD0 97 0 Z
bit 97 C 0 *
bit 96 I 1 P_AD0
bit 95 O 0 *
bit 94 O 0 *
bit 93 O 0 *
bit 92 O 1 P_AD1 91 0 Z
bit 91 C 0 *
bit 90 I 1 P_AD1
bit 89 O 1 P_AD2 88 0 Z
bit 88 C 0 *
bit 87 I 1 P_AD2
bit 86 O 1 P_AD7 85 0 Z
bit 85 C 0 *
bit 84 I 1 P_AD7
bit 83 O 1 P_AD3 82 0 Z
bit 82 C 0 *
bit 81 I 1 P_AD3
bit 80 O 1 P_AD8 79 0 Z
bit 79 C 0 *
bit 78 I 1 P_AD8
bit 77 O 1 P_AD4 76 0 Z
bit 76 C 0 *
bit 75 I 1 P_AD4
bit 74 O 1 P_AD9 73 0 Z
bit 73 C 0 *
bit 72 I 1 P_AD9
bit 71 O 1 P_AD5 70 0 Z
bit 70 C 0 *
bit 69 I 1 P_AD5
bit 68 O 1 P_AD10 67 0 Z
bit 67 C 0 *
bit 66 I 1 P_AD10
bit 65 O 1 P_AD6 64 0 Z
bit 64 C 0 *
bit 63 I 1 P_AD6
bit 62 O 1 P_AD13 61 0 Z
bit 61 C 0 *
bit 60 I 1 P_AD13
bit 59 O 1 P_AD11 58 0 Z
bit 58 C 0 *
bit 57 I 1 P_AD11
bit 56 O 1 P_AD16 55 0 Z
bit 55 C 0 *
bit 54 I 1 P_AD16
bit 53 O 1 P_AD12 52 0 Z
bit 52 C 0 *
bit 51 I 1 P_AD12
bit 50 O 1 P_AD17 49 0 Z
bit 49 C 0 *
bit 48 I 1 P_AD17
bit 47 O 1 P_AD15 46 0 Z
bit 46 C 0 *
bit 45 I 1 P_AD15
bit 44 O 1 P_AD18 43 0 Z
bit 43 C 0 *
bit 42 I 1 P_AD18
bit 41 O 1 P_AD14 40 0 Z
bit 40 C 0 *
bit 39 I 1 P_AD14
bit 38 O 1 P_AD21 37 0 Z
bit 37 C 0 *
bit 36 I 1 P_AD21
bit 35 O 1 P_AD19 34 0 Z
bit 34 C 0 *
bit 33 I 1 P_AD19
bit 32 O 1 P_AD24 31 0 Z
bit 31 C 0 *
bit 30 I 1 P_AD24
bit 29 O 1 P_AD22 28 0 Z
bit 28 C 0 *
bit 27 I 1 P_AD22
bit 26 O 1 P_AD25 25 0 Z
bit 25 C 0 *
bit 24 I 1 P_AD25
bit 23 O 1 P_AD23 22 0 Z
bit 22 C 0 *
bit 21 I 1 P_AD23
bit 20 O 1 P_AD28 19 0 Z
bit 19 C 0 *
bit 18 I 1 P_AD28
bit 17 O 1 P_AD20 16 0 Z
bit 16 C 0 *
bit 15 I 1 P_AD20
bit 14 O 1 P_AD27 13 0 Z
bit 13 C 0 *
bit 12 I 1 P_AD27
bit 11 O 1 P_AD26 10 0 Z
bit 10 C 0 *
bit 9 I 1 P_AD26
bit 8 O 1 P_AD30 7 0 Z
bit 7 C 0 *
bit 6 I 1 P_AD30
bit 5 O 1 P_AD29 4 0 Z
bit 4 C 0 *
bit 3 I 1 P_AD29
bit 2 O 1 P_AD31 1 0 Z
bit 1 C 0 *
bit 0 I 1 P_AD31

initbus bcm1250
