signal TCK
signal TDI
signal TDO
signal TMS
signal PAD56
signal PAD92
signal PAD38
signal PAD93
signal PAD75
signal PAD39
signal PAD58
signal PAD94
signal PAD76
signal PAD59
signal PAD96
signal PAD78
signal PAD97
signal PAD79
signal PAD98
signal PAD1
signal PAD99
signal PAD2
signal IPAD66
signal IPAD67
signal PAD7
signal PAD8
signal PAD9
signal PROG_B
signal PAD40
signal PAD24
signal PAD42
signal PAD25
signal PAD61
signal PAD43
signal PAD62
signal PAD44
signal PAD63
signal PAD45
signal PAD64
signal PAD82
signal PAD65
signal PAD83
signal PAD48
signal IPAD12
signal PAD49
signal IPAD13
signal PAD68
signal PAD69
signal DONE
signal IPAD36
signal IPAD73
signal PAD105
signal PAD106
signal IPAD95
signal PAD107
signal PAD108
signal PAD10
signal PAD11
signal PAD14
signal PAD15
signal PAD34
signal PAD70
signal PAD35
signal PAD71
signal PAD53
signal PAD17
signal PAD72
signal PAD54
signal PAD18
signal PAD37
signal PAD55
signal PAD91
signal GND0
signal GND1
signal GND2
signal GND3
signal GND4
signal GND5
signal GND6
signal GND7
signal GND8
signal GND9
signal GND10
signal GND11
signal VDD0
signal VDD1
signal VDD2
signal VDD3
signal VDD4
signal VDD5
signal VDD6
signal VDD7
signal VDD8
signal VDD9
signal VDD10
signal VDD11
signal Vaux0
signal Vaux1
signal Vaux2

register	BSR	272
register	BR	1
register	DIR	32

instruction length 6

instruction SAMPLE/PRELOAD 100000 BSR
instruction IDCODE 100100 DIR
instruction EXTEST 111100 BSR
instruction BYPASS 111111 BR

bit 271 O 1 *
bit 270 O 1 *
bit 269 O 1 *
bit 268 O 1 *
bit 267 O 1 *
bit 266 O 1 *
bit 265 O 1 *
bit 264 O 1 *
bit 263 O 1 *
bit 262 O 1 *
bit 261 O 1 *
bit 260 O 1 *
bit 259 O 1 *
bit 258 O 1 *
bit 257 O 1 *
bit 256 O 1 *
bit 255 O 1 *
bit 254 I 1 PAD34
bit 253 O 1 PAD34 252 0 Z
bit 252 C 0 *
bit 251 I 1 PAD35
bit 250 O 1 PAD35 249 0 Z
bit 249 C 0 *
bit 248 I 1 IPAD36
bit 247 I 1 PAD37
bit 246 O 1 PAD37 245 0 Z
bit 245 C 0 *
bit 244 I 1 PAD38
bit 243 O 1 PAD38 242 0 Z
bit 242 C 0 *
bit 241 I 1 PAD39
bit 240 O 1 PAD39 239 0 Z
bit 239 C 0 *
bit 238 I 1 PAD40
bit 237 O 1 PAD40 236 0 Z
bit 236 C 0 *
bit 235 O 1 *
bit 234 I 1 PAD42
bit 233 O 1 PAD42 232 0 Z
bit 232 C 0 *
bit 231 I 1 PAD43
bit 230 O 1 PAD43 229 0 Z
bit 229 C 0 *
bit 228 I 1 PAD44
bit 227 O 1 PAD44 226 0 Z
bit 226 C 0 *
bit 225 I 1 PAD45
bit 224 O 1 PAD45 223 0 Z
bit 223 C 0 *
bit 222 O 1 *
bit 221 O 1 *
bit 220 O 1 *
bit 219 O 1 *
bit 218 I 1 PAD48
bit 217 O 1 PAD48 216 0 Z
bit 216 C 0 *
bit 215 I 1 PAD49
bit 214 O 1 PAD49 213 0 Z
bit 213 C 0 *
bit 212 O 1 *
bit 211 O 1 *
bit 210 O 1 *
bit 209 O 1 *
bit 208 O 1 *
bit 207 O 1 *
bit 206 O 1 *
bit 205 I 1 PAD53
bit 204 O 1 PAD53 203 0 Z
bit 203 C 0 *
bit 202 I 1 PAD54
bit 201 O 1 PAD54 200 0 Z
bit 200 C 0 *
bit 199 I 1 DONE
bit 198 O 1 *
bit 197 O 1 *
bit 196 I 1 PAD55
bit 195 O 1 PAD55 194 0 Z
bit 194 C 0 *
bit 193 I 1 PAD56
bit 192 O 1 PAD56 191 0 Z
bit 191 C 0 *
bit 190 O 1 *
bit 189 I 1 PAD58
bit 188 O 1 PAD58 187 0 Z
bit 187 C 0 *
bit 186 I 1 PAD59
bit 185 O 1 PAD59 184 0 Z
bit 184 C 0 *
bit 183 O 1 *
bit 182 I 1 PAD61
bit 181 O 1 PAD61 180 0 Z
bit 180 C 0 *
bit 179 I 1 PAD62
bit 178 O 1 PAD62 177 0 Z
bit 177 C 0 *
bit 176 I 1 PAD63
bit 175 O 1 PAD63 174 0 Z
bit 174 C 0 *
bit 173 I 1 PAD64
bit 172 O 1 PAD64 171 0 Z
bit 171 C 0 *
bit 170 I 1 PAD65
bit 169 O 1 PAD65 168 0 Z
bit 168 C 0 *
bit 167 I 1 IPAD66
bit 166 I 1 IPAD67
bit 165 I 1 PAD68
bit 164 O 1 PAD68 163 0 Z
bit 163 C 0 *
bit 162 I 1 PAD69
bit 161 O 1 PAD69 160 0 Z
bit 160 C 0 *
bit 159 I 1 PAD70
bit 158 O 1 PAD70 157 0 Z
bit 157 C 0 *
bit 156 I 1 PAD71
bit 155 O 1 PAD71 154 0 Z
bit 154 C 0 *
bit 153 I 1 PAD72
bit 152 O 1 PAD72 151 0 Z
bit 151 C 0 *
bit 150 I 1 IPAD73
bit 149 O 1 *
bit 148 I 1 PAD75
bit 147 O 1 PAD75 146 0 Z
bit 146 C 0 *
bit 145 I 1 PAD76
bit 144 O 1 PAD76 143 0 Z
bit 143 C 0 *
bit 142 O 1 *
bit 141 I 1 PAD78
bit 140 O 1 PAD78 139 0 Z
bit 139 C 0 *
bit 138 I 1 PAD79
bit 137 O 1 PAD79 136 0 Z
bit 136 C 0 *
bit 135 O 1 *
bit 134 O 1 *
bit 133 I 1 PAD82
bit 132 O 1 PAD82 131 0 Z
bit 131 C 0 *
bit 130 I 1 PAD83
bit 129 O 1 PAD83 128 0 Z
bit 128 C 0 *
bit 127 O 1 *
bit 126 O 1 *
bit 125 O 1 *
bit 124 O 1 *
bit 123 O 1 *
bit 122 O 1 *
bit 121 O 1 *
bit 120 O 1 *
bit 119 O 1 *
bit 118 O 1 *
bit 117 O 1 *
bit 116 O 1 *
bit 115 O 1 *
bit 114 O 1 *
bit 113 O 1 *
bit 112 O 1 *
bit 111 O 1 *
bit 110 I 1 PAD91
bit 109 O 1 PAD91 108 0 Z
bit 108 C 0 *
bit 107 I 1 PAD92
bit 106 O 1 PAD92 105 0 Z
bit 105 C 0 *
bit 104 I 1 PAD93
bit 103 O 1 PAD93 102 0 Z
bit 102 C 0 *
bit 101 I 1 PAD94
bit 100 O 1 PAD94 99 0 Z
bit 99 C 0 *
bit 98 I 1 IPAD95
bit 97 I 1 PAD96
bit 96 O 1 PAD96 95 0 Z
bit 95 C 0 *
bit 94 I 1 PAD97
bit 93 O 1 PAD97 92 0 Z
bit 92 C 0 *
bit 91 I 1 PAD98
bit 90 O 1 PAD98 89 0 Z
bit 89 C 0 *
bit 88 I 1 PAD99
bit 87 O 1 PAD99 86 0 Z
bit 86 C 0 *
bit 85 O 1 *
bit 84 O 1 *
bit 83 O 1 *
bit 82 O 1 *
bit 81 O 1 *
bit 80 O 1 *
bit 79 O 1 *
bit 78 O 1 *
bit 77 O 1 *
bit 76 O 1 *
bit 75 O 1 *
bit 74 I 1 PAD105
bit 73 O 1 PAD105 72 0 Z
bit 72 C 0 *
bit 71 I 1 PAD106
bit 70 O 1 PAD106 69 0 Z
bit 69 C 0 *
bit 68 I 1 PAD107
bit 67 O 1 PAD107 66 0 Z
bit 66 C 0 *
bit 65 I 1 PAD108
bit 64 O 1 PAD108 63 0 Z
bit 63 C 0 *
bit 62 I 1 PROG_B
bit 61 I 1 PAD1
bit 60 O 1 PAD1 59 0 Z
bit 59 C 0 *
bit 58 I 1 PAD2
bit 57 O 1 PAD2 56 0 Z
bit 56 C 0 *
bit 55 O 1 *
bit 54 O 1 *
bit 53 O 1 *
bit 52 O 1 *
bit 51 O 1 *
bit 50 O 1 *
bit 49 O 1 *
bit 48 O 1 *
bit 47 I 1 PAD7
bit 46 O 1 PAD7 45 0 Z
bit 45 C 0 *
bit 44 I 1 PAD8
bit 43 O 1 PAD8 42 0 Z
bit 42 C 0 *
bit 41 I 1 PAD9
bit 40 O 1 PAD9 39 0 Z
bit 39 C 0 *
bit 38 I 1 PAD10
bit 37 O 1 PAD10 36 0 Z
bit 36 C 0 *
bit 35 I 1 PAD11
bit 34 O 1 PAD11 33 0 Z
bit 33 C 0 *
bit 32 I 1 IPAD12
bit 31 I 1 IPAD13
bit 30 I 1 PAD14
bit 29 O 1 PAD14 28 0 Z
bit 28 C 0 *
bit 27 I 1 PAD15
bit 26 O 1 PAD15 25 0 Z
bit 25 C 0 *
bit 24 O 1 *
bit 23 O 1 *
bit 22 O 1 *
bit 21 I 1 PAD17
bit 20 O 1 PAD17 19 0 Z
bit 19 C 0 *
bit 18 I 1 PAD18
bit 17 O 1 PAD18 16 0 Z
bit 16 C 0 *
bit 15 O 1 *
bit 14 O 1 *
bit 13 O 1 *
bit 12 O 1 *
bit 11 O 1 *
bit 10 O 1 *
bit 9 O 1 *
bit 8 O 1 *
bit 7 O 1 *
bit 6 I 1 PAD24
bit 5 O 1 PAD24 4 0 Z
bit 4 C 0 *
bit 3 I 1 PAD25
bit 2 O 1 PAD25 1 0 Z
bit 1 C 0 *
bit 0 O 1 *
