signal GND1
signal GND2
signal GND3
signal GND4
signal GND5
signal GND6
signal GND7
signal GND8
signal GND9
signal GND10
signal GND11
signal GND12
signal GND13
signal GND14
signal GND15
signal GND16
signal GND17
signal GND18
signal GND19
signal GND20
signal GND21
signal GND22
signal GND23
signal GND24
signal GND25
signal GND26
signal GND27
signal GND28
signal CCLK_P104
signal DONE_P103
signal HSWAP_EN_P206
signal M0_P55
signal M1_P54
signal M2_P56
signal PROG_B
signal TCK
signal TDI
signal TDO
signal TMS
signal VCCAUX1
signal VCCAUX2
signal VCCAUX3
signal VCCAUX4
signal VCCAUX5
signal VCCAUX6
signal VCCAUX7
signal VCCAUX8
signal VCCINT1
signal VCCINT2
signal VCCINT3
signal VCCINT4
signal VCCO01
signal VCCO02
signal VCCO11
signal VCCO12
signal VCCO21
signal VCCO22
signal VCCO31
signal VCCO32
signal VCCO41
signal VCCO42
signal VCCO51
signal VCCO52
signal VCCO61
signal VCCO62
signal VCCO71
signal VCCO72
signal IO_P2
signal IO_P3
signal IO_P7
signal IO_P9
signal IO_P10
signal IO_P11
signal IO_P12
signal IO_P13
signal IO_P15
signal IO_P16
signal IO_P18
signal IO_P19
signal IO_P20
signal IO_P21
signal IO_P26
signal IO_P27
signal IO_P28
signal IO_P29
signal IO_P34
signal IO_P35
signal IO_P36
signal IO_P37
signal IO_P39
signal IO_P40
signal IO_P42
signal IO_P43
signal IO_P44
signal IO_P45
signal IO_P46
signal IO_P48
signal IO_P51
signal IO_P52
signal IO_P57
signal IO_P58
signal IO_P61
signal IO_P62
signal IO_P63
signal IO_P64
signal IO_P65
signal IO_P67
signal IO_P68
signal IO_P71
signal IO_P72
signal IO_P74
signal IO_P76
signal IO_P77
signal IO_P78
signal IO_P79
signal IO_P80
signal IO_P81
signal IO_P83
signal IO_P85
signal IO_P86
signal IO_P87
signal IO_P90
signal IO_P92
signal IO_P93
signal IO_P94
signal IO_P95
signal IO_P100
signal IO_P101
signal IO_P102
signal IO_P106
signal IO_P107
signal IO_P111
signal IO_P113
signal IO_P114
signal IO_P115
signal IO_P116
signal IO_P117
signal IO_P119
signal IO_P120
signal IO_P122
signal IO_P123
signal IO_P124
signal IO_P125
signal IO_P130
signal IO_P131
signal IO_P132
signal IO_P133
signal IO_P138
signal IO_P139
signal IO_P140
signal IO_P141
signal IO_P143
signal IO_P144
signal IO_P146
signal IO_P147
signal IO_P148
signal IO_P149
signal IO_P150
signal IO_P152
signal IO_P155
signal IO_P156
signal IO_P161
signal IO_P162
signal IO_P165
signal IO_P166
signal IO_P167
signal IO_P168
signal IO_P169
signal IO_P171
signal IO_P172
signal IO_P175
signal IO_P176
signal IO_P178
signal IO_P180
signal IO_P181
signal IO_P182
signal IO_P183
signal IO_P184
signal IO_P185
signal IO_P187
signal IO_P189
signal IO_P190
signal IO_P191
signal IO_P194
signal IO_P196
signal IO_P197
signal IO_P198
signal IO_P199
signal IO_P203
signal IO_P204

register	BSR	383
register	BR	1
register	DIR	32

instruction length 6

instruction EXTEST 000000 BSR
instruction SAMPLE/PRELOAD 000001 BSR
instruction IDCODE 001001 DIR
instruction BYPASS 111111 BR

bit 382 I 1 IO_P156
bit 381 O 1 IO_P156 380 1 Z
bit 380 C 1 *
bit 379 I 1 IO_P155
bit 378 O 1 IO_P155 377 1 Z
bit 377 C 1 *
bit 376 I 1 IO_P152
bit 375 O 1 IO_P152 374 1 Z
bit 374 C 1 *
bit 373 I 1 IO_P150
bit 372 O 1 IO_P150 371 1 Z
bit 371 C 1 *
bit 370 I 1 IO_P149
bit 369 O 1 IO_P149 368 1 Z
bit 368 C 1 *
bit 367 I 1 IO_P148
bit 366 O 1 IO_P148 365 1 Z
bit 365 C 1 *
bit 364 I 1 IO_P147
bit 363 O 1 IO_P147 362 1 Z
bit 362 C 1 *
bit 361 I 1 IO_P146
bit 360 O 1 IO_P146 359 1 Z
bit 359 C 1 *
bit 358 I 1 IO_P144
bit 357 O 1 IO_P144 356 1 Z
bit 356 C 1 *
bit 355 I 1 IO_P143
bit 354 O 1 IO_P143 353 1 Z
bit 353 C 1 *
bit 352 I 1 IO_P141
bit 351 O 1 IO_P141 350 1 Z
bit 350 C 1 *
bit 349 I 1 IO_P140
bit 348 O 1 IO_P140 347 1 Z
bit 347 C 1 *
bit 346 I 1 IO_P139
bit 345 O 1 IO_P139 344 1 Z
bit 344 C 1 *
bit 343 I 1 IO_P138
bit 342 O 1 IO_P138 341 1 Z
bit 341 C 1 *
bit 340 I 1 IO_P133
bit 339 O 1 IO_P133 338 1 Z
bit 338 C 1 *
bit 337 I 1 IO_P132
bit 336 O 1 IO_P132 335 1 Z
bit 335 C 1 *
bit 334 I 1 IO_P131
bit 333 O 1 IO_P131 332 1 Z
bit 332 C 1 *
bit 331 I 1 IO_P130
bit 330 O 1 IO_P130 329 1 Z
bit 329 C 1 *
bit 328 I 1 IO_P125
bit 327 O 1 IO_P125 326 1 Z
bit 326 C 1 *
bit 325 I 1 IO_P124
bit 324 O 1 IO_P124 323 1 Z
bit 323 C 1 *
bit 322 I 1 IO_P123
bit 321 O 1 IO_P123 320 1 Z
bit 320 C 1 *
bit 319 I 1 IO_P122
bit 318 O 1 IO_P122 317 1 Z
bit 317 C 1 *
bit 316 I 1 IO_P120
bit 315 O 1 IO_P120 314 1 Z
bit 314 C 1 *
bit 313 I 1 IO_P119
bit 312 O 1 IO_P119 311 1 Z
bit 311 C 1 *
bit 310 I 1 IO_P117
bit 309 O 1 IO_P117 308 1 Z
bit 308 C 1 *
bit 307 I 1 IO_P116
bit 306 O 1 IO_P116 305 1 Z
bit 305 C 1 *
bit 304 I 1 IO_P115
bit 303 O 1 IO_P115 302 1 Z
bit 302 C 1 *
bit 301 I 1 IO_P114
bit 300 O 1 IO_P114 299 1 Z
bit 299 C 1 *
bit 298 I 1 IO_P113
bit 297 O 1 IO_P113 296 1 Z
bit 296 C 1 *
bit 295 I 1 IO_P111
bit 294 O 1 IO_P111 293 1 Z
bit 293 C 1 *
bit 292 I 1 IO_P107
bit 291 O 1 IO_P107 290 1 Z
bit 290 C 1 *
bit 289 I 1 IO_P106
bit 288 O 1 IO_P106 287 1 Z
bit 287 C 1 *
bit 286 I 1 CCLK_P104
bit 285 O 1 CCLK_P104 284 1 Z
bit 284 C 1 *
bit 283 I 1 DONE_P103
bit 282 O 1 DONE_P103 281 1 Z
bit 281 C 1 *
bit 280 I 1 IO_P102
bit 279 O 1 IO_P102 278 1 Z
bit 278 C 1 *
bit 277 I 1 IO_P101
bit 276 O 1 IO_P101 275 1 Z
bit 275 C 1 *
bit 274 I 1 IO_P100
bit 273 O 1 IO_P100 272 1 Z
bit 272 C 1 *
bit 271 I 1 IO_P95
bit 270 O 1 IO_P95 269 1 Z
bit 269 C 1 *
bit 268 I 1 IO_P94
bit 267 O 1 IO_P94 266 1 Z
bit 266 C 1 *
bit 265 I 1 IO_P93
bit 264 O 1 IO_P93 263 1 Z
bit 263 C 1 *
bit 262 I 1 IO_P92
bit 261 O 1 IO_P92 260 1 Z
bit 260 C 1 *
bit 259 I 1 IO_P90
bit 258 O 1 IO_P90 257 1 Z
bit 257 C 1 *
bit 256 I 1 IO_P87
bit 255 O 1 IO_P87 254 1 Z
bit 254 C 1 *
bit 253 I 1 IO_P86
bit 252 O 1 IO_P86 251 1 Z
bit 251 C 1 *
bit 250 I 1 IO_P85
bit 249 O 1 IO_P85 248 1 Z
bit 248 C 1 *
bit 247 I 1 IO_P83
bit 246 O 1 IO_P83 245 1 Z
bit 245 C 1 *
bit 244 I 1 IO_P81
bit 243 O 1 IO_P81 242 1 Z
bit 242 C 1 *
bit 241 I 1 IO_P80
bit 240 O 1 IO_P80 239 1 Z
bit 239 C 1 *
bit 238 I 1 IO_P79
bit 237 O 1 IO_P79 236 1 Z
bit 236 C 1 *
bit 235 I 1 IO_P78
bit 234 O 1 IO_P78 233 1 Z
bit 233 C 1 *
bit 232 I 1 IO_P77
bit 231 O 1 IO_P77 230 1 Z
bit 230 C 1 *
bit 229 I 1 IO_P76
bit 228 O 1 IO_P76 227 1 Z
bit 227 C 1 *
bit 226 I 1 IO_P74
bit 225 O 1 IO_P74 224 1 Z
bit 224 C 1 *
bit 223 I 1 IO_P72
bit 222 O 1 IO_P72 221 1 Z
bit 221 C 1 *
bit 220 I 1 IO_P71
bit 219 O 1 IO_P71 218 1 Z
bit 218 C 1 *
bit 217 I 1 IO_P68
bit 216 O 1 IO_P68 215 1 Z
bit 215 C 1 *
bit 214 I 1 IO_P67
bit 213 O 1 IO_P67 212 1 Z
bit 212 C 1 *
bit 211 I 1 IO_P65
bit 210 O 1 IO_P65 209 1 Z
bit 209 C 1 *
bit 208 I 1 IO_P64
bit 207 O 1 IO_P64 206 1 Z
bit 206 C 1 *
bit 205 I 1 IO_P63
bit 204 O 1 IO_P63 203 1 Z
bit 203 C 1 *
bit 202 I 1 IO_P62
bit 201 O 1 IO_P62 200 1 Z
bit 200 C 1 *
bit 199 I 1 IO_P61
bit 198 O 1 IO_P61 197 1 Z
bit 197 C 1 *
bit 196 I 1 IO_P58
bit 195 O 1 IO_P58 194 1 Z
bit 194 C 1 *
bit 193 I 1 IO_P57
bit 192 O 1 IO_P57 191 1 Z
bit 191 C 1 *
bit 190 I 1 M2_P56
bit 189 I 1 M0_P55
bit 188 I 1 M1_P54
bit 187 I 1 IO_P52
bit 186 O 1 IO_P52 185 1 Z
bit 185 C 1 *
bit 184 I 1 IO_P51
bit 183 O 1 IO_P51 182 1 Z
bit 182 C 1 *
bit 181 I 1 IO_P48
bit 180 O 1 IO_P48 179 1 Z
bit 179 C 1 *
bit 178 I 1 IO_P46
bit 177 O 1 IO_P46 176 1 Z
bit 176 C 1 *
bit 175 I 1 IO_P45
bit 174 O 1 IO_P45 173 1 Z
bit 173 C 1 *
bit 172 I 1 IO_P44
bit 171 O 1 IO_P44 170 1 Z
bit 170 C 1 *
bit 169 I 1 IO_P43
bit 168 O 1 IO_P43 167 1 Z
bit 167 C 1 *
bit 166 I 1 IO_P42
bit 165 O 1 IO_P42 164 1 Z
bit 164 C 1 *
bit 163 I 1 IO_P40
bit 162 O 1 IO_P40 161 1 Z
bit 161 C 1 *
bit 160 I 1 IO_P39
bit 159 O 1 IO_P39 158 1 Z
bit 158 C 1 *
bit 157 I 1 IO_P37
bit 156 O 1 IO_P37 155 1 Z
bit 155 C 1 *
bit 154 I 1 IO_P36
bit 153 O 1 IO_P36 152 1 Z
bit 152 C 1 *
bit 151 I 1 IO_P35
bit 150 O 1 IO_P35 149 1 Z
bit 149 C 1 *
bit 148 I 1 IO_P34
bit 147 O 1 IO_P34 146 1 Z
bit 146 C 1 *
bit 145 I 1 IO_P29
bit 144 O 1 IO_P29 143 1 Z
bit 143 C 1 *
bit 142 I 1 IO_P28
bit 141 O 1 IO_P28 140 1 Z
bit 140 C 1 *
bit 139 I 1 IO_P27
bit 138 O 1 IO_P27 137 1 Z
bit 137 C 1 *
bit 136 I 1 IO_P26
bit 135 O 1 IO_P26 134 1 Z
bit 134 C 1 *
bit 133 I 1 IO_P21
bit 132 O 1 IO_P21 131 1 Z
bit 131 C 1 *
bit 130 I 1 IO_P20
bit 129 O 1 IO_P20 128 1 Z
bit 128 C 1 *
bit 127 I 1 IO_P19
bit 126 O 1 IO_P19 125 1 Z
bit 125 C 1 *
bit 124 I 1 IO_P18
bit 123 O 1 IO_P18 122 1 Z
bit 122 C 1 *
bit 121 I 1 IO_P16
bit 120 O 1 IO_P16 119 1 Z
bit 119 C 1 *
bit 118 I 1 IO_P15
bit 117 O 1 IO_P15 116 1 Z
bit 116 C 1 *
bit 115 I 1 IO_P13
bit 114 O 1 IO_P13 113 1 Z
bit 113 C 1 *
bit 112 I 1 IO_P12
bit 111 O 1 IO_P12 110 1 Z
bit 110 C 1 *
bit 109 I 1 IO_P11
bit 108 O 1 IO_P11 107 1 Z
bit 107 C 1 *
bit 106 I 1 IO_P10
bit 105 O 1 IO_P10 104 1 Z
bit 104 C 1 *
bit 103 I 1 IO_P9
bit 102 O 1 IO_P9 101 1 Z
bit 101 C 1 *
bit 100 I 1 IO_P7
bit 99 O 1 IO_P7 98 1 Z
bit 98 C 1 *
bit 97 I 1 IO_P3
bit 96 O 1 IO_P3 95 1 Z
bit 95 C 1 *
bit 94 I 1 IO_P2
bit 93 O 1 IO_P2 92 1 Z
bit 92 C 1 *
bit 91 O 1 *
bit 90 I 1 HSWAP_EN_P206
bit 89 I 1 IO_P205
bit 88 O 1 IO_P205 87 1 Z
bit 87 C 1 *
bit 86 I 1 IO_P204
bit 85 O 1 IO_P204 84 1 Z
bit 84 C 1 *
bit 83 I 1 IO_P203
bit 82 O 1 IO_P203 81 1 Z
bit 81 C 1 *
bit 80 I 1 IO_P199
bit 79 O 1 IO_P199 78 1 Z
bit 78 C 1 *
bit 77 I 1 IO_P198
bit 76 O 1 IO_P198 75 1 Z
bit 75 C 1 *
bit 74 I 1 IO_P197
bit 73 O 1 IO_P197 72 1 Z
bit 72 C 1 *
bit 71 I 1 IO_P196
bit 70 O 1 IO_P196 69 1 Z
bit 69 C 1 *
bit 68 I 1 IO_P194
bit 67 O 1 IO_P194 66 1 Z
bit 66 C 1 *
bit 65 I 1 IO_P191
bit 64 O 1 IO_P191 63 1 Z
bit 63 C 1 *
bit 62 I 1 IO_P190
bit 61 O 1 IO_P190 60 1 Z
bit 60 C 1 *
bit 59 I 1 IO_P189
bit 58 O 1 IO_P189 57 1 Z
bit 57 C 1 *
bit 56 I 1 IO_P187
bit 55 O 1 IO_P187 54 1 Z
bit 54 C 1 *
bit 53 I 1 IO_P185
bit 52 O 1 IO_P185 51 1 Z
bit 51 C 1 *
bit 50 I 1 IO_P184
bit 49 O 1 IO_P184 48 1 Z
bit 48 C 1 *
bit 47 I 1 IO_P183
bit 46 O 1 IO_P183 45 1 Z
bit 45 C 1 *
bit 44 I 1 IO_P182
bit 43 O 1 IO_P182 42 1 Z
bit 42 C 1 *
bit 41 I 1 IO_P181
bit 40 O 1 IO_P181 39 1 Z
bit 39 C 1 *
bit 38 I 1 IO_P180
bit 37 O 1 IO_P180 36 1 Z
bit 36 C 1 *
bit 35 I 1 IO_P178
bit 34 O 1 IO_P178 33 1 Z
bit 33 C 1 *
bit 32 I 1 IO_P176
bit 31 O 1 IO_P176 30 1 Z
bit 30 C 1 *
bit 29 I 1 IO_P175
bit 28 O 1 IO_P175 27 1 Z
bit 27 C 1 *
bit 26 I 1 IO_P172
bit 25 O 1 IO_P172 24 1 Z
bit 24 C 1 *
bit 23 I 1 IO_P171
bit 22 O 1 IO_P171 21 1 Z
bit 21 C 1 *
bit 20 I 1 IO_P169
bit 19 O 1 IO_P169 18 1 Z
bit 18 C 1 *
bit 17 I 1 IO_P168
bit 16 O 1 IO_P168 15 1 Z
bit 15 C 1 *
bit 14 I 1 IO_P167
bit 13 O 1 IO_P167 12 1 Z
bit 12 C 1 *
bit 11 I 1 IO_P166
bit 10 O 1 IO_P166 9 1 Z
bit 9 C 1 *
bit 8 I 1 IO_P165
bit 7 O 1 IO_P165 6 1 Z
bit 6 C 1 *
bit 5 I 1 IO_P162
bit 4 O 1 IO_P162 3 1 Z
bit 3 C 1 *
bit 2 I 1 IO_P161
bit 1 O 1 IO_P161 0 1 Z
bit 0 C 1 *
