signal ADDR1
signal ADDR2
signal ADDR3
signal ADDR4
signal ADDR5
signal ADDR6
signal ADDR7
signal ADDR8
signal ADDR9
signal ADDR10
signal ADDR11
signal ADDR12
signal ADDR13
signal ADDR14
signal ADDR15
signal ADDR16
signal ADDR17
signal ADDR18
signal ADDR19
signal DATA0
signal DATA1
signal DATA2
signal DATA3
signal DATA4
signal DATA5
signal DATA6
signal DATA7
signal DATA8
signal DATA9
signal DATA10
signal DATA11
signal DATA12
signal DATA13
signal DATA14
signal DATA15
signal PF0
signal PF1
signal PF2
signal PF3
signal PF4
signal PF5
signal PF6
signal PF7
signal PF8
signal PF9
signal PF10
signal PF11
signal PF12
signal PF13
signal PF14
signal PF15
signal PG0
signal PG1
signal PG2
signal PG3
signal PG4
signal PG5
signal PG6
signal PG7
signal PG8
signal PG9
signal PG10
signal PG11
signal PG12
signal PG13
signal PG14
signal PG15
signal PH0
signal PH1
signal PH2
signal PH3
signal PH4
signal PH5
signal PH6
signal PH7
signal PH8
signal PH9
signal PH10
signal PH11
signal PH12
signal PH13
signal PH14
signal PH15
signal BMODE0
signal BMODE1
signal BMODE2
signal BMODE3
signal PJ1
signal PJ0
signal PJ2
signal PJ3
signal NMI_B
signal RESET_B
signal CLKOUT
signal AMS_B0
signal AMS_B1
signal AMS_B2
signal AMS_B3
signal AOE_B
signal ARE_B
signal AWE_B
signal ARDY
signal SCKE
signal SMS_B
signal SRAS_B
signal SCAS_B
signal SWE_B
signal SA10
signal ABE_B0
signal ABE_B1
signal TCK
signal TDI
signal TDO
signal TMS
signal TRST_B
signal GND0
signal GND1
signal GND2
signal GND3
signal GND4
signal GND5
signal GND6
signal GND7
signal GND8
signal GND9
signal GND10
signal GND11
signal GND12
signal GND13
signal GND14
signal GND15
signal GND16
signal GND17
signal GND18
signal GND19
signal GND20
signal GND21
signal GND22
signal GND23
signal GND24
signal GND25
signal GND26
signal GND27
signal GND28
signal GND29
signal GND30
signal GND31
signal GND32
signal GND33
signal GND34
signal GND35
signal GND36
signal GND37
signal GND38
signal GND39
signal GND40
signal GND41
signal GND42
signal GND43
signal GND44
signal GND45
signal GND46
signal GND47
signal GND48
signal GND49
signal GND50
signal GND51
signal GND52
signal GND53
signal GND54
signal VDDOTP
signal OTPVPP
signal USB_ID
signal USB_RSET
signal VDDUSB0
signal VDDUSB1
signal USB_VREF
signal USB_XTALIN
signal USB_XTALOUT
signal VDDEXT0
signal VDDEXT1
signal VDDEXT2
signal VDDEXT3
signal VDDEXT4
signal VDDEXT5
signal VDDEXT6
signal VDDEXT7
signal VDDEXT8
signal VDDEXT9
signal VDDEXT10
signal VDDEXT11
signal VDDEXT12
signal VDDEXT13
signal VDDEXT14
signal VDDEXT15
signal VDDEXT16
signal VDDEXT17
signal VDDEXT18
signal VDDEXT19
signal RTXI
signal RTXO
signal SSPG
signal CLKIN
signal VROUT
signal EXT_WAKE
signal USB_DM
signal USB_DP
signal USB_VBUS
signal CLKBUF
signal VDDRTC
signal VDDMEM0
signal VDDMEM1
signal VDDMEM2
signal VDDMEM3
signal VDDMEM4
signal VDDMEM5
signal VDDMEM6
signal VDDMEM7
signal VDDMEM8
signal VDDMEM9
signal VDDMEM10
signal VDDMEM11
signal VDDMEM12
signal VDDMEM13
signal VDDMEM14
signal VDDMEM15
signal VDDMEM16
signal VDDMEM17
signal VDDINT0
signal VDDINT1
signal VDDINT2
signal VDDINT3
signal VDDINT4
signal VDDINT5
signal VDDINT6
signal VDDINT7
signal VDDINT8
signal VDDINT9
signal VDDINT10
signal VDDINT11
signal VDDINT12
signal VDDINT13
signal VDDINT14
signal VDDINT15
signal VDDINT16
signal VDDINT17
signal VDDINT18
signal VDDINT19
signal VDDINT20
signal VDDINT21
signal VDDINT22
signal VDDINT23
signal VDDINT24
signal VDDINT25
signal VDDINT26
signal VDDINT27
signal VDDINT28
signal VDDINT29
signal VDDINT30
signal VDDINT31
signal VDDINT32
signal VRSEL
signal XTAL
signal ADCLRC
signal ADCDAT
signal DACLRC
signal DACDAT
signal BCLK
signal XTO
signal XTI_MCLK
signal LHPOUT
signal RHPOUT
signal CSCL
signal CSDA
signal CCLKOUT
signal CSB
signal CMODE
signal LLINEIN
signal LOUT
signal RLINEIN
signal ROUT
signal VMID
signal MICBIAS
signal MICIN
signal AVDD0
signal AVDD1
signal AGND0
signal AGND1

register	BSR	233
register	BR	1
register	DIR	32
register	DBGSTAT	16
register	DBGCTL	16
register	EMUIR	32
register	EMUDAT	32
register	EMUPC	32

instruction length 5

instruction EXTEST 00000 BSR
instruction SAMPLE/PRELOAD 10000 BSR
instruction IDCODE 00010 DIR
instruction BYPASS 11111 BR
instruction DBGSTAT_SCAN 01100 DBGSTAT
instruction DBGCTL_SCAN 00100 DBGCTL
instruction EMUIR_SCAN 01000 EMUIR
instruction EMUDAT_SCAN 10100 EMUDAT
instruction EMUPC_SCAN 11110 EMUPC

bit 232 C 0 *
bit 231 O 1 ADDR14 8 0 Z
bit 230 O 1 ADDR15 8 0 Z
bit 229 O 1 ADDR16 8 0 Z
bit 228 O 1 ADDR17 8 0 Z
bit 227 O 1 ADDR18 8 0 Z
bit 226 O 1 ADDR19 8 0 Z
bit 225 O 1 DATA0 232 0 Z
bit 224 I 1 DATA0
bit 223 O 1 DATA1 232 0 Z
bit 222 I 1 DATA1
bit 221 O 1 DATA2 232 0 Z
bit 220 I 1 DATA2
bit 219 O 1 DATA3 232 0 Z
bit 218 I 1 DATA3
bit 217 O 1 DATA4 232 0 Z
bit 216 I 1 DATA4
bit 215 O 1 DATA5 232 0 Z
bit 214 I 1 DATA5
bit 213 O 1 DATA6 232 0 Z
bit 212 I 1 DATA6
bit 211 O 1 DATA7 232 0 Z
bit 210 I 1 DATA7
bit 209 O 1 DATA8 232 0 Z
bit 208 I 1 DATA8
bit 207 O 1 DATA9 232 0 Z
bit 206 I 1 DATA9
bit 205 O 1 DATA10 232 0 Z
bit 204 I 1 DATA10
bit 203 O 1 DATA11 232 0 Z
bit 202 I 1 DATA11
bit 201 O 1 DATA12 232 0 Z
bit 200 I 1 DATA12
bit 199 O 1 DATA13 232 0 Z
bit 198 I 1 DATA13
bit 197 O 1 DATA14 232 0 Z
bit 196 I 1 DATA14
bit 195 O 1 DATA15 232 0 Z
bit 194 I 1 DATA15
bit 193 C 0 *
bit 192 O 1 PG0 193 0 Z
bit 191 I 1 PG0
bit 190 C 0 *
bit 189 O 1 PG1 190 0 Z
bit 188 I 1 PG1
bit 187 C 0 *
bit 186 O 1 PG2 187 0 Z
bit 185 I 1 PG2
bit 184 C 0 *
bit 183 O 1 PG3 184 0 Z
bit 182 I 1 PG3
bit 181 I 1 BMODE0
bit 180 I 1 BMODE1
bit 179 I 1 BMODE2
bit 178 I 1 BMODE3
bit 177 C 0 *
bit 176 O 1 PG4 177 0 Z
bit 175 I 1 PG4
bit 174 C 0 *
bit 173 O 1 PG5 174 0 Z
bit 172 I 1 PG5
bit 171 C 0 *
bit 170 O 1 PG6 171 0 Z
bit 169 I 1 PG6
bit 168 C 0 *
bit 167 O 1 PG7 168 0 Z
bit 166 I 1 PG7
bit 165 C 0 *
bit 164 O 1 PG8 165 0 Z
bit 163 I 1 PG8
bit 162 C 0 *
bit 161 O 1 PG9 162 0 Z
bit 160 I 1 PG9
bit 159 C 0 *
bit 158 O 1 PG10 159 0 Z
bit 157 I 1 PG10
bit 156 C 0 *
bit 155 O 1 PG11 156 0 Z
bit 154 I 1 PG11
bit 153 C 0 *
bit 152 O 1 PG12 153 0 Z
bit 151 I 1 PG12
bit 150 C 0 *
bit 149 O 1 PG13 150 0 Z
bit 148 I 1 PG13
bit 147 C 0 *
bit 146 O 1 PG14 147 0 Z
bit 145 I 1 PG14
bit 144 C 0 *
bit 143 O 1 PG15 144 0 Z
bit 142 I 1 PG15
bit 141 I 1 PJ1
bit 140 C 0 *
bit 139 O 1 PJ0 140 0 Z
bit 138 I 1 PJ0
bit 137 C 0 *
bit 136 O 1 PF0 137 0 Z
bit 135 I 1 PF0
bit 134 C 0 *
bit 133 O 1 PF1 134 0 Z
bit 132 I 1 PF1
bit 131 C 0 *
bit 130 O 1 PF2 131 0 Z
bit 129 I 1 PF2
bit 128 C 0 *
bit 127 O 1 PF3 128 0 Z
bit 126 I 1 PF3
bit 125 C 0 *
bit 124 O 1 PF4 125 0 Z
bit 123 I 1 PF4
bit 122 C 0 *
bit 121 O 1 PF5 122 0 Z
bit 120 I 1 PF5
bit 119 C 0 *
bit 118 O 1 PF6 119 0 Z
bit 117 I 1 PF6
bit 116 C 0 *
bit 115 O 1 PF7 116 0 Z
bit 114 I 1 PF7
bit 113 C 0 *
bit 112 O 1 PF8 113 0 Z
bit 111 I 1 PF8
bit 110 C 0 *
bit 109 O 1 PF9 110 0 Z
bit 108 I 1 PF9
bit 107 C 0 *
bit 106 O 1 PF10 107 0 Z
bit 105 I 1 PF10
bit 104 C 0 *
bit 103 O 1 PF11 104 0 Z
bit 102 I 1 PF11
bit 101 O 1 *
bit 100 O 1 PJ2 100 1 Z
bit 99 I 1 PJ2
bit 98 O 1 *
bit 97 O 1 PJ3 97 1 Z
bit 96 I 1 PJ3
bit 95 C 0 *
bit 94 O 1 PF12 95 0 Z
bit 93 I 1 PF12
bit 92 C 0 *
bit 91 O 1 PF13 92 0 Z
bit 90 I 1 PF13
bit 89 C 0 *
bit 88 O 1 PF14 89 0 Z
bit 87 I 1 PF14
bit 86 C 0 *
bit 85 O 1 PF15 86 0 Z
bit 84 I 1 PF15
bit 83 C 0 *
bit 82 O 1 PH0 83 0 Z
bit 81 I 1 PH0
bit 80 C 0 *
bit 79 O 1 PH1 80 0 Z
bit 78 I 1 PH1
bit 77 C 0 *
bit 76 O 1 PH2 77 0 Z
bit 75 I 1 PH2
bit 74 C 0 *
bit 73 O 1 PH3 74 0 Z
bit 72 I 1 PH3
bit 71 C 0 *
bit 70 O 1 PH4 71 0 Z
bit 69 I 1 PH4
bit 68 C 0 *
bit 67 O 1 PH5 68 0 Z
bit 66 I 1 PH5
bit 65 C 0 *
bit 64 O 1 PH6 65 0 Z
bit 63 I 1 PH6
bit 62 C 0 *
bit 61 O 1 PH7 62 0 Z
bit 60 I 1 PH7
bit 59 C 0 *
bit 58 O 1 PH8 59 0 Z
bit 57 I 1 PH8
bit 56 O 0 *
bit 55 C 0 *
bit 54 O 1 PH9 55 0 Z
bit 53 I 1 PH9
bit 52 C 0 *
bit 51 O 1 PH10 52 0 Z
bit 50 I 1 PH10
bit 49 C 0 *
bit 48 O 1 PH11 49 0 Z
bit 47 I 1 PH11
bit 46 C 0 *
bit 45 O 1 PH12 46 0 Z
bit 44 I 1 PH12
bit 43 C 0 *
bit 42 O 1 PH13 43 0 Z
bit 41 I 1 PH13
bit 40 C 0 *
bit 39 O 1 PH14 40 0 Z
bit 38 I 1 PH14
bit 37 C 0 *
bit 36 O 1 PH15 37 0 Z
bit 35 I 1 PH15
bit 34 I 1 NMI_B
bit 33 I 1 RESET_B
bit 32 C 0 *
bit 31 O 1 CLKOUT 32 0 Z
bit 30 O 1 AMS_B0 25 0 Z
bit 29 O 1 AMS_B1 25 0 Z
bit 28 O 1 AMS_B2 25 0 Z
bit 27 O 1 AMS_B3 25 0 Z
bit 26 O 1 AOE_B 25 0 Z
bit 25 C 0 *
bit 24 O 1 ARE_B 25 0 Z
bit 23 O 1 AWE_B 25 0 Z
bit 22 I 1 ARDY
bit 21 O 1 SCKE 32 0 Z
bit 20 O 1 SMS_B 32 0 Z
bit 19 O 1 SRAS_B 32 0 Z
bit 18 O 1 SCAS_B 32 0 Z
bit 17 O 1 SWE_B 32 0 Z
bit 16 O 1 SA10 32 0 Z
bit 15 O 1 ABE_B0 8 0 Z
bit 14 O 1 ABE_B1 8 0 Z
bit 13 O 1 ADDR1 8 0 Z
bit 12 O 1 ADDR2 8 0 Z
bit 11 O 1 ADDR3 8 0 Z
bit 10 O 1 ADDR4 8 0 Z
bit 9 O 1 ADDR5 8 0 Z
bit 8 C 0 *
bit 7 O 1 ADDR6 8 0 Z
bit 6 O 1 ADDR7 8 0 Z
bit 5 O 1 ADDR8 8 0 Z
bit 4 O 1 ADDR9 8 0 Z
bit 3 O 1 ADDR10 8 0 Z
bit 2 O 1 ADDR11 8 0 Z
bit 1 O 1 ADDR12 8 0 Z
bit 0 O 1 ADDR13 8 0 Z
