signal GND1
signal GND2
signal GND3
signal GND4
signal GND5
signal GND6
signal GND7
signal GND8
signal GND9
signal GND10
signal CCLK_P52
signal DONE_P51
signal HSWAP_EN_P98
signal M0_P25
signal M1_P24
signal M2_P26
signal PROG_B
signal TCK
signal TDI
signal TDO
signal TMS
signal VCCAUX1
signal VCCAUX2
signal VCCAUX3
signal VCCAUX4
signal VCCINT1
signal VCCINT2
signal VCCINT3
signal VCCINT4
signal VCCO0
signal VCCO1
signal VCCO2
signal VCCO3
signal VCCO4
signal VCCO5
signal VCCO6
signal VCCO7
signal IO_P1
signal IO_P2
signal IO_P4
signal IO_P5
signal IO_P8
signal IO_P9
signal IO_P11
signal IO_P12
signal IO_P13
signal IO_P14
signal IO_P15
signal IO_P16
signal IO_P17
signal IO_P21
signal IO_P22
signal IO_P23
signal IO_P27
signal IO_P28
signal IO_P30
signal IO_P32
signal IO_P34
signal IO_P35
signal IO_P36
signal IO_P37
signal IO_P38
signal IO_P39
signal IO_P40
signal IO_P42
signal IO_P43
signal IO_P44
signal IO_P47
signal IO_P48
signal IO_P49
signal IO_P50
signal IO_P53
signal IO_P54
signal IO_P55
signal IO_P59
signal IO_P60
signal IO_P61
signal IO_P62
signal IO_P63
signal IO_P64
signal IO_P65
signal IO_P67
signal IO_P68
signal IO_P71
signal IO_P72
signal IO_P74
signal IO_P75
signal IO_P79
signal IO_P80
signal IO_P81
signal IO_P85
signal IO_P86
signal IO_P87
signal IO_P88
signal IO_P89
signal IO_P90
signal IO_P91
signal IO_P92
signal IO_P96

register	BSR	383
register	BR	1
register	DIR	32

instruction length 6

instruction EXTEST 000000 BSR
instruction SAMPLE/PRELOAD 000001 BSR
instruction IDCODE 001001 DIR
instruction BYPASS 111111 BR

bit 382 I 1 IO_P75
bit 381 O 1 IO_P75 380 1 Z
bit 380 C 1 *
bit 379 I 1 IO_P74
bit 378 O 1 IO_P74 377 1 Z
bit 377 C 1 *
bit 376 O 1 *
bit 375 O 1 *
bit 374 O 1 *
bit 373 O 1 *
bit 372 O 1 *
bit 371 O 1 *
bit 370 O 1 *
bit 369 O 1 *
bit 368 O 1 *
bit 367 O 1 *
bit 366 O 1 *
bit 365 O 1 *
bit 364 I 1 IO_P72
bit 363 O 1 IO_P72 362 1 Z
bit 362 C 1 *
bit 361 I 1 IO_P71
bit 360 O 1 IO_P71 359 1 Z
bit 359 C 1 *
bit 358 O 1 *
bit 357 O 1 *
bit 356 O 1 *
bit 355 O 1 *
bit 354 O 1 *
bit 353 O 1 *
bit 352 O 1 *
bit 351 O 1 *
bit 350 O 1 *
bit 349 O 1 *
bit 348 O 1 *
bit 347 O 1 *
bit 346 I 1 IO_P68
bit 345 O 1 IO_P68 344 1 Z
bit 344 C 1 *
bit 343 I 1 IO_P67
bit 342 O 1 IO_P67 341 1 Z
bit 341 C 1 *
bit 340 I 1 IO_P65
bit 339 O 1 IO_P65 338 1 Z
bit 338 C 1 *
bit 337 I 1 IO_P64
bit 336 O 1 IO_P64 335 1 Z
bit 335 C 1 *
bit 334 I 1 IO_P63
bit 333 O 1 IO_P63 332 1 Z
bit 332 C 1 *
bit 331 I 1 IO_P62
bit 330 O 1 IO_P62 329 1 Z
bit 329 C 1 *
bit 328 I 1 IO_P61
bit 327 O 1 IO_P61 326 1 Z
bit 326 C 1 *
bit 325 I 1 IO_P60
bit 324 O 1 IO_P60 323 1 Z
bit 323 C 1 *
bit 322 I 1 IO_P59
bit 321 O 1 IO_P59 320 1 Z
bit 320 C 1 *
bit 319 O 1 *
bit 318 O 1 *
bit 317 O 1 *
bit 316 O 1 *
bit 315 O 1 *
bit 314 O 1 *
bit 313 O 1 *
bit 312 O 1 *
bit 311 O 1 *
bit 310 O 1 *
bit 309 O 1 *
bit 308 O 1 *
bit 307 O 1 *
bit 306 O 1 *
bit 305 O 1 *
bit 304 I 1 IO_P55
bit 303 O 1 IO_P55 302 1 Z
bit 302 C 1 *
bit 301 O 1 *
bit 300 O 1 *
bit 299 O 1 *
bit 298 O 1 *
bit 297 O 1 *
bit 296 O 1 *
bit 295 O 1 *
bit 294 O 1 *
bit 293 O 1 *
bit 292 I 1 IO_P54
bit 291 O 1 IO_P54 290 1 Z
bit 290 C 1 *
bit 289 I 1 IO_P53
bit 288 O 1 IO_P53 287 1 Z
bit 287 C 1 *
bit 286 I 1 CCLK_P52
bit 285 O 1 CCLK_P52 284 1 Z
bit 284 C 1 *
bit 283 I 1 DONE_P51
bit 282 O 1 DONE_P51 281 1 Z
bit 281 C 1 *
bit 280 O 1 *
bit 279 O 1 *
bit 278 O 1 *
bit 277 I 1 IO_P50
bit 276 O 1 IO_P50 275 1 Z
bit 275 C 1 *
bit 274 I 1 IO_P49
bit 273 O 1 IO_P49 272 1 Z
bit 272 C 1 *
bit 271 O 1 *
bit 270 O 1 *
bit 269 O 1 *
bit 268 O 1 *
bit 267 O 1 *
bit 266 O 1 *
bit 265 O 1 *
bit 264 O 1 *
bit 263 O 1 *
bit 262 I 1 IO_P48
bit 261 O 1 IO_P48 260 1 Z
bit 260 C 1 *
bit 259 I 1 IO_P47
bit 258 O 1 IO_P47 257 1 Z
bit 257 C 1 *
bit 256 I 1 IO_P44
bit 255 O 1 IO_P44 254 1 Z
bit 254 C 1 *
bit 253 I 1 IO_P43
bit 252 O 1 IO_P43 251 1 Z
bit 251 C 1 *
bit 250 O 1 *
bit 249 O 1 *
bit 248 O 1 *
bit 247 I 1 IO_P42
bit 246 O 1 IO_P42 245 1 Z
bit 245 C 1 *
bit 244 I 1 IO_P40
bit 243 O 1 IO_P40 242 1 Z
bit 242 C 1 *
bit 241 I 1 IO_P39
bit 240 O 1 IO_P39 239 1 Z
bit 239 C 1 *
bit 238 I 1 IO_P38
bit 237 O 1 IO_P38 236 1 Z
bit 236 C 1 *
bit 235 O 1 *
bit 234 O 1 *
bit 233 O 1 *
bit 232 I 1 IO_P37
bit 231 O 1 IO_P37 230 1 Z
bit 230 C 1 *
bit 229 I 1 IO_P36
bit 228 O 1 IO_P36 227 1 Z
bit 227 C 1 *
bit 226 I 1 IO_P35
bit 225 O 1 IO_P35 224 1 Z
bit 224 C 1 *
bit 223 I 1 IO_P34
bit 222 O 1 IO_P34 221 1 Z
bit 221 C 1 *
bit 220 O 1 *
bit 219 O 1 *
bit 218 O 1 *
bit 217 I 1 IO_P32
bit 216 O 1 IO_P32 215 1 Z
bit 215 C 1 *
bit 214 I 1 IO_P30
bit 213 O 1 IO_P30 212 1 Z
bit 212 C 1 *
bit 211 O 1 *
bit 210 O 1 *
bit 209 O 1 *
bit 208 O 1 *
bit 207 O 1 *
bit 206 O 1 *
bit 205 O 1 *
bit 204 O 1 *
bit 203 O 1 *
bit 202 O 1 *
bit 201 O 1 *
bit 200 O 1 *
bit 199 O 1 *
bit 198 O 1 *
bit 197 O 1 *
bit 196 I 1 IO_P28
bit 195 O 1 IO_P28 194 1 Z
bit 194 C 1 *
bit 193 I 1 IO_P27
bit 192 O 1 IO_P27 191 1 Z
bit 191 C 1 *
bit 190 I 1 M2_P26
bit 189 I 1 M0_P25
bit 188 I 1 M1_P24
bit 187 I 1 IO_P23
bit 186 O 1 IO_P23 185 1 Z
bit 185 C 1 *
bit 184 I 1 IO_P22
bit 183 O 1 IO_P22 182 1 Z
bit 182 C 1 *
bit 181 O 1 *
bit 180 O 1 *
bit 179 O 1 *
bit 178 O 1 *
bit 177 O 1 *
bit 176 O 1 *
bit 175 O 1 *
bit 174 O 1 *
bit 173 O 1 *
bit 172 I 1 IO_P21
bit 171 O 1 IO_P21 170 1 Z
bit 170 C 1 *
bit 169 O 1 *
bit 168 O 1 *
bit 167 O 1 *
bit 166 O 1 *
bit 165 O 1 *
bit 164 O 1 *
bit 163 O 1 *
bit 162 O 1 *
bit 161 O 1 *
bit 160 O 1 *
bit 159 O 1 *
bit 158 O 1 *
bit 157 O 1 *
bit 156 O 1 *
bit 155 O 1 *
bit 154 I 1 IO_P17
bit 153 O 1 IO_P17 152 1 Z
bit 152 C 1 *
bit 151 I 1 IO_P16
bit 150 O 1 IO_P16 149 1 Z
bit 149 C 1 *
bit 148 I 1 IO_P15
bit 147 O 1 IO_P15 146 1 Z
bit 146 C 1 *
bit 145 I 1 IO_P14
bit 144 O 1 IO_P14 143 1 Z
bit 143 C 1 *
bit 142 I 1 IO_P13
bit 141 O 1 IO_P13 140 1 Z
bit 140 C 1 *
bit 139 I 1 IO_P12
bit 138 O 1 IO_P12 137 1 Z
bit 137 C 1 *
bit 136 I 1 IO_P11
bit 135 O 1 IO_P11 134 1 Z
bit 134 C 1 *
bit 133 O 1 *
bit 132 O 1 *
bit 131 O 1 *
bit 130 O 1 *
bit 129 O 1 *
bit 128 O 1 *
bit 127 I 1 IO_P9
bit 126 O 1 IO_P9 125 1 Z
bit 125 C 1 *
bit 124 I 1 IO_P8
bit 123 O 1 IO_P8 122 1 Z
bit 122 C 1 *
bit 121 O 1 *
bit 120 O 1 *
bit 119 O 1 *
bit 118 O 1 *
bit 117 O 1 *
bit 116 O 1 *
bit 115 I 1 IO_P5
bit 114 O 1 IO_P5 113 1 Z
bit 113 C 1 *
bit 112 I 1 IO_P4
bit 111 O 1 IO_P4 110 1 Z
bit 110 C 1 *
bit 109 O 1 *
bit 108 O 1 *
bit 107 O 1 *
bit 106 O 1 *
bit 105 O 1 *
bit 104 O 1 *
bit 103 O 1 *
bit 102 O 1 *
bit 101 O 1 *
bit 100 O 1 *
bit 99 O 1 *
bit 98 O 1 *
bit 97 I 1 IO_P2
bit 96 O 1 IO_P2 95 1 Z
bit 95 C 1 *
bit 94 I 1 IO_P1
bit 93 O 1 IO_P1 92 1 Z
bit 92 C 1 *
bit 91 O 1 *
bit 90 I 1 HSWAP_EN_P98
bit 89 O 1 *
bit 88 O 1 *
bit 87 O 1 *
bit 86 I 1 IO_P97
bit 85 O 1 IO_P97 84 1 Z
bit 84 C 1 *
bit 83 I 1 IO_P96
bit 82 O 1 IO_P96 81 1 Z
bit 81 C 1 *
bit 80 O 1 *
bit 79 O 1 *
bit 78 O 1 *
bit 77 O 1 *
bit 76 O 1 *
bit 75 O 1 *
bit 74 O 1 *
bit 73 O 1 *
bit 72 O 1 *
bit 71 O 1 *
bit 70 O 1 *
bit 69 O 1 *
bit 68 O 1 *
bit 67 O 1 *
bit 66 O 1 *
bit 65 O 1 *
bit 64 O 1 *
bit 63 O 1 *
bit 62 O 1 *
bit 61 O 1 *
bit 60 O 1 *
bit 59 O 1 *
bit 58 O 1 *
bit 57 O 1 *
bit 56 I 1 IO_P92
bit 55 O 1 IO_P92 54 1 Z
bit 54 C 1 *
bit 53 I 1 IO_P91
bit 52 O 1 IO_P91 51 1 Z
bit 51 C 1 *
bit 50 I 1 IO_P90
bit 49 O 1 IO_P90 48 1 Z
bit 48 C 1 *
bit 47 I 1 IO_P89
bit 46 O 1 IO_P89 45 1 Z
bit 45 C 1 *
bit 44 O 1 *
bit 43 O 1 *
bit 42 O 1 *
bit 41 I 1 IO_P88
bit 40 O 1 IO_P88 39 1 Z
bit 39 C 1 *
bit 38 I 1 IO_P87
bit 37 O 1 IO_P87 36 1 Z
bit 36 C 1 *
bit 35 I 1 IO_P86
bit 34 O 1 IO_P86 33 1 Z
bit 33 C 1 *
bit 32 I 1 IO_P85
bit 31 O 1 IO_P85 30 1 Z
bit 30 C 1 *
bit 29 O 1 *
bit 28 O 1 *
bit 27 O 1 *
bit 26 O 1 *
bit 25 O 1 *
bit 24 O 1 *
bit 23 O 1 *
bit 22 O 1 *
bit 21 O 1 *
bit 20 O 1 *
bit 19 O 1 *
bit 18 O 1 *
bit 17 O 1 *
bit 16 O 1 *
bit 15 O 1 *
bit 14 I 1 IO_P81
bit 13 O 1 IO_P81 12 1 Z
bit 12 C 1 *
bit 11 O 1 *
bit 10 O 1 *
bit 9 O 1 *
bit 8 O 1 *
bit 7 O 1 *
bit 6 O 1 *
bit 5 I 1 IO_P80
bit 4 O 1 IO_P80 3 1 Z
bit 3 C 1 *
bit 2 I 1 IO_P79
bit 1 O 1 IO_P79 0 1 Z
bit 0 C 1 *
