#
# $Id: q208 897 2007-12-29 13:02:32Z arniml $
#
# JTAG package script for EP2C8Q208
#
# This program is free software; you can redistribute it and/or
# modify it under the terms of the GNU General Public License
# as published by the Free Software Foundation; either version 2
# of the License, or (at your option) any later version.
#
# This program is distributed in the hope that it will be useful,
# but WITHOUT ANY WARRANTY; without even the implied warranty of
# MERCHANTABILITY or FITNESS FOR A PARTICULAR PURPOSE.  See the
# GNU General Public License for more details.
#
# You should have received a copy of the GNU General Public License
# along with this program; if not, write to the Free Software
# Foundation, Inc., 59 Temple Place - Suite 330, Boston, MA
# 02111-1307, USA.
#
# Written by H Hartley Sweeten <hsweeten@visionengravers.com>
#
# Note:
#   The signals defined in this file as unused pad are specified as
#   I/O pins in the main configuration file ep2c8.
#

salias	IO1	BSC198	# Note: this pin is specified as I/O. If AS mode is specified by MSEL it is output only (ASDO)
salias	IO2	BSC197	# Note: this pin is specified as I/O. If AS mode is specified by MSEL it is output only (nCSO)
salias	IO3	BSC196
salias	IO4	BSC195
salias	IO5	BSC194
salias	IO6	BSC193
salias	IO8	BSC192
salias	IO10	BSC191
salias	IO11	BSC190
salias	IO12	BSC189
salias	IO13	BSC188
#		BSC187	# unused pad
#		BSC186	# unused pad
#		BSC185	# unused pad
#		BSC184	# unused pad
#		BSC183	# unused pad
#		BSC182	# unused pad
#		BSC181	# unused pad
salias	IO14	BSC180
salias	IO15	BSC179
salias	DATA0	BSC178	# Family-specific input pin 20
salias	DCLK	BSC177	# Family-specific input pin 21
#	nCE	BSC176	# untestable Family-specific pin 22
salias	CLK0	BSC175	# Family-specific input pin 23
salias	CLK1	BSC174	# Family-specific input pin 24
#	nCONFIG	BSC173	# untestable Family-specific pin 26
salias	CLK2	BSC172	# Family-specific input pin 27
salias	CLK3	BSC171	# Family-specific input pin 28
salias	IO30	BSC170
salias	IO31	BSC169
#		BSC168	# unused pad
salias	IO33	BSC167
salias	IO34	BSC166
salias	IO35	BSC165
#		BSC164	# unused pad
salias	IO37	BSC163
#		BSC162	# unused pad
#		BSC161	# unused pad
#		BSC160	# unused pad
salias	IO39	BSC159
salias	IO40	BSC158
salias	IO41	BSC157
#		BSC156	# unused pad
#		BSC155	# unused pad
salias	IO43	BSC154
salias	IO44	BSC153
salias	IO45	BSC152
salias	IO46	BSC151
salias	IO47	BSC150
salias	IO48	BSC149
salias	IO56	BSC148
salias	IO57	BSC147
salias	IO58	BSC146
salias	IO59	BSC145
salias	IO60	BSC144
salias	IO61	BSC143
salias	IO63	BSC142
salias	IO64	BSC141
#		BSC140	# unused pad
#		BSC139	# unused pad
#		BSC138	# unused pad
#		BSC137	# unused pad
#		BSC136	# unused pad
#		BSC135	# unused pad
#		BSC134	# unused pad
salias	IO67	BSC133
salias	IO68	BSC132
salias	IO69	BSC131
#		BSC130	# unused pad
#		BSC129	# unused pad
salias	IO70	BSC128
salias	IO72	BSC127
salias	IO74	BSC126
salias	IO75	BSC125
salias	IO76	BSC124
salias	IO77	BSC123
#		BSC122	# unused pad
#		BSC121	# unused pad
salias	IO80	BSC120
salias	IO81	BSC119
salias	IO82	BSC118
salias	IO84	BSC117
salias	IO86	BSC116
salias	IO87	BSC115
salias	IO88	BSC114
salias	IO89	BSC113
salias	IO90	BSC112
salias	IO92	BSC111
salias	IO94	BSC110
salias	IO95	BSC109
salias	IO96	BSC108
salias	IO97	BSC107
salias	IO99	BSC106
salias	IO101	BSC105
salias	IO102	BSC104
salias	IO103	BSC103
salias	IO104	BSC102
salias	IO105	BSC101
salias	IO106	BSC100
#		BSC099	# unused pad
#		BSC098	# unused pad
salias	IO107	BSC097
salias	IO108	BSC096
salias	IO110	BSC095
salias	IO112	BSC094
salias	IO113	BSC093
salias	IO114	BSC092
#		BSC091	# unused pad
salias	IO115	BSC090
salias	IO116	BSC089
salias	IO117	BSC088
#		BSC087	# unused pad
#		BSC086	# unused pad
salias	IO118	BSC085
#		BSC084	# unused pad
#		BSC083	# unused pad
#		BSC082	# unused pad
#	nSTATUS	BSC081	# untestable Family-specific pin 121
#	CONF_DONE	BSC080	# untestable Family-specific pin 123
salias	MSEL1	BSC079	# Family-specific input pin 125
salias	MSEL0	BSC078	# Family-specific input pin 126
salias	IO127	BSC077
salias	IO128	BSC076
salias	CLK7	BSC075	# Family-specific input pin 129
salias	CLK6	BSC074	# Family-specific input pin 130
salias	CLK5	BSC073	# Family-specific input pin 131
salias	CLK4	BSC072	# Family-specific input pin 132
salias	IO133	BSC071
salias	IO134	BSC070
salias	IO135	BSC069
salias	IO137	BSC068
salias	IO138	BSC067
salias	IO139	BSC066
salias	IO141	BSC065
salias	IO142	BSC064
#		BSC063	# unused pad
#		BSC062	# unused pad
salias	IO143	BSC061
salias	IO144	BSC060
salias	IO145	BSC059
#		BSC058	# unused pad
#		BSC057	# unused pad
#		BSC056	# unused pad
#		BSC055	# unused pad
#		BSC054	# unused pad
salias	IO146	BSC053
salias	IO147	BSC052
salias	IO149	BSC051
salias	IO150	BSC050
salias	IO151	BSC049
salias	IO152	BSC048
salias	IO160	BSC047
salias	IO161	BSC046
salias	IO162	BSC045
salias	IO163	BSC044
salias	IO164	BSC043
salias	IO165	BSC042
salias	IO168	BSC041
salias	IO169	BSC040
salias	IO170	BSC039
salias	IO171	BSC038
salias	IO173	BSC037
#		BSC036	# unused pad
#		BSC035	# unused pad
salias	IO175	BSC034
salias	IO176	BSC033
#		BSC032	# unused pad
#		BSC031	# unused pad
#		BSC030	# unused pad
salias	IO179	BSC029
salias	IO180	BSC028
salias	IO181	BSC027
salias	IO182	BSC026
#		BSC025	# unused pad
#		BSC024	# unused pad
#		BSC023	# unused pad
salias	IO185	BSC022
salias	IO187	BSC021
salias	IO188	BSC020
salias	IO189	BSC019
salias	IO191	BSC018
salias	IO192	BSC017
salias	IO193	BSC016
salias	IO195	BSC015
#		BSC014	# unused pad
#		BSC013	# unused pad
#		BSC012	# unused pad
salias	IO197	BSC011
salias	IO198	BSC010
#		BSC009	# unused pad
#		BSC008	# unused pad
salias	IO199	BSC007
salias	IO200	BSC006
salias	IO201	BSC005
salias	IO203	BSC004
salias	IO205	BSC003
salias	IO206	BSC002
salias	IO207	BSC001
salias	IO208	BSC000
