signal GND1
signal GND2
signal GND3
signal GND4
signal GND5
signal GND6
signal GND7
signal GND8
signal GND9
signal GND10
signal CCLK_P52
signal DONE_P51
signal HSWAP_EN_P98
signal M0_P25
signal M1_P24
signal M2_P26
signal PROG_B
signal TCK
signal TDI
signal TDO
signal TMS
signal VCCAUX1
signal VCCAUX2
signal VCCAUX3
signal VCCAUX4
signal VCCINT1
signal VCCINT2
signal VCCINT3
signal VCCINT4
signal VCCO0
signal VCCO1
signal VCCO2
signal VCCO3
signal VCCO4
signal VCCO5
signal VCCO6
signal VCCO7
signal IO_P1
signal IO_P2
signal IO_P4
signal IO_P5
signal IO_P8
signal IO_P9
signal IO_P11
signal IO_P12
signal IO_P13
signal IO_P14
signal IO_P15
signal IO_P16
signal IO_P17
signal IO_P21
signal IO_P22
signal IO_P23
signal IO_P27
signal IO_P28
signal IO_P30
signal IO_P32
signal IO_P34
signal IO_P35
signal IO_P36
signal IO_P37
signal IO_P38
signal IO_P39
signal IO_P40
signal IO_P42
signal IO_P43
signal IO_P44
signal IO_P47
signal IO_P48
signal IO_P49
signal IO_P50
signal IO_P53
signal IO_P54
signal IO_P55
signal IO_P59
signal IO_P60
signal IO_P61
signal IO_P62
signal IO_P63
signal IO_P64
signal IO_P65
signal IO_P67
signal IO_P68
signal IO_P71
signal IO_P72
signal IO_P74
signal IO_P75
signal IO_P79
signal IO_P80
signal IO_P81
signal IO_P85
signal IO_P86
signal IO_P87
signal IO_P88
signal IO_P89
signal IO_P90
signal IO_P91
signal IO_P92
signal IO_P96

register	BSR	599
register	BR	1
register	DIR	32

instruction length 6

instruction EXTEST 000000 BSR
instruction SAMPLE/PRELOAD 000001 BSR
instruction IDCODE 001001 DIR
instruction BYPASS 111111 BR

bit 598 I 1 IO_P75
bit 597 O 1 IO_P75 596 1 Z
bit 596 C 1 *
bit 595 I 1 IO_P74
bit 594 O 1 IO_P74 593 1 Z
bit 593 C 1 *
bit 592 O 1 *
bit 591 O 1 *
bit 590 O 1 *
bit 589 O 1 *
bit 588 O 1 *
bit 587 O 1 *
bit 586 O 1 *
bit 585 O 1 *
bit 584 O 1 *
bit 583 O 1 *
bit 582 O 1 *
bit 581 O 1 *
bit 580 O 1 *
bit 579 O 1 *
bit 578 O 1 *
bit 577 O 1 *
bit 576 O 1 *
bit 575 O 1 *
bit 574 O 1 *
bit 573 O 1 *
bit 572 O 1 *
bit 571 O 1 *
bit 570 O 1 *
bit 569 O 1 *
bit 568 I 1 IO_P72
bit 567 O 1 IO_P72 566 1 Z
bit 566 C 1 *
bit 565 I 1 IO_P71
bit 564 O 1 IO_P71 563 1 Z
bit 563 C 1 *
bit 562 O 1 *
bit 561 O 1 *
bit 560 O 1 *
bit 559 O 1 *
bit 558 O 1 *
bit 557 O 1 *
bit 556 O 1 *
bit 555 O 1 *
bit 554 O 1 *
bit 553 O 1 *
bit 552 O 1 *
bit 551 O 1 *
bit 550 I 1 IO_P68
bit 549 O 1 IO_P68 548 1 Z
bit 548 C 1 *
bit 547 I 1 IO_P67
bit 546 O 1 IO_P67 545 1 Z
bit 545 C 1 *
bit 544 O 1 *
bit 543 O 1 *
bit 542 O 1 *
bit 541 O 1 *
bit 540 O 1 *
bit 539 O 1 *
bit 538 O 1 *
bit 537 O 1 *
bit 536 O 1 *
bit 535 O 1 *
bit 534 O 1 *
bit 533 O 1 *
bit 532 I 1 IO_P65
bit 531 O 1 IO_P65 530 1 Z
bit 530 C 1 *
bit 529 I 1 IO_P64
bit 528 O 1 IO_P64 527 1 Z
bit 527 C 1 *
bit 526 I 1 IO_P63
bit 525 O 1 IO_P63 524 1 Z
bit 524 C 1 *
bit 523 I 1 IO_P62
bit 522 O 1 IO_P62 521 1 Z
bit 521 C 1 *
bit 520 O 1 *
bit 519 O 1 *
bit 518 O 1 *
bit 517 O 1 *
bit 516 O 1 *
bit 515 O 1 *
bit 514 O 1 *
bit 513 O 1 *
bit 512 O 1 *
bit 511 O 1 *
bit 510 O 1 *
bit 509 O 1 *
bit 508 I 1 IO_P61
bit 507 O 1 IO_P61 506 1 Z
bit 506 C 1 *
bit 505 I 1 IO_P60
bit 504 O 1 IO_P60 503 1 Z
bit 503 C 1 *
bit 502 I 1 IO_P59
bit 501 O 1 IO_P59 500 1 Z
bit 500 C 1 *
bit 499 O 1 *
bit 498 O 1 *
bit 497 O 1 *
bit 496 O 1 *
bit 495 O 1 *
bit 494 O 1 *
bit 493 O 1 *
bit 492 O 1 *
bit 491 O 1 *
bit 490 O 1 *
bit 489 O 1 *
bit 488 O 1 *
bit 487 O 1 *
bit 486 O 1 *
bit 485 O 1 *
bit 484 I 1 IO_P55
bit 483 O 1 IO_P55 482 1 Z
bit 482 C 1 *
bit 481 O 1 *
bit 480 O 1 *
bit 479 O 1 *
bit 478 O 1 *
bit 477 O 1 *
bit 476 O 1 *
bit 475 O 1 *
bit 474 O 1 *
bit 473 O 1 *
bit 472 O 1 *
bit 471 O 1 *
bit 470 O 1 *
bit 469 O 1 *
bit 468 O 1 *
bit 467 O 1 *
bit 466 O 1 *
bit 465 O 1 *
bit 464 O 1 *
bit 463 O 1 *
bit 462 O 1 *
bit 461 O 1 *
bit 460 I 1 IO_P54
bit 459 O 1 IO_P54 458 1 Z
bit 458 C 1 *
bit 457 I 1 IO_P53
bit 456 O 1 IO_P53 455 1 Z
bit 455 C 1 *
bit 454 I 1 CCLK_P52
bit 453 O 1 CCLK_P52 452 1 Z
bit 452 C 1 *
bit 451 I 1 DONE_P51
bit 450 O 1 DONE_P51 449 1 Z
bit 449 C 1 *
bit 448 O 1 *
bit 447 O 1 *
bit 446 O 1 *
bit 445 I 1 IO_P50
bit 444 O 1 IO_P50 443 1 Z
bit 443 C 1 *
bit 442 I 1 IO_P49
bit 441 O 1 IO_P49 440 1 Z
bit 440 C 1 *
bit 439 O 1 *
bit 438 O 1 *
bit 437 O 1 *
bit 436 O 1 *
bit 435 O 1 *
bit 434 O 1 *
bit 433 O 1 *
bit 432 O 1 *
bit 431 O 1 *
bit 430 O 1 *
bit 429 O 1 *
bit 428 O 1 *
bit 427 O 1 *
bit 426 O 1 *
bit 425 O 1 *
bit 424 O 1 *
bit 423 O 1 *
bit 422 O 1 *
bit 421 O 1 *
bit 420 O 1 *
bit 419 O 1 *
bit 418 O 1 *
bit 417 O 1 *
bit 416 O 1 *
bit 415 I 1 IO_P48
bit 414 O 1 IO_P48 413 1 Z
bit 413 C 1 *
bit 412 I 1 IO_P47
bit 411 O 1 IO_P47 410 1 Z
bit 410 C 1 *
bit 409 O 1 *
bit 408 O 1 *
bit 407 O 1 *
bit 406 O 1 *
bit 405 O 1 *
bit 404 O 1 *
bit 403 O 1 *
bit 402 O 1 *
bit 401 O 1 *
bit 400 O 1 *
bit 399 O 1 *
bit 398 O 1 *
bit 397 O 1 *
bit 396 O 1 *
bit 395 O 1 *
bit 394 I 1 IO_P44
bit 393 O 1 IO_P44 392 1 Z
bit 392 C 1 *
bit 391 I 1 IO_P43
bit 390 O 1 IO_P43 389 1 Z
bit 389 C 1 *
bit 388 O 1 *
bit 387 O 1 *
bit 386 O 1 *
bit 385 I 1 IO_P42
bit 384 O 1 IO_P42 383 1 Z
bit 383 C 1 *
bit 382 I 1 IO_P40
bit 381 O 1 IO_P40 380 1 Z
bit 380 C 1 *
bit 379 I 1 IO_P39
bit 378 O 1 IO_P39 377 1 Z
bit 377 C 1 *
bit 376 I 1 IO_P38
bit 375 O 1 IO_P38 374 1 Z
bit 374 C 1 *
bit 373 O 1 *
bit 372 O 1 *
bit 371 O 1 *
bit 370 I 1 IO_P37
bit 369 O 1 IO_P37 368 1 Z
bit 368 C 1 *
bit 367 I 1 IO_P36
bit 366 O 1 IO_P36 365 1 Z
bit 365 C 1 *
bit 364 I 1 IO_P35
bit 363 O 1 IO_P35 362 1 Z
bit 362 C 1 *
bit 361 I 1 IO_P34
bit 360 O 1 IO_P34 359 1 Z
bit 359 C 1 *
bit 358 O 1 *
bit 357 O 1 *
bit 356 O 1 *
bit 355 O 1 *
bit 354 O 1 *
bit 353 O 1 *
bit 352 O 1 *
bit 351 O 1 *
bit 350 O 1 *
bit 349 O 1 *
bit 348 O 1 *
bit 347 O 1 *
bit 346 O 1 *
bit 345 O 1 *
bit 344 O 1 *
bit 343 O 1 *
bit 342 O 1 *
bit 341 O 1 *
bit 340 I 1 IO_P32
bit 339 O 1 IO_P32 338 1 Z
bit 338 C 1 *
bit 337 I 1 IO_P30
bit 336 O 1 IO_P30 335 1 Z
bit 335 C 1 *
bit 334 O 1 *
bit 333 O 1 *
bit 332 O 1 *
bit 331 O 1 *
bit 330 O 1 *
bit 329 O 1 *
bit 328 O 1 *
bit 327 O 1 *
bit 326 O 1 *
bit 325 O 1 *
bit 324 O 1 *
bit 323 O 1 *
bit 322 O 1 *
bit 321 O 1 *
bit 320 O 1 *
bit 319 O 1 *
bit 318 O 1 *
bit 317 O 1 *
bit 316 O 1 *
bit 315 O 1 *
bit 314 O 1 *
bit 313 O 1 *
bit 312 O 1 *
bit 311 O 1 *
bit 310 O 1 *
bit 309 O 1 *
bit 308 O 1 *
bit 307 O 1 *
bit 306 O 1 *
bit 305 O 1 *
bit 304 I 1 IO_P28
bit 303 O 1 IO_P28 302 1 Z
bit 302 C 1 *
bit 301 I 1 IO_P27
bit 300 O 1 IO_P27 299 1 Z
bit 299 C 1 *
bit 298 I 1 M2_P26
bit 297 I 1 M0_P25
bit 296 I 1 M1_P24
bit 295 I 1 IO_P23
bit 294 O 1 IO_P23 293 1 Z
bit 293 C 1 *
bit 292 I 1 IO_P22
bit 291 O 1 IO_P22 290 1 Z
bit 290 C 1 *
bit 289 O 1 *
bit 288 O 1 *
bit 287 O 1 *
bit 286 O 1 *
bit 285 O 1 *
bit 284 O 1 *
bit 283 O 1 *
bit 282 O 1 *
bit 281 O 1 *
bit 280 O 1 *
bit 279 O 1 *
bit 278 O 1 *
bit 277 O 1 *
bit 276 O 1 *
bit 275 O 1 *
bit 274 O 1 *
bit 273 O 1 *
bit 272 O 1 *
bit 271 O 1 *
bit 270 O 1 *
bit 269 O 1 *
bit 268 I 1 IO_P21
bit 267 O 1 IO_P21 266 1 Z
bit 266 C 1 *
bit 265 O 1 *
bit 264 O 1 *
bit 263 O 1 *
bit 262 O 1 *
bit 261 O 1 *
bit 260 O 1 *
bit 259 O 1 *
bit 258 O 1 *
bit 257 O 1 *
bit 256 O 1 *
bit 255 O 1 *
bit 254 O 1 *
bit 253 O 1 *
bit 252 O 1 *
bit 251 O 1 *
bit 250 I 1 IO_P17
bit 249 O 1 IO_P17 248 1 Z
bit 248 C 1 *
bit 247 I 1 IO_P16
bit 246 O 1 IO_P16 245 1 Z
bit 245 C 1 *
bit 244 I 1 IO_P15
bit 243 O 1 IO_P15 242 1 Z
bit 242 C 1 *
bit 241 O 1 *
bit 240 O 1 *
bit 239 O 1 *
bit 238 O 1 *
bit 237 O 1 *
bit 236 O 1 *
bit 235 O 1 *
bit 234 O 1 *
bit 233 O 1 *
bit 232 O 1 *
bit 231 O 1 *
bit 230 O 1 *
bit 229 I 1 IO_P14
bit 228 O 1 IO_P14 227 1 Z
bit 227 C 1 *
bit 226 I 1 IO_P13
bit 225 O 1 IO_P13 224 1 Z
bit 224 C 1 *
bit 223 I 1 IO_P12
bit 222 O 1 IO_P12 221 1 Z
bit 221 C 1 *
bit 220 I 1 IO_P11
bit 219 O 1 IO_P11 218 1 Z
bit 218 C 1 *
bit 217 O 1 *
bit 216 O 1 *
bit 215 O 1 *
bit 214 O 1 *
bit 213 O 1 *
bit 212 O 1 *
bit 211 O 1 *
bit 210 O 1 *
bit 209 O 1 *
bit 208 O 1 *
bit 207 O 1 *
bit 206 O 1 *
bit 205 O 1 *
bit 204 O 1 *
bit 203 O 1 *
bit 202 O 1 *
bit 201 O 1 *
bit 200 O 1 *
bit 199 I 1 IO_P9
bit 198 O 1 IO_P9 197 1 Z
bit 197 C 1 *
bit 196 I 1 IO_P8
bit 195 O 1 IO_P8 194 1 Z
bit 194 C 1 *
bit 193 O 1 *
bit 192 O 1 *
bit 191 O 1 *
bit 190 O 1 *
bit 189 O 1 *
bit 188 O 1 *
bit 187 I 1 IO_P5
bit 186 O 1 IO_P5 185 1 Z
bit 185 C 1 *
bit 184 I 1 IO_P4
bit 183 O 1 IO_P4 182 1 Z
bit 182 C 1 *
bit 181 O 1 *
bit 180 O 1 *
bit 179 O 1 *
bit 178 O 1 *
bit 177 O 1 *
bit 176 O 1 *
bit 175 O 1 *
bit 174 O 1 *
bit 173 O 1 *
bit 172 O 1 *
bit 171 O 1 *
bit 170 O 1 *
bit 169 O 1 *
bit 168 O 1 *
bit 167 O 1 *
bit 166 O 1 *
bit 165 O 1 *
bit 164 O 1 *
bit 163 O 1 *
bit 162 O 1 *
bit 161 O 1 *
bit 160 O 1 *
bit 159 O 1 *
bit 158 O 1 *
bit 157 I 1 IO_P2
bit 156 O 1 IO_P2 155 1 Z
bit 155 C 1 *
bit 154 I 1 IO_P1
bit 153 O 1 IO_P1 152 1 Z
bit 152 C 1 *
bit 151 O 1 *
bit 150 I 1 HSWAP_EN_P98
bit 149 O 1 *
bit 148 O 1 *
bit 147 O 1 *
bit 146 I 1 IO_P97
bit 145 O 1 IO_P97 144 1 Z
bit 144 C 1 *
bit 143 I 1 IO_P96
bit 142 O 1 IO_P96 141 1 Z
bit 141 C 1 *
bit 140 O 1 *
bit 139 O 1 *
bit 138 O 1 *
bit 137 O 1 *
bit 136 O 1 *
bit 135 O 1 *
bit 134 O 1 *
bit 133 O 1 *
bit 132 O 1 *
bit 131 O 1 *
bit 130 O 1 *
bit 129 O 1 *
bit 128 O 1 *
bit 127 O 1 *
bit 126 O 1 *
bit 125 O 1 *
bit 124 O 1 *
bit 123 O 1 *
bit 122 O 1 *
bit 121 O 1 *
bit 120 O 1 *
bit 119 O 1 *
bit 118 O 1 *
bit 117 O 1 *
bit 116 O 1 *
bit 115 O 1 *
bit 114 O 1 *
bit 113 O 1 *
bit 112 O 1 *
bit 111 O 1 *
bit 110 O 1 *
bit 109 O 1 *
bit 108 O 1 *
bit 107 O 1 *
bit 106 O 1 *
bit 105 O 1 *
bit 104 O 1 *
bit 103 O 1 *
bit 102 O 1 *
bit 101 O 1 *
bit 100 O 1 *
bit 99 O 1 *
bit 98 O 1 *
bit 97 O 1 *
bit 96 O 1 *
bit 95 O 1 *
bit 94 O 1 *
bit 93 O 1 *
bit 92 O 1 *
bit 91 O 1 *
bit 90 O 1 *
bit 89 O 1 *
bit 88 O 1 *
bit 87 O 1 *
bit 86 I 1 IO_P92
bit 85 O 1 IO_P92 84 1 Z
bit 84 C 1 *
bit 83 I 1 IO_P91
bit 82 O 1 IO_P91 81 1 Z
bit 81 C 1 *
bit 80 I 1 IO_P90
bit 79 O 1 IO_P90 78 1 Z
bit 78 C 1 *
bit 77 I 1 IO_P89
bit 76 O 1 IO_P89 75 1 Z
bit 75 C 1 *
bit 74 O 1 *
bit 73 O 1 *
bit 72 O 1 *
bit 71 I 1 IO_P88
bit 70 O 1 IO_P88 69 1 Z
bit 69 C 1 *
bit 68 I 1 IO_P87
bit 67 O 1 IO_P87 66 1 Z
bit 66 C 1 *
bit 65 I 1 IO_P86
bit 64 O 1 IO_P86 63 1 Z
bit 63 C 1 *
bit 62 I 1 IO_P85
bit 61 O 1 IO_P85 60 1 Z
bit 60 C 1 *
bit 59 O 1 *
bit 58 O 1 *
bit 57 O 1 *
bit 56 O 1 *
bit 55 O 1 *
bit 54 O 1 *
bit 53 O 1 *
bit 52 O 1 *
bit 51 O 1 *
bit 50 O 1 *
bit 49 O 1 *
bit 48 O 1 *
bit 47 O 1 *
bit 46 O 1 *
bit 45 O 1 *
bit 44 O 1 *
bit 43 O 1 *
bit 42 O 1 *
bit 41 O 1 *
bit 40 O 1 *
bit 39 O 1 *
bit 38 O 1 *
bit 37 O 1 *
bit 36 O 1 *
bit 35 O 1 *
bit 34 O 1 *
bit 33 O 1 *
bit 32 O 1 *
bit 31 O 1 *
bit 30 O 1 *
bit 29 I 1 IO_P81
bit 28 O 1 IO_P81 27 1 Z
bit 27 C 1 *
bit 26 O 1 *
bit 25 O 1 *
bit 24 O 1 *
bit 23 O 1 *
bit 22 O 1 *
bit 21 O 1 *
bit 20 O 1 *
bit 19 O 1 *
bit 18 O 1 *
bit 17 O 1 *
bit 16 O 1 *
bit 15 O 1 *
bit 14 O 1 *
bit 13 O 1 *
bit 12 O 1 *
bit 11 O 1 *
bit 10 O 1 *
bit 9 O 1 *
bit 8 O 1 *
bit 7 O 1 *
bit 6 O 1 *
bit 5 I 1 IO_P80
bit 4 O 1 IO_P80 3 1 Z
bit 3 C 1 *
bit 2 I 1 IO_P79
bit 1 O 1 IO_P79 0 1 Z
bit 0 C 1 *
