#
# $Id: sa1100 448 2003-05-29 09:18:54Z telka $
#
# JTAG declarations for SA-1100
# Copyright (C) 2003 ETC s.r.o.
#
# This program is free software; you can redistribute it and/or
# modify it under the terms of the GNU General Public License
# as published by the Free Software Foundation; either version 2
# of the License, or (at your option) any later version.
#
# This program is distributed in the hope that it will be useful,
# but WITHOUT ANY WARRANTY; without even the implied warranty of
# MERCHANTABILITY or FITNESS FOR A PARTICULAR PURPOSE.  See the
# GNU General Public License for more details.
#
# You should have received a copy of the GNU General Public License
# along with this program; if not, write to the Free Software
# Foundation, Inc., 59 Temple Place - Suite 330, Boston, MA
# 02111-1307, USA.
#
# Written by Marcel Telka <marcel@telka.sk>, 2003.
#

signal	A(0)
signal	A(1)
signal	A(2)
signal	A(3)
signal	A(4)
signal	A(5)
signal	A(6)
signal	A(7)
signal	A(8)
signal	A(9)
signal	A(10)
signal	A(11)
signal	A(12)
signal	A(13)
signal	A(14)
signal	A(15)
signal	A(16)
signal	A(17)
signal	A(18)
signal	A(19)
signal	A(20)
signal	A(21)
signal	A(22)
signal	A(23)
signal	A(24)
signal	A(25)
signal	BATTF
signal	CAS(0)
signal	CAS(1)
signal	CAS(2)
signal	CAS(3)
signal	CS(0)
signal	CS(1)
signal	CS(2)
signal	CS(3)
signal	D(0)
signal	D(1)
signal	D(2)
signal	D(3)
signal	D(4)
signal	D(5)
signal	D(6)
signal	D(7)
signal	D(8)
signal	D(9)
signal	D(10)
signal	D(11)
signal	D(12)
signal	D(13)
signal	D(14)
signal	D(15)
signal	D(16)
signal	D(17)
signal	D(18)
signal	D(19)
signal	D(20)
signal	D(21)
signal	D(22)
signal	D(23)
signal	D(24)
signal	D(25)
signal	D(26)
signal	D(27)
signal	D(28)
signal	D(29)
signal	D(30)
signal	D(31)
signal	GP(0)
signal	GP(1)
signal	GP(2)
signal	GP(3)
signal	GP(4)
signal	GP(5)
signal	GP(6)
signal	GP(7)
signal	GP(8)
signal	GP(9)
signal	GP(10)
signal	GP(11)
signal	GP(12)
signal	GP(13)
signal	GP(14)
signal	GP(15)
signal	GP(16)
signal	GP(17)
signal	GP(18)
signal	GP(19)
signal	GP(20)
signal	GP(21)
signal	GP(22)
signal	GP(23)
signal	GP(24)
signal	GP(25)
signal	GP(26)
signal	GP(27)
signal	IOIS16
signal	LBIAS
signal	LDD(0)
signal	LDD(1)
signal	LDD(2)
signal	LDD(3)
signal	LDD(4)
signal	LDD(5)
signal	LDD(6)
signal	LDD(7)
signal	LFCLK
signal	LLCLK
signal	LPCLK
signal	OE
signal	PCE1
signal	PCE2
signal	PIOR
signal	PIOW
signal	POE
signal	PREG
signal	PSKTSEL
signal	PWAIT
signal	PWE
signal	RAS(0)
signal	RAS(1)
signal	RAS(2)
signal	RAS(3)
signal	RESET
signal	RESETO
signal	ROMSEL
signal	RXD1
signal	RXD2
signal	RXD3
signal	RXDC
signal	SCLKC
signal	SFRMC
signal	TXD1
signal	TXD2
signal	TXD3
signal	TXDC
signal	UDCN
signal	UDCP
signal	VDDFA
signal	WE

# mandatory data registers
register	BSR	279	# Boundary Scan Register
register	BR	1	# Bypass Register
# optional data registers
register	DIR	32	# Device Identification Register

instruction length 5

# mandatory instructions
instruction EXTEST		00000	BSR
instruction SAMPLE/PRELOAD	00001	BSR
instruction BYPASS		11111	BR

# optional instructions
instruction CLAMP		00100	BR
instruction HIGHZ		00101	BR
instruction IDCODE		00110	DIR

# BSR bits
bit 278 I ? BATTF
bit 277 I ? VDDFA
bit 276 X ? .
bit 275 C 0 .
bit 274 O ? SFRMC 275 0 Z
bit 273 I ? SFRMC
bit 272 C 0 .
bit 271 O ? SCLKC 272 0 Z
bit 270 I ? SCLKC
bit 269 C 0 .
bit 268 O ? RXDC 269 0 Z
bit 267 I ? RXDC
bit 266 C ? .
bit 265 O ? TXDC 266 0 Z
bit 264 I ? TXDC
bit 263 O ? D(0) 199 1 Z
bit 262 I ? D(0)
bit 261 O ? D(8) 199 1 Z
bit 260 I ? D(8)
bit 259 O ? D(16) 199 1 Z
bit 258 I ? D(16)
bit 257 O ? D(24) 199 1 Z
bit 256 I ? D(24)
bit 255 O ? D(1) 199 1 Z
bit 254 I ? D(1)
bit 253 O ? D(9) 199 1 Z
bit 252 I ? D(9)
bit 251 O ? D(17) 199 1 Z
bit 250 I ? D(17)
bit 249 O ? D(25) 199 1 Z
bit 248 I ? D(25)
bit 247 O ? D(2) 199 1 Z
bit 246 I ? D(2)
bit 245 O ? D(10) 199 1 Z
bit 244 I ? D(10)
bit 243 O ? D(18) 199 1 Z
bit 242 I ? D(18)
bit 241 O ? D(26) 199 1 Z
bit 240 I ? D(26)
bit 239 O ? D(3) 199 1 Z
bit 238 I ? D(3)
bit 237 O ? D(11) 199 1 Z
bit 236 I ? D(11)
bit 235 O ? D(19) 199 1 Z
bit 234 I ? D(19)
bit 233 O ? D(27) 199 1 Z
bit 232 I ? D(27)
bit 231 O ? D(4) 199 1 Z
bit 230 I ? D(4)
bit 229 O ? D(12) 199 1 Z
bit 228 I ? D(12)
bit 227 O ? D(20) 199 1 Z
bit 226 I ? D(20)
bit 225 O ? D(28) 199 1 Z
bit 224 I ? D(28)
bit 223 O ? D(5) 199 1 Z
bit 222 I ? D(5)
bit 221 O ? D(13) 199 1 Z
bit 220 I ? D(13)
bit 219 O ? D(21) 199 1 Z
bit 218 I ? D(21)
bit 217 O ? D(29) 199 1 Z
bit 216 I ? D(29)
bit 215 O ? D(6) 199 1 Z
bit 214 I ? D(6)
bit 213 O ? D(14) 199 1 Z
bit 212 I ? D(14)
bit 211 O ? D(22) 199 1 Z
bit 210 I ? D(22)
bit 209 O ? D(30) 199 1 Z
bit 208 I ? D(30)
bit 207 O ? D(7) 199 1 Z
bit 206 I ? D(7)
bit 205 O ? D(15) 199 1 Z
bit 204 I ? D(15)
bit 203 O ? D(23) 199 1 Z
bit 202 I ? D(23)
bit 201 O ? D(31) 199 1 Z
bit 200 I ? D(31)
bit 199 C 1 .
bit 198 C 0 .
bit 197 O ? GP(27) 198 0 Z
bit 196 I ? GP(27)
bit 195 C 0 .
bit 194 O ? GP(26) 195 0 Z
bit 193 I ? GP(26)
bit 192 C 0 .
bit 191 O ? GP(25) 192 0 Z
bit 190 I ? GP(25)
bit 189 C 0 .
bit 188 O ? GP(24) 189 0 Z
bit 187 I ? GP(24)
bit 186 C 0 .
bit 185 O ? GP(23) 186 0 Z
bit 184 I ? GP(23)
bit 183 C 0 .
bit 182 O ? GP(22) 183 0 Z
bit 181 I ? GP(22)
bit 180 C 0 .
bit 179 O ? GP(21) 180 0 Z
bit 178 I ? GP(21)
bit 177 C 0 .
bit 176 O ? GP(20) 177 0 Z
bit 175 I ? GP(20)
bit 174 C 0 .
bit 173 O ? GP(19) 174 0 Z
bit 172 I ? GP(19)
bit 171 C 0 .
bit 170 O ? GP(18) 171 0 Z
bit 169 I ? GP(18)
bit 168 C 0 .
bit 167 O ? GP(17) 168 0 Z
bit 166 I ? GP(17)
bit 165 C 0 .
bit 164 O ? GP(16) 165 0 Z
bit 163 I ? GP(16)
bit 162 C 0 .
bit 161 O ? GP(15) 162 0 Z
bit 160 I ? GP(15)
bit 159 C 0 .
bit 158 O ? GP(14) 159 0 Z
bit 157 I ? GP(14)
bit 156 C 0 .
bit 155 O ? GP(13) 156 0 Z
bit 154 I ? GP(13)
bit 153 C 0 .
bit 152 O ? GP(12) 153 0 Z
bit 151 I ? GP(12)
bit 150 C 0 .
bit 149 O ? GP(11) 150 0 Z
bit 148 I ? GP(11)
bit 147 C 0 .
bit 146 O ? GP(10) 147 0 Z
bit 145 I ? GP(10)
bit 144 C 0 .
bit 143 O ? GP(9) 144 0 Z
bit 142 I ? GP(9)
bit 141 C 0 .
bit 140 O ? GP(8) 141 0 Z
bit 139 I ? GP(8)
bit 138 C 0 .
bit 137 O ? GP(7) 138 0 Z
bit 136 I ? GP(7)
bit 135 C 0 .
bit 134 O ? GP(6) 135 0 Z
bit 133 I ? GP(6)
bit 132 C 0 .
bit 131 O ? GP(5) 132 0 Z
bit 130 I ? GP(5)
bit 129 C 0 .
bit 128 O ? GP(4) 129 0 Z
bit 127 I ? GP(4)
bit 126 C 0 .
bit 125 O ? GP(3) 126 0 Z
bit 124 I ? GP(3)
bit 123 C 0 .
bit 122 O ? GP(2) 123 0 Z
bit 121 I ? GP(2)
bit 120 C 0 .
bit 119 O ? GP(1) 120 0 Z
bit 118 I ? GP(1)
bit 117 C 0 .
bit 116 O ? GP(0) 117 0 Z
bit 115 I ? GP(0)
bit 114 C 0 .
bit 113 O ? LBIAS 114 0 Z
bit 112 I ? LBIAS
bit 111 C 0 .
bit 110 O ? LPCLK 111 0 Z
bit 109 I ? LPCLK
bit 108 C 0 .
bit 107 O ? LDD(0) 108 0 Z
bit 106 I ? LDD(0)
bit 105 C 0 .
bit 104 O ? LDD(1) 105 0 Z
bit 103 I ? LDD(1)
bit 102 C 0 .
bit 101 O ? LDD(2) 102 0 Z
bit 100 I ? LDD(2)
bit 99 C 0 .
bit 98 O ? LDD(3) 99 0 Z
bit 97 I ? LDD(3)
bit 96 C 0 .
bit 95 O ? LDD(4) 96 0 Z
bit 94 I ? LDD(4)
bit 93 C 0 .
bit 92 O ? LDD(5) 93 0 Z
bit 91 I ? LDD(5)
bit 90 C 0 .
bit 89 O ? LDD(6) 90 0 Z
bit 88 I ? LDD(6)
bit 87 C 0 .
bit 86 O ? LDD(7) 87 0 Z
bit 85 I ? LDD(7)
bit 84 C 0 .
bit 83 O ? LLCLK 84 0 Z
bit 82 I ? LLCLK
bit 81 C 0 .
bit 80 O ? LFCLK 81 0 Z
bit 79 I ? LFCLK
bit 78 O ? POE
bit 77 O ? PWE
bit 76 O ? PIOR
bit 75 O ? PIOW
bit 74 O ? PSKTSEL
bit 73 I ? IOIS16
bit 72 I ? PWAIT
bit 71 O ? PREG
bit 70 O ? PCE2
bit 69 O ? PCE1
bit 68 C 1 .
bit 67 O ? WE 68 1 Z
bit 66 O ? OE 68 1 Z
bit 65 O ? RAS(3) 68 1 Z
bit 64 O ? RAS(2) 68 1 Z
bit 63 O ? RAS(1) 68 1 Z
bit 62 O ? RAS(0) 68 1 Z
bit 61 O ? CAS(3) 68 1 Z
bit 60 O ? CAS(2) 68 1 Z
bit 59 O ? CAS(1) 68 1 Z
bit 58 O ? CAS(0) 68 1 Z
bit 57 O ? CS(3) 68 1 Z
bit 56 O ? CS(2) 68 1 Z
bit 55 O ? CS(1) 68 1 Z
bit 54 O ? CS(0) 68 1 Z
bit 53 O ? A(25) 68 1 Z
bit 52 O ? A(24) 68 1 Z
bit 51 O ? A(23) 68 1 Z
bit 50 O ? A(22) 68 1 Z
bit 49 O ? A(21) 68 1 Z
bit 48 O ? A(20) 68 1 Z
bit 47 O ? A(19) 68 1 Z
bit 46 O ? A(18) 68 1 Z
bit 45 O ? A(17) 68 1 Z
bit 44 O ? A(16) 68 1 Z
bit 43 O ? A(15) 68 1 Z
bit 42 O ? A(14) 68 1 Z
bit 41 O ? A(13) 68 1 Z
bit 40 O ? A(12) 68 1 Z
bit 39 O ? A(11) 68 1 Z
bit 38 O ? A(10) 68 1 Z
bit 37 O ? A(9) 68 1 Z
bit 36 O ? A(8) 68 1 Z
bit 35 O ? A(7) 68 1 Z
bit 34 O ? A(6) 68 1 Z
bit 33 O ? A(5) 68 1 Z
bit 32 O ? A(4) 68 1 Z
bit 31 O ? A(3) 68 1 Z
bit 30 O ? A(2) 68 1 Z
bit 29 O ? A(1) 68 1 Z
bit 28 O ? A(0) 68 1 Z
bit 27 C 1 .
bit 26 O ? UDCN 27 1 Z
bit 25 I ? UDCN
bit 24 X ? .
bit 23 C 1 .
bit 22 O ? UDCP 23 1 Z
bit 21 I ? UDCP
bit 20 C 0 .
bit 19 O ? RXD1 20 0 Z
bit 18 I ? RXD1
bit 17 C 0 .
bit 16 O ? TXD1 17 0 Z
bit 15 I ? TXD1
bit 14 C 0 .
bit 13 O ? RXD2 14 0 Z
bit 12 I ? RXD2
bit 11 C 0 .
bit 10 O ? TXD2 11 0 Z
bit 9 I ? TXD2
bit 8 C 0 .
bit 7 O ? RXD3 8 0 Z
bit 6 I ? RXD3
bit 5 C 0 .
bit 4 O ? TXD3 5 0 Z
bit 3 I ? TXD3
bit 2 I ? RESET
bit 1 O ? RESETO
bit 0 I ? ROMSEL
