#
# $Id: ixp425 558 2003-09-05 21:09:14Z telka $
#
# JTAG declarations for IXP425
# Copyright (C) 2002 ETC s.r.o.
#
# This program is free software; you can redistribute it and/or
# modify it under the terms of the GNU General Public License
# as published by the Free Software Foundation; either version 2
# of the License, or (at your option) any later version.
#
# This program is distributed in the hope that it will be useful,
# but WITHOUT ANY WARRANTY; without even the implied warranty of
# MERCHANTABILITY or FITNESS FOR A PARTICULAR PURPOSE.  See the
# GNU General Public License for more details.
#
# You should have received a copy of the GNU General Public License
# along with this program; if not, write to the Free Software
# Foundation, Inc., 59 Temple Place - Suite 330, Boston, MA
# 02111-1307, USA.
#
# Written by Christian Pellegrin <chri@ascensit.com>, 2003.
#

signal	EX_CS[0]	K26
signal	EX_CS[1]	L24
signal	EX_CS[2]	M22
signal	EX_CS[3]	J26
signal	EX_CS[4]	K24
signal	EX_CS[5]	J25
signal	EX_CS[6]	H26
signal	EX_CS[7]	K23
signal	EX_WR		F22
signal	EX_RD		A23
signal	EX_RDY[0]	V26
signal	EX_RDY[1]	U24
signal	EX_RDY[2]	U23
signal	EX_RDY[3]	T22
signal	EX_IOWAIT	B23
signal	EX_CLK		M23
signal	EX_ALE		D22
signal	EX_ADDR[0]		G1
signal	EX_ADDR[1]		H2
signal	EX_ADDR[2]		H1
signal	EX_ADDR[3]		H6
signal	EX_ADDR[4]		J6
signal	EX_ADDR[5]		J5
signal	EX_ADDR[6]		J3
signal	EX_ADDR[7]		J1
signal	EX_ADDR[8]		K1
signal	EX_ADDR[9]		K2
signal	EX_ADDR[10]		K5
signal	EX_ADDR[11]		K6
signal	EX_ADDR[12]		L1
signal	EX_ADDR[13]		L3
signal	EX_ADDR[14]		M1
signal	EX_ADDR[15]		M3
signal	EX_ADDR[16]		N3
signal	EX_ADDR[17]		P1
signal	EX_ADDR[18]		R1
signal	EX_ADDR[19]		P2
signal	EX_ADDR[20]		R3
signal	EX_ADDR[21]		T4
signal	EX_ADDR[22]		R5
signal	EX_ADDR[23]		P5
signal	EX_ADDR[24]		T5
signal	EX_ADDR[25]		P4
signal	EX_DATA[0]		N4
signal	EX_DATA[1]		M5
signal	EX_DATA[2]		L5
signal	EX_DATA[3]		T6
signal	EX_DATA[4]		N6
signal	EX_DATA[5]		T7
signal	EX_DATA[6]		M6
signal	EX_DATA[7]		M7
signal	EX_DATA[8]		M9
signal	EX_DATA[9]		T10
signal	EX_DATA[10]		R9
signal	EX_DATA[11]		T11
signal	EX_DATA[12]		P11
signal	EX_DATA[13]		N10
signal	EX_DATA[14]		T12
signal	EX_DATA[15]		M10
signal	EX_DATA[16]		H3
signal	EX_DATA[17]		H5
signal	EX_DATA[18]		J4
signal	EX_DATA[19]		K3
signal	EX_DATA[20]		L4
signal	EX_DATA[21]		M2
signal	EX_DATA[22]		N1
signal	EX_DATA[23]		T3
signal	EX_DATA[24]		P6
signal	EX_DATA[25]		R7
signal	EX_DATA[26]		P7
signal	EX_DATA[27]		P8
signal	EX_DATA[28]		L8
signal	EX_DATA[29]		P10
signal	EX_DATA[30]		R11
signal	EX_DATA[31]		P12
signal	GPIO[0]		U25
signal	GPIO[1]		U22
signal	GPIO[2]		V24
signal	GPIO[3]		W26
signal	GPIO[4]		W25
signal	GPIO[5]		Y26
signal	GPIO[6]		V22
signal	GPIO[7]		W23
signal	GPIO[8]		AA26
signal	GPIO[9]		V21
signal	GPIO[10]	Y24
signal	GPIO[11]	AB26
signal	GPIO[12]	AA24
signal	GPIO[13]	AC26
signal	GPIO[14]	W21
signal	GPIO[15]	Y22

# mandatory data registers
register	BSR		498	# Boundary Scan Register
register	BR		1	# Bypass Register
# optional data registers
register	DIR		32	# Device Identification Register

instruction length 7
# mandatory instructions
instruction EXTEST		0000000	BSR
instruction SAMPLE/PRELOAD	0000001	BSR
instruction BYPASS		1111111	BR
# optional instructions
instruction CLAMP		1001001	BR
instruction HIGHZ		1001010	BR
instruction IDCODE		1111110	DIR

# boundary scan register

bit 497 C ? .
bit 496 C ? .
bit 495 C ? .
bit 494 C ? .
bit 493 C ? .
bit 492 C ? .
bit 491 C ? .
bit 490 C ? .
bit 489 C ? .
bit 488 C ? .
bit 487 C ? .
bit 486 C ? .
bit 485 C ? .
bit 484 C ? .
bit 483 C ? .
bit 482 C ? .
bit 481 C ? .
bit 480 C ? .
bit 479 C ? .
bit 478 C ? .
bit 477 C ? .
bit 476 C ? .
bit 475 C ? .
bit 474 C ? .
bit 473 C ? .
bit 472 C ? .
bit 471 C ? .
bit 470 C ? .
bit 469 C ? .
bit 468 C ? .
bit 467 C ? .
bit 466 C ? .
bit 465 C ? .
bit 464 C ? .
bit 463 C ? .
bit 462 C ? .
bit 461 C ? .
bit 460 C ? .
bit 459 C ? .
bit 458 C ? .
bit 457 C ? .
bit 456 C ? .
bit 455 C ? .
bit 454 C ? .
bit 453 C ? .
bit 452 C ? .
bit 451 C ? .
bit 450 C ? .
bit 449 C ? .
bit 448 C ? .
bit 447 C ? .
bit 446 C ? .
bit 445 C ? .
bit 444 C ? .
bit 443 C ? .
bit 442 C ? .
bit 441 C ? .
bit 440 C ? .
bit 439 C ? .
bit 438 C ? .
bit 437 C ? .
bit 436 C ? .
bit 435 C ? .
bit 434 C ? .
bit 433 C ? .
bit 432 C ? .
bit 431 C ? .
bit 430 C ? .
bit 429 C ? .
bit 428 C ? .
bit 427 C ? .
bit 426 C ? .
bit 425 C ? .
bit 424 C ? .
bit 423 C ? .
bit 422 C ? .
bit 421 C ? .
bit 420 C ? .
bit 419 C ? .
bit 418 C ? .
bit 417 C ? .
bit 416 C ? .
bit 415 C ? .
bit 414 C ? .
bit 413 C ? .
bit 412 C ? .
bit 411 C ? .
bit 410 C ? .
bit 409 C ? .
bit 408 C ? .
bit 407 C ? .
bit 406 C ? .
bit 405 C ? .
bit 404 C ? .
bit 403 C ? .
bit 402 C ? .
bit 401 C ? .
bit 400 C ? .
bit 399 C ? .
bit 398 C ? .
bit 397 C ? .
bit 396 C ? .
bit 395 C ? .
bit 394 C ? .
bit 393 C ? .
bit 392 C ? .
bit 391 C ? .
bit 390 C ? .
bit 389 C ? .
bit 388 C ? .
bit 387 C ? .
bit 386 C ? .
bit 385 C ? .
bit 384 B ? GPIO[1] 369 1 Z
bit 383 B ? GPIO[2] 368 1 Z
bit 382 B ? GPIO[3] 367 1 Z
bit 381 B ? GPIO[4] 366 1 Z
bit 380 B ? GPIO[5] 365 1 Z
bit 379 B ? GPIO[6] 364 1 Z
bit 378 B ? GPIO[7] 363 1 Z
bit 377 B ? GPIO[8] 362 1 Z
bit 376 B ? GPIO[9] 361 1 Z
bit 375 B ? GPIO[10] 360 1 Z
bit 374 B ? GPIO[11] 359 1 Z
bit 373 B ? GPIO[12] 358 1 Z
bit 372 B ? GPIO[13] 357 1 Z
bit 371 B ? GPIO[14] 356 1 Z
bit 370 B ? GPIO[15] 355 1 Z
bit 369 C ? .
bit 368 C ? .
bit 367 C ? .
bit 366 C ? .
bit 365 C ? .
bit 364 C ? .
bit 363 C ? .
bit 362 C ? .
bit 361 C ? .
bit 360 C ? .
bit 359 C ? .
bit 358 C ? .
bit 357 C ? .
bit 356 C ? .
bit 355 C ? .
bit 354 I ? EX_IOWAIT
bit 353 I ? EX_CLK 
bit 352 O ? EX_ALE 297 1 Z
bit 351 O ? EX_ADDR[0] 296 1 Z
bit 350 O ? EX_ADDR[1] 295 1 Z
bit 349 O ? EX_ADDR[2] 294 1 Z
bit 348 O ? EX_ADDR[3] 293 1 Z
bit 347 O ? EX_ADDR[4] 292 1 Z
bit 346 O ? EX_ADDR[5] 291 1 Z
bit 345 O ? EX_ADDR[6] 290 1 Z
bit 344 O ? EX_ADDR[7] 289 1 Z
bit 343 O ? EX_ADDR[8] 288 1 Z
bit 342 O ? EX_ADDR[9] 287 1 Z
bit 341 O ? EX_ADDR[10] 286 1 Z
bit 340 O ? EX_ADDR[11] 285 1 Z
bit 339 O ? EX_ADDR[12] 284 1 Z
bit 338 O ? EX_ADDR[13] 283 1 Z
bit 337 O ? EX_ADDR[14] 282 1 Z
bit 336 O ? EX_ADDR[15] 281 1 Z
bit 335 O ? EX_ADDR[16] 280 1 Z
bit 334 O ? EX_ADDR[17] 279 1 Z
bit 333 O ? EX_ADDR[18] 278 1 Z
bit 332 O ? EX_ADDR[19] 277 1 Z
bit 331 O ? EX_ADDR[20] 276 1 Z
bit 330 O ? EX_ADDR[21] 275 1 Z
bit 329 O ? EX_ADDR[22] 274 1 Z
bit 328 O ? EX_ADDR[23] 273 1 Z
bit 327 O ? EX_WR 272 1 Z
bit 326 O ? EX_RD 271 1 Z
bit 325 O ? EX_CS[0] 270 1 Z
bit 324 O ? EX_CS[1] 269 1 Z
bit 323 O ? EX_CS[2] 268 1 Z
bit 322 O ? EX_CS[3] 267 1 Z
bit 321 O ? EX_CS[4] 266 1 Z
bit 320 O ? EX_CS[5] 265 1 Z
bit 319 O ? EX_CS[6] 264 1 Z
bit 318 O ? EX_CS[7] 263 1 Z
bit 317 B ? EX_DATA[0] 262 1 Z
bit 316 B ? EX_DATA[1] 261 1 Z
bit 315 B ? EX_DATA[2] 260 1 Z
bit 314 B ? EX_DATA[3] 259 1 Z
bit 313 B ? EX_DATA[4] 258 1 Z
bit 312 B ? EX_DATA[5] 257 1 Z
bit 311 B ? EX_DATA[6] 256 1 Z
bit 310 B ? EX_DATA[7] 255 1 Z
bit 309 B ? EX_DATA[8] 254 1 Z
bit 308 B ? EX_DATA[9] 253 1 Z
bit 307 B ? EX_DATA[10] 252 1 Z
bit 306 B ? EX_DATA[11] 251 1 Z
bit 305 B ? EX_DATA[12] 250 1 Z
bit 304 B ? EX_DATA[13] 249 1 Z
bit 303 B ? EX_DATA[14] 248 1 Z
bit 302 B ? EX_DATA[15] 247 1 Z
bit 301 I ? EX_RDY[0]
bit 300 I ? EX_RDY[1]
bit 299 I ? EX_RDY[2]
bit 298 I ? EX_RDY[3]
bit 297 C ? .
bit 296 C ? .
bit 295 C ? .
bit 294 C ? .
bit 293 C ? .
bit 292 C ? .
bit 291 C ? .
bit 290 C ? .
bit 289 C ? .
bit 288 C ? .
bit 287 C ? .
bit 286 C ? .
bit 285 C ? .
bit 284 C ? .
bit 283 C ? .
bit 282 C ? .
bit 281 C ? .
bit 280 C ? .
bit 279 C ? .
bit 278 C ? .
bit 277 C ? .
bit 276 C ? .
bit 275 C ? .
bit 274 C ? .
bit 273 C ? .
bit 272 C ? .
bit 271 C ? .
bit 270 C ? .
bit 269 C ? .
bit 268 C ? .
bit 267 C ? .
bit 266 C ? .
bit 265 C ? .
bit 264 C ? .
bit 263 C ? .
bit 262 C ? .
bit 261 C ? .
bit 260 C ? .
bit 259 C ? .
bit 258 C ? .
bit 257 C ? .
bit 256 C ? .
bit 255 C ? .
bit 254 C ? .
bit 253 C ? .
bit 252 C ? .
bit 251 C ? .
bit 250 C ? .
bit 249 C ? .
bit 248 C ? .
bit 247 C ? .
bit 246 C ? .
bit 245 C ? .
bit 244 C ? .
bit 243 C ? .
bit 242 C ? .
bit 241 C ? .
bit 240 C ? .
bit 239 C ? .
bit 238 C ? .
bit 237 C ? .
bit 236 C ? .
bit 235 C ? .
bit 234 C ? .
bit 233 C ? .
bit 232 C ? .
bit 231 C ? .
bit 230 C ? .
bit 229 C ? .
bit 228 C ? .
bit 227 C ? .
bit 226 C ? .
bit 225 C ? .
bit 224 C ? .
bit 223 C ? .
bit 222 C ? .
bit 221 C ? .
bit 220 C ? .
bit 219 C ? .
bit 218 C ? .
bit 217 C ? .
bit 216 C ? .
bit 215 C ? .
bit 214 C ? .
bit 213 C ? .
bit 212 C ? .
bit 211 C ? .
bit 210 C ? .
bit 209 C ? .
bit 208 C ? .
bit 207 C ? .
bit 206 C ? .
bit 205 C ? .
bit 204 C ? .
bit 203 C ? .
bit 202 C ? .
bit 201 C ? .
bit 200 C ? .
bit 199 C ? .
bit 198 C ? .
bit 197 C ? .
bit 196 C ? .
bit 195 C ? .
bit 194 C ? .
bit 193 C ? .
bit 192 C ? .
bit 191 C ? .
bit 190 C ? .
bit 189 C ? .
bit 188 C ? .
bit 187 C ? .
bit 186 C ? .
bit 185 C ? .
bit 184 C ? .
bit 183 C ? .
bit 182 C ? .
bit 181 C ? .
bit 180 C ? .
bit 179 C ? .
bit 178 C ? .
bit 177 C ? .
bit 176 C ? .
bit 175 C ? .
bit 174 C ? .
bit 173 C ? .
bit 172 C ? .
bit 171 C ? .
bit 170 C ? .
bit 169 C ? .
bit 168 C ? .
bit 167 C ? .
bit 166 C ? .
bit 165 C ? .
bit 164 C ? .
bit 163 C ? .
bit 162 C ? .
bit 161 C ? .
bit 160 C ? .
bit 159 C ? .
bit 158 C ? .
bit 157 C ? .
bit 156 C ? .
bit 155 C ? .
bit 154 C ? .
bit 153 C ? .
bit 152 C ? .
bit 151 C ? .
bit 150 C ? .
bit 149 C ? .
bit 148 C ? .
bit 147 C ? .
bit 146 C ? .
bit 145 C ? .
bit 144 C ? .
bit 143 C ? .
bit 142 C ? .
bit 141 C ? .
bit 140 C ? .
bit 139 C ? .
bit 138 C ? .
bit 137 C ? .
bit 136 C ? .
bit 135 C ? .
bit 134 C ? .
bit 133 C ? .
bit 132 C ? .
bit 131 C ? .
bit 130 C ? .
bit 129 C ? .
bit 128 C ? .
bit 127 C ? .
bit 126 C ? .
bit 125 C ? .
bit 124 C ? .
bit 123 C ? .
bit 122 C ? .
bit 121 C ? .
bit 120 C ? .
bit 119 C ? .
bit 118 C ? .
bit 117 C ? .
bit 116 C ? .
bit 115 C ? .
bit 114 C ? .
bit 113 C ? .
bit 112 C ? .
bit 111 C ? .
bit 110 C ? .
bit 109 C ? .
bit 108 C ? .
bit 107 C ? .
bit 106 C ? .
bit 105 C ? .
bit 104 C ? .
bit 103 C ? .
bit 102 C ? .
bit 101 C ? .
bit 100 C ? .
bit 99 C ? .
bit 98 C ? .
bit 97 C ? .
bit 96 C ? .
bit 95 C ? .
bit 94 C ? .
bit 93 C ? .
bit 92 C ? .
bit 91 C ? .
bit 90 C ? .
bit 89 C ? .
bit 88 C ? .
bit 87 C ? .
bit 86 C ? .
bit 85 C ? .
bit 84 C ? .
bit 83 C ? .
bit 82 C ? .
bit 81 C ? .
bit 80 C ? .
bit 79 C ? .
bit 78 C ? .
bit 77 C ? .
bit 76 C ? .
bit 75 C ? .
bit 74 C ? .
bit 73 C ? .
bit 72 C ? .
bit 71 C ? .
bit 70 C ? .
bit 69 C ? .
bit 68 C ? .
bit 67 C ? .
bit 66 C ? .
bit 65 C ? .
bit 64 C ? .
bit 63 C ? .
bit 62 C ? .
bit 61 C ? .
bit 60 C ? .
bit 59 C ? .
bit 58 C ? .
bit 57 C ? .
bit 56 C ? .
bit 55 C ? .
bit 54 C ? .
bit 53 C ? .
bit 52 C ? .
bit 51 C ? .
bit 50 C ? .
bit 49 C ? .
bit 48 C ? .
bit 47 C ? .
bit 46 C ? .
bit 45 C ? .
bit 44 C ? .
bit 43 C ? .
bit 42 C ? .
bit 41 C ? .
bit 40 C ? .
bit 39 C ? .
bit 38 C ? .
bit 37 C ? .
bit 36 C ? .
bit 35 C ? .
bit 34 C ? .
bit 33 C ? .
bit 32 C ? .
bit 31 C ? .
bit 30 C ? .
bit 29 C ? .
bit 28 C ? .
bit 27 C ? .
bit 26 C ? .
bit 25 C ? .
bit 24 C ? .
bit 23 C ? .
bit 22 C ? .
bit 21 C ? .
bit 20 C ? .
bit 19 C ? .
bit 18 C ? .
bit 17 C ? .
bit 16 C ? .
bit 15 C ? .
bit 14 C ? .
bit 13 C ? .
bit 12 C ? .
bit 11 C ? .
bit 10 C ? .
bit 9 C ? .
bit 8 C ? .
bit 7 C ? .
bit 6 C ? .
bit 5 C ? .
bit 4 C ? .
bit 3 C ? .
bit 2 C ? .
bit 1 C ? .
bit 0 C ? .

initbus ixp425
