From c93c2bbf0cc96da5a47d77f01daf6c983cfe4216 Mon Sep 17 00:00:00 2001
From: Jonas Gorski <jonas.gorski@gmail.com>
Date: Tue, 29 May 2012 10:52:25 +0200
Subject: [PATCH] MIPS: BCM63XX: add 96328avng reference board

---
 arch/mips/bcm63xx/boards/board_bcm963xx.c |   77 +++++++++++++++++++++++++++++
 1 files changed, 77 insertions(+), 0 deletions(-)

--- a/arch/mips/bcm63xx/boards/board_bcm963xx.c
+++ b/arch/mips/bcm63xx/boards/board_bcm963xx.c
@@ -65,13 +65,45 @@ static struct board_info __initdata boar
 	.has_uart0			= 1,
 	.has_pci			= 1,
 
+	.has_enetsw			= 1,
+
+	.enetsw = {
+		.used_ports = {
+			[0] = {
+				.used	= 1,
+				.phy_id = 1,
+				.name	= "Port 1",
+			},
+			[1] = {
+				.used	= 1,
+				.phy_id	= 2,
+				.name	= "Port 2",
+			},
+			[2] = {
+				.used	= 1,
+				.phy_id	= 3,
+				.name	= "Port 3",
+			},
+			[3] = {
+				.used	= 1,
+				.phy_id	= 4,
+				.name	= "Port 4",
+			},
+		},
+	},
+
 	.leds = {
 		{
-			.name		= "96328avng::ppp-fail",
+			.name		= "96328avng::internet-fail",
 			.gpio		= 2,
 			.active_low	= 1,
 		},
 		{
+			.name		= "96328avng::dsl",
+			.gpio		= 3,
+			.active_low	= 1,
+		},
+		{
 			.name		= "96328avng::power",
 			.gpio		= 4,
 			.active_low	= 1,
@@ -88,7 +120,7 @@ static struct board_info __initdata boar
 			.active_low	= 1,
 		},
 		{
-			.name		= "96328avng::ppp",
+			.name		= "96328avng::internet",
 			.gpio		= 11,
 			.active_low	= 1,
 		},
