From 7751684dc81d357bc9a226f12b9f12b14c824c54 Mon Sep 17 00:00:00 2001
From: Alison Wang <b18965@freescale.com>
Date: Thu, 4 Aug 2011 09:59:54 +0800
Subject: [PATCH 47/52] Fix DSPI compile error for MCF547x/MCF548x

Signed-off-by: Alison Wang <b18965@freescale.com>
---
 arch/m68k/coldfire/m547x/devices.c |    2 +-
 arch/m68k/include/asm/mcfdspi.h    |    8 ++++++++
 2 files changed, 9 insertions(+), 1 deletions(-)

--- a/arch/m68k/coldfire/m547x/devices.c
+++ b/arch/m68k/coldfire/m547x/devices.c
@@ -17,7 +17,7 @@
 
 #include <asm/coldfire.h>
 #include <asm/mcfsim.h>
-#include <asm/mcfqspi.h>
+#include <asm/mcfdspi.h>
 
 
 #ifdef CONFIG_SPI
--- a/arch/m68k/include/asm/mcfdspi.h
+++ b/arch/m68k/include/asm/mcfdspi.h
@@ -56,4 +56,12 @@ struct coldfire_spi_master {
 	u32 *irq_list;
 	void (*cs_control)(u8 cs, u8 command);
 };
+
+struct coldfire_spi_chip {
+	u8 mode;
+	u8 bits_per_word;
+	u8 del_cs_to_clk;
+	u8 del_after_trans;
+	u16 void_write_data;
+};
 #endif /*MCFDSPI_H_*/
