--- a/arch/mips/bcm47xx/Makefile
+++ b/arch/mips/bcm47xx/Makefile
@@ -4,4 +4,3 @@
 #
 
 obj-y 				+= gpio.o irq.o nvram.o prom.o serial.o setup.o time.o sprom.o
-obj-$(CONFIG_BCM47XX_SSB)	+= wgt634u.o
--- a/arch/mips/bcm47xx/wgt634u.c
+++ /dev/null
@@ -1,177 +0,0 @@
-/*
- * This file is subject to the terms and conditions of the GNU General Public
- * License.  See the file "COPYING" in the main directory of this archive
- * for more details.
- *
- * Copyright (C) 2007 Aurelien Jarno <aurelien@aurel32.net>
- */
-
-#include <linux/platform_device.h>
-#include <linux/module.h>
-#include <linux/leds.h>
-#include <linux/mtd/physmap.h>
-#include <linux/ssb/ssb.h>
-#include <linux/interrupt.h>
-#include <linux/reboot.h>
-#include <linux/gpio.h>
-#include <asm/mach-bcm47xx/bcm47xx.h>
-
-/* GPIO definitions for the WGT634U */
-#define WGT634U_GPIO_LED	3
-#define WGT634U_GPIO_RESET	2
-#define WGT634U_GPIO_TP1	7
-#define WGT634U_GPIO_TP2	6
-#define WGT634U_GPIO_TP3	5
-#define WGT634U_GPIO_TP4	4
-#define WGT634U_GPIO_TP5	1
-
-static struct gpio_led wgt634u_leds[] = {
-	{
-		.name = "power",
-		.gpio = WGT634U_GPIO_LED,
-		.active_low = 1,
-		.default_trigger = "heartbeat",
-	},
-};
-
-static struct gpio_led_platform_data wgt634u_led_data = {
-	.num_leds =     ARRAY_SIZE(wgt634u_leds),
-	.leds =         wgt634u_leds,
-};
-
-static struct platform_device wgt634u_gpio_leds = {
-	.name =         "leds-gpio",
-	.id =           -1,
-	.dev = {
-		.platform_data = &wgt634u_led_data,
-	}
-};
-
-
-/* 8MiB flash. The struct mtd_partition matches original Netgear WGT634U
-   firmware. */
-static struct mtd_partition wgt634u_partitions[] = {
-	{
-		.name       = "cfe",
-		.offset     = 0,
-		.size       = 0x60000,		/* 384k */
-		.mask_flags = MTD_WRITEABLE 	/* force read-only */
-	},
-	{
-		.name   = "config",
-		.offset = 0x60000,
-		.size   = 0x20000		/* 128k */
-	},
-	{
-		.name   = "linux",
-		.offset = 0x80000,
-		.size   = 0x140000 		/* 1280k */
-	},
-	{
-		.name   = "jffs",
-		.offset = 0x1c0000,
-		.size   = 0x620000 		/* 6272k */
-	},
-	{
-		.name   = "nvram",
-		.offset = 0x7e0000,
-		.size   = 0x20000		/* 128k */
-	},
-};
-
-static struct physmap_flash_data wgt634u_flash_data = {
-	.parts    = wgt634u_partitions,
-	.nr_parts = ARRAY_SIZE(wgt634u_partitions)
-};
-
-static struct resource wgt634u_flash_resource = {
-	.flags = IORESOURCE_MEM,
-};
-
-static struct platform_device wgt634u_flash = {
-	.name          = "physmap-flash",
-	.id            = 0,
-	.dev           = { .platform_data = &wgt634u_flash_data, },
-	.resource      = &wgt634u_flash_resource,
-	.num_resources = 1,
-};
-
-/* Platform devices */
-static struct platform_device *wgt634u_devices[] __initdata = {
-	&wgt634u_flash,
-	&wgt634u_gpio_leds,
-};
-
-static irqreturn_t gpio_interrupt(int irq, void *ignored)
-{
-	int state;
-
-	/* Interrupts are shared, check if the current one is
-	   a GPIO interrupt. */
-	if (!ssb_chipco_irq_status(&bcm47xx_bus.ssb.chipco,
-				   SSB_CHIPCO_IRQ_GPIO))
-		return IRQ_NONE;
-
-	state = gpio_get_value(WGT634U_GPIO_RESET);
-
-	/* Interrupt are level triggered, revert the interrupt polarity
-	   to clear the interrupt. */
-	gpio_polarity(WGT634U_GPIO_RESET, state);
-
-	if (!state) {
-		printk(KERN_INFO "Reset button pressed");
-		ctrl_alt_del();
-	}
-
-	return IRQ_HANDLED;
-}
-
-static int __init wgt634u_init(void)
-{
-	/* There is no easy way to detect that we are running on a WGT634U
-	 * machine. Use the MAC address as an heuristic. Netgear Inc. has
-	 * been allocated ranges 00:09:5b:xx:xx:xx and 00:0f:b5:xx:xx:xx.
-	 */
-	u8 *et0mac;
-	int err;
-
-	if (bcm47xx_bus_type != BCM47XX_BUS_TYPE_SSB)
-		return -ENODEV;
-
-	et0mac = bcm47xx_bus.ssb.sprom.et0mac;
-
-	if (et0mac[0] == 0x00 &&
-	    ((et0mac[1] == 0x09 && et0mac[2] == 0x5b) ||
-	     (et0mac[1] == 0x0f && et0mac[2] == 0xb5))) {
-		struct ssb_mipscore *mcore = &bcm47xx_bus.ssb.mipscore;
-
-		printk(KERN_INFO "WGT634U machine detected.\n");
-
-		err = gpio_request(WGT634U_GPIO_RESET, "reset-buton");
-		if (err) {
-			printk(KERN_INFO "Can not register gpio for reset button\n");
-			return 0;
-		}
-
-		if (!request_irq(gpio_to_irq(WGT634U_GPIO_RESET),
-				 gpio_interrupt, IRQF_SHARED,
-				 "WGT634U GPIO", &bcm47xx_bus.ssb.chipco)) {
-			gpio_direction_input(WGT634U_GPIO_RESET);
-			gpio_intmask(WGT634U_GPIO_RESET, 1);
-			ssb_chipco_irq_mask(&bcm47xx_bus.ssb.chipco,
-					    SSB_CHIPCO_IRQ_GPIO,
-					    SSB_CHIPCO_IRQ_GPIO);
-		}
-
-		wgt634u_flash_data.width = mcore->pflash.buswidth;
-		wgt634u_flash_resource.start = mcore->pflash.window;
-		wgt634u_flash_resource.end = mcore->pflash.window
-					   + mcore->pflash.window_size
-					   - 1;
-		return platform_add_devices(wgt634u_devices,
-					    ARRAY_SIZE(wgt634u_devices));
-	} else
-		return -ENODEV;
-}
-
-module_init(wgt634u_init);
