--- a/drivers/net/wireless/rt2x00/rt2800lib.c
+++ b/drivers/net/wireless/rt2x00/rt2800lib.c
@@ -5090,7 +5090,8 @@ static int rt2800_probe_hw_mode(struct r
 	    IEEE80211_HW_SUPPORTS_PS |
 	    IEEE80211_HW_PS_NULLFUNC_STACK |
 	    IEEE80211_HW_AMPDU_AGGREGATION |
-	    IEEE80211_HW_REPORTS_TX_ACK_STATUS;
+	    IEEE80211_HW_REPORTS_TX_ACK_STATUS |
+	    IEEE80211_HW_TEARDOWN_AGGR_ON_BAR_FAIL;
 
 	/*
 	 * Don't set IEEE80211_HW_HOST_BROADCAST_PS_BUFFERING for USB devices
--- a/drivers/net/wireless/rt2x00/rt2x00dev.c
+++ b/drivers/net/wireless/rt2x00/rt2x00dev.c
@@ -392,10 +392,9 @@ void rt2x00lib_txdone(struct queue_entry
 		tx_info->flags |= IEEE80211_TX_STAT_AMPDU;
 		tx_info->status.ampdu_len = 1;
 		tx_info->status.ampdu_ack_len = success ? 1 : 0;
-		/*
-		 * TODO: Need to tear down BA session here
-		 * if not successful.
-		 */
+
+		if (!success)
+			tx_info->flags |= IEEE80211_TX_STAT_AMPDU_NO_BACK;
 	}
 
 	if (rate_flags & IEEE80211_TX_RC_USE_RTS_CTS) {
--- a/include/net/mac80211.h
+++ b/include/net/mac80211.h
@@ -1369,6 +1369,10 @@ struct ieee80211_tx_control {
  * @IEEE80211_HW_P2P_DEV_ADDR_FOR_INTF: Use the P2P Device address for any
  *	P2P Interface. This will be honoured even if more than one interface
  *	is supported.
+ *
+ * @IEEE80211_HW_TEARDOWN_AGGR_ON_BAR_FAIL: On this hardware TX BA session
+ *	should be tear down once BAR frame will not be acked.
+ *
  */
 enum ieee80211_hw_flags {
 	IEEE80211_HW_HAS_RATE_CONTROL			= 1<<0,
@@ -1397,6 +1401,7 @@ enum ieee80211_hw_flags {
 	IEEE80211_HW_TX_AMPDU_SETUP_IN_HW		= 1<<23,
 	IEEE80211_HW_SCAN_WHILE_IDLE			= 1<<24,
 	IEEE80211_HW_P2P_DEV_ADDR_FOR_INTF		= 1<<25,
+	IEEE80211_HW_TEARDOWN_AGGR_ON_BAR_FAIL		= 1<<26,
 };
 
 /**
--- a/net/mac80211/agg-rx.c
+++ b/net/mac80211/agg-rx.c
@@ -203,6 +203,8 @@ static void ieee80211_send_addba_resp(st
 		memcpy(mgmt->bssid, sdata->u.mgd.bssid, ETH_ALEN);
 	else if (sdata->vif.type == NL80211_IFTYPE_ADHOC)
 		memcpy(mgmt->bssid, sdata->u.ibss.bssid, ETH_ALEN);
+	else if (sdata->vif.type == NL80211_IFTYPE_WDS)
+		memcpy(mgmt->bssid, da, ETH_ALEN);
 
 	mgmt->frame_control = cpu_to_le16(IEEE80211_FTYPE_MGMT |
 					  IEEE80211_STYPE_ACTION);
--- a/net/mac80211/agg-tx.c
+++ b/net/mac80211/agg-tx.c
@@ -81,7 +81,8 @@ static void ieee80211_send_addba_request
 	memcpy(mgmt->sa, sdata->vif.addr, ETH_ALEN);
 	if (sdata->vif.type == NL80211_IFTYPE_AP ||
 	    sdata->vif.type == NL80211_IFTYPE_AP_VLAN ||
-	    sdata->vif.type == NL80211_IFTYPE_MESH_POINT)
+	    sdata->vif.type == NL80211_IFTYPE_MESH_POINT ||
+	    sdata->vif.type == NL80211_IFTYPE_WDS)
 		memcpy(mgmt->bssid, sdata->vif.addr, ETH_ALEN);
 	else if (sdata->vif.type == NL80211_IFTYPE_STATION)
 		memcpy(mgmt->bssid, sdata->u.mgd.bssid, ETH_ALEN);
@@ -460,6 +461,7 @@ int ieee80211_start_tx_ba_session(struct
 	    sdata->vif.type != NL80211_IFTYPE_MESH_POINT &&
 	    sdata->vif.type != NL80211_IFTYPE_AP_VLAN &&
 	    sdata->vif.type != NL80211_IFTYPE_AP &&
+	    sdata->vif.type != NL80211_IFTYPE_WDS &&
 	    sdata->vif.type != NL80211_IFTYPE_ADHOC)
 		return -EINVAL;
 
--- a/net/mac80211/debugfs_sta.c
+++ b/net/mac80211/debugfs_sta.c
@@ -65,11 +65,11 @@ static ssize_t sta_flags_read(struct fil
 	test_sta_flag(sta, WLAN_STA_##flg) ? #flg "\n" : ""
 
 	int res = scnprintf(buf, sizeof(buf),
-			    "%s%s%s%s%s%s%s%s%s%s%s%s%s%s%s%s%s%s%s%s",
+			    "%s%s%s%s%s%s%s%s%s%s%s%s%s%s%s%s%s%s%s",
 			    TEST(AUTH), TEST(ASSOC), TEST(PS_STA),
 			    TEST(PS_DRIVER), TEST(AUTHORIZED),
 			    TEST(SHORT_PREAMBLE),
-			    TEST(WME), TEST(WDS), TEST(CLEAR_PS_FILT),
+			    TEST(WME), TEST(CLEAR_PS_FILT),
 			    TEST(MFP), TEST(BLOCK_BA), TEST(PSPOLL),
 			    TEST(UAPSD), TEST(SP), TEST(TDLS_PEER),
 			    TEST(TDLS_PEER_AUTH), TEST(4ADDR_EVENT),
--- a/net/mac80211/ibss.c
+++ b/net/mac80211/ibss.c
@@ -201,6 +201,20 @@ static void __ieee80211_sta_join_ibss(st
 	bss_change |= BSS_CHANGED_BASIC_RATES;
 	bss_change |= BSS_CHANGED_HT;
 	bss_change |= BSS_CHANGED_IBSS;
+
+	/*
+	 * In 5 GHz/802.11a, we can always use short slot time.
+	 * (IEEE 802.11-2012 18.3.8.7)
+	 *
+	 * In 2.4GHz, we must always use long slots in IBSS for compatibility
+	 * reasons.
+	 * (IEEE 802.11-2012 19.4.5)
+	 *
+	 * HT follows these specifications (IEEE 802.11-2012 20.3.18)
+	 */
+	sdata->vif.bss_conf.use_short_slot = chan->band == IEEE80211_BAND_5GHZ;
+	bss_change |= BSS_CHANGED_ERP_SLOT;
+
 	sdata->vif.bss_conf.ibss_joined = true;
 	sdata->vif.bss_conf.ibss_creator = creator;
 	ieee80211_bss_info_change_notify(sdata, bss_change);
--- a/net/mac80211/iface.c
+++ b/net/mac80211/iface.c
@@ -508,9 +508,9 @@ static void ieee80211_del_virtual_monito
 int ieee80211_do_open(struct wireless_dev *wdev, bool coming_up)
 {
 	struct ieee80211_sub_if_data *sdata = IEEE80211_WDEV_TO_SUB_IF(wdev);
+	struct ieee80211_sub_if_data *ap_sdata;
 	struct net_device *dev = wdev->netdev;
 	struct ieee80211_local *local = sdata->local;
-	struct sta_info *sta;
 	u32 changed = 0;
 	int res;
 	u32 hw_reconf_flags = 0;
@@ -587,10 +587,14 @@ int ieee80211_do_open(struct wireless_de
 	switch (sdata->vif.type) {
 	case NL80211_IFTYPE_AP_VLAN:
 		/* no need to tell driver, but set carrier */
-		if (rtnl_dereference(sdata->bss->beacon))
-			netif_carrier_on(dev);
-		else
+		if (!rtnl_dereference(sdata->bss->beacon)) {
 			netif_carrier_off(dev);
+			break;
+		}
+
+		ap_sdata = get_bss_sdata(sdata);
+		ieee80211_vif_copy_channel(sdata, ap_sdata);
+		netif_carrier_on(dev);
 		break;
 	case NL80211_IFTYPE_MONITOR:
 		if (sdata->u.mntr_flags & MONITOR_FLAG_COOK_FRAMES) {
@@ -665,30 +669,8 @@ int ieee80211_do_open(struct wireless_de
 
 	set_bit(SDATA_STATE_RUNNING, &sdata->state);
 
-	if (sdata->vif.type == NL80211_IFTYPE_WDS) {
-		/* Create STA entry for the WDS peer */
-		sta = sta_info_alloc(sdata, sdata->u.wds.remote_addr,
-				     GFP_KERNEL);
-		if (!sta) {
-			res = -ENOMEM;
-			goto err_del_interface;
-		}
-
-		sta_info_pre_move_state(sta, IEEE80211_STA_AUTH);
-		sta_info_pre_move_state(sta, IEEE80211_STA_ASSOC);
-		sta_info_pre_move_state(sta, IEEE80211_STA_AUTHORIZED);
-
-		res = sta_info_insert(sta);
-		if (res) {
-			/* STA has been freed */
-			goto err_del_interface;
-		}
-
-		rate_control_rate_init(sta);
-		netif_carrier_on(dev);
-	} else if (sdata->vif.type == NL80211_IFTYPE_P2P_DEVICE) {
+	if (sdata->vif.type == NL80211_IFTYPE_P2P_DEVICE)
 		rcu_assign_pointer(local->p2p_sdata, sdata);
-	}
 
 	/*
 	 * set_multicast_list will be invoked by the networking core
@@ -844,6 +826,8 @@ static void ieee80211_do_stop(struct iee
 	switch (sdata->vif.type) {
 	case NL80211_IFTYPE_AP_VLAN:
 		list_del(&sdata->u.vlan.list);
+		netif_carrier_off(sdata->dev);
+		ieee80211_vif_release_channel(sdata);
 		/* no need to tell driver */
 		break;
 	case NL80211_IFTYPE_MONITOR:
@@ -1072,6 +1056,72 @@ static void ieee80211_if_setup(struct ne
 	dev->destructor = free_netdev;
 }
 
+static void ieee80211_wds_rx_queued_mgmt(struct ieee80211_sub_if_data *sdata,
+					 struct sk_buff *skb)
+{
+	struct ieee80211_local *local = sdata->local;
+	struct ieee80211_rx_status *rx_status;
+	struct ieee802_11_elems elems;
+	struct ieee80211_mgmt *mgmt;
+	struct sta_info *sta;
+	size_t baselen;
+	u32 rates = 0;
+	u16 stype;
+	bool new = false;
+	enum ieee80211_band band = local->hw.conf.channel->band;
+	struct ieee80211_supported_band *sband = local->hw.wiphy->bands[band];
+
+	rx_status = IEEE80211_SKB_RXCB(skb);
+	mgmt = (struct ieee80211_mgmt *) skb->data;
+	stype = le16_to_cpu(mgmt->frame_control) & IEEE80211_FCTL_STYPE;
+
+	if (stype != IEEE80211_STYPE_BEACON)
+		return;
+
+	baselen = (u8 *) mgmt->u.probe_resp.variable - (u8 *) mgmt;
+	if (baselen > skb->len)
+		return;
+
+	ieee802_11_parse_elems(mgmt->u.probe_resp.variable,
+			       skb->len - baselen, &elems);
+
+	rates = ieee80211_sta_get_rates(local, &elems, band, NULL);
+
+	rcu_read_lock();
+
+	sta = sta_info_get(sdata, sdata->u.wds.remote_addr);
+
+	if (!sta) {
+		rcu_read_unlock();
+		sta = sta_info_alloc(sdata, sdata->u.wds.remote_addr,
+				     GFP_KERNEL);
+		if (!sta)
+			return;
+
+		new = true;
+	}
+
+	sta->last_rx = jiffies;
+	sta->sta.supp_rates[local->hw.conf.channel->band] = rates;
+
+	if (elems.ht_cap_elem)
+		ieee80211_ht_cap_ie_to_sta_ht_cap(sdata, sband,
+				elems.ht_cap_elem, &sta->sta.ht_cap);
+
+	if (elems.wmm_param)
+		set_sta_flag(sta, WLAN_STA_WME);
+
+	if (new) {
+		sta_info_pre_move_state(sta, IEEE80211_STA_AUTH);
+		sta_info_pre_move_state(sta, IEEE80211_STA_ASSOC);
+		sta_info_pre_move_state(sta, IEEE80211_STA_AUTHORIZED);
+		rate_control_rate_init(sta);
+		sta_info_insert_rcu(sta);
+	}
+
+	rcu_read_unlock();
+}
+
 static void ieee80211_iface_work(struct work_struct *work)
 {
 	struct ieee80211_sub_if_data *sdata =
@@ -1176,6 +1226,9 @@ static void ieee80211_iface_work(struct 
 				break;
 			ieee80211_mesh_rx_queued_mgmt(sdata, skb);
 			break;
+		case NL80211_IFTYPE_WDS:
+			ieee80211_wds_rx_queued_mgmt(sdata, skb);
+			break;
 		default:
 			WARN(1, "frame for unexpected interface type");
 			break;
--- a/net/mac80211/rx.c
+++ b/net/mac80211/rx.c
@@ -378,9 +378,6 @@ ieee80211_rx_monitor(struct ieee80211_lo
 	 * the SKB because it has a bad FCS/PLCP checksum.
 	 */
 
-	/* room for the radiotap header based on driver features */
-	needed_headroom = ieee80211_rx_radiotap_space(local, status);
-
 	if (local->hw.flags & IEEE80211_HW_RX_INCLUDES_FCS)
 		present_fcs_len = FCS_LEN;
 
@@ -399,6 +396,9 @@ ieee80211_rx_monitor(struct ieee80211_lo
 		return remove_monitor_info(local, origskb);
 	}
 
+	/* room for the radiotap header based on driver features */
+	needed_headroom = ieee80211_rx_radiotap_space(local, status);
+
 	if (should_drop_frame(origskb, present_fcs_len)) {
 		/* only need to expand headroom if necessary */
 		skb = origskb;
@@ -2333,7 +2333,8 @@ ieee80211_rx_h_action(struct ieee80211_r
 	if (len < IEEE80211_MIN_ACTION_SIZE)
 		return RX_DROP_UNUSABLE;
 
-	if (!rx->sta && mgmt->u.action.category != WLAN_CATEGORY_PUBLIC)
+	if (!rx->sta && mgmt->u.action.category != WLAN_CATEGORY_PUBLIC &&
+	    mgmt->u.action.category != WLAN_CATEGORY_SELF_PROTECTED)
 		return RX_DROP_UNUSABLE;
 
 	if (!(status->rx_flags & IEEE80211_RX_RA_MATCH))
@@ -2349,6 +2350,7 @@ ieee80211_rx_h_action(struct ieee80211_r
 		    sdata->vif.type != NL80211_IFTYPE_MESH_POINT &&
 		    sdata->vif.type != NL80211_IFTYPE_AP_VLAN &&
 		    sdata->vif.type != NL80211_IFTYPE_AP &&
+		    sdata->vif.type != NL80211_IFTYPE_WDS &&
 		    sdata->vif.type != NL80211_IFTYPE_ADHOC)
 			break;
 
@@ -2625,14 +2627,15 @@ ieee80211_rx_h_mgmt(struct ieee80211_rx_
 
 	if (!ieee80211_vif_is_mesh(&sdata->vif) &&
 	    sdata->vif.type != NL80211_IFTYPE_ADHOC &&
-	    sdata->vif.type != NL80211_IFTYPE_STATION)
+	    sdata->vif.type != NL80211_IFTYPE_STATION &&
+	    sdata->vif.type != NL80211_IFTYPE_WDS)
 		return RX_DROP_MONITOR;
 
 	switch (stype) {
 	case cpu_to_le16(IEEE80211_STYPE_AUTH):
 	case cpu_to_le16(IEEE80211_STYPE_BEACON):
 	case cpu_to_le16(IEEE80211_STYPE_PROBE_RESP):
-		/* process for all: mesh, mlme, ibss */
+		/* process for all: mesh, mlme, ibss, wds */
 		break;
 	case cpu_to_le16(IEEE80211_STYPE_ASSOC_RESP):
 	case cpu_to_le16(IEEE80211_STYPE_REASSOC_RESP):
@@ -2957,10 +2960,16 @@ static int prepare_for_handlers(struct i
 		}
 		break;
 	case NL80211_IFTYPE_WDS:
-		if (bssid || !ieee80211_is_data(hdr->frame_control))
-			return 0;
 		if (!ether_addr_equal(sdata->u.wds.remote_addr, hdr->addr2))
 			return 0;
+
+		if (ieee80211_is_data(hdr->frame_control) ||
+		    ieee80211_is_action(hdr->frame_control)) {
+			if (compare_ether_addr(sdata->vif.addr, hdr->addr1))
+				return 0;
+		} else if (!ieee80211_is_beacon(hdr->frame_control))
+			return 0;
+
 		break;
 	case NL80211_IFTYPE_P2P_DEVICE:
 		if (!ieee80211_is_public_action(hdr, skb->len) &&
--- a/net/mac80211/sta_info.h
+++ b/net/mac80211/sta_info.h
@@ -32,7 +32,6 @@
  * @WLAN_STA_SHORT_PREAMBLE: Station is capable of receiving short-preamble
  *	frames.
  * @WLAN_STA_WME: Station is a QoS-STA.
- * @WLAN_STA_WDS: Station is one of our WDS peers.
  * @WLAN_STA_CLEAR_PS_FILT: Clear PS filter in hardware (using the
  *	IEEE80211_TX_CTL_CLEAR_PS_FILT control flag) when the next
  *	frame to this station is transmitted.
@@ -64,7 +63,6 @@ enum ieee80211_sta_info_flags {
 	WLAN_STA_AUTHORIZED,
 	WLAN_STA_SHORT_PREAMBLE,
 	WLAN_STA_WME,
-	WLAN_STA_WDS,
 	WLAN_STA_CLEAR_PS_FILT,
 	WLAN_STA_MFP,
 	WLAN_STA_BLOCK_BA,
--- a/net/mac80211/status.c
+++ b/net/mac80211/status.c
@@ -502,7 +502,11 @@ void ieee80211_tx_status(struct ieee8021
 				       IEEE80211_BAR_CTRL_TID_INFO_MASK) >>
 				      IEEE80211_BAR_CTRL_TID_INFO_SHIFT;
 
-				ieee80211_set_bar_pending(sta, tid, ssn);
+				if (local->hw.flags &
+				    IEEE80211_HW_TEARDOWN_AGGR_ON_BAR_FAIL)
+					ieee80211_stop_tx_ba_session(&sta->sta, tid);
+				else
+					ieee80211_set_bar_pending(sta, tid, ssn);
 			}
 		}
 
--- a/drivers/net/wireless/ath/ath9k/ar9003_2p2_initvals.h
+++ b/drivers/net/wireless/ath/ath9k/ar9003_2p2_initvals.h
@@ -534,98 +534,98 @@ static const u32 ar9300_2p2_baseband_cor
 
 static const u32 ar9300Modes_high_power_tx_gain_table_2p2[][5] = {
 	/* Addr      5G_HT20     5G_HT40     2G_HT40     2G_HT20   */
-	{0x0000a2dc, 0x00033800, 0x00033800, 0x03aaa352, 0x03aaa352},
-	{0x0000a2e0, 0x0003c000, 0x0003c000, 0x03ccc584, 0x03ccc584},
-	{0x0000a2e4, 0x03fc0000, 0x03fc0000, 0x03f0f800, 0x03f0f800},
+	{0x0000a2dc, 0x0380c7fc, 0x0380c7fc, 0x03aaa352, 0x03aaa352},
+	{0x0000a2e0, 0x0000f800, 0x0000f800, 0x03ccc584, 0x03ccc584},
+	{0x0000a2e4, 0x03ff0000, 0x03ff0000, 0x03f0f800, 0x03f0f800},
 	{0x0000a2e8, 0x00000000, 0x00000000, 0x03ff0000, 0x03ff0000},
-	{0x0000a410, 0x000050d9, 0x000050d9, 0x000050d9, 0x000050d9},
-	{0x0000a500, 0x00000000, 0x00000000, 0x00000000, 0x00000000},
-	{0x0000a504, 0x06000003, 0x06000003, 0x04000002, 0x04000002},
-	{0x0000a508, 0x0a000020, 0x0a000020, 0x08000004, 0x08000004},
-	{0x0000a50c, 0x10000023, 0x10000023, 0x0b000200, 0x0b000200},
-	{0x0000a510, 0x16000220, 0x16000220, 0x0f000202, 0x0f000202},
-	{0x0000a514, 0x1c000223, 0x1c000223, 0x12000400, 0x12000400},
-	{0x0000a518, 0x21002220, 0x21002220, 0x16000402, 0x16000402},
-	{0x0000a51c, 0x27002223, 0x27002223, 0x19000404, 0x19000404},
-	{0x0000a520, 0x2b022220, 0x2b022220, 0x1c000603, 0x1c000603},
-	{0x0000a524, 0x2f022222, 0x2f022222, 0x21000a02, 0x21000a02},
-	{0x0000a528, 0x34022225, 0x34022225, 0x25000a04, 0x25000a04},
-	{0x0000a52c, 0x3a02222a, 0x3a02222a, 0x28000a20, 0x28000a20},
-	{0x0000a530, 0x3e02222c, 0x3e02222c, 0x2c000e20, 0x2c000e20},
-	{0x0000a534, 0x4202242a, 0x4202242a, 0x30000e22, 0x30000e22},
-	{0x0000a538, 0x4702244a, 0x4702244a, 0x34000e24, 0x34000e24},
-	{0x0000a53c, 0x4b02244c, 0x4b02244c, 0x38001640, 0x38001640},
-	{0x0000a540, 0x4e02246c, 0x4e02246c, 0x3c001660, 0x3c001660},
-	{0x0000a544, 0x52022470, 0x52022470, 0x3f001861, 0x3f001861},
-	{0x0000a548, 0x55022490, 0x55022490, 0x43001a81, 0x43001a81},
-	{0x0000a54c, 0x59022492, 0x59022492, 0x47001a83, 0x47001a83},
-	{0x0000a550, 0x5d022692, 0x5d022692, 0x4a001c84, 0x4a001c84},
-	{0x0000a554, 0x61022892, 0x61022892, 0x4e001ce3, 0x4e001ce3},
-	{0x0000a558, 0x65024890, 0x65024890, 0x52001ce5, 0x52001ce5},
-	{0x0000a55c, 0x69024892, 0x69024892, 0x56001ce9, 0x56001ce9},
-	{0x0000a560, 0x6e024c92, 0x6e024c92, 0x5a001ceb, 0x5a001ceb},
-	{0x0000a564, 0x74026e92, 0x74026e92, 0x5d001eec, 0x5d001eec},
-	{0x0000a568, 0x74026e92, 0x74026e92, 0x5d001eec, 0x5d001eec},
-	{0x0000a56c, 0x74026e92, 0x74026e92, 0x5d001eec, 0x5d001eec},
-	{0x0000a570, 0x74026e92, 0x74026e92, 0x5d001eec, 0x5d001eec},
-	{0x0000a574, 0x74026e92, 0x74026e92, 0x5d001eec, 0x5d001eec},
-	{0x0000a578, 0x74026e92, 0x74026e92, 0x5d001eec, 0x5d001eec},
-	{0x0000a57c, 0x74026e92, 0x74026e92, 0x5d001eec, 0x5d001eec},
-	{0x0000a580, 0x00800000, 0x00800000, 0x00800000, 0x00800000},
-	{0x0000a584, 0x06800003, 0x06800003, 0x04800002, 0x04800002},
-	{0x0000a588, 0x0a800020, 0x0a800020, 0x08800004, 0x08800004},
-	{0x0000a58c, 0x10800023, 0x10800023, 0x0b800200, 0x0b800200},
-	{0x0000a590, 0x16800220, 0x16800220, 0x0f800202, 0x0f800202},
-	{0x0000a594, 0x1c800223, 0x1c800223, 0x12800400, 0x12800400},
-	{0x0000a598, 0x21802220, 0x21802220, 0x16800402, 0x16800402},
-	{0x0000a59c, 0x27802223, 0x27802223, 0x19800404, 0x19800404},
-	{0x0000a5a0, 0x2b822220, 0x2b822220, 0x1c800603, 0x1c800603},
-	{0x0000a5a4, 0x2f822222, 0x2f822222, 0x21800a02, 0x21800a02},
-	{0x0000a5a8, 0x34822225, 0x34822225, 0x25800a04, 0x25800a04},
-	{0x0000a5ac, 0x3a82222a, 0x3a82222a, 0x28800a20, 0x28800a20},
-	{0x0000a5b0, 0x3e82222c, 0x3e82222c, 0x2c800e20, 0x2c800e20},
-	{0x0000a5b4, 0x4282242a, 0x4282242a, 0x30800e22, 0x30800e22},
-	{0x0000a5b8, 0x4782244a, 0x4782244a, 0x34800e24, 0x34800e24},
-	{0x0000a5bc, 0x4b82244c, 0x4b82244c, 0x38801640, 0x38801640},
-	{0x0000a5c0, 0x4e82246c, 0x4e82246c, 0x3c801660, 0x3c801660},
-	{0x0000a5c4, 0x52822470, 0x52822470, 0x3f801861, 0x3f801861},
-	{0x0000a5c8, 0x55822490, 0x55822490, 0x43801a81, 0x43801a81},
-	{0x0000a5cc, 0x59822492, 0x59822492, 0x47801a83, 0x47801a83},
-	{0x0000a5d0, 0x5d822692, 0x5d822692, 0x4a801c84, 0x4a801c84},
-	{0x0000a5d4, 0x61822892, 0x61822892, 0x4e801ce3, 0x4e801ce3},
-	{0x0000a5d8, 0x65824890, 0x65824890, 0x52801ce5, 0x52801ce5},
-	{0x0000a5dc, 0x69824892, 0x69824892, 0x56801ce9, 0x56801ce9},
-	{0x0000a5e0, 0x6e824c92, 0x6e824c92, 0x5a801ceb, 0x5a801ceb},
-	{0x0000a5e4, 0x74826e92, 0x74826e92, 0x5d801eec, 0x5d801eec},
-	{0x0000a5e8, 0x74826e92, 0x74826e92, 0x5d801eec, 0x5d801eec},
-	{0x0000a5ec, 0x74826e92, 0x74826e92, 0x5d801eec, 0x5d801eec},
-	{0x0000a5f0, 0x74826e92, 0x74826e92, 0x5d801eec, 0x5d801eec},
-	{0x0000a5f4, 0x74826e92, 0x74826e92, 0x5d801eec, 0x5d801eec},
-	{0x0000a5f8, 0x74826e92, 0x74826e92, 0x5d801eec, 0x5d801eec},
-	{0x0000a5fc, 0x74826e92, 0x74826e92, 0x5d801eec, 0x5d801eec},
+	{0x0000a410, 0x000050d8, 0x000050d8, 0x000050d9, 0x000050d9},
+	{0x0000a500, 0x00002220, 0x00002220, 0x00000000, 0x00000000},
+	{0x0000a504, 0x04002222, 0x04002222, 0x04000002, 0x04000002},
+	{0x0000a508, 0x09002421, 0x09002421, 0x08000004, 0x08000004},
+	{0x0000a50c, 0x0d002621, 0x0d002621, 0x0b000200, 0x0b000200},
+	{0x0000a510, 0x13004620, 0x13004620, 0x0f000202, 0x0f000202},
+	{0x0000a514, 0x19004a20, 0x19004a20, 0x11000400, 0x11000400},
+	{0x0000a518, 0x1d004e20, 0x1d004e20, 0x15000402, 0x15000402},
+	{0x0000a51c, 0x21005420, 0x21005420, 0x19000404, 0x19000404},
+	{0x0000a520, 0x26005e20, 0x26005e20, 0x1b000603, 0x1b000603},
+	{0x0000a524, 0x2b005e40, 0x2b005e40, 0x1f000a02, 0x1f000a02},
+	{0x0000a528, 0x2f005e42, 0x2f005e42, 0x23000a04, 0x23000a04},
+	{0x0000a52c, 0x33005e44, 0x33005e44, 0x26000a20, 0x26000a20},
+	{0x0000a530, 0x38005e65, 0x38005e65, 0x2a000e20, 0x2a000e20},
+	{0x0000a534, 0x3c005e69, 0x3c005e69, 0x2e000e22, 0x2e000e22},
+	{0x0000a538, 0x40005e6b, 0x40005e6b, 0x31000e24, 0x31000e24},
+	{0x0000a53c, 0x44005e6d, 0x44005e6d, 0x34001640, 0x34001640},
+	{0x0000a540, 0x49005e72, 0x49005e72, 0x38001660, 0x38001660},
+	{0x0000a544, 0x4e005eb2, 0x4e005eb2, 0x3b001861, 0x3b001861},
+	{0x0000a548, 0x53005f12, 0x53005f12, 0x3e001a81, 0x3e001a81},
+	{0x0000a54c, 0x59025eb2, 0x59025eb2, 0x42001a83, 0x42001a83},
+	{0x0000a550, 0x5e025f12, 0x5e025f12, 0x44001c84, 0x44001c84},
+	{0x0000a554, 0x61027f12, 0x61027f12, 0x48001ce3, 0x48001ce3},
+	{0x0000a558, 0x6702bf12, 0x6702bf12, 0x4c001ce5, 0x4c001ce5},
+	{0x0000a55c, 0x6b02bf14, 0x6b02bf14, 0x50001ce9, 0x50001ce9},
+	{0x0000a560, 0x6f02bf16, 0x6f02bf16, 0x54001ceb, 0x54001ceb},
+	{0x0000a564, 0x6f02bf16, 0x6f02bf16, 0x56001eec, 0x56001eec},
+	{0x0000a568, 0x6f02bf16, 0x6f02bf16, 0x56001eec, 0x56001eec},
+	{0x0000a56c, 0x6f02bf16, 0x6f02bf16, 0x56001eec, 0x56001eec},
+	{0x0000a570, 0x6f02bf16, 0x6f02bf16, 0x56001eec, 0x56001eec},
+	{0x0000a574, 0x6f02bf16, 0x6f02bf16, 0x56001eec, 0x56001eec},
+	{0x0000a578, 0x6f02bf16, 0x6f02bf16, 0x56001eec, 0x56001eec},
+	{0x0000a57c, 0x6f02bf16, 0x6f02bf16, 0x56001eec, 0x56001eec},
+	{0x0000a580, 0x00802220, 0x00802220, 0x00800000, 0x00800000},
+	{0x0000a584, 0x04802222, 0x04802222, 0x04800002, 0x04800002},
+	{0x0000a588, 0x09802421, 0x09802421, 0x08800004, 0x08800004},
+	{0x0000a58c, 0x0d802621, 0x0d802621, 0x0b800200, 0x0b800200},
+	{0x0000a590, 0x13804620, 0x13804620, 0x0f800202, 0x0f800202},
+	{0x0000a594, 0x19804a20, 0x19804a20, 0x11800400, 0x11800400},
+	{0x0000a598, 0x1d804e20, 0x1d804e20, 0x15800402, 0x15800402},
+	{0x0000a59c, 0x21805420, 0x21805420, 0x19800404, 0x19800404},
+	{0x0000a5a0, 0x26805e20, 0x26805e20, 0x1b800603, 0x1b800603},
+	{0x0000a5a4, 0x2b805e40, 0x2b805e40, 0x1f800a02, 0x1f800a02},
+	{0x0000a5a8, 0x2f805e42, 0x2f805e42, 0x23800a04, 0x23800a04},
+	{0x0000a5ac, 0x33805e44, 0x33805e44, 0x26800a20, 0x26800a20},
+	{0x0000a5b0, 0x38805e65, 0x38805e65, 0x2a800e20, 0x2a800e20},
+	{0x0000a5b4, 0x3c805e69, 0x3c805e69, 0x2e800e22, 0x2e800e22},
+	{0x0000a5b8, 0x40805e6b, 0x40805e6b, 0x31800e24, 0x31800e24},
+	{0x0000a5bc, 0x44805e6d, 0x44805e6d, 0x34801640, 0x34801640},
+	{0x0000a5c0, 0x49805e72, 0x49805e72, 0x38801660, 0x38801660},
+	{0x0000a5c4, 0x4e805eb2, 0x4e805eb2, 0x3b801861, 0x3b801861},
+	{0x0000a5c8, 0x53805f12, 0x53805f12, 0x3e801a81, 0x3e801a81},
+	{0x0000a5cc, 0x59825eb2, 0x59825eb2, 0x42801a83, 0x42801a83},
+	{0x0000a5d0, 0x5e825f12, 0x5e825f12, 0x44801c84, 0x44801c84},
+	{0x0000a5d4, 0x61827f12, 0x61827f12, 0x48801ce3, 0x48801ce3},
+	{0x0000a5d8, 0x6782bf12, 0x6782bf12, 0x4c801ce5, 0x4c801ce5},
+	{0x0000a5dc, 0x6b82bf14, 0x6b82bf14, 0x50801ce9, 0x50801ce9},
+	{0x0000a5e0, 0x6f82bf16, 0x6f82bf16, 0x54801ceb, 0x54801ceb},
+	{0x0000a5e4, 0x6f82bf16, 0x6f82bf16, 0x56801eec, 0x56801eec},
+	{0x0000a5e8, 0x6f82bf16, 0x6f82bf16, 0x56801eec, 0x56801eec},
+	{0x0000a5ec, 0x6f82bf16, 0x6f82bf16, 0x56801eec, 0x56801eec},
+	{0x0000a5f0, 0x6f82bf16, 0x6f82bf16, 0x56801eec, 0x56801eec},
+	{0x0000a5f4, 0x6f82bf16, 0x6f82bf16, 0x56801eec, 0x56801eec},
+	{0x0000a5f8, 0x6f82bf16, 0x6f82bf16, 0x56801eec, 0x56801eec},
+	{0x0000a5fc, 0x6f82bf16, 0x6f82bf16, 0x56801eec, 0x56801eec},
 	{0x0000a600, 0x00000000, 0x00000000, 0x00000000, 0x00000000},
 	{0x0000a604, 0x00000000, 0x00000000, 0x00000000, 0x00000000},
 	{0x0000a608, 0x00000000, 0x00000000, 0x00000000, 0x00000000},
 	{0x0000a60c, 0x00000000, 0x00000000, 0x00000000, 0x00000000},
-	{0x0000a610, 0x00000000, 0x00000000, 0x00000000, 0x00000000},
-	{0x0000a614, 0x02004000, 0x02004000, 0x01404000, 0x01404000},
-	{0x0000a618, 0x02004801, 0x02004801, 0x01404501, 0x01404501},
-	{0x0000a61c, 0x02808a02, 0x02808a02, 0x02008501, 0x02008501},
-	{0x0000a620, 0x0380ce03, 0x0380ce03, 0x0280ca03, 0x0280ca03},
-	{0x0000a624, 0x04411104, 0x04411104, 0x03010c04, 0x03010c04},
-	{0x0000a628, 0x04411104, 0x04411104, 0x04014c04, 0x04014c04},
-	{0x0000a62c, 0x04411104, 0x04411104, 0x04015005, 0x04015005},
-	{0x0000a630, 0x04411104, 0x04411104, 0x04015005, 0x04015005},
-	{0x0000a634, 0x04411104, 0x04411104, 0x04015005, 0x04015005},
-	{0x0000a638, 0x04411104, 0x04411104, 0x04015005, 0x04015005},
-	{0x0000a63c, 0x04411104, 0x04411104, 0x04015005, 0x04015005},
-	{0x0000b2dc, 0x00033800, 0x00033800, 0x03aaa352, 0x03aaa352},
-	{0x0000b2e0, 0x0003c000, 0x0003c000, 0x03ccc584, 0x03ccc584},
-	{0x0000b2e4, 0x03fc0000, 0x03fc0000, 0x03f0f800, 0x03f0f800},
+	{0x0000a610, 0x00804000, 0x00804000, 0x00000000, 0x00000000},
+	{0x0000a614, 0x00804201, 0x00804201, 0x01404000, 0x01404000},
+	{0x0000a618, 0x0280c802, 0x0280c802, 0x01404501, 0x01404501},
+	{0x0000a61c, 0x0280ca03, 0x0280ca03, 0x02008501, 0x02008501},
+	{0x0000a620, 0x04c15104, 0x04c15104, 0x0280ca03, 0x0280ca03},
+	{0x0000a624, 0x04c15305, 0x04c15305, 0x03010c04, 0x03010c04},
+	{0x0000a628, 0x04c15305, 0x04c15305, 0x04014c04, 0x04014c04},
+	{0x0000a62c, 0x04c15305, 0x04c15305, 0x04015005, 0x04015005},
+	{0x0000a630, 0x04c15305, 0x04c15305, 0x04015005, 0x04015005},
+	{0x0000a634, 0x04c15305, 0x04c15305, 0x04015005, 0x04015005},
+	{0x0000a638, 0x04c15305, 0x04c15305, 0x04015005, 0x04015005},
+	{0x0000a63c, 0x04c15305, 0x04c15305, 0x04015005, 0x04015005},
+	{0x0000b2dc, 0x0380c7fc, 0x0380c7fc, 0x03aaa352, 0x03aaa352},
+	{0x0000b2e0, 0x0000f800, 0x0000f800, 0x03ccc584, 0x03ccc584},
+	{0x0000b2e4, 0x03ff0000, 0x03ff0000, 0x03f0f800, 0x03f0f800},
 	{0x0000b2e8, 0x00000000, 0x00000000, 0x03ff0000, 0x03ff0000},
-	{0x0000c2dc, 0x00033800, 0x00033800, 0x03aaa352, 0x03aaa352},
-	{0x0000c2e0, 0x0003c000, 0x0003c000, 0x03ccc584, 0x03ccc584},
-	{0x0000c2e4, 0x03fc0000, 0x03fc0000, 0x03f0f800, 0x03f0f800},
+	{0x0000c2dc, 0x0380c7fc, 0x0380c7fc, 0x03aaa352, 0x03aaa352},
+	{0x0000c2e0, 0x0000f800, 0x0000f800, 0x03ccc584, 0x03ccc584},
+	{0x0000c2e4, 0x03ff0000, 0x03ff0000, 0x03f0f800, 0x03f0f800},
 	{0x0000c2e8, 0x00000000, 0x00000000, 0x03ff0000, 0x03ff0000},
 	{0x00016044, 0x012492d4, 0x012492d4, 0x012492d4, 0x012492d4},
 	{0x00016048, 0x66480001, 0x66480001, 0x66480001, 0x66480001},
--- a/drivers/net/wireless/ath/ath9k/debug.h
+++ b/drivers/net/wireless/ath/ath9k/debug.h
@@ -242,7 +242,7 @@ struct ath_rx_stats {
 
 struct ath_stats {
 	struct ath_interrupt_stats istats;
-	struct ath_tx_stats txstats[IEEE80211_NUM_ACS];
+	struct ath_tx_stats txstats[ATH9K_NUM_TX_QUEUES];
 	struct ath_rx_stats rxstats;
 	struct ath_dfs_stats dfs_stats;
 	u32 reset[__RESET_TYPE_MAX];
--- a/drivers/net/wireless/ath/carl9170/rx.c
+++ b/drivers/net/wireless/ath/carl9170/rx.c
@@ -684,7 +684,7 @@ static int carl9170_handle_mpdu(struct a
 	if (!skb)
 		return -ENOMEM;
 
-	memcpy(IEEE80211_SKB_RXCB(skb), &status, sizeof(status));
+	memcpy(IEEE80211_SKB_RXCB(skb), status, sizeof(*status));
 	ieee80211_rx(ar->hw, skb);
 	return 0;
 }
--- a/drivers/net/wireless/ath/ath9k/calib.c
+++ b/drivers/net/wireless/ath/ath9k/calib.c
@@ -69,6 +69,7 @@ s16 ath9k_hw_getchan_noise(struct ath_hw
 
 	if (chan && chan->noisefloor) {
 		s8 delta = chan->noisefloor -
+			   ATH9K_NF_CAL_NOISE_THRESH -
 			   ath9k_hw_get_default_nf(ah, chan);
 		if (delta > 0)
 			noise += delta;
--- a/drivers/net/wireless/ath/ath9k/calib.h
+++ b/drivers/net/wireless/ath/ath9k/calib.h
@@ -21,6 +21,9 @@
 
 #define AR_PHY_CCA_FILTERWINDOW_LENGTH          5
 
+/* Internal noise floor can vary by about 6db depending on the frequency */
+#define ATH9K_NF_CAL_NOISE_THRESH		6
+
 #define NUM_NF_READINGS       6
 #define ATH9K_NF_CAL_HIST_MAX 5
 
--- a/drivers/net/wireless/ath/ath5k/base.c
+++ b/drivers/net/wireless/ath/ath5k/base.c
@@ -851,7 +851,7 @@ ath5k_txbuf_free_skb(struct ath5k_hw *ah
 		return;
 	dma_unmap_single(ah->dev, bf->skbaddr, bf->skb->len,
 			DMA_TO_DEVICE);
-	dev_kfree_skb_any(bf->skb);
+	ieee80211_free_txskb(ah->hw, bf->skb);
 	bf->skb = NULL;
 	bf->skbaddr = 0;
 	bf->desc->ds_data = 0;
@@ -1578,7 +1578,7 @@ ath5k_tx_queue(struct ieee80211_hw *hw, 
 	return;
 
 drop_packet:
-	dev_kfree_skb_any(skb);
+	ieee80211_free_txskb(hw, skb);
 }
 
 static void
--- a/drivers/net/wireless/ath/ath5k/mac80211-ops.c
+++ b/drivers/net/wireless/ath/ath5k/mac80211-ops.c
@@ -65,7 +65,7 @@ ath5k_tx(struct ieee80211_hw *hw, struct
 	u16 qnum = skb_get_queue_mapping(skb);
 
 	if (WARN_ON(qnum >= ah->ah_capabilities.cap_queues.q_tx_num)) {
-		dev_kfree_skb_any(skb);
+		ieee80211_free_txskb(hw, skb);
 		return;
 	}
 
--- a/drivers/net/wireless/b43/dma.c
+++ b/drivers/net/wireless/b43/dma.c
@@ -409,7 +409,10 @@ static inline
 				struct b43_dmadesc_meta *meta)
 {
 	if (meta->skb) {
-		dev_kfree_skb_any(meta->skb);
+		if (ring->tx)
+			ieee80211_free_txskb(ring->dev->wl->hw, meta->skb);
+		else
+			dev_kfree_skb_any(meta->skb);
 		meta->skb = NULL;
 	}
 }
@@ -1454,7 +1457,7 @@ int b43_dma_tx(struct b43_wldev *dev, st
 	if (unlikely(err == -ENOKEY)) {
 		/* Drop this packet, as we don't have the encryption key
 		 * anymore and must not transmit it unencrypted. */
-		dev_kfree_skb_any(skb);
+		ieee80211_free_txskb(dev->wl->hw, skb);
 		err = 0;
 		goto out;
 	}
--- a/drivers/net/wireless/b43/main.c
+++ b/drivers/net/wireless/b43/main.c
@@ -3397,7 +3397,7 @@ static void b43_tx_work(struct work_stru
 				break;
 			}
 			if (unlikely(err))
-				dev_kfree_skb(skb); /* Drop it */
+				ieee80211_free_txskb(wl->hw, skb);
 			err = 0;
 		}
 
@@ -3419,7 +3419,7 @@ static void b43_op_tx(struct ieee80211_h
 
 	if (unlikely(skb->len < 2 + 2 + 6)) {
 		/* Too short, this can't be a valid frame. */
-		dev_kfree_skb_any(skb);
+		ieee80211_free_txskb(hw, skb);
 		return;
 	}
 	B43_WARN_ON(skb_shinfo(skb)->nr_frags);
@@ -4234,8 +4234,12 @@ redo:
 
 	/* Drain all TX queues. */
 	for (queue_num = 0; queue_num < B43_QOS_QUEUE_NUM; queue_num++) {
-		while (skb_queue_len(&wl->tx_queue[queue_num]))
-			dev_kfree_skb(skb_dequeue(&wl->tx_queue[queue_num]));
+		while (skb_queue_len(&wl->tx_queue[queue_num])) {
+			struct sk_buff *skb;
+
+			skb = skb_dequeue(&wl->tx_queue[queue_num]);
+			ieee80211_free_txskb(wl->hw, skb);
+		}
 	}
 
 	b43_mac_suspend(dev);
--- a/drivers/net/wireless/b43/pio.c
+++ b/drivers/net/wireless/b43/pio.c
@@ -196,7 +196,7 @@ static void b43_pio_cancel_tx_packets(st
 	for (i = 0; i < ARRAY_SIZE(q->packets); i++) {
 		pack = &(q->packets[i]);
 		if (pack->skb) {
-			dev_kfree_skb_any(pack->skb);
+			ieee80211_free_txskb(q->dev->wl->hw, pack->skb);
 			pack->skb = NULL;
 		}
 	}
@@ -552,7 +552,7 @@ int b43_pio_tx(struct b43_wldev *dev, st
 	if (unlikely(err == -ENOKEY)) {
 		/* Drop this packet, as we don't have the encryption key
 		 * anymore and must not transmit it unencrypted. */
-		dev_kfree_skb_any(skb);
+		ieee80211_free_txskb(dev->wl->hw, skb);
 		err = 0;
 		goto out;
 	}
--- a/net/mac80211/cfg.c
+++ b/net/mac80211/cfg.c
@@ -915,6 +915,12 @@ static int ieee80211_start_ap(struct wip
 	if (err)
 		return err;
 
+	list_for_each_entry(vlan, &sdata->u.ap.vlans, u.vlan.list) {
+		err = ieee80211_vif_copy_channel(vlan, sdata);
+		if (err)
+			return err;
+	}
+
 	/*
 	 * Apply control port protocol, this allows us to
 	 * not encrypt dynamic WEP control frames.
@@ -998,8 +1004,11 @@ static int ieee80211_stop_ap(struct wiph
 	old_probe_resp = rtnl_dereference(sdata->u.ap.probe_resp);
 
 	/* turn off carrier for this interface and dependent VLANs */
-	list_for_each_entry(vlan, &sdata->u.ap.vlans, u.vlan.list)
+	list_for_each_entry(vlan, &sdata->u.ap.vlans, u.vlan.list) {
+		sta_info_flush(local, vlan);
 		netif_carrier_off(vlan->dev);
+		ieee80211_vif_release_channel(vlan);
+	}
 	netif_carrier_off(dev);
 
 	/* remove beacon and probe response */
--- a/net/mac80211/chan.c
+++ b/net/mac80211/chan.c
@@ -119,14 +119,17 @@ static int ieee80211_assign_vif_chanctx(
 
 	lockdep_assert_held(&local->chanctx_mtx);
 
-	ret = drv_assign_vif_chanctx(local, sdata, ctx);
-	if (ret)
-		return ret;
+	if (sdata->vif.type != NL80211_IFTYPE_AP_VLAN) {
+		ret = drv_assign_vif_chanctx(local, sdata, ctx);
+		if (ret)
+			return ret;
+	}
 
 	rcu_assign_pointer(sdata->vif.chanctx_conf, &ctx->conf);
 	ctx->refcount++;
 
-	ieee80211_recalc_txpower(sdata);
+	if (sdata->vif.type != NL80211_IFTYPE_AP_VLAN)
+		ieee80211_recalc_txpower(sdata);
 
 	return 0;
 }
@@ -174,7 +177,8 @@ static void ieee80211_unassign_vif_chanc
 	ctx->refcount--;
 	rcu_assign_pointer(sdata->vif.chanctx_conf, NULL);
 
-	drv_unassign_vif_chanctx(local, sdata, ctx);
+	if (sdata->vif.type != NL80211_IFTYPE_AP_VLAN)
+		drv_unassign_vif_chanctx(local, sdata, ctx);
 
 	if (ctx->refcount > 0) {
 		ieee80211_recalc_chanctx_chantype(sdata->local, ctx);
@@ -285,6 +289,30 @@ void ieee80211_recalc_smps_chanctx(struc
 	drv_change_chanctx(local, chanctx, IEEE80211_CHANCTX_CHANGE_RX_CHAINS);
 }
 
+int ieee80211_vif_copy_channel(struct ieee80211_sub_if_data *sdata,
+			       struct ieee80211_sub_if_data *parent)
+{
+	struct ieee80211_local *local = sdata->local;
+	struct ieee80211_chanctx_conf *conf;
+	struct ieee80211_chanctx *ctx;
+
+	int ret;
+
+	mutex_lock(&local->chanctx_mtx);
+	conf = rcu_dereference_protected(parent->vif.chanctx_conf,
+					 lockdep_is_held(&local->chanctx_mtx));
+	if (!conf) {
+		ret = -ENOENT;
+		goto out;
+	}
+
+	ctx = container_of(conf, struct ieee80211_chanctx, conf);
+	ret = ieee80211_assign_vif_chanctx(sdata, ctx);
+out:
+	mutex_unlock(&local->chanctx_mtx);
+	return ret;
+}
+
 int ieee80211_vif_use_channel(struct ieee80211_sub_if_data *sdata,
 			      const struct cfg80211_chan_def *chandef,
 			      enum ieee80211_chanctx_mode mode)
--- a/net/mac80211/ieee80211_i.h
+++ b/net/mac80211/ieee80211_i.h
@@ -1633,6 +1633,8 @@ ieee80211_vif_use_channel(struct ieee802
 			  const struct cfg80211_chan_def *chandef,
 			  enum ieee80211_chanctx_mode mode);
 void ieee80211_vif_release_channel(struct ieee80211_sub_if_data *sdata);
+int ieee80211_vif_copy_channel(struct ieee80211_sub_if_data *sdata,
+			       struct ieee80211_sub_if_data *parent);
 
 void ieee80211_recalc_smps_chanctx(struct ieee80211_local *local,
 				   struct ieee80211_chanctx *chanctx);
