--- a/arch/arm/mach-cns3xxx/core.c
+++ b/arch/arm/mach-cns3xxx/core.c
@@ -19,6 +19,7 @@
 #include <asm/mach/time.h>
 #include <asm/mach/irq.h>
 #include <asm/hardware/gic.h>
+#include <asm/smp_twd.h>
 #include <asm/hardware/cache-l2x0.h>
 #include <mach/cns3xxx.h>
 #include "core.h"
@@ -73,6 +74,9 @@ static struct map_desc cns3xxx_io_desc[]
 
 void __init cns3xxx_map_io(void)
 {
+#ifdef CONFIG_LOCAL_TIMERS
+	twd_base = (void __iomem *) CNS3XXX_TC11MP_TWD_BASE_VIRT;
+#endif
 	iotable_init(cns3xxx_io_desc, ARRAY_SIZE(cns3xxx_io_desc));
 }
 
