From 05d6c964722224e8cf2902606744e29a835e7d5f Mon Sep 17 00:00:00 2001
From: John Crispin <blogic@openwrt.org>
Date: Mon, 3 Dec 2012 21:35:01 +0100
Subject: [PATCH 102/123] MIPS: lantiq: add GPHY clock gate bits

Explicitly enable the clock gate of the internal GPHYs found on xrx200.

Signed-off-by: John Crispin <blogic@openwrt.org>
---
 arch/mips/lantiq/xway/reset.c   |    9 +++++++++
 arch/mips/lantiq/xway/sysctrl.c |    1 +
 2 files changed, 10 insertions(+)

diff --git a/arch/mips/lantiq/xway/reset.c b/arch/mips/lantiq/xway/reset.c
index 544dbb7..1fa0f17 100644
--- a/arch/mips/lantiq/xway/reset.c
+++ b/arch/mips/lantiq/xway/reset.c
@@ -78,10 +78,19 @@ static struct ltq_xrx200_gphy_reset {
 /* reset and boot a gphy. these phys only exist on xrx200 SoC */
 int xrx200_gphy_boot(struct device *dev, unsigned int id, dma_addr_t dev_addr)
 {
+	struct clk *clk;
+
 	if (!of_device_is_compatible(ltq_rcu_np, "lantiq,rcu-xrx200")) {
 		dev_err(dev, "this SoC has no GPHY\n");
 		return -EINVAL;
 	}
+
+	clk = clk_get_sys("1f203000.rcu", "gphy");
+	if (IS_ERR(clk))
+		return PTR_ERR(clk);
+
+	clk_enable(clk);
+
 	if (id > 1) {
 		dev_err(dev, "%u is an invalid gphy id\n", id);
 		return -EINVAL;
diff --git a/arch/mips/lantiq/xway/sysctrl.c b/arch/mips/lantiq/xway/sysctrl.c
index 3925e66..6e0e135 100644
--- a/arch/mips/lantiq/xway/sysctrl.c
+++ b/arch/mips/lantiq/xway/sysctrl.c
@@ -374,6 +374,7 @@ void __init ltq_soc_init(void)
 				PMU_SWITCH | PMU_PPE_DPLUS | PMU_PPE_DPLUM |
 				PMU_PPE_EMA | PMU_PPE_TC | PMU_PPE_SLL01 |
 				PMU_PPE_QSB | PMU_PPE_TOP);
+		clkdev_add_pmu("1f203000.rcu", "gphy", 0, PMU_GPHY);
 	} else if (of_machine_is_compatible("lantiq,ar9")) {
 		clkdev_add_static(ltq_ar9_cpu_hz(), ltq_ar9_fpi_hz(),
 				ltq_ar9_fpi_hz());
-- 
1.7.10.4

