From bfd78dda2ad5afb4434ebe99c05528614065bdb1 Mon Sep 17 00:00:00 2001
From: Florian Fainelli <florian@openwrt.org>
Date: Wed, 25 Jan 2012 17:39:56 +0100
Subject: [PATCH 06/63] MIPS: BCM63XX: define BCM6358 SPI base address

Signed-off-by: Florian Fainelli <florian@openwrt.org>
---
 arch/mips/include/asm/mach-bcm63xx/bcm63xx_cpu.h |    2 +-
 1 files changed, 1 insertions(+), 1 deletions(-)

--- a/arch/mips/include/asm/mach-bcm63xx/bcm63xx_cpu.h
+++ b/arch/mips/include/asm/mach-bcm63xx/bcm63xx_cpu.h
@@ -289,7 +289,7 @@ enum bcm63xx_regs_set {
 #define BCM_6358_UART0_BASE		(0xfffe0100)
 #define BCM_6358_UART1_BASE		(0xfffe0120)
 #define BCM_6358_GPIO_BASE		(0xfffe0080)
-#define BCM_6358_SPI_BASE		(0xdeadbeef)
+#define BCM_6358_SPI_BASE		(0xfffe0800)
 #define BCM_6358_SPI2_BASE		(0xfffe0800)
 #define BCM_6358_UDC0_BASE		(0xfffe0800)
 #define BCM_6358_OHCI0_BASE		(0xfffe1400)
