#!/bin/sh
#
# Copyright (C) 2010 OpenWrt.org
#

. /lib/ar71xx.sh

board=$(ar71xx_board_name)

wrt160nl_fixtrx() {
	mtd -o 32 fixtrx firmware
}

wrt160nl_setup_leds() {
	uci batch <<EOF
set system.wlan_led=led
set system.wlan_led.name='WLAN'
set system.wlan_led.sysfs='wrt160nl:blue:wlan'
set system.wlan_led.trigger='phy0tpt'
commit system
EOF
}

if [ "${board}" == "wrt160nl" ]; then
	wrt160nl_fixtrx
	wrt160nl_setup_leds
fi
