--- a/drivers/ssb/driver_pcicore.c
+++ b/drivers/ssb/driver_pcicore.c
@@ -476,30 +476,6 @@ static void ssb_pcie_mdio_write(struct s
 	pcicore_write32(pc, mdio_control, 0);
 }
 
-static void ssb_broadcast_value(struct ssb_device *dev,
-				u32 address, u32 data)
-{
-	/* This is used for both, PCI and ChipCommon core, so be careful. */
-	BUILD_BUG_ON(SSB_PCICORE_BCAST_ADDR != SSB_CHIPCO_BCAST_ADDR);
-	BUILD_BUG_ON(SSB_PCICORE_BCAST_DATA != SSB_CHIPCO_BCAST_DATA);
-
-	ssb_write32(dev, SSB_PCICORE_BCAST_ADDR, address);
-	ssb_read32(dev, SSB_PCICORE_BCAST_ADDR); /* flush */
-	ssb_write32(dev, SSB_PCICORE_BCAST_DATA, data);
-	ssb_read32(dev, SSB_PCICORE_BCAST_DATA); /* flush */
-}
-
-static void ssb_commit_settings(struct ssb_bus *bus)
-{
-	struct ssb_device *dev;
-
-	dev = bus->chipco.dev ? bus->chipco.dev : bus->pcicore.dev;
-	if (WARN_ON(!dev))
-		return;
-	/* This forces an update of the cached registers. */
-	ssb_broadcast_value(dev, 0xFD8, 0);
-}
-
 int ssb_pcicore_dev_irqvecs_enable(struct ssb_pcicore *pc,
 				   struct ssb_device *dev)
 {
--- a/drivers/ssb/main.c
+++ b/drivers/ssb/main.c
@@ -1330,6 +1330,31 @@ error:
 }
 EXPORT_SYMBOL(ssb_bus_powerup);
 
+static void ssb_broadcast_value(struct ssb_device *dev,
+				u32 address, u32 data)
+{
+	/* This is used for both, PCI and ChipCommon core, so be careful. */
+	BUILD_BUG_ON(SSB_PCICORE_BCAST_ADDR != SSB_CHIPCO_BCAST_ADDR);
+	BUILD_BUG_ON(SSB_PCICORE_BCAST_DATA != SSB_CHIPCO_BCAST_DATA);
+
+	ssb_write32(dev, SSB_PCICORE_BCAST_ADDR, address);
+	ssb_read32(dev, SSB_PCICORE_BCAST_ADDR); /* flush */
+	ssb_write32(dev, SSB_PCICORE_BCAST_DATA, data);
+	ssb_read32(dev, SSB_PCICORE_BCAST_DATA); /* flush */
+}
+
+void ssb_commit_settings(struct ssb_bus *bus)
+{
+	struct ssb_device *dev;
+
+	dev = bus->chipco.dev ? bus->chipco.dev : bus->pcicore.dev;
+	if (WARN_ON(!dev))
+		return;
+	/* This forces an update of the cached registers. */
+	ssb_broadcast_value(dev, 0xFD8, 0);
+}
+EXPORT_SYMBOL(ssb_commit_settings);
+
 u32 ssb_admatch_base(u32 adm)
 {
 	u32 base = 0;
--- a/include/linux/ssb/ssb.h
+++ b/include/linux/ssb/ssb.h
@@ -518,6 +518,7 @@ extern int ssb_bus_may_powerdown(struct 
  * Otherwise static always-on powercontrol will be used. */
 extern int ssb_bus_powerup(struct ssb_bus *bus, bool dynamic_pctl);
 
+extern void ssb_commit_settings(struct ssb_bus *bus);
 
 /* Various helper functions */
 extern u32 ssb_admatch_base(u32 adm);
