
--- /dev/null
+++ b/arch/mips/lantiq/xway/Kconfig
@@ -0,0 +1,19 @@
+if SOC_LANTIQ_XWAY
+
+menu "Mips Machine"
+
+config LANTIQ_MACH_EASY50812
+	bool "Easy50812"
+	default y
+
+config LANTIQ_MACH_EASY50712
+	bool "Easy50712"
+	default y
+
+config LANTIQ_MACH_EASY4010
+	bool "Easy4010"
+	default y
+
+endmenu
+
+endif
--- /dev/null
+++ b/arch/mips/lantiq/xway/gpio_ebu.c
@@ -0,0 +1,116 @@
+/*
+ *  This program is free software; you can redistribute it and/or modify it
+ *  under the terms of the GNU General Public License version 2 as published
+ *  by the Free Software Foundation.
+ *
+ *  Copyright (C) 2010 John Crispin <blogic@openwrt.org>
+ */
+
+#include <linux/init.h>
+#include <linux/module.h>
+#include <linux/types.h>
+#include <linux/platform_device.h>
+#include <linux/mutex.h>
+#include <linux/gpio.h>
+
+#include <xway.h>
+
+#define LQ_EBU_BUSCON	0x1e7ff
+#define LQ_EBU_WP		0x80000000
+
+static int shadow = 0x0000;
+static void __iomem *virt;
+
+static int
+lq_ebu_direction_output(struct gpio_chip *chip, unsigned offset, int value)
+{
+	return 0;
+}
+
+static void
+lq_ebu_apply(void)
+{
+	unsigned long flags;
+	spin_lock_irqsave(&ebu_lock, flags);
+	lq_w32(LQ_EBU_BUSCON, LQ_EBU_BUSCON1);
+	*((__u16*)virt) = shadow;
+	lq_w32(LQ_EBU_BUSCON | LQ_EBU_WP, LQ_EBU_BUSCON1);
+	spin_unlock_irqrestore(&ebu_lock, flags);
+}
+
+static void
+lq_ebu_set(struct gpio_chip *chip, unsigned offset, int value)
+{
+	if(value)
+		shadow |= (1 << offset);
+	else
+		shadow &= ~(1 << offset);
+	lq_ebu_apply();
+}
+
+static struct gpio_chip
+lq_ebu_chip =
+{
+	.label = "lq_ebu",
+	.direction_output = lq_ebu_direction_output,
+	.set = lq_ebu_set,
+	.base = 32,
+	.ngpio = 16,
+	.can_sleep = 0,
+	.owner = THIS_MODULE,
+};
+
+static int __devinit
+lq_ebu_probe(struct platform_device *pdev)
+{
+	struct resource *res = platform_get_resource(pdev, IORESOURCE_MEM, 0);
+	int ret = 0;
+	if (!res)
+		return -ENOENT;
+	res = request_mem_region(res->start, resource_size(res),
+		dev_name(&pdev->dev));
+	if (!res)
+		return -EBUSY;
+
+	/* tell the ebu controller which mem addr we will be using */
+	lq_w32(pdev->resource->start | 0x1, LQ_EBU_ADDRSEL1);
+	lq_w32(LQ_EBU_BUSCON | LQ_EBU_WP, LQ_EBU_BUSCON1);
+
+	virt = ioremap_nocache(res->start, resource_size(res));
+	if (!virt)
+	{
+		dev_err(&pdev->dev, "Failed to ioremap mem region\n");
+		ret = -ENOMEM;
+		goto err_release_mem_region;
+	}
+	/* grab the default settings passed form the platform code */
+	shadow = (unsigned int) pdev->dev.platform_data;
+
+	ret = gpiochip_add(&lq_ebu_chip);
+	if (!ret)
+	{
+		lq_ebu_apply();
+		return 0;
+	}
+
+err_release_mem_region:
+	release_mem_region(res->start, resource_size(res));
+	return ret;
+}
+
+static struct platform_driver
+lq_ebu_driver = {
+	.probe = lq_ebu_probe,
+	.driver = {
+		.name = "lq_ebu",
+		.owner = THIS_MODULE,
+	},
+};
+
+static int __init
+init_lq_ebu(void)
+{
+	return platform_driver_register(&lq_ebu_driver);
+}
+
+postcore_initcall(init_lq_ebu);
--- /dev/null
+++ b/arch/mips/lantiq/xway/gpio_leds.c
@@ -0,0 +1,161 @@
+/*
+ *  This program is free software; you can redistribute it and/or modify it
+ *  under the terms of the GNU General Public License version 2 as published
+ *  by the Free Software Foundation.
+ *
+ *  Copyright (C) 2007 John Crispin <blogic@openwrt.org>
+ *
+ */
+
+#include <linux/slab.h>
+#include <linux/init.h>
+#include <linux/module.h>
+#include <linux/types.h>
+#include <linux/platform_device.h>
+#include <linux/mutex.h>
+#include <linux/gpio.h>
+
+#include <xway.h>
+
+#define LQ_STP_BASE			0x1E100BB0
+#define LQ_STP_SIZE			0x40
+
+#define LQ_STP_CON0			0x00
+#define LQ_STP_CON1			0x04
+#define LQ_STP_CPU0			0x08
+#define LQ_STP_CPU1			0x0C
+#define LQ_STP_AR			0x10
+
+#define STP_CON0_SWU		(1 << 31)
+
+#define LQ_STP_2HZ			(0)
+#define LQ_STP_4HZ			(1 << 23)
+#define LQ_STP_8HZ			(2 << 23)
+#define LQ_STP_10HZ			(3 << 23)
+#define LQ_STP_MASK			(0xf << 23)
+
+#define LQ_STP_UPD_SRC_FPI	(1 << 31)
+#define LQ_STP_UPD_MASK		(3 << 30)
+#define LQ_STP_ADSL_SRC		(3 << 24)
+
+#define LQ_STP_GROUP0		(1 << 0)
+
+#define LQ_STP_RISING		0
+#define LQ_STP_FALLING		(1 << 26)
+#define LQ_STP_EDGE_MASK	(1 << 26)
+
+#define lq_stp_r32(reg)				__raw_readl(virt + reg)
+#define lq_stp_w32(val, reg)		__raw_writel(val, virt + reg)
+#define lq_stp_w32_mask(clear, set, reg) \
+        lq_w32((lq_r32(virt + reg) & ~clear) | set, virt + reg)
+
+static int shadow = 0xffff;
+static void __iomem *virt;
+
+static int
+lq_stp_direction_output(struct gpio_chip *chip, unsigned offset, int value)
+{
+	return 0;
+}
+
+static void
+lq_stp_set(struct gpio_chip *chip, unsigned offset, int value)
+{
+	if(value)
+		shadow |= (1 << offset);
+	else
+		shadow &= ~(1 << offset);
+	lq_stp_w32(shadow, LQ_STP_CPU0);
+}
+
+static struct gpio_chip lq_stp_chip =
+{
+	.label = "lq_stp",
+	.direction_output = lq_stp_direction_output,
+	.set = lq_stp_set,
+	.base = 48,
+	.ngpio = 24,
+	.can_sleep = 0,
+	.owner = THIS_MODULE,
+};
+
+static int
+lq_stp_hw_init(void)
+{
+	/* the 3 pins used to control the external stp */
+	lq_gpio_request(4, 1, 0, 1, "stp-st");
+	lq_gpio_request(5, 1, 0, 1, "stp-d");
+	lq_gpio_request(6, 1, 0, 1, "stp-sh");
+
+	/* sane defaults */
+	lq_stp_w32(0, LQ_STP_AR);
+	lq_stp_w32(0, LQ_STP_CPU0);
+	lq_stp_w32(0, LQ_STP_CPU1);
+	lq_stp_w32(STP_CON0_SWU, LQ_STP_CON0);
+	lq_stp_w32(0, LQ_STP_CON1);
+
+	/* rising or falling edge */
+	lq_stp_w32_mask(LQ_STP_EDGE_MASK, LQ_STP_FALLING, LQ_STP_CON0);
+
+	/* per default stp 15-0 are set */
+	lq_stp_w32_mask(0, LQ_STP_GROUP0, LQ_STP_CON1);
+
+	/* stp are update periodically by the FPID */
+	lq_stp_w32_mask(LQ_STP_UPD_MASK, LQ_STP_UPD_SRC_FPI, LQ_STP_CON1);
+
+	/* set stp update speed */
+	lq_stp_w32_mask(LQ_STP_MASK, LQ_STP_8HZ, LQ_STP_CON1);
+
+	/* adsl 0 and 1 stp are updated by the arc */
+	lq_stp_w32_mask(0, LQ_STP_ADSL_SRC, LQ_STP_CON0);
+
+	lq_pmu_enable(PMU_LED);
+	return 0;
+}
+
+static int
+lq_stp_probe(struct platform_device *pdev)
+{
+	struct resource *res = platform_get_resource(pdev, IORESOURCE_MEM, 0);
+	int ret = 0;
+	if (!res)
+		return -ENOENT;
+	res = request_mem_region(res->start, resource_size(res),
+		dev_name(&pdev->dev));
+	if (!res)
+		return -EBUSY;
+	virt = ioremap_nocache(res->start, resource_size(res));
+	if(!virt)
+	{
+		ret = -ENOMEM;
+		goto err_release_mem_region;
+	}
+	ret = gpiochip_add(&lq_stp_chip);
+	if(!ret)
+		return lq_stp_hw_init();
+
+	iounmap(virt);
+err_release_mem_region:
+	release_mem_region(res->start, resource_size(res));
+	return ret;
+}
+
+static struct platform_driver lq_stp_driver = {
+	.probe = lq_stp_probe,
+	.driver = {
+		.name = "lq_stp",
+		.owner = THIS_MODULE,
+	},
+};
+
+int __init
+init_lq_stp(void)
+{
+	int ret = platform_driver_register(&lq_stp_driver);
+	if (ret)
+		printk(KERN_INFO
+			"lq_stp: error registering platfom driver");
+	return ret;
+}
+
+postcore_initcall(init_lq_stp);
--- /dev/null
+++ b/arch/mips/lantiq/xway/mach-easy4010.c
@@ -0,0 +1,82 @@
+/*
+ *  This program is free software; you can redistribute it and/or modify it
+ *  under the terms of the GNU General Public License version 2 as published
+ *  by the Free Software Foundation.
+ *
+ *  Copyright (C) 2010 John Crispin <blogic@openwrt.org>
+ */
+
+#include <linux/init.h>
+#include <linux/platform_device.h>
+#include <linux/leds.h>
+#include <linux/gpio.h>
+#include <linux/gpio_buttons.h>
+#include <linux/mtd/mtd.h>
+#include <linux/mtd/partitions.h>
+#include <linux/mtd/physmap.h>
+#include <linux/input.h>
+
+#include <machine.h>
+
+#include <xway.h>
+#include <lantiq_platform.h>
+
+#include "devices.h"
+
+#ifdef CONFIG_MTD_PARTITIONS
+static struct mtd_partition easy4010_partitions[] =
+{
+	{
+		.name	= "uboot",
+		.offset	= 0x0,
+		.size	= 0x20000,
+	},
+	{
+		.name	= "uboot_env",
+		.offset	= 0x20000,
+		.size	= 0x10000,
+	},
+	{
+		.name	= "linux",
+		.offset	= 0x30000,
+		.size	= 0x3D0000,
+	},
+};
+#endif
+
+static struct physmap_flash_data easy4010_flash_data = {
+#ifdef CONFIG_MTD_PARTITIONS
+	.nr_parts	= ARRAY_SIZE(easy4010_partitions),
+	.parts		= easy4010_partitions,
+#endif
+};
+
+static struct lq_pci_data lq_pci_data = {
+	.clock      = PCI_CLOCK_INT,
+	.gpio   = PCI_GNT1 | PCI_REQ1,
+	.irq    = {
+		[14] = INT_NUM_IM0_IRL0 + 22,
+	},
+};
+
+static struct lq_eth_data lq_eth_data = {
+	.mii_mode = REV_MII_MODE,
+};
+
+static void __init
+easy4010_init(void)
+{
+	lq_register_gpio();
+	lq_register_gpio_stp();
+	lq_register_asc(0);
+	lq_register_asc(1);
+	lq_register_nor(&easy4010_flash_data);
+	lq_register_wdt();
+	lq_register_pci(&lq_pci_data);
+	lq_register_ethernet(&lq_eth_data);
+}
+
+MIPS_MACHINE(LANTIQ_MACH_EASY4010,
+			"EASY4010",
+			"EASY4010 Eval Board",
+			easy4010_init);
--- /dev/null
+++ b/arch/mips/lantiq/xway/mach-easy50712.c
@@ -0,0 +1,82 @@
+/*
+ *  This program is free software; you can redistribute it and/or modify it
+ *  under the terms of the GNU General Public License version 2 as published
+ *  by the Free Software Foundation.
+ *
+ *  Copyright (C) 2010 John Crispin <blogic@openwrt.org>
+ */
+
+#include <linux/init.h>
+#include <linux/platform_device.h>
+#include <linux/leds.h>
+#include <linux/gpio.h>
+#include <linux/gpio_buttons.h>
+#include <linux/mtd/mtd.h>
+#include <linux/mtd/partitions.h>
+#include <linux/mtd/physmap.h>
+#include <linux/input.h>
+
+#include <machine.h>
+
+#include <xway.h>
+#include <lantiq_platform.h>
+
+#include "devices.h"
+
+#ifdef CONFIG_MTD_PARTITIONS
+static struct mtd_partition easy50712_partitions[] =
+{
+	{
+		.name	= "uboot",
+		.offset	= 0x0,
+		.size	= 0x20000,
+	},
+	{
+		.name	= "uboot_env",
+		.offset	= 0x20000,
+		.size	= 0x10000,
+	},
+	{
+		.name	= "linux",
+		.offset	= 0x30000,
+		.size	= 0x3D0000,
+	},
+};
+#endif
+
+static struct physmap_flash_data easy50712_flash_data = {
+#ifdef CONFIG_MTD_PARTITIONS
+	.nr_parts	= ARRAY_SIZE(easy50712_partitions),
+	.parts		= easy50712_partitions,
+#endif
+};
+
+static struct lq_pci_data lq_pci_data = {
+	.clock      = PCI_CLOCK_INT,
+	.gpio   = PCI_GNT1 | PCI_REQ1,
+	.irq    = {
+		[14] = INT_NUM_IM0_IRL0 + 22,
+	},
+};
+
+static struct lq_eth_data lq_eth_data = {
+	.mii_mode = REV_MII_MODE,
+};
+
+static void __init
+easy50712_init(void)
+{
+	lq_register_asc(0);
+	lq_register_asc(1);
+	lq_register_gpio();
+	lq_register_gpio_stp();
+	lq_register_nor(&easy50712_flash_data);
+	lq_register_wdt();
+	lq_register_pci(&lq_pci_data);
+	lq_register_ethernet(&lq_eth_data);
+}
+
+MIPS_MACHINE(LANTIQ_MACH_EASY50712,
+			"EASY50712",
+			"EASY50712 Eval Board",
+			easy50712_init);
--- /dev/null
+++ b/arch/mips/lantiq/xway/mach-easy50812.c
@@ -0,0 +1,81 @@
+/*
+ *  This program is free software; you can redistribute it and/or modify it
+ *  under the terms of the GNU General Public License version 2 as published
+ *  by the Free Software Foundation.
+ *
+ *  Copyright (C) 2010 John Crispin <blogic@openwrt.org>
+ */
+
+#include <linux/init.h>
+#include <linux/platform_device.h>
+#include <linux/leds.h>
+#include <linux/gpio.h>
+#include <linux/gpio_buttons.h>
+#include <linux/mtd/mtd.h>
+#include <linux/mtd/partitions.h>
+#include <linux/mtd/physmap.h>
+#include <linux/input.h>
+
+#include <machine.h>
+
+#include <xway.h>
+#include <lantiq_platform.h>
+
+#include "devices.h"
+
+#ifdef CONFIG_MTD_PARTITIONS
+static struct mtd_partition easy50812_partitions[] =
+{
+	{
+		.name	= "uboot",
+		.offset	= 0x0,
+		.size	= 0x40000,
+	},
+	{
+		.name	= "uboot_env",
+		.offset	= 0x40000,
+		.size	= 0x10000,
+	},
+	{
+		.name	= "linux",
+		.offset	= 0x50000,
+		.size	= 0x3B0000,
+	},
+};
+#endif
+
+static struct physmap_flash_data easy50812_flash_data = {
+#ifdef CONFIG_MTD_PARTITIONS
+	.nr_parts	= ARRAY_SIZE(easy50812_partitions),
+	.parts		= easy50812_partitions,
+#endif
+};
+
+static struct lq_pci_data lq_pci_data = {
+	.clock      = PCI_CLOCK_INT,
+	.gpio   = PCI_GNT1 | PCI_REQ1,
+	.irq    = {
+		[14] = INT_NUM_IM0_IRL0 + 22,
+	},
+};
+
+static struct lq_eth_data lq_eth_data = {
+	.mii_mode = REV_MII_MODE,
+};
+
+static void __init
+easy50812_init(void)
+{
+	lq_register_gpio();
+	lq_register_asc(0);
+	lq_register_asc(1);
+	lq_register_nor(&easy50812_flash_data);
+	lq_register_wdt();
+	lq_register_pci(&lq_pci_data);
+	lq_register_ethernet(&lq_eth_data);
+}
+
+MIPS_MACHINE(LANTIQ_MACH_EASY50812,
+			"EASY50812",
+			"EASY50812 Eval Board",
+			easy50812_init);
--- /dev/null
+++ b/arch/mips/lantiq/xway/prom.c
@@ -0,0 +1,52 @@
+/*
+ *  This program is free software; you can redistribute it and/or modify it
+ *  under the terms of the GNU General Public License version 2 as published
+ *  by the Free Software Foundation.
+ *
+ *  Copyright (C) 2010 John Crispin <blogic@openwrt.org>
+ */
+
+#include <linux/module.h>
+#include <linux/clk.h>
+#include <asm/bootinfo.h>
+#include <asm/time.h>
+
+#include <xway.h>
+
+#include "../prom.h"
+
+#define SOC_DANUBE		"Danube"
+#define SOC_TWINPASS	"Twinpass"
+#define SOC_AR9			"AR9"
+
+void __init
+lq_soc_detect(struct lq_soc_info *i)
+{
+	i->partnum = (lq_r32(LQ_MPS_CHIPID) & 0x0FFFFFFF) >> 12;
+	i->rev = (lq_r32(LQ_MPS_CHIPID) & 0xF0000000) >> 28;
+	switch (i->partnum)
+	{
+	case SOC_ID_DANUBE1:
+	case SOC_ID_DANUBE2:
+		i->name = SOC_DANUBE;
+		i->type = SOC_TYPE_DANUBE;
+		break;
+
+	case SOC_ID_TWINPASS:
+		i->name = SOC_TWINPASS;
+		i->type = SOC_TYPE_DANUBE;
+		break;
+
+	case SOC_ID_ARX188:
+	case SOC_ID_ARX168:
+	case SOC_ID_ARX182:
+		i->name = SOC_AR9;
+		i->type = SOC_TYPE_AR9;
+		break;
+
+	default:
+		printk(KERN_ERR "unknown chiprev : 0x%08X\n", i->partnum);
+		while(1) {	};
+		break;
+	}
+}
--- /dev/null
+++ b/arch/mips/lantiq/xway/devices.c
@@ -0,0 +1,336 @@
+/*
+ *  This program is free software; you can redistribute it and/or modify it
+ *  under the terms of the GNU General Public License version 2 as published
+ *  by the Free Software Foundation.
+ *
+ *  Copyright (C) 2010 John Crispin <blogic@openwrt.org>
+ */
+
+#include <linux/init.h>
+#include <linux/module.h>
+#include <linux/types.h>
+#include <linux/string.h>
+#include <linux/mtd/physmap.h>
+#include <linux/kernel.h>
+#include <linux/reboot.h>
+#include <linux/platform_device.h>
+#include <linux/leds.h>
+#include <linux/etherdevice.h>
+#include <linux/reboot.h>
+#include <linux/time.h>
+#include <linux/io.h>
+#include <linux/gpio.h>
+#include <linux/gpio_buttons.h>
+#include <linux/leds.h>
+
+#include <asm/bootinfo.h>
+#include <asm/irq.h>
+
+#include <xway.h>
+#include <xway_irq.h>
+#include <lantiq_platform.h>
+
+#define IRQ_RES(resname,irq) {.name=#resname,.start=(irq),.flags=IORESOURCE_IRQ}
+
+/* gpio leds */
+static struct gpio_led_platform_data lq_gpio_led_data;
+
+static struct platform_device lq_gpio_leds =
+{
+	.name = "leds-gpio",
+	.dev = {
+		.platform_data = (void *) &lq_gpio_led_data,
+	}
+};
+
+void __init
+lq_register_gpio_leds(struct gpio_led *leds, int cnt)
+{
+	lq_gpio_led_data.leds = leds;
+	lq_gpio_led_data.num_leds = cnt;
+	platform_device_register(&lq_gpio_leds);
+}
+
+/* gpio buttons */
+static struct gpio_buttons_platform_data lq_gpio_buttons_platform_data;
+
+static struct platform_device lq_gpio_buttons_platform_device =
+{
+	.name = "gpio-buttons",
+	.id = 0,
+	.dev = {
+		.platform_data = (void *) &lq_gpio_buttons_platform_data,
+	},
+};
+
+void __init
+lq_register_gpio_buttons(struct gpio_button *buttons, int cnt)
+{
+	lq_gpio_buttons_platform_data.buttons = buttons;
+	lq_gpio_buttons_platform_data.nbuttons = cnt;
+	platform_device_register(&lq_gpio_buttons_platform_device);
+}
+
+/* serial to parallel conversion */
+static struct resource lq_stp_resource =
+{
+	.name	= "stp",
+	.start	= LQ_STP_BASE,
+	.end	= LQ_STP_BASE + LQ_STP_SIZE - 1,
+	.flags	= IORESOURCE_MEM,
+};
+
+void __init
+lq_register_gpio_stp(void)
+{
+	platform_device_register_simple("lq_stp", 0, &lq_stp_resource, 1);
+}
+
+/* nor flash */
+static struct resource lq_nor_resource =
+{
+	.name	= "nor",
+	.start	= LQ_FLASH_START,
+	.end	= LQ_FLASH_START + LQ_FLASH_MAX - 1,
+	.flags  = IORESOURCE_MEM,
+};
+
+static struct platform_device lq_nor =
+{
+	.name			= "lq_nor",
+	.resource		= &lq_nor_resource,
+	.num_resources	= 1,
+};
+
+void __init
+lq_register_nor(struct physmap_flash_data *data)
+{
+	lq_nor.dev.platform_data = data;
+	platform_device_register(&lq_nor);
+}
+
+/* watchdog */
+static struct resource lq_wdt_resource =
+{
+	.name	= "watchdog",
+	.start  = LQ_WDT_BASE,
+	.end    = LQ_WDT_BASE + LQ_WDT_SIZE - 1,
+	.flags  = IORESOURCE_MEM,
+};
+
+void __init
+lq_register_wdt(void)
+{
+	platform_device_register_simple("lq_wdt", 0, &lq_wdt_resource, 1);
+}
+
+/* gpio */
+static struct resource lq_gpio_resource[] = {
+	{
+		.name	= "gpio0",
+		.start  = LQ_GPIO0_BASE_ADDR,
+		.end    = LQ_GPIO0_BASE_ADDR + LQ_GPIO_SIZE - 1,
+		.flags  = IORESOURCE_MEM,
+	}, {
+		.name	= "gpio1",
+		.start  = LQ_GPIO1_BASE_ADDR,
+		.end    = LQ_GPIO1_BASE_ADDR + LQ_GPIO_SIZE - 1,
+		.flags  = IORESOURCE_MEM,
+	}
+};
+
+void __init
+lq_register_gpio(void)
+{
+	platform_device_register_simple("lq_gpio", 0, &lq_gpio_resource[0], 1);
+	platform_device_register_simple("lq_gpio", 1, &lq_gpio_resource[1], 1);
+}
+
+/* pci */
+static struct platform_device lq_pci =
+{
+	.name			= "lq_pci",
+	.num_resources	= 0,
+};
+
+void __init
+lq_register_pci(struct lq_pci_data *data)
+{
+	lq_pci.dev.platform_data = data;
+	platform_device_register(&lq_pci);
+}
+
+/* ebu */
+static struct resource lq_ebu_resource =
+{
+	.name	= "gpio_ebu",
+	.start	= LQ_EBU_GPIO_START,
+	.end	= LQ_EBU_GPIO_START + LQ_EBU_GPIO_SIZE - 1,
+	.flags	= IORESOURCE_MEM,
+};
+
+static struct platform_device lq_ebu =
+{
+	.name		= "lq_ebu",
+	.resource	= &lq_ebu_resource,
+	.num_resources	= 1,
+};
+
+void __init
+lq_register_gpio_ebu(unsigned int value)
+{
+	lq_ebu.dev.platform_data = (void*) value;
+	platform_device_register(&lq_ebu);
+}
+
+/* ethernet */
+unsigned char lq_ethaddr[6] = {0xff, 0xff, 0xff, 0xff, 0xff, 0xff};
+
+static int __init
+lq_set_ethaddr(char *str)
+{
+	sscanf(&str[8], "0%02hhx:0%02hhx:0%02hhx:0%02hhx:0%02hhx:0%02hhx",
+		&lq_ethaddr[0], &lq_ethaddr[1], &lq_ethaddr[2],
+		&lq_ethaddr[3], &lq_ethaddr[4], &lq_ethaddr[5]);
+	return 0;
+}
+__setup("ethaddr=", lq_set_ethaddr);
+
+static struct resource lq_ethernet_resources =
+{
+	.name	= "etop",
+	.start  = LQ_PPE32_BASE_ADDR,
+	.end    = LQ_PPE32_BASE_ADDR + LQ_PPE32_SIZE - 1,
+	.flags  = IORESOURCE_MEM,
+};
+
+static struct platform_device lq_ethernet =
+{
+	.name			= "lq_etop",
+	.resource		= &lq_ethernet_resources,
+	.num_resources	= 1,
+};
+
+void __init
+lq_register_ethernet(struct lq_eth_data *eth)
+{
+	if(!eth)
+		return;
+	if(!eth->mac)
+		eth->mac = lq_ethaddr;
+	if(!is_valid_ether_addr(eth->mac))
+		random_ether_addr(eth->mac);
+	lq_ethernet.dev.platform_data = eth;
+	platform_device_register(&lq_ethernet);
+}
+
+/* tapi */
+static struct resource mps_resources[] = {
+	{
+		.name = "voice-mem",
+		.flags = IORESOURCE_MEM,
+		.start = 0x1f107000,
+		.end =   0x1f1073ff,
+	},
+	{
+		.name = "voice-mailbox",
+		.flags = IORESOURCE_MEM,
+		.start = 0x1f200000,
+		.end =   0x1f2007ff,
+	},
+};
+
+static struct platform_device mps_device = {
+	.name = "mps",
+	.resource = mps_resources,
+	.num_resources = ARRAY_SIZE(mps_resources),
+};
+
+static struct platform_device vmmc_device = {
+	.name = "vmmc",
+	.dev = {
+		.parent = &mps_device.dev,
+	},
+};
+
+static unsigned int *cp1_base;
+unsigned int*
+lq_get_cp1_base(void)
+{
+	return cp1_base;
+}
+EXPORT_SYMBOL(lq_get_cp1_base);
+
+void __init
+lq_register_tapi(void)
+{
+#define CP1_SIZE	(1 << 20)
+	dma_addr_t dma;
+	mps_device.dev.platform_data =
+	cp1_base =
+		(void*)CPHYSADDR(dma_alloc_coherent(NULL, CP1_SIZE, &dma, GFP_ATOMIC));
+	mps_device.dev.platform_data = cp1_base;
+	platform_device_register(&mps_device);
+	platform_device_register(&vmmc_device);
+}
+
+/* asc ports */
+static struct resource lq_asc0_resources[] =
+{
+	{
+		.start  = LQ_ASC0_BASE,
+		.end    = LQ_ASC0_BASE + LQ_ASC_SIZE - 1,
+		.flags  = IORESOURCE_MEM,
+	},
+	IRQ_RES(tx, INT_NUM_IM3_IRL0),
+	IRQ_RES(rx, INT_NUM_IM3_IRL0 + 1),
+	IRQ_RES(err, INT_NUM_IM3_IRL0 + 2),
+};
+
+static struct resource lq_asc1_resources[] =
+{
+	{
+		.start  = LQ_ASC1_BASE,
+		.end    = LQ_ASC1_BASE + LQ_ASC_SIZE - 1,
+		.flags  = IORESOURCE_MEM,
+	},
+	IRQ_RES(tx, INT_NUM_IM3_IRL0 + 8),
+	IRQ_RES(rx, INT_NUM_IM3_IRL0 + 9),
+	IRQ_RES(err, INT_NUM_IM3_IRL0 + 10),
+};
+
+void __init
+lq_register_asc(int port)
+{
+	switch (port) {
+	case 0:
+		platform_device_register_simple("lq_asc", 0,
+			lq_asc0_resources, ARRAY_SIZE(lq_asc0_resources));
+		break;
+	case 1:
+		platform_device_register_simple("lq_asc", 1,
+			lq_asc1_resources, ARRAY_SIZE(lq_asc1_resources));
+		break;
+	default:
+		break;
+	}
+}
+
+void __init
+lq_register_crypto(const char *name)
+{
+	platform_device_register_simple(name, 0, 0, 0);
+}
+
+/* madwifi */
+int lantiq_emulate_madwifi_eep = 0;
+EXPORT_SYMBOL(lantiq_emulate_madwifi_eep);
+
+void __init
+lq_register_madwifi_eep(void)
+{
+	lantiq_emulate_madwifi_eep = 1;
+}
+
+
+
--- /dev/null
+++ b/arch/mips/lantiq/xway/devices.h
@@ -0,0 +1,28 @@
+/*
+ *  This program is free software; you can redistribute it and/or modify it
+ *  under the terms of the GNU General Public License version 2 as published
+ *  by the Free Software Foundation.
+ *
+ *  Copyright (C) 2010 John Crispin <blogic@openwrt.org>
+ */
+
+#ifndef _LQ_DEVICES_H__
+#define _LQ_DEVICES_H__
+
+#include <lantiq_platform.h>
+#include <xway_irq.h>
+
+extern void __init lq_register_gpio(void);
+extern void __init lq_register_gpio_stp(void);
+extern void __init lq_register_gpio_ebu(unsigned int value);
+extern void __init lq_register_gpio_leds(struct gpio_led *leds, int cnt);
+extern void __init lq_register_pci(struct lq_pci_data *data);
+extern void __init lq_register_nor(struct physmap_flash_data *data);
+extern void __init lq_register_tapi(void);
+extern void __init lq_register_madwifi_eep(void);
+extern void __init lq_register_wdt(void);
+extern void __init lq_register_ethernet(struct lq_eth_data *eth);
+extern void __init lq_register_asc(int port);
+extern void __init lq_register_gpio_buttons(struct gpio_button *buttons, int cnt);
+
+#endif
--- /dev/null
+++ b/arch/mips/lantiq/xway/dma.c
@@ -0,0 +1,701 @@
+#include <linux/module.h>
+#include <linux/init.h>
+#include <linux/sched.h>
+#include <linux/kernel.h>
+#include <linux/slab.h>
+#include <linux/string.h>
+#include <linux/timer.h>
+#include <linux/fs.h>
+#include <linux/errno.h>
+#include <linux/stat.h>
+#include <linux/mm.h>
+#include <linux/tty.h>
+#include <linux/selection.h>
+#include <linux/kmod.h>
+#include <linux/vmalloc.h>
+#include <linux/interrupt.h>
+#include <linux/delay.h>
+#include <linux/uaccess.h>
+#include <linux/errno.h>
+#include <linux/io.h>
+
+#include <xway.h>
+#include <xway_irq.h>
+#include <xway_dma.h>
+
+#define LQ_DMA_CS			((u32 *)(LQ_DMA_BASE_ADDR + 0x18))
+#define LQ_DMA_CIE			((u32 *)(LQ_DMA_BASE_ADDR + 0x2C))
+#define LQ_DMA_IRNEN		((u32 *)(LQ_DMA_BASE_ADDR + 0xf4))
+#define LQ_DMA_CCTRL		((u32 *)(LQ_DMA_BASE_ADDR + 0x1C))
+#define LQ_DMA_CIS			((u32 *)(LQ_DMA_BASE_ADDR + 0x28))
+#define LQ_DMA_CDLEN		((u32 *)(LQ_DMA_BASE_ADDR + 0x24))
+#define LQ_DMA_PS			((u32 *)(LQ_DMA_BASE_ADDR + 0x40))
+#define LQ_DMA_PCTRL		((u32 *)(LQ_DMA_BASE_ADDR + 0x44))
+#define LQ_DMA_CTRL		((u32 *)(LQ_DMA_BASE_ADDR + 0x10))
+#define LQ_DMA_CPOLL		((u32 *)(LQ_DMA_BASE_ADDR + 0x14))
+#define LQ_DMA_CDBA		((u32 *)(LQ_DMA_BASE_ADDR + 0x20))
+
+/*25 descriptors for each dma channel,4096/8/20=25.xx*/
+#define LQ_DMA_DESCRIPTOR_OFFSET 25
+
+#define MAX_DMA_DEVICE_NUM  6	/*max ports connecting to dma */
+#define MAX_DMA_CHANNEL_NUM 20	/*max dma channels */
+#define DMA_INT_BUDGET      100	/*budget for interrupt handling */
+#define DMA_POLL_COUNTER    4	/*fix me, set the correct counter value here! */
+
+extern void lq_mask_and_ack_irq(unsigned int irq_nr);
+extern void lq_enable_irq(unsigned int irq_nr);
+extern void lq_disable_irq(unsigned int irq_nr);
+
+u64 *g_desc_list;
+struct dma_device_info dma_devs[MAX_DMA_DEVICE_NUM];
+struct dma_channel_info dma_chan[MAX_DMA_CHANNEL_NUM];
+
+static const char *global_device_name[MAX_DMA_DEVICE_NUM] =
+	{ "PPE", "DEU", "SPI", "SDIO", "MCTRL0", "MCTRL1" };
+
+struct dma_chan_map default_dma_map[MAX_DMA_CHANNEL_NUM] = {
+	{"PPE", LQ_DMA_RX, 0, LQ_DMA_CH0_INT, 0},
+	{"PPE", LQ_DMA_TX, 0, LQ_DMA_CH1_INT, 0},
+	{"PPE", LQ_DMA_RX, 1, LQ_DMA_CH2_INT, 1},
+	{"PPE", LQ_DMA_TX, 1, LQ_DMA_CH3_INT, 1},
+	{"PPE", LQ_DMA_RX, 2, LQ_DMA_CH4_INT, 2},
+	{"PPE", LQ_DMA_TX, 2, LQ_DMA_CH5_INT, 2},
+	{"PPE", LQ_DMA_RX, 3, LQ_DMA_CH6_INT, 3},
+	{"PPE", LQ_DMA_TX, 3, LQ_DMA_CH7_INT, 3},
+	{"DEU", LQ_DMA_RX, 0, LQ_DMA_CH8_INT, 0},
+	{"DEU", LQ_DMA_TX, 0, LQ_DMA_CH9_INT, 0},
+	{"DEU", LQ_DMA_RX, 1, LQ_DMA_CH10_INT, 1},
+	{"DEU", LQ_DMA_TX, 1, LQ_DMA_CH11_INT, 1},
+	{"SPI", LQ_DMA_RX, 0, LQ_DMA_CH12_INT, 0},
+	{"SPI", LQ_DMA_TX, 0, LQ_DMA_CH13_INT, 0},
+	{"SDIO", LQ_DMA_RX, 0, LQ_DMA_CH14_INT, 0},
+	{"SDIO", LQ_DMA_TX, 0, LQ_DMA_CH15_INT, 0},
+	{"MCTRL0", LQ_DMA_RX, 0, LQ_DMA_CH16_INT, 0},
+	{"MCTRL0", LQ_DMA_TX, 0, LQ_DMA_CH17_INT, 0},
+	{"MCTRL1", LQ_DMA_RX, 1, LQ_DMA_CH18_INT, 1},
+	{"MCTRL1", LQ_DMA_TX, 1, LQ_DMA_CH19_INT, 1}
+};
+
+struct dma_chan_map *chan_map = default_dma_map;
+volatile u32 g_lq_dma_int_status;
+volatile int g_lq_dma_in_process; /* 0=not in process, 1=in process */
+
+void do_dma_tasklet(unsigned long);
+DECLARE_TASKLET(dma_tasklet, do_dma_tasklet, 0);
+
+u8 *common_buffer_alloc(int len, int *byte_offset, void **opt)
+{
+	u8 *buffer = kmalloc(len * sizeof(u8), GFP_KERNEL);
+
+	*byte_offset = 0;
+
+	return buffer;
+}
+
+void common_buffer_free(u8 *dataptr, void *opt)
+{
+	kfree(dataptr);
+}
+
+void enable_ch_irq(struct dma_channel_info *pCh)
+{
+	int chan_no = (int)(pCh - dma_chan);
+	unsigned long flag;
+
+	local_irq_save(flag);
+	lq_w32(chan_no, LQ_DMA_CS);
+	lq_w32(0x4a, LQ_DMA_CIE);
+	lq_w32(lq_r32(LQ_DMA_IRNEN) | (1 << chan_no), LQ_DMA_IRNEN);
+	local_irq_restore(flag);
+	lq_enable_irq(pCh->irq);
+}
+
+void disable_ch_irq(struct dma_channel_info *pCh)
+{
+	unsigned long flag;
+	int chan_no = (int) (pCh - dma_chan);
+
+	local_irq_save(flag);
+	g_lq_dma_int_status &= ~(1 << chan_no);
+	lq_w32(chan_no, LQ_DMA_CS);
+	lq_w32(0, LQ_DMA_CIE);
+	lq_w32(lq_r32(LQ_DMA_IRNEN) & ~(1 << chan_no), LQ_DMA_IRNEN);
+	local_irq_restore(flag);
+	lq_mask_and_ack_irq(pCh->irq);
+}
+
+void open_chan(struct dma_channel_info *pCh)
+{
+	unsigned long flag;
+	int chan_no = (int)(pCh - dma_chan);
+
+	local_irq_save(flag);
+	lq_w32(chan_no, LQ_DMA_CS);
+	lq_w32(lq_r32(LQ_DMA_CCTRL) | 1, LQ_DMA_CCTRL);
+	if (pCh->dir == LQ_DMA_RX)
+		enable_ch_irq(pCh);
+	local_irq_restore(flag);
+}
+
+void close_chan(struct dma_channel_info *pCh)
+{
+	unsigned long flag;
+	int chan_no = (int) (pCh - dma_chan);
+
+	local_irq_save(flag);
+	lq_w32(chan_no, LQ_DMA_CS);
+	lq_w32(lq_r32(LQ_DMA_CCTRL) & ~1, LQ_DMA_CCTRL);
+	disable_ch_irq(pCh);
+	local_irq_restore(flag);
+}
+
+void reset_chan(struct dma_channel_info *pCh)
+{
+	int chan_no = (int) (pCh - dma_chan);
+
+	lq_w32(chan_no, LQ_DMA_CS);
+	lq_w32(lq_r32(LQ_DMA_CCTRL) | 2, LQ_DMA_CCTRL);
+}
+
+void rx_chan_intr_handler(int chan_no)
+{
+	struct dma_device_info *pDev = (struct dma_device_info *)dma_chan[chan_no].dma_dev;
+	struct dma_channel_info *pCh = &dma_chan[chan_no];
+	struct rx_desc *rx_desc_p;
+	int tmp;
+	unsigned long flag;
+
+	/*handle command complete interrupt */
+	rx_desc_p = (struct rx_desc *)pCh->desc_base + pCh->curr_desc;
+	if (rx_desc_p->status.field.OWN == CPU_OWN
+	    && rx_desc_p->status.field.C
+	    && rx_desc_p->status.field.data_length < 1536){
+		/* Every thing is correct, then we inform the upper layer */
+		pDev->current_rx_chan = pCh->rel_chan_no;
+		if (pDev->intr_handler)
+			pDev->intr_handler(pDev, RCV_INT);
+		pCh->weight--;
+	} else {
+		local_irq_save(flag);
+		tmp = lq_r32(LQ_DMA_CS);
+		lq_w32(chan_no, LQ_DMA_CS);
+		lq_w32(lq_r32(LQ_DMA_CIS) | 0x7e, LQ_DMA_CIS);
+		lq_w32(tmp, LQ_DMA_CS);
+		g_lq_dma_int_status &= ~(1 << chan_no);
+		local_irq_restore(flag);
+		lq_enable_irq(dma_chan[chan_no].irq);
+	}
+}
+
+inline void tx_chan_intr_handler(int chan_no)
+{
+	struct dma_device_info *pDev = (struct dma_device_info *)dma_chan[chan_no].dma_dev;
+	struct dma_channel_info *pCh = &dma_chan[chan_no];
+	int tmp;
+	unsigned long flag;
+
+	local_irq_save(flag);
+	tmp = lq_r32(LQ_DMA_CS);
+	lq_w32(chan_no, LQ_DMA_CS);
+	lq_w32(lq_r32(LQ_DMA_CIS) | 0x7e, LQ_DMA_CIS);
+	lq_w32(tmp, LQ_DMA_CS);
+	g_lq_dma_int_status &= ~(1 << chan_no);
+	local_irq_restore(flag);
+	pDev->current_tx_chan = pCh->rel_chan_no;
+	if (pDev->intr_handler)
+		pDev->intr_handler(pDev, TRANSMIT_CPT_INT);
+}
+
+void do_dma_tasklet(unsigned long unused)
+{
+	int i;
+	int chan_no = 0;
+	int budget = DMA_INT_BUDGET;
+	int weight = 0;
+	unsigned long flag;
+
+	while (g_lq_dma_int_status) {
+		if (budget-- < 0) {
+			tasklet_schedule(&dma_tasklet);
+			return;
+		}
+		chan_no = -1;
+		weight = 0;
+		for (i = 0; i < MAX_DMA_CHANNEL_NUM; i++) {
+			if ((g_lq_dma_int_status & (1 << i)) && dma_chan[i].weight > 0) {
+				if (dma_chan[i].weight > weight) {
+					chan_no = i;
+					weight = dma_chan[chan_no].weight;
+				}
+			}
+		}
+
+		if (chan_no >= 0) {
+			if (chan_map[chan_no].dir == LQ_DMA_RX)
+				rx_chan_intr_handler(chan_no);
+			else
+				tx_chan_intr_handler(chan_no);
+		} else {
+			for (i = 0; i < MAX_DMA_CHANNEL_NUM; i++)
+				dma_chan[i].weight = dma_chan[i].default_weight;
+		}
+	}
+
+	local_irq_save(flag);
+	g_lq_dma_in_process = 0;
+	if (g_lq_dma_int_status) {
+		g_lq_dma_in_process = 1;
+		tasklet_schedule(&dma_tasklet);
+	}
+	local_irq_restore(flag);
+}
+
+irqreturn_t dma_interrupt(int irq, void *dev_id)
+{
+	struct dma_channel_info *pCh;
+	int chan_no = 0;
+	int tmp;
+
+	pCh = (struct dma_channel_info *)dev_id;
+	chan_no = (int)(pCh - dma_chan);
+	if (chan_no < 0 || chan_no > 19)
+		BUG();
+
+	tmp = lq_r32(LQ_DMA_IRNEN);
+	lq_w32(0, LQ_DMA_IRNEN);
+	g_lq_dma_int_status |= 1 << chan_no;
+	lq_w32(tmp, LQ_DMA_IRNEN);
+	lq_mask_and_ack_irq(irq);
+
+	if (!g_lq_dma_in_process) {
+		g_lq_dma_in_process = 1;
+		tasklet_schedule(&dma_tasklet);
+	}
+
+	return IRQ_HANDLED;
+}
+
+struct dma_device_info *dma_device_reserve(char *dev_name)
+{
+	int i;
+
+	for (i = 0; i < MAX_DMA_DEVICE_NUM; i++) {
+		if (strcmp(dev_name, dma_devs[i].device_name) == 0) {
+			if (dma_devs[i].reserved)
+				return NULL;
+			dma_devs[i].reserved = 1;
+			break;
+		}
+	}
+
+	return &dma_devs[i];
+}
+EXPORT_SYMBOL(dma_device_reserve);
+
+void dma_device_release(struct dma_device_info *dev)
+{
+	dev->reserved = 0;
+}
+EXPORT_SYMBOL(dma_device_release);
+
+void dma_device_register(struct dma_device_info *dev)
+{
+	int i, j;
+	int chan_no = 0;
+	u8 *buffer;
+	int byte_offset;
+	unsigned long flag;
+	struct dma_device_info *pDev;
+	struct dma_channel_info *pCh;
+	struct rx_desc *rx_desc_p;
+	struct tx_desc *tx_desc_p;
+
+	for (i = 0; i < dev->max_tx_chan_num; i++) {
+		pCh = dev->tx_chan[i];
+		if (pCh->control == LQ_DMA_CH_ON) {
+			chan_no = (int)(pCh - dma_chan);
+			for (j = 0; j < pCh->desc_len; j++) {
+				tx_desc_p = (struct tx_desc *)pCh->desc_base + j;
+				memset(tx_desc_p, 0, sizeof(struct tx_desc));
+			}
+			local_irq_save(flag);
+			lq_w32(chan_no, LQ_DMA_CS);
+			/* check if the descriptor length is changed */
+			if (lq_r32(LQ_DMA_CDLEN) != pCh->desc_len)
+				lq_w32(pCh->desc_len, LQ_DMA_CDLEN);
+
+			lq_w32(lq_r32(LQ_DMA_CCTRL) & ~1, LQ_DMA_CCTRL);
+			lq_w32(lq_r32(LQ_DMA_CCTRL) | 2, LQ_DMA_CCTRL);
+			while (lq_r32(LQ_DMA_CCTRL) & 2)
+				;
+			lq_w32(lq_r32(LQ_DMA_IRNEN) | (1 << chan_no), LQ_DMA_IRNEN);
+			lq_w32(0x30100, LQ_DMA_CCTRL); /* reset and enable channel,enable channel later */
+			local_irq_restore(flag);
+		}
+	}
+
+	for (i = 0; i < dev->max_rx_chan_num; i++) {
+		pCh = dev->rx_chan[i];
+		if (pCh->control == LQ_DMA_CH_ON) {
+			chan_no = (int)(pCh - dma_chan);
+
+			for (j = 0; j < pCh->desc_len; j++) {
+				rx_desc_p = (struct rx_desc *)pCh->desc_base + j;
+				pDev = (struct dma_device_info *)(pCh->dma_dev);
+				buffer = pDev->buffer_alloc(pCh->packet_size, &byte_offset, (void *)&(pCh->opt[j]));
+				if (!buffer)
+					break;
+
+				dma_cache_inv((unsigned long) buffer, pCh->packet_size);
+
+				rx_desc_p->Data_Pointer = (u32)CPHYSADDR((u32)buffer);
+				rx_desc_p->status.word = 0;
+				rx_desc_p->status.field.byte_offset = byte_offset;
+				rx_desc_p->status.field.OWN = DMA_OWN;
+				rx_desc_p->status.field.data_length = pCh->packet_size;
+			}
+
+			local_irq_save(flag);
+			lq_w32(chan_no, LQ_DMA_CS);
+			/* check if the descriptor length is changed */
+			if (lq_r32(LQ_DMA_CDLEN) != pCh->desc_len)
+				lq_w32(pCh->desc_len, LQ_DMA_CDLEN);
+			lq_w32(lq_r32(LQ_DMA_CCTRL) & ~1, LQ_DMA_CCTRL);
+			lq_w32(lq_r32(LQ_DMA_CCTRL) | 2, LQ_DMA_CCTRL);
+			while (lq_r32(LQ_DMA_CCTRL) & 2)
+				;
+			lq_w32(0x0a, LQ_DMA_CIE); /* fix me, should enable all the interrupts here? */
+			lq_w32(lq_r32(LQ_DMA_IRNEN) | (1 << chan_no), LQ_DMA_IRNEN);
+			lq_w32(0x30000, LQ_DMA_CCTRL);
+			local_irq_restore(flag);
+			lq_enable_irq(dma_chan[chan_no].irq);
+		}
+	}
+}
+EXPORT_SYMBOL(dma_device_register);
+
+void dma_device_unregister(struct dma_device_info *dev)
+{
+	int i, j;
+	int chan_no;
+	struct dma_channel_info *pCh;
+	struct rx_desc *rx_desc_p;
+	struct tx_desc *tx_desc_p;
+	unsigned long flag;
+
+	for (i = 0; i < dev->max_tx_chan_num; i++) {
+		pCh = dev->tx_chan[i];
+		if (pCh->control == LQ_DMA_CH_ON) {
+			chan_no = (int)(dev->tx_chan[i] - dma_chan);
+			local_irq_save(flag);
+			lq_w32(chan_no, LQ_DMA_CS);
+			pCh->curr_desc = 0;
+			pCh->prev_desc = 0;
+			pCh->control = LQ_DMA_CH_OFF;
+			lq_w32(0, LQ_DMA_CIE); /* fix me, should disable all the interrupts here? */
+			lq_w32(lq_r32(LQ_DMA_IRNEN) & ~(1 << chan_no), LQ_DMA_IRNEN); /* disable interrupts */
+			lq_w32(lq_r32(LQ_DMA_CCTRL) & ~1, LQ_DMA_CCTRL);
+			while (lq_r32(LQ_DMA_CCTRL) & 1)
+				;
+			local_irq_restore(flag);
+
+			for (j = 0; j < pCh->desc_len; j++) {
+				tx_desc_p = (struct tx_desc *)pCh->desc_base + j;
+				if ((tx_desc_p->status.field.OWN == CPU_OWN && tx_desc_p->status.field.C)
+						|| (tx_desc_p->status.field.OWN == DMA_OWN && tx_desc_p->status.field.data_length > 0)) {
+					dev->buffer_free((u8 *) __va(tx_desc_p->Data_Pointer), (void *)pCh->opt[j]);
+				}
+				tx_desc_p->status.field.OWN = CPU_OWN;
+				memset(tx_desc_p, 0, sizeof(struct tx_desc));
+			}
+			/* TODO should free buffer that is not transferred by dma */
+		}
+	}
+
+	for (i = 0; i < dev->max_rx_chan_num; i++) {
+		pCh = dev->rx_chan[i];
+		chan_no = (int)(dev->rx_chan[i] - dma_chan);
+		lq_disable_irq(pCh->irq);
+
+		local_irq_save(flag);
+		g_lq_dma_int_status &= ~(1 << chan_no);
+		pCh->curr_desc = 0;
+		pCh->prev_desc = 0;
+		pCh->control = LQ_DMA_CH_OFF;
+
+		lq_w32(chan_no, LQ_DMA_CS);
+		lq_w32(0, LQ_DMA_CIE); /* fix me, should disable all the interrupts here? */
+		lq_w32(lq_r32(LQ_DMA_IRNEN) & ~(1 << chan_no), LQ_DMA_IRNEN); /* disable interrupts */
+		lq_w32(lq_r32(LQ_DMA_CCTRL) & ~1, LQ_DMA_CCTRL);
+		while (lq_r32(LQ_DMA_CCTRL) & 1)
+			;
+
+		local_irq_restore(flag);
+		for (j = 0; j < pCh->desc_len; j++) {
+			rx_desc_p = (struct rx_desc *) pCh->desc_base + j;
+			if ((rx_desc_p->status.field.OWN == CPU_OWN
+			     && rx_desc_p->status.field.C)
+			    || (rx_desc_p->status.field.OWN == DMA_OWN
+				&& rx_desc_p->status.field.data_length > 0)) {
+				dev->buffer_free((u8 *)
+						 __va(rx_desc_p->Data_Pointer),
+						 (void *) pCh->opt[j]);
+			}
+		}
+	}
+}
+EXPORT_SYMBOL(dma_device_unregister);
+
+int dma_device_read(struct dma_device_info *dma_dev, u8 **dataptr, void **opt)
+{
+	u8 *buf;
+	int len;
+	int byte_offset = 0;
+	void *p = NULL;
+	struct dma_channel_info *pCh = dma_dev->rx_chan[dma_dev->current_rx_chan];
+	struct rx_desc *rx_desc_p;
+
+	/* get the rx data first */
+	rx_desc_p = (struct rx_desc *) pCh->desc_base + pCh->curr_desc;
+	if (!(rx_desc_p->status.field.OWN == CPU_OWN && rx_desc_p->status.field.C))
+		return 0;
+
+	buf = (u8 *) __va(rx_desc_p->Data_Pointer);
+	*(u32 *)dataptr = (u32)buf;
+	len = rx_desc_p->status.field.data_length;
+
+	if (opt)
+		*(int *)opt = (int)pCh->opt[pCh->curr_desc];
+
+	/* replace with a new allocated buffer */
+	buf = dma_dev->buffer_alloc(pCh->packet_size, &byte_offset, &p);
+
+	if (buf) {
+		dma_cache_inv((unsigned long) buf, pCh->packet_size);
+		pCh->opt[pCh->curr_desc] = p;
+		wmb();
+
+		rx_desc_p->Data_Pointer = (u32) CPHYSADDR((u32) buf);
+		rx_desc_p->status.word = (DMA_OWN << 31) | ((byte_offset) << 23) | pCh->packet_size;
+		wmb();
+	} else {
+		*(u32 *) dataptr = 0;
+		if (opt)
+			*(int *) opt = 0;
+		len = 0;
+	}
+
+	/* increase the curr_desc pointer */
+	pCh->curr_desc++;
+	if (pCh->curr_desc == pCh->desc_len)
+		pCh->curr_desc = 0;
+
+	return len;
+}
+EXPORT_SYMBOL(dma_device_read);
+
+int dma_device_write(struct dma_device_info *dma_dev, u8 *dataptr, int len, void *opt)
+{
+	unsigned long flag;
+	u32 tmp, byte_offset;
+	struct dma_channel_info *pCh;
+	int chan_no;
+	struct tx_desc *tx_desc_p;
+	local_irq_save(flag);
+
+	pCh = dma_dev->tx_chan[dma_dev->current_tx_chan];
+	chan_no = (int)(pCh - (struct dma_channel_info *) dma_chan);
+
+	tx_desc_p = (struct tx_desc *)pCh->desc_base + pCh->prev_desc;
+	while (tx_desc_p->status.field.OWN == CPU_OWN && tx_desc_p->status.field.C) {
+		dma_dev->buffer_free((u8 *) __va(tx_desc_p->Data_Pointer), pCh->opt[pCh->prev_desc]);
+		memset(tx_desc_p, 0, sizeof(struct tx_desc));
+		pCh->prev_desc = (pCh->prev_desc + 1) % (pCh->desc_len);
+		tx_desc_p = (struct tx_desc *)pCh->desc_base + pCh->prev_desc;
+	}
+	tx_desc_p = (struct tx_desc *)pCh->desc_base + pCh->curr_desc;
+	/* Check whether this descriptor is available */
+	if (tx_desc_p->status.field.OWN == DMA_OWN || tx_desc_p->status.field.C) {
+		/* if not, the tell the upper layer device */
+		dma_dev->intr_handler (dma_dev, TX_BUF_FULL_INT);
+		local_irq_restore(flag);
+		printk(KERN_INFO "%s %d: failed to write!\n", __func__, __LINE__);
+
+		return 0;
+	}
+	pCh->opt[pCh->curr_desc] = opt;
+	/* byte offset----to adjust the starting address of the data buffer, should be multiple of the burst length. */
+	byte_offset = ((u32) CPHYSADDR((u32) dataptr)) % ((dma_dev->tx_burst_len) * 4);
+	dma_cache_wback((unsigned long) dataptr, len);
+	wmb();
+	tx_desc_p->Data_Pointer = (u32) CPHYSADDR((u32) dataptr) - byte_offset;
+	wmb();
+	tx_desc_p->status.word = (DMA_OWN << 31) | DMA_DESC_SOP_SET | DMA_DESC_EOP_SET | ((byte_offset) << 23) | len;
+	wmb();
+
+	pCh->curr_desc++;
+	if (pCh->curr_desc == pCh->desc_len)
+		pCh->curr_desc = 0;
+
+	/*Check whether this descriptor is available */
+	tx_desc_p = (struct tx_desc *) pCh->desc_base + pCh->curr_desc;
+	if (tx_desc_p->status.field.OWN == DMA_OWN) {
+		/*if not , the tell the upper layer device */
+		dma_dev->intr_handler (dma_dev, TX_BUF_FULL_INT);
+	}
+
+	lq_w32(chan_no, LQ_DMA_CS);
+	tmp = lq_r32(LQ_DMA_CCTRL);
+
+	if (!(tmp & 1))
+		pCh->open(pCh);
+
+	local_irq_restore(flag);
+
+	return len;
+}
+EXPORT_SYMBOL(dma_device_write);
+
+int map_dma_chan(struct dma_chan_map *map)
+{
+	int i, j;
+	int result;
+
+	for (i = 0; i < MAX_DMA_DEVICE_NUM; i++)
+		strcpy(dma_devs[i].device_name, global_device_name[i]);
+
+	for (i = 0; i < MAX_DMA_CHANNEL_NUM; i++) {
+		dma_chan[i].irq = map[i].irq;
+		result = request_irq(dma_chan[i].irq, dma_interrupt, IRQF_DISABLED, map[i].dev_name, (void *)&dma_chan[i]);
+		if (result) {
+			printk(KERN_WARNING "error, cannot get dma_irq!\n");
+			free_irq(dma_chan[i].irq, (void *) &dma_interrupt);
+
+			return -EFAULT;
+		}
+	}
+
+	for (i = 0; i < MAX_DMA_DEVICE_NUM; i++) {
+		dma_devs[i].num_tx_chan = 0;	/*set default tx channel number to be one */
+		dma_devs[i].num_rx_chan = 0;	/*set default rx channel number to be one */
+		dma_devs[i].max_rx_chan_num = 0;
+		dma_devs[i].max_tx_chan_num = 0;
+		dma_devs[i].buffer_alloc = &common_buffer_alloc;
+		dma_devs[i].buffer_free = &common_buffer_free;
+		dma_devs[i].intr_handler = NULL;
+		dma_devs[i].tx_burst_len = 4;
+		dma_devs[i].rx_burst_len = 4;
+		if (i == 0) {
+			lq_w32(0, LQ_DMA_PS);
+			lq_w32(lq_r32(LQ_DMA_PCTRL) | ((0xf << 8) | (1 << 6)), LQ_DMA_PCTRL);	/*enable dma drop */
+		}
+
+		if (i == 1) {
+			lq_w32(1, LQ_DMA_PS);
+			lq_w32(0x14, LQ_DMA_PCTRL);	/*deu port setting */
+		}
+
+		for (j = 0; j < MAX_DMA_CHANNEL_NUM; j++) {
+			dma_chan[j].byte_offset = 0;
+			dma_chan[j].open = &open_chan;
+			dma_chan[j].close = &close_chan;
+			dma_chan[j].reset = &reset_chan;
+			dma_chan[j].enable_irq = &enable_ch_irq;
+			dma_chan[j].disable_irq = &disable_ch_irq;
+			dma_chan[j].rel_chan_no = map[j].rel_chan_no;
+			dma_chan[j].control = LQ_DMA_CH_OFF;
+			dma_chan[j].default_weight = LQ_DMA_CH_DEFAULT_WEIGHT;
+			dma_chan[j].weight = dma_chan[j].default_weight;
+			dma_chan[j].curr_desc = 0;
+			dma_chan[j].prev_desc = 0;
+		}
+
+		for (j = 0; j < MAX_DMA_CHANNEL_NUM; j++) {
+			if (strcmp(dma_devs[i].device_name, map[j].dev_name) == 0) {
+				if (map[j].dir == LQ_DMA_RX) {
+					dma_chan[j].dir = LQ_DMA_RX;
+					dma_devs[i].max_rx_chan_num++;
+					dma_devs[i].rx_chan[dma_devs[i].max_rx_chan_num - 1] = &dma_chan[j];
+					dma_devs[i].rx_chan[dma_devs[i].max_rx_chan_num - 1]->pri = map[j].pri;
+					dma_chan[j].dma_dev = (void *)&dma_devs[i];
+				} else if (map[j].dir == LQ_DMA_TX) {
+					/*TX direction */
+					dma_chan[j].dir = LQ_DMA_TX;
+					dma_devs[i].max_tx_chan_num++;
+					dma_devs[i].tx_chan[dma_devs[i].max_tx_chan_num - 1] = &dma_chan[j];
+					dma_devs[i].tx_chan[dma_devs[i].max_tx_chan_num - 1]->pri = map[j].pri;
+					dma_chan[j].dma_dev = (void *)&dma_devs[i];
+				} else {
+					printk(KERN_WARNING "WRONG DMA MAP!\n");
+				}
+			}
+		}
+	}
+
+	return 0;
+}
+
+void dma_chip_init(void)
+{
+	int i;
+
+	/* enable DMA from PMU */
+	lq_pmu_enable(PMU_DMA);
+
+	/* reset DMA */
+	lq_w32(lq_r32(LQ_DMA_CTRL) | 1, LQ_DMA_CTRL);
+
+	/* disable all interrupts */
+	lq_w32(0, LQ_DMA_IRNEN);
+
+	for (i = 0; i < MAX_DMA_CHANNEL_NUM; i++) {
+		lq_w32(i, LQ_DMA_CS);
+		lq_w32(0x2, LQ_DMA_CCTRL);
+		lq_w32(0x80000040, LQ_DMA_CPOLL);
+		lq_w32(lq_r32(LQ_DMA_CCTRL) & ~0x1, LQ_DMA_CCTRL);
+	}
+}
+
+int lq_dma_init(void)
+{
+	int i;
+
+	dma_chip_init();
+
+	if (map_dma_chan(default_dma_map))
+		BUG();
+
+	g_desc_list = (u64 *)KSEG1ADDR(__get_free_page(GFP_DMA));
+
+	if (g_desc_list == NULL) {
+		printk(KERN_WARNING "no memory for desriptor\n");
+		return -ENOMEM;
+	}
+
+	memset(g_desc_list, 0, PAGE_SIZE);
+
+	for (i = 0; i < MAX_DMA_CHANNEL_NUM; i++) {
+		dma_chan[i].desc_base = (u32)g_desc_list + i * LQ_DMA_DESCRIPTOR_OFFSET * 8;
+		dma_chan[i].curr_desc = 0;
+		dma_chan[i].desc_len = LQ_DMA_DESCRIPTOR_OFFSET;
+
+		lq_w32(i, LQ_DMA_CS);
+		lq_w32((u32)CPHYSADDR(dma_chan[i].desc_base), LQ_DMA_CDBA);
+		lq_w32(dma_chan[i].desc_len, LQ_DMA_CDLEN);
+	}
+	return 0;
+}
+
+arch_initcall(lq_dma_init);
+
+void dma_cleanup(void)
+{
+	int i;
+
+	free_page(KSEG0ADDR((unsigned long) g_desc_list));
+	for (i = 0; i < MAX_DMA_CHANNEL_NUM; i++)
+		free_irq(dma_chan[i].irq, (void  *)&dma_interrupt);
+}
+
+MODULE_LICENSE("GPL");
--- /dev/null
+++ b/arch/mips/lantiq/xway/pmu.c
@@ -0,0 +1,36 @@
+/*
+ *  This program is free software; you can redistribute it and/or modify it
+ *  under the terms of the GNU General Public License version 2 as published
+ *  by the Free Software Foundation.
+ *
+ *  Copyright (C) 2010 John Crispin <blogic@openwrt.org>
+ */
+
+#include <linux/kernel.h>
+#include <linux/module.h>
+#include <linux/version.h>
+
+#include <xway.h>
+
+#define LQ_PMU_PWDCR        ((u32 *)(LQ_PMU_BASE_ADDR + 0x001C))
+#define LQ_PMU_PWDSR        ((u32 *)(LQ_PMU_BASE_ADDR + 0x0020))
+
+void
+lq_pmu_enable(unsigned int module)
+{
+	int err = 1000000;
+
+	lq_w32(lq_r32(LQ_PMU_PWDCR) & ~module, LQ_PMU_PWDCR);
+	while (--err && (lq_r32(LQ_PMU_PWDSR) & module));
+
+	if (!err)
+		panic("activating PMU module failed!");
+}
+EXPORT_SYMBOL(lq_pmu_enable);
+
+void
+lq_pmu_disable(unsigned int module)
+{
+	lq_w32(lq_r32(LQ_PMU_PWDCR) | module, LQ_PMU_PWDCR);
+}
+EXPORT_SYMBOL(lq_pmu_disable);
--- /dev/null
+++ b/arch/mips/lantiq/xway/timer.c
@@ -0,0 +1,828 @@
+#include <linux/kernel.h>
+#include <linux/module.h>
+#include <linux/version.h>
+#include <linux/types.h>
+#include <linux/fs.h>
+#include <linux/miscdevice.h>
+#include <linux/init.h>
+#include <linux/uaccess.h>
+#include <linux/unistd.h>
+#include <linux/errno.h>
+#include <linux/interrupt.h>
+#include <linux/sched.h>
+
+#include <asm/irq.h>
+#include <asm/div64.h>
+
+#include <xway.h>
+#include <xway_irq.h>
+#include <lantiq_timer.h>
+
+#define MAX_NUM_OF_32BIT_TIMER_BLOCKS	6
+
+#ifdef TIMER1A
+#define FIRST_TIMER			TIMER1A
+#else
+#define FIRST_TIMER			2
+#endif
+
+/*
+ *  GPTC divider is set or not.
+ */
+#define GPTU_CLC_RMC_IS_SET		0
+
+/*
+ *  Timer Interrupt (IRQ)
+ */
+/*  Must be adjusted when ICU driver is available */
+#define TIMER_INTERRUPT			(INT_NUM_IM3_IRL0 + 22)
+
+/*
+ *  Bits Operation
+ */
+#define GET_BITS(x, msb, lsb)		\
+	(((x) & ((1 << ((msb) + 1)) - 1)) >> (lsb))
+#define SET_BITS(x, msb, lsb, value)	\
+	(((x) & ~(((1 << ((msb) + 1)) - 1) ^ ((1 << (lsb)) - 1))) | \
+	(((value) & ((1 << (1 + (msb) - (lsb))) - 1)) << (lsb)))
+
+/*
+ *  GPTU Register Mapping
+ */
+#define LQ_GPTU			(KSEG1 + 0x1E100A00)
+#define LQ_GPTU_CLC		((volatile u32 *)(LQ_GPTU + 0x0000))
+#define LQ_GPTU_ID			((volatile u32 *)(LQ_GPTU + 0x0008))
+#define LQ_GPTU_CON(n, X)		((volatile u32 *)(LQ_GPTU + 0x0010 + ((X) * 4) + ((n) - 1) * 0x0020))	/* X must be either A or B */
+#define LQ_GPTU_RUN(n, X)		((volatile u32 *)(LQ_GPTU + 0x0018 + ((X) * 4) + ((n) - 1) * 0x0020))	/* X must be either A or B */
+#define LQ_GPTU_RELOAD(n, X)	((volatile u32 *)(LQ_GPTU + 0x0020 + ((X) * 4) + ((n) - 1) * 0x0020))	/* X must be either A or B */
+#define LQ_GPTU_COUNT(n, X)	((volatile u32 *)(LQ_GPTU + 0x0028 + ((X) * 4) + ((n) - 1) * 0x0020))	/* X must be either A or B */
+#define LQ_GPTU_IRNEN		((volatile u32 *)(LQ_GPTU + 0x00F4))
+#define LQ_GPTU_IRNICR		((volatile u32 *)(LQ_GPTU + 0x00F8))
+#define LQ_GPTU_IRNCR		((volatile u32 *)(LQ_GPTU + 0x00FC))
+
+/*
+ *  Clock Control Register
+ */
+#define GPTU_CLC_SMC			GET_BITS(*LQ_GPTU_CLC, 23, 16)
+#define GPTU_CLC_RMC			GET_BITS(*LQ_GPTU_CLC, 15, 8)
+#define GPTU_CLC_FSOE			(*LQ_GPTU_CLC & (1 << 5))
+#define GPTU_CLC_EDIS			(*LQ_GPTU_CLC & (1 << 3))
+#define GPTU_CLC_SPEN			(*LQ_GPTU_CLC & (1 << 2))
+#define GPTU_CLC_DISS			(*LQ_GPTU_CLC & (1 << 1))
+#define GPTU_CLC_DISR			(*LQ_GPTU_CLC & (1 << 0))
+
+#define GPTU_CLC_SMC_SET(value)		SET_BITS(0, 23, 16, (value))
+#define GPTU_CLC_RMC_SET(value)		SET_BITS(0, 15, 8, (value))
+#define GPTU_CLC_FSOE_SET(value)	((value) ? (1 << 5) : 0)
+#define GPTU_CLC_SBWE_SET(value)	((value) ? (1 << 4) : 0)
+#define GPTU_CLC_EDIS_SET(value)	((value) ? (1 << 3) : 0)
+#define GPTU_CLC_SPEN_SET(value)	((value) ? (1 << 2) : 0)
+#define GPTU_CLC_DISR_SET(value)	((value) ? (1 << 0) : 0)
+
+/*
+ *  ID Register
+ */
+#define GPTU_ID_ID			GET_BITS(*LQ_GPTU_ID, 15, 8)
+#define GPTU_ID_CFG			GET_BITS(*LQ_GPTU_ID, 7, 5)
+#define GPTU_ID_REV			GET_BITS(*LQ_GPTU_ID, 4, 0)
+
+/*
+ *  Control Register of Timer/Counter nX
+ *    n is the index of block (1 based index)
+ *    X is either A or B
+ */
+#define GPTU_CON_SRC_EG(n, X)		(*LQ_GPTU_CON(n, X) & (1 << 10))
+#define GPTU_CON_SRC_EXT(n, X)		(*LQ_GPTU_CON(n, X) & (1 << 9))
+#define GPTU_CON_SYNC(n, X)		(*LQ_GPTU_CON(n, X) & (1 << 8))
+#define GPTU_CON_EDGE(n, X)		GET_BITS(*LQ_GPTU_CON(n, X), 7, 6)
+#define GPTU_CON_INV(n, X)		(*LQ_GPTU_CON(n, X) & (1 << 5))
+#define GPTU_CON_EXT(n, X)		(*LQ_GPTU_CON(n, A) & (1 << 4))	/* Timer/Counter B does not have this bit */
+#define GPTU_CON_STP(n, X)		(*LQ_GPTU_CON(n, X) & (1 << 3))
+#define GPTU_CON_CNT(n, X)		(*LQ_GPTU_CON(n, X) & (1 << 2))
+#define GPTU_CON_DIR(n, X)		(*LQ_GPTU_CON(n, X) & (1 << 1))
+#define GPTU_CON_EN(n, X)		(*LQ_GPTU_CON(n, X) & (1 << 0))
+
+#define GPTU_CON_SRC_EG_SET(value)	((value) ? 0 : (1 << 10))
+#define GPTU_CON_SRC_EXT_SET(value)	((value) ? (1 << 9) : 0)
+#define GPTU_CON_SYNC_SET(value)	((value) ? (1 << 8) : 0)
+#define GPTU_CON_EDGE_SET(value)	SET_BITS(0, 7, 6, (value))
+#define GPTU_CON_INV_SET(value)		((value) ? (1 << 5) : 0)
+#define GPTU_CON_EXT_SET(value)		((value) ? (1 << 4) : 0)
+#define GPTU_CON_STP_SET(value)		((value) ? (1 << 3) : 0)
+#define GPTU_CON_CNT_SET(value)		((value) ? (1 << 2) : 0)
+#define GPTU_CON_DIR_SET(value)		((value) ? (1 << 1) : 0)
+
+#define GPTU_RUN_RL_SET(value)		((value) ? (1 << 2) : 0)
+#define GPTU_RUN_CEN_SET(value)		((value) ? (1 << 1) : 0)
+#define GPTU_RUN_SEN_SET(value)		((value) ? (1 << 0) : 0)
+
+#define GPTU_IRNEN_TC_SET(n, X, value)	((value) ? (1 << (((n) - 1) * 2 + (X))) : 0)
+#define GPTU_IRNCR_TC_SET(n, X, value)	((value) ? (1 << (((n) - 1) * 2 + (X))) : 0)
+
+#define TIMER_FLAG_MASK_SIZE(x)		(x & 0x0001)
+#define TIMER_FLAG_MASK_TYPE(x)		(x & 0x0002)
+#define TIMER_FLAG_MASK_STOP(x)		(x & 0x0004)
+#define TIMER_FLAG_MASK_DIR(x)		(x & 0x0008)
+#define TIMER_FLAG_NONE_EDGE		0x0000
+#define TIMER_FLAG_MASK_EDGE(x)		(x & 0x0030)
+#define TIMER_FLAG_REAL			0x0000
+#define TIMER_FLAG_INVERT		0x0040
+#define TIMER_FLAG_MASK_INVERT(x)	(x & 0x0040)
+#define TIMER_FLAG_MASK_TRIGGER(x)	(x & 0x0070)
+#define TIMER_FLAG_MASK_SYNC(x)		(x & 0x0080)
+#define TIMER_FLAG_CALLBACK_IN_HB	0x0200
+#define TIMER_FLAG_MASK_HANDLE(x)	(x & 0x0300)
+#define TIMER_FLAG_MASK_SRC(x)		(x & 0x1000)
+
+struct timer_dev_timer {
+	unsigned int f_irq_on;
+	unsigned int irq;
+	unsigned int flag;
+	unsigned long arg1;
+	unsigned long arg2;
+};
+
+struct timer_dev {
+	struct mutex gptu_mutex;
+	unsigned int number_of_timers;
+	unsigned int occupation;
+	unsigned int f_gptu_on;
+	struct timer_dev_timer timer[MAX_NUM_OF_32BIT_TIMER_BLOCKS * 2];
+};
+
+static long gptu_ioctl(struct file *, unsigned int, unsigned long);
+static int gptu_open(struct inode *, struct file *);
+static int gptu_release(struct inode *, struct file *);
+
+static struct file_operations gptu_fops = {
+	.owner = THIS_MODULE,
+	.unlocked_ioctl = gptu_ioctl,
+	.open = gptu_open,
+	.release = gptu_release
+};
+
+static struct miscdevice gptu_miscdev = {
+	.minor = MISC_DYNAMIC_MINOR,
+	.name = "gptu",
+	.fops = &gptu_fops,
+};
+
+static struct timer_dev timer_dev;
+
+static irqreturn_t timer_irq_handler(int irq, void *p)
+{
+	unsigned int timer;
+	unsigned int flag;
+	struct timer_dev_timer *dev_timer = (struct timer_dev_timer *)p;
+
+	timer = irq - TIMER_INTERRUPT;
+	if (timer < timer_dev.number_of_timers
+		&& dev_timer == &timer_dev.timer[timer]) {
+		/*  Clear interrupt.    */
+		lq_w32(1 << timer, LQ_GPTU_IRNCR);
+
+		/*  Call user hanler or signal. */
+		flag = dev_timer->flag;
+		if (!(timer & 0x01)
+			|| TIMER_FLAG_MASK_SIZE(flag) == TIMER_FLAG_16BIT) {
+			/* 16-bit timer or timer A of 32-bit timer  */
+			switch (TIMER_FLAG_MASK_HANDLE(flag)) {
+			case TIMER_FLAG_CALLBACK_IN_IRQ:
+			case TIMER_FLAG_CALLBACK_IN_HB:
+				if (dev_timer->arg1)
+					(*(timer_callback)dev_timer->arg1)(dev_timer->arg2);
+				break;
+			case TIMER_FLAG_SIGNAL:
+				send_sig((int)dev_timer->arg2, (struct task_struct *)dev_timer->arg1, 0);
+				break;
+			}
+		}
+	}
+	return IRQ_HANDLED;
+}
+
+static inline void lq_enable_gptu(void)
+{
+	lq_pmu_enable(PMU_GPT);
+
+	/*  Set divider as 1, disable write protection for SPEN, enable module. */
+	*LQ_GPTU_CLC =
+		GPTU_CLC_SMC_SET(0x00) |
+		GPTU_CLC_RMC_SET(0x01) |
+		GPTU_CLC_FSOE_SET(0) |
+		GPTU_CLC_SBWE_SET(1) |
+		GPTU_CLC_EDIS_SET(0) |
+		GPTU_CLC_SPEN_SET(0) |
+		GPTU_CLC_DISR_SET(0);
+}
+
+static inline void lq_disable_gptu(void)
+{
+	lq_w32(0x00, LQ_GPTU_IRNEN);
+	lq_w32(0xfff, LQ_GPTU_IRNCR);
+
+	/*  Set divider as 0, enable write protection for SPEN, disable module. */
+	*LQ_GPTU_CLC =
+		GPTU_CLC_SMC_SET(0x00) |
+		GPTU_CLC_RMC_SET(0x00) |
+		GPTU_CLC_FSOE_SET(0) |
+		GPTU_CLC_SBWE_SET(0) |
+		GPTU_CLC_EDIS_SET(0) |
+		GPTU_CLC_SPEN_SET(0) |
+		GPTU_CLC_DISR_SET(1);
+
+	lq_pmu_disable(PMU_GPT);
+}
+
+int lq_request_timer(unsigned int timer, unsigned int flag,
+	unsigned long value, unsigned long arg1, unsigned long arg2)
+{
+	int ret = 0;
+	unsigned int con_reg, irnen_reg;
+	int n, X;
+
+	if (timer >= FIRST_TIMER + timer_dev.number_of_timers)
+		return -EINVAL;
+
+	printk(KERN_INFO "request_timer(%d, 0x%08X, %lu)...",
+		timer, flag, value);
+
+	if (TIMER_FLAG_MASK_SIZE(flag) == TIMER_FLAG_16BIT)
+		value &= 0xFFFF;
+	else
+		timer &= ~0x01;
+
+	mutex_lock(&timer_dev.gptu_mutex);
+
+	/*
+	 *  Allocate timer.
+	 */
+	if (timer < FIRST_TIMER) {
+		unsigned int mask;
+		unsigned int shift;
+		/* This takes care of TIMER1B which is the only choice for Voice TAPI system */
+		unsigned int offset = TIMER2A;
+
+		/*
+		 *  Pick up a free timer.
+		 */
+		if (TIMER_FLAG_MASK_SIZE(flag) == TIMER_FLAG_16BIT) {
+			mask = 1 << offset;
+			shift = 1;
+		} else {
+			mask = 3 << offset;
+			shift = 2;
+		}
+		for (timer = offset;
+		     timer < offset + timer_dev.number_of_timers;
+		     timer += shift, mask <<= shift)
+			if (!(timer_dev.occupation & mask)) {
+				timer_dev.occupation |= mask;
+				break;
+			}
+		if (timer >= offset + timer_dev.number_of_timers) {
+			printk("failed![%d]\n", __LINE__);
+			mutex_unlock(&timer_dev.gptu_mutex);
+			return -EINVAL;
+		} else
+			ret = timer;
+	} else {
+		register unsigned int mask;
+
+		/*
+		 *  Check if the requested timer is free.
+		 */
+		mask = (TIMER_FLAG_MASK_SIZE(flag) == TIMER_FLAG_16BIT ? 1 : 3) << timer;
+		if ((timer_dev.occupation & mask)) {
+			printk("failed![%d] mask %#x, timer_dev.occupation %#x\n",
+				__LINE__, mask, timer_dev.occupation);
+			mutex_unlock(&timer_dev.gptu_mutex);
+			return -EBUSY;
+		} else {
+			timer_dev.occupation |= mask;
+			ret = 0;
+		}
+	}
+
+	/*
+	 *  Prepare control register value.
+	 */
+	switch (TIMER_FLAG_MASK_EDGE(flag)) {
+	default:
+	case TIMER_FLAG_NONE_EDGE:
+		con_reg = GPTU_CON_EDGE_SET(0x00);
+		break;
+	case TIMER_FLAG_RISE_EDGE:
+		con_reg = GPTU_CON_EDGE_SET(0x01);
+		break;
+	case TIMER_FLAG_FALL_EDGE:
+		con_reg = GPTU_CON_EDGE_SET(0x02);
+		break;
+	case TIMER_FLAG_ANY_EDGE:
+		con_reg = GPTU_CON_EDGE_SET(0x03);
+		break;
+	}
+	if (TIMER_FLAG_MASK_TYPE(flag) == TIMER_FLAG_TIMER)
+		con_reg |=
+			TIMER_FLAG_MASK_SRC(flag) ==
+			TIMER_FLAG_EXT_SRC ? GPTU_CON_SRC_EXT_SET(1) :
+			GPTU_CON_SRC_EXT_SET(0);
+	else
+		con_reg |=
+			TIMER_FLAG_MASK_SRC(flag) ==
+			TIMER_FLAG_EXT_SRC ? GPTU_CON_SRC_EG_SET(1) :
+			GPTU_CON_SRC_EG_SET(0);
+	con_reg |=
+		TIMER_FLAG_MASK_SYNC(flag) ==
+		TIMER_FLAG_UNSYNC ? GPTU_CON_SYNC_SET(0) :
+		GPTU_CON_SYNC_SET(1);
+	con_reg |=
+		TIMER_FLAG_MASK_INVERT(flag) ==
+		TIMER_FLAG_REAL ? GPTU_CON_INV_SET(0) : GPTU_CON_INV_SET(1);
+	con_reg |=
+		TIMER_FLAG_MASK_SIZE(flag) ==
+		TIMER_FLAG_16BIT ? GPTU_CON_EXT_SET(0) :
+		GPTU_CON_EXT_SET(1);
+	con_reg |=
+		TIMER_FLAG_MASK_STOP(flag) ==
+		TIMER_FLAG_ONCE ? GPTU_CON_STP_SET(1) : GPTU_CON_STP_SET(0);
+	con_reg |=
+		TIMER_FLAG_MASK_TYPE(flag) ==
+		TIMER_FLAG_TIMER ? GPTU_CON_CNT_SET(0) :
+		GPTU_CON_CNT_SET(1);
+	con_reg |=
+		TIMER_FLAG_MASK_DIR(flag) ==
+		TIMER_FLAG_UP ? GPTU_CON_DIR_SET(1) : GPTU_CON_DIR_SET(0);
+
+	/*
+	 *  Fill up running data.
+	 */
+	timer_dev.timer[timer - FIRST_TIMER].flag = flag;
+	timer_dev.timer[timer - FIRST_TIMER].arg1 = arg1;
+	timer_dev.timer[timer - FIRST_TIMER].arg2 = arg2;
+	if (TIMER_FLAG_MASK_SIZE(flag) != TIMER_FLAG_16BIT)
+		timer_dev.timer[timer - FIRST_TIMER + 1].flag = flag;
+
+	/*
+	 *  Enable GPTU module.
+	 */
+	if (!timer_dev.f_gptu_on) {
+		lq_enable_gptu();
+		timer_dev.f_gptu_on = 1;
+	}
+
+	/*
+	 *  Enable IRQ.
+	 */
+	if (TIMER_FLAG_MASK_HANDLE(flag) != TIMER_FLAG_NO_HANDLE) {
+		if (TIMER_FLAG_MASK_HANDLE(flag) == TIMER_FLAG_SIGNAL)
+			timer_dev.timer[timer - FIRST_TIMER].arg1 =
+				(unsigned long) find_task_by_vpid((int) arg1);
+
+		irnen_reg = 1 << (timer - FIRST_TIMER);
+
+		if (TIMER_FLAG_MASK_HANDLE(flag) == TIMER_FLAG_SIGNAL
+		    || (TIMER_FLAG_MASK_HANDLE(flag) ==
+			TIMER_FLAG_CALLBACK_IN_IRQ
+			&& timer_dev.timer[timer - FIRST_TIMER].arg1)) {
+			enable_irq(timer_dev.timer[timer - FIRST_TIMER].irq);
+			timer_dev.timer[timer - FIRST_TIMER].f_irq_on = 1;
+		}
+	} else
+		irnen_reg = 0;
+
+	/*
+	 *  Write config register, reload value and enable interrupt.
+	 */
+	n = timer >> 1;
+	X = timer & 0x01;
+	*LQ_GPTU_CON(n, X) = con_reg;
+	*LQ_GPTU_RELOAD(n, X) = value;
+	/* printk("reload value = %d\n", (u32)value); */
+	*LQ_GPTU_IRNEN |= irnen_reg;
+
+	mutex_unlock(&timer_dev.gptu_mutex);
+	printk("successful!\n");
+	return ret;
+}
+EXPORT_SYMBOL(lq_request_timer);
+
+int lq_free_timer(unsigned int timer)
+{
+	unsigned int flag;
+	unsigned int mask;
+	int n, X;
+
+	if (!timer_dev.f_gptu_on)
+		return -EINVAL;
+
+	if (timer < FIRST_TIMER || timer >= FIRST_TIMER + timer_dev.number_of_timers)
+		return -EINVAL;
+
+	mutex_lock(&timer_dev.gptu_mutex);
+
+	flag = timer_dev.timer[timer - FIRST_TIMER].flag;
+	if (TIMER_FLAG_MASK_SIZE(flag) != TIMER_FLAG_16BIT)
+		timer &= ~0x01;
+
+	mask = (TIMER_FLAG_MASK_SIZE(flag) == TIMER_FLAG_16BIT ? 1 : 3) << timer;
+	if (((timer_dev.occupation & mask) ^ mask)) {
+		mutex_unlock(&timer_dev.gptu_mutex);
+		return -EINVAL;
+	}
+
+	n = timer >> 1;
+	X = timer & 0x01;
+
+	if (GPTU_CON_EN(n, X))
+		*LQ_GPTU_RUN(n, X) = GPTU_RUN_CEN_SET(1);
+
+	*LQ_GPTU_IRNEN &= ~GPTU_IRNEN_TC_SET(n, X, 1);
+	*LQ_GPTU_IRNCR |= GPTU_IRNCR_TC_SET(n, X, 1);
+
+	if (timer_dev.timer[timer - FIRST_TIMER].f_irq_on) {
+		disable_irq(timer_dev.timer[timer - FIRST_TIMER].irq);
+		timer_dev.timer[timer - FIRST_TIMER].f_irq_on = 0;
+	}
+
+	timer_dev.occupation &= ~mask;
+	if (!timer_dev.occupation && timer_dev.f_gptu_on) {
+		lq_disable_gptu();
+		timer_dev.f_gptu_on = 0;
+	}
+
+	mutex_unlock(&timer_dev.gptu_mutex);
+
+	return 0;
+}
+EXPORT_SYMBOL(lq_free_timer);
+
+int lq_start_timer(unsigned int timer, int is_resume)
+{
+	unsigned int flag;
+	unsigned int mask;
+	int n, X;
+
+	if (!timer_dev.f_gptu_on)
+		return -EINVAL;
+
+	if (timer < FIRST_TIMER || timer >= FIRST_TIMER + timer_dev.number_of_timers)
+		return -EINVAL;
+
+	mutex_lock(&timer_dev.gptu_mutex);
+
+	flag = timer_dev.timer[timer - FIRST_TIMER].flag;
+	if (TIMER_FLAG_MASK_SIZE(flag) != TIMER_FLAG_16BIT)
+		timer &= ~0x01;
+
+	mask = (TIMER_FLAG_MASK_SIZE(flag) ==
+	TIMER_FLAG_16BIT ? 1 : 3) << timer;
+	if (((timer_dev.occupation & mask) ^ mask)) {
+		mutex_unlock(&timer_dev.gptu_mutex);
+		return -EINVAL;
+	}
+
+	n = timer >> 1;
+	X = timer & 0x01;
+
+	*LQ_GPTU_RUN(n, X) = GPTU_RUN_RL_SET(!is_resume) | GPTU_RUN_SEN_SET(1);
+
+	mutex_unlock(&timer_dev.gptu_mutex);
+
+	return 0;
+}
+EXPORT_SYMBOL(lq_start_timer);
+
+int lq_stop_timer(unsigned int timer)
+{
+	unsigned int flag;
+	unsigned int mask;
+	int n, X;
+
+	if (!timer_dev.f_gptu_on)
+		return -EINVAL;
+
+	if (timer < FIRST_TIMER
+	    || timer >= FIRST_TIMER + timer_dev.number_of_timers)
+		return -EINVAL;
+
+	mutex_lock(&timer_dev.gptu_mutex);
+
+	flag = timer_dev.timer[timer - FIRST_TIMER].flag;
+	if (TIMER_FLAG_MASK_SIZE(flag) != TIMER_FLAG_16BIT)
+		timer &= ~0x01;
+
+	mask = (TIMER_FLAG_MASK_SIZE(flag) == TIMER_FLAG_16BIT ? 1 : 3) << timer;
+	if (((timer_dev.occupation & mask) ^ mask)) {
+		mutex_unlock(&timer_dev.gptu_mutex);
+		return -EINVAL;
+	}
+
+	n = timer >> 1;
+	X = timer & 0x01;
+
+	*LQ_GPTU_RUN(n, X) = GPTU_RUN_CEN_SET(1);
+
+	mutex_unlock(&timer_dev.gptu_mutex);
+
+	return 0;
+}
+EXPORT_SYMBOL(lq_stop_timer);
+
+int lq_reset_counter_flags(u32 timer, u32 flags)
+{
+	unsigned int oflag;
+	unsigned int mask, con_reg;
+	int n, X;
+
+	if (!timer_dev.f_gptu_on)
+		return -EINVAL;
+
+	if (timer < FIRST_TIMER || timer >= FIRST_TIMER + timer_dev.number_of_timers)
+		return -EINVAL;
+
+	mutex_lock(&timer_dev.gptu_mutex);
+
+	oflag = timer_dev.timer[timer - FIRST_TIMER].flag;
+	if (TIMER_FLAG_MASK_SIZE(oflag) != TIMER_FLAG_16BIT)
+		timer &= ~0x01;
+
+	mask = (TIMER_FLAG_MASK_SIZE(oflag) == TIMER_FLAG_16BIT ? 1 : 3) << timer;
+	if (((timer_dev.occupation & mask) ^ mask)) {
+		mutex_unlock(&timer_dev.gptu_mutex);
+		return -EINVAL;
+	}
+
+	switch (TIMER_FLAG_MASK_EDGE(flags)) {
+	default:
+	case TIMER_FLAG_NONE_EDGE:
+		con_reg = GPTU_CON_EDGE_SET(0x00);
+		break;
+	case TIMER_FLAG_RISE_EDGE:
+		con_reg = GPTU_CON_EDGE_SET(0x01);
+		break;
+	case TIMER_FLAG_FALL_EDGE:
+		con_reg = GPTU_CON_EDGE_SET(0x02);
+		break;
+	case TIMER_FLAG_ANY_EDGE:
+		con_reg = GPTU_CON_EDGE_SET(0x03);
+		break;
+	}
+	if (TIMER_FLAG_MASK_TYPE(flags) == TIMER_FLAG_TIMER)
+		con_reg |= TIMER_FLAG_MASK_SRC(flags) == TIMER_FLAG_EXT_SRC ? GPTU_CON_SRC_EXT_SET(1) : GPTU_CON_SRC_EXT_SET(0);
+	else
+		con_reg |= TIMER_FLAG_MASK_SRC(flags) == TIMER_FLAG_EXT_SRC ? GPTU_CON_SRC_EG_SET(1) : GPTU_CON_SRC_EG_SET(0);
+	con_reg |= TIMER_FLAG_MASK_SYNC(flags) == TIMER_FLAG_UNSYNC ? GPTU_CON_SYNC_SET(0) : GPTU_CON_SYNC_SET(1);
+	con_reg |= TIMER_FLAG_MASK_INVERT(flags) == TIMER_FLAG_REAL ? GPTU_CON_INV_SET(0) : GPTU_CON_INV_SET(1);
+	con_reg |= TIMER_FLAG_MASK_SIZE(flags) == TIMER_FLAG_16BIT ? GPTU_CON_EXT_SET(0) : GPTU_CON_EXT_SET(1);
+	con_reg |= TIMER_FLAG_MASK_STOP(flags) == TIMER_FLAG_ONCE ? GPTU_CON_STP_SET(1) : GPTU_CON_STP_SET(0);
+	con_reg |= TIMER_FLAG_MASK_TYPE(flags) == TIMER_FLAG_TIMER ? GPTU_CON_CNT_SET(0) : GPTU_CON_CNT_SET(1);
+	con_reg |= TIMER_FLAG_MASK_DIR(flags) == TIMER_FLAG_UP ? GPTU_CON_DIR_SET(1) : GPTU_CON_DIR_SET(0);
+
+	timer_dev.timer[timer - FIRST_TIMER].flag = flags;
+	if (TIMER_FLAG_MASK_SIZE(flags) != TIMER_FLAG_16BIT)
+		timer_dev.timer[timer - FIRST_TIMER + 1].flag = flags;
+
+	n = timer >> 1;
+	X = timer & 0x01;
+
+	*LQ_GPTU_CON(n, X) = con_reg;
+	smp_wmb();
+	printk(KERN_INFO "[%s]: counter%d oflags %#x, nflags %#x, GPTU_CON %#x\n", __func__, timer, oflag, flags, *LQ_GPTU_CON(n, X));
+	mutex_unlock(&timer_dev.gptu_mutex);
+	return 0;
+}
+EXPORT_SYMBOL(lq_reset_counter_flags);
+
+int lq_get_count_value(unsigned int timer, unsigned long *value)
+{
+	unsigned int flag;
+	unsigned int mask;
+	int n, X;
+
+	if (!timer_dev.f_gptu_on)
+		return -EINVAL;
+
+	if (timer < FIRST_TIMER
+	    || timer >= FIRST_TIMER + timer_dev.number_of_timers)
+		return -EINVAL;
+
+	mutex_lock(&timer_dev.gptu_mutex);
+
+	flag = timer_dev.timer[timer - FIRST_TIMER].flag;
+	if (TIMER_FLAG_MASK_SIZE(flag) != TIMER_FLAG_16BIT)
+		timer &= ~0x01;
+
+	mask = (TIMER_FLAG_MASK_SIZE(flag) == TIMER_FLAG_16BIT ? 1 : 3) << timer;
+	if (((timer_dev.occupation & mask) ^ mask)) {
+		mutex_unlock(&timer_dev.gptu_mutex);
+		return -EINVAL;
+	}
+
+	n = timer >> 1;
+	X = timer & 0x01;
+
+	*value = *LQ_GPTU_COUNT(n, X);
+
+	mutex_unlock(&timer_dev.gptu_mutex);
+
+	return 0;
+}
+EXPORT_SYMBOL(lq_get_count_value);
+
+u32 lq_cal_divider(unsigned long freq)
+{
+	u64 module_freq, fpi = lq_get_fpi_bus_clock(2);
+	u32 clock_divider = 1;
+	module_freq = fpi * 1000;
+	do_div(module_freq, clock_divider * freq);
+	return module_freq;
+}
+EXPORT_SYMBOL(lq_cal_divider);
+
+int lq_set_timer(unsigned int timer, unsigned int freq, int is_cyclic,
+	int is_ext_src, unsigned int handle_flag, unsigned long arg1,
+	unsigned long arg2)
+{
+	unsigned long divider;
+	unsigned int flag;
+
+	divider = lq_cal_divider(freq);
+	if (divider == 0)
+		return -EINVAL;
+	flag = ((divider & ~0xFFFF) ? TIMER_FLAG_32BIT : TIMER_FLAG_16BIT)
+		| (is_cyclic ? TIMER_FLAG_CYCLIC : TIMER_FLAG_ONCE)
+		| (is_ext_src ? TIMER_FLAG_EXT_SRC : TIMER_FLAG_INT_SRC)
+		| TIMER_FLAG_TIMER | TIMER_FLAG_DOWN
+		| TIMER_FLAG_MASK_HANDLE(handle_flag);
+
+	printk(KERN_INFO "lq_set_timer(%d, %d), divider = %lu\n",
+		timer, freq, divider);
+	return lq_request_timer(timer, flag, divider, arg1, arg2);
+}
+EXPORT_SYMBOL(lq_set_timer);
+
+int lq_set_counter(unsigned int timer, unsigned int flag, u32 reload,
+	unsigned long arg1, unsigned long arg2)
+{
+	printk(KERN_INFO "lq_set_counter(%d, %#x, %d)\n", timer, flag, reload);
+	return lq_request_timer(timer, flag, reload, arg1, arg2);
+}
+EXPORT_SYMBOL(lq_set_counter);
+
+static long gptu_ioctl(struct file *file, unsigned int cmd,
+	unsigned long arg)
+{
+	int ret;
+	struct gptu_ioctl_param param;
+
+	if (!access_ok(VERIFY_READ, arg, sizeof(struct gptu_ioctl_param)))
+		return -EFAULT;
+	copy_from_user(&param, (void *) arg, sizeof(param));
+
+	if ((((cmd == GPTU_REQUEST_TIMER || cmd == GPTU_SET_TIMER
+	       || GPTU_SET_COUNTER) && param.timer < 2)
+	     || cmd == GPTU_GET_COUNT_VALUE || cmd == GPTU_CALCULATE_DIVIDER)
+	    && !access_ok(VERIFY_WRITE, arg,
+			   sizeof(struct gptu_ioctl_param)))
+		return -EFAULT;
+
+	switch (cmd) {
+	case GPTU_REQUEST_TIMER:
+		ret = lq_request_timer(param.timer, param.flag, param.value,
+				     (unsigned long) param.pid,
+				     (unsigned long) param.sig);
+		if (ret > 0) {
+			copy_to_user(&((struct gptu_ioctl_param *) arg)->
+				      timer, &ret, sizeof(&ret));
+			ret = 0;
+		}
+		break;
+	case GPTU_FREE_TIMER:
+		ret = lq_free_timer(param.timer);
+		break;
+	case GPTU_START_TIMER:
+		ret = lq_start_timer(param.timer, param.flag);
+		break;
+	case GPTU_STOP_TIMER:
+		ret = lq_stop_timer(param.timer);
+		break;
+	case GPTU_GET_COUNT_VALUE:
+		ret = lq_get_count_value(param.timer, &param.value);
+		if (!ret)
+			copy_to_user(&((struct gptu_ioctl_param *) arg)->
+				      value, &param.value,
+				      sizeof(param.value));
+		break;
+	case GPTU_CALCULATE_DIVIDER:
+		param.value = lq_cal_divider(param.value);
+		if (param.value == 0)
+			ret = -EINVAL;
+		else {
+			copy_to_user(&((struct gptu_ioctl_param *) arg)->
+				      value, &param.value,
+				      sizeof(param.value));
+			ret = 0;
+		}
+		break;
+	case GPTU_SET_TIMER:
+		ret = lq_set_timer(param.timer, param.value,
+				 TIMER_FLAG_MASK_STOP(param.flag) !=
+				 TIMER_FLAG_ONCE ? 1 : 0,
+				 TIMER_FLAG_MASK_SRC(param.flag) ==
+				 TIMER_FLAG_EXT_SRC ? 1 : 0,
+				 TIMER_FLAG_MASK_HANDLE(param.flag) ==
+				 TIMER_FLAG_SIGNAL ? TIMER_FLAG_SIGNAL :
+				 TIMER_FLAG_NO_HANDLE,
+				 (unsigned long) param.pid,
+				 (unsigned long) param.sig);
+		if (ret > 0) {
+			copy_to_user(&((struct gptu_ioctl_param *) arg)->
+				      timer, &ret, sizeof(&ret));
+			ret = 0;
+		}
+		break;
+	case GPTU_SET_COUNTER:
+		lq_set_counter(param.timer, param.flag, param.value, 0, 0);
+		if (ret > 0) {
+			copy_to_user(&((struct gptu_ioctl_param *) arg)->
+				      timer, &ret, sizeof(&ret));
+			ret = 0;
+		}
+		break;
+	default:
+		ret = -ENOTTY;
+	}
+
+	return ret;
+}
+
+static int gptu_open(struct inode *inode, struct file *file)
+{
+	return 0;
+}
+
+static int gptu_release(struct inode *inode, struct file *file)
+{
+	return 0;
+}
+
+int __init lq_gptu_init(void)
+{
+	int ret;
+	unsigned int i;
+
+	lq_w32(0, LQ_GPTU_IRNEN);
+	lq_w32(0xfff, LQ_GPTU_IRNCR);
+
+	memset(&timer_dev, 0, sizeof(timer_dev));
+	mutex_init(&timer_dev.gptu_mutex);
+
+	lq_enable_gptu();
+	timer_dev.number_of_timers = GPTU_ID_CFG * 2;
+	lq_disable_gptu();
+	if (timer_dev.number_of_timers > MAX_NUM_OF_32BIT_TIMER_BLOCKS * 2)
+		timer_dev.number_of_timers = MAX_NUM_OF_32BIT_TIMER_BLOCKS * 2;
+	printk(KERN_INFO "gptu: totally %d 16-bit timers/counters\n", timer_dev.number_of_timers);
+
+	ret = misc_register(&gptu_miscdev);
+	if (ret) {
+		printk(KERN_ERR "gptu: can't misc_register, get error %d\n", -ret);
+		return ret;
+	} else {
+		printk(KERN_INFO "gptu: misc_register on minor %d\n", gptu_miscdev.minor);
+	}
+
+	for (i = 0; i < timer_dev.number_of_timers; i++) {
+		ret = request_irq(TIMER_INTERRUPT + i, timer_irq_handler, IRQF_TIMER, gptu_miscdev.name, &timer_dev.timer[i]);
+		if (ret) {
+			for (; i >= 0; i--)
+				free_irq(TIMER_INTERRUPT + i, &timer_dev.timer[i]);
+			misc_deregister(&gptu_miscdev);
+			printk(KERN_ERR "gptu: failed in requesting irq (%d), get error %d\n", i, -ret);
+			return ret;
+		} else {
+			timer_dev.timer[i].irq = TIMER_INTERRUPT + i;
+			disable_irq(timer_dev.timer[i].irq);
+			printk(KERN_INFO "gptu: succeeded to request irq %d\n", timer_dev.timer[i].irq);
+		}
+	}
+
+	return 0;
+}
+
+void __exit lq_gptu_exit(void)
+{
+	unsigned int i;
+
+	for (i = 0; i < timer_dev.number_of_timers; i++) {
+		if (timer_dev.timer[i].f_irq_on)
+			disable_irq(timer_dev.timer[i].irq);
+		free_irq(timer_dev.timer[i].irq, &timer_dev.timer[i]);
+	}
+	lq_disable_gptu();
+	misc_deregister(&gptu_miscdev);
+}
+
+module_init(lq_gptu_init);
+module_exit(lq_gptu_exit);
--- /dev/null
+++ b/arch/mips/lantiq/xway/timer.h
@@ -0,0 +1,155 @@
+#ifndef __DANUBE_GPTU_DEV_H__2005_07_26__10_19__
+#define __DANUBE_GPTU_DEV_H__2005_07_26__10_19__
+
+
+/******************************************************************************
+       Copyright (c) 2002, Infineon Technologies.  All rights reserved.
+
+                               No Warranty
+   Because the program is licensed free of charge, there is no warranty for
+   the program, to the extent permitted by applicable law.  Except when
+   otherwise stated in writing the copyright holders and/or other parties
+   provide the program "as is" without warranty of any kind, either
+   expressed or implied, including, but not limited to, the implied
+   warranties of merchantability and fitness for a particular purpose. The
+   entire risk as to the quality and performance of the program is with
+   you.  should the program prove defective, you assume the cost of all
+   necessary servicing, repair or correction.
+
+   In no event unless required by applicable law or agreed to in writing
+   will any copyright holder, or any other party who may modify and/or
+   redistribute the program as permitted above, be liable to you for
+   damages, including any general, special, incidental or consequential
+   damages arising out of the use or inability to use the program
+   (including but not limited to loss of data or data being rendered
+   inaccurate or losses sustained by you or third parties or a failure of
+   the program to operate with any other programs), even if such holder or
+   other party has been advised of the possibility of such damages.
+******************************************************************************/
+
+
+/*
+ * ####################################
+ *              Definition
+ * ####################################
+ */
+
+/*
+ *  Available Timer/Counter Index
+ */
+#define TIMER(n, X)                     (n * 2 + (X ? 1 : 0))
+#define TIMER_ANY                       0x00
+#define TIMER1A                         TIMER(1, 0)
+#define TIMER1B                         TIMER(1, 1)
+#define TIMER2A                         TIMER(2, 0)
+#define TIMER2B                         TIMER(2, 1)
+#define TIMER3A                         TIMER(3, 0)
+#define TIMER3B                         TIMER(3, 1)
+
+/*
+ *  Flag of Timer/Counter
+ *  These flags specify the way in which timer is configured.
+ */
+/*  Bit size of timer/counter.                      */
+#define TIMER_FLAG_16BIT                0x0000
+#define TIMER_FLAG_32BIT                0x0001
+/*  Switch between timer and counter.               */
+#define TIMER_FLAG_TIMER                0x0000
+#define TIMER_FLAG_COUNTER              0x0002
+/*  Stop or continue when overflowing/underflowing. */
+#define TIMER_FLAG_ONCE                 0x0000
+#define TIMER_FLAG_CYCLIC               0x0004
+/*  Count up or counter down.                       */
+#define TIMER_FLAG_UP                   0x0000
+#define TIMER_FLAG_DOWN                 0x0008
+/*  Count on specific level or edge.                */
+#define TIMER_FLAG_HIGH_LEVEL_SENSITIVE 0x0000
+#define TIMER_FLAG_LOW_LEVEL_SENSITIVE  0x0040
+#define TIMER_FLAG_RISE_EDGE            0x0010
+#define TIMER_FLAG_FALL_EDGE            0x0020
+#define TIMER_FLAG_ANY_EDGE             0x0030
+/*  Signal is syncronous to module clock or not.    */
+#define TIMER_FLAG_UNSYNC               0x0000
+#define TIMER_FLAG_SYNC                 0x0080
+/*  Different interrupt handle type.                */
+#define TIMER_FLAG_NO_HANDLE            0x0000
+#if defined(__KERNEL__)
+    #define TIMER_FLAG_CALLBACK_IN_IRQ  0x0100
+#endif  //  defined(__KERNEL__)
+#define TIMER_FLAG_SIGNAL               0x0300
+/*  Internal clock source or external clock source  */
+#define TIMER_FLAG_INT_SRC              0x0000
+#define TIMER_FLAG_EXT_SRC              0x1000
+
+
+/*
+ *  ioctl Command
+ */
+#define GPTU_REQUEST_TIMER              0x01    /*  General method to setup timer/counter.  */
+#define GPTU_FREE_TIMER                 0x02    /*  Free timer/counter.                     */
+#define GPTU_START_TIMER                0x03    /*  Start or resume timer/counter.          */
+#define GPTU_STOP_TIMER                 0x04    /*  Suspend timer/counter.                  */
+#define GPTU_GET_COUNT_VALUE            0x05    /*  Get current count value.                */
+#define GPTU_CALCULATE_DIVIDER          0x06    /*  Calculate timer divider from given freq.*/
+#define GPTU_SET_TIMER                  0x07    /*  Simplified method to setup timer.       */
+#define GPTU_SET_COUNTER                0x08    /*  Simplified method to setup counter.     */
+
+/*
+ *  Data Type Used to Call ioctl
+ */
+struct gptu_ioctl_param {
+    unsigned int                        timer;  /*  In command GPTU_REQUEST_TIMER, GPTU_SET_TIMER, and  *
+                                                 *  GPTU_SET_COUNTER, this field is ID of expected      *
+                                                 *  timer/counter. If it's zero, a timer/counter would  *
+                                                 *  be dynamically allocated and ID would be stored in  *
+                                                 *  this field.                                         *
+                                                 *  In command GPTU_GET_COUNT_VALUE, this field is      *
+                                                 *  ignored.                                            *
+                                                 *  In other command, this field is ID of timer/counter *
+                                                 *  allocated.                                          */
+    unsigned int                        flag;   /*  In command GPTU_REQUEST_TIMER, GPTU_SET_TIMER, and  *
+                                                 *  GPTU_SET_COUNTER, this field contains flags to      *
+                                                 *  specify how to configure timer/counter.             *
+                                                 *  In command GPTU_START_TIMER, zero indicate start    *
+                                                 *  and non-zero indicate resume timer/counter.         *
+                                                 *  In other command, this field is ignored.            */
+    unsigned long                       value;  /*  In command GPTU_REQUEST_TIMER, this field contains  *
+                                                 *  init/reload value.                                  *
+                                                 *  In command GPTU_SET_TIMER, this field contains      *
+                                                 *  frequency (0.001Hz) of timer.                       *
+                                                 *  In command GPTU_GET_COUNT_VALUE, current count      *
+                                                 *  value would be stored in this field.                *
+                                                 *  In command GPTU_CALCULATE_DIVIDER, this field       *
+                                                 *  contains frequency wanted, and after calculation,   *
+                                                 *  divider would be stored in this field to overwrite  *
+                                                 *  the frequency.                                      *
+                                                 *  In other command, this field is ignored.            */
+    int                                 pid;    /*  In command GPTU_REQUEST_TIMER and GPTU_SET_TIMER,   *
+                                                 *  if signal is required, this field contains process  *
+                                                 *  ID to which signal would be sent.                   *
+                                                 *  In other command, this field is ignored.            */
+    int                                 sig;    /*  In command GPTU_REQUEST_TIMER and GPTU_SET_TIMER,   *
+                                                 *  if signal is required, this field contains signal   *
+                                                 *  number which would be sent.                         *
+                                                 *  In other command, this field is ignored.            */
+};
+
+/*
+ * ####################################
+ *              Data Type
+ * ####################################
+ */
+typedef void (*timer_callback)(unsigned long arg);
+
+extern int ifxmips_request_timer(unsigned int, unsigned int, unsigned long, unsigned long, unsigned long);
+extern int ifxmips_free_timer(unsigned int);
+extern int ifxmips_start_timer(unsigned int, int);
+extern int ifxmips_stop_timer(unsigned int);
+extern int ifxmips_reset_counter_flags(u32 timer, u32 flags);
+extern int ifxmips_get_count_value(unsigned int, unsigned long *);
+extern u32 ifxmips_cal_divider(unsigned long);
+extern int ifxmips_set_timer(unsigned int, unsigned int, int, int, unsigned int, unsigned long, unsigned long);
+extern int ifxmips_set_counter(unsigned int timer, unsigned int flag,
+	u32 reload, unsigned long arg1, unsigned long arg2);
+
+#endif /* __DANUBE_GPTU_DEV_H__2005_07_26__10_19__ */
--- /dev/null
+++ b/arch/mips/lantiq/xway/Makefile
@@ -0,0 +1,5 @@
+obj-y := pmu.o prom.o dma.o timer.o reset.o clk-xway.o
+obj-y += gpio.o gpio_ebu.o gpio_leds.o devices.o
+obj-$(CONFIG_LANTIQ_MACH_EASY50812) += mach-easy50812.o
+obj-$(CONFIG_LANTIQ_MACH_EASY50712) += mach-easy50712.o
+obj-$(CONFIG_LANTIQ_MACH_EASY4010) += mach-easy4010.o
--- /dev/null
+++ b/arch/mips/lantiq/xway/clk-xway.c
@@ -0,0 +1,219 @@
+/*
+ *  This program is free software; you can redistribute it and/or modify it
+ *  under the terms of the GNU General Public License version 2 as published
+ *  by the Free Software Foundation.
+ *
+ *  Copyright (C) 2007 Xu Liang, infineon
+ *  Copyright (C) 2010 John Crispin <blogic@openwrt.org>
+ */
+
+#include <linux/io.h>
+#include <linux/module.h>
+#include <linux/init.h>
+#include <linux/clk.h>
+
+#include <asm/time.h>
+#include <asm/irq.h>
+#include <asm/div64.h>
+
+#include <xway.h>
+
+static unsigned int lq_ram_clocks[] = {CLOCK_167M, CLOCK_133M, CLOCK_111M, CLOCK_83M };
+#define DDR_HZ lq_ram_clocks[lq_r32(LQ_CGU_SYS) & 0x3]
+
+#define BASIC_FREQUENCY_1	35328000
+#define BASIC_FREQUENCY_2	36000000
+#define BASIS_REQUENCY_USB	12000000
+
+#define GET_BITS(x, msb, lsb)           (((x) & ((1 << ((msb) + 1)) - 1)) >> (lsb))
+
+#define CGU_PLL0_PHASE_DIVIDER_ENABLE   (lq_r32(LQ_CGU_PLL0_CFG) & (1 << 31))
+#define CGU_PLL0_BYPASS                 (lq_r32(LQ_CGU_PLL0_CFG) & (1 << 30))
+#define CGU_PLL0_CFG_DSMSEL             (lq_r32(LQ_CGU_PLL0_CFG) & (1 << 28))
+#define CGU_PLL0_CFG_FRAC_EN            (lq_r32(LQ_CGU_PLL0_CFG) & (1 << 27))
+#define CGU_PLL1_SRC                    (lq_r32(LQ_CGU_PLL1_CFG) & (1 << 31))
+#define CGU_PLL2_PHASE_DIVIDER_ENABLE   (lq_r32(LQ_CGU_PLL2_CFG) & (1 << 20))
+#define CGU_SYS_FPI_SEL                 (1 << 6)
+#define CGU_SYS_DDR_SEL                 0x3
+#define CGU_PLL0_SRC                    (1 << 29)
+
+#define CGU_PLL0_CFG_PLLK               GET_BITS(*LQ_CGU_PLL0_CFG, 26, 17)
+#define CGU_PLL0_CFG_PLLN               GET_BITS(*LQ_CGU_PLL0_CFG, 12, 6)
+#define CGU_PLL0_CFG_PLLM               GET_BITS(*LQ_CGU_PLL0_CFG, 5, 2)
+#define CGU_PLL2_SRC                    GET_BITS(*LQ_CGU_PLL2_CFG, 18, 17)
+#define CGU_PLL2_CFG_INPUT_DIV          GET_BITS(*LQ_CGU_PLL2_CFG, 16, 13)
+
+#define LQ_GPTU_GPT_CLC		((u32 *)(LQ_GPTU_BASE_ADDR + 0x0000))
+#define LQ_CGU_PLL0_CFG		((u32 *)(LQ_CGU_BASE_ADDR + 0x0004))
+#define LQ_CGU_PLL1_CFG		((u32 *)(LQ_CGU_BASE_ADDR + 0x0008))
+#define LQ_CGU_PLL2_CFG		((u32 *)(LQ_CGU_BASE_ADDR + 0x000C))
+#define LQ_CGU_SYS			((u32 *)(LQ_CGU_BASE_ADDR + 0x0010))
+#define LQ_CGU_UPDATE		((u32 *)(LQ_CGU_BASE_ADDR + 0x0014))
+#define LQ_CGU_IF_CLK		((u32 *)(LQ_CGU_BASE_ADDR + 0x0018))
+#define LQ_CGU_OSC_CON		((u32 *)(LQ_CGU_BASE_ADDR + 0x001C))
+#define LQ_CGU_SMD			((u32 *)(LQ_CGU_BASE_ADDR + 0x0020))
+#define LQ_CGU_CT1SR		((u32 *)(LQ_CGU_BASE_ADDR + 0x0028))
+#define LQ_CGU_CT2SR		((u32 *)(LQ_CGU_BASE_ADDR + 0x002C))
+#define LQ_CGU_PCMCR		((u32 *)(LQ_CGU_BASE_ADDR + 0x0030))
+#define LQ_CGU_PCI_CR		((u32 *)(LQ_CGU_BASE_ADDR + 0x0034))
+#define LQ_CGU_PD_PC		((u32 *)(LQ_CGU_BASE_ADDR + 0x0038))
+#define LQ_CGU_FMR			((u32 *)(LQ_CGU_BASE_ADDR + 0x003C))
+
+static unsigned int lq_get_pll0_fdiv(void);
+
+static inline unsigned int
+get_input_clock(int pll)
+{
+	switch (pll) {
+	case 0:
+		if (lq_r32(LQ_CGU_PLL0_CFG) & CGU_PLL0_SRC)
+			return BASIS_REQUENCY_USB;
+		else if (CGU_PLL0_PHASE_DIVIDER_ENABLE)
+			return BASIC_FREQUENCY_1;
+		else
+			return BASIC_FREQUENCY_2;
+	case 1:
+		if (CGU_PLL1_SRC)
+			return BASIS_REQUENCY_USB;
+		else if (CGU_PLL0_PHASE_DIVIDER_ENABLE)
+			return BASIC_FREQUENCY_1;
+		else
+			return BASIC_FREQUENCY_2;
+	case 2:
+		switch (CGU_PLL2_SRC) {
+		case 0:
+			return lq_get_pll0_fdiv();
+		case 1:
+			return CGU_PLL2_PHASE_DIVIDER_ENABLE ?
+				BASIC_FREQUENCY_1 :
+				BASIC_FREQUENCY_2;
+		case 2:
+			return BASIS_REQUENCY_USB;
+		}
+	default:
+		return 0;
+	}
+}
+
+static inline unsigned int
+cal_dsm(int pll, unsigned int num, unsigned int den)
+{
+	u64 res, clock = get_input_clock(pll);
+	res = num * clock;
+	do_div(res, den);
+	return res;
+}
+
+static inline unsigned int
+mash_dsm(int pll, unsigned int M, unsigned int N, unsigned int K)
+{
+	unsigned int num = ((N + 1) << 10) + K;
+	unsigned int den = (M + 1) << 10;
+	return cal_dsm(pll, num, den);
+}
+
+static inline unsigned int
+ssff_dsm_1(int pll, unsigned int M, unsigned int N,	unsigned int K)
+{
+	unsigned int num = ((N + 1) << 11) + K + 512;
+	unsigned int den = (M + 1) << 11;
+	return cal_dsm(pll, num, den);
+}
+
+static inline unsigned int
+ssff_dsm_2(int pll, unsigned int M, unsigned int N, unsigned int K)
+{
+	unsigned int num = K >= 512 ?
+		((N + 1) << 12) + K - 512 : ((N + 1) << 12) + K + 3584;
+	unsigned int den = (M + 1) << 12;
+	return cal_dsm(pll, num, den);
+}
+
+static inline unsigned int
+dsm(int pll, unsigned int M, unsigned int N, unsigned int K,
+	unsigned int dsmsel, unsigned int phase_div_en)
+{
+	if (!dsmsel)
+		return mash_dsm(pll, M, N, K);
+	else if (!phase_div_en)
+		return mash_dsm(pll, M, N, K);
+	else
+		return ssff_dsm_2(pll, M, N, K);
+}
+
+static inline unsigned int
+lq_get_pll0_fosc(void)
+{
+	if (CGU_PLL0_BYPASS)
+		return get_input_clock(0);
+	else
+		return !CGU_PLL0_CFG_FRAC_EN
+			? dsm(0, CGU_PLL0_CFG_PLLM, CGU_PLL0_CFG_PLLN, 0, CGU_PLL0_CFG_DSMSEL,
+				CGU_PLL0_PHASE_DIVIDER_ENABLE)
+			: dsm(0, CGU_PLL0_CFG_PLLM, CGU_PLL0_CFG_PLLN, CGU_PLL0_CFG_PLLK,
+				CGU_PLL0_CFG_DSMSEL, CGU_PLL0_PHASE_DIVIDER_ENABLE);
+}
+
+static unsigned int
+lq_get_pll0_fdiv(void)
+{
+	unsigned int div = CGU_PLL2_CFG_INPUT_DIV + 1;
+	return (lq_get_pll0_fosc() + (div >> 1)) / div;
+}
+
+unsigned int
+lq_get_io_region_clock(void)
+{
+	unsigned int ret = lq_get_pll0_fosc();
+	switch (lq_r32(LQ_CGU_PLL2_CFG) & CGU_SYS_DDR_SEL) {
+	default:
+	case 0:
+		return (ret + 1) / 2;
+	case 1:
+		return (ret * 2 + 2) / 5;
+	case 2:
+		return (ret + 1) / 3;
+	case 3:
+		return (ret + 2) / 4;
+	}
+}
+EXPORT_SYMBOL(lq_get_io_region_clock);
+
+unsigned int
+lq_get_fpi_bus_clock(int fpi)
+{
+	unsigned int ret = lq_get_io_region_clock();
+	if ((fpi == 2) && (lq_r32(LQ_CGU_SYS) & CGU_SYS_FPI_SEL))
+		ret >>= 1;
+	return ret;
+}
+EXPORT_SYMBOL(lq_get_fpi_bus_clock);
+
+unsigned int
+lq_get_cpu_hz(void)
+{
+	switch (lq_r32(LQ_CGU_SYS) & 0xc)
+	{
+	case 0:
+		return CLOCK_333M;
+	case 4:
+		return DDR_HZ;
+	case 8:
+		return DDR_HZ << 1;
+	default:
+		return DDR_HZ >> 1;
+	}
+}
+EXPORT_SYMBOL(lq_get_cpu_hz);
+
+unsigned int
+lq_get_fpi_hz(void)
+{
+	unsigned int ddr_clock = DDR_HZ;
+	if (lq_r32(LQ_CGU_SYS) & 0x40)
+		return ddr_clock >> 1;
+	return ddr_clock;
+}
+EXPORT_SYMBOL(lq_get_fpi_hz);
+
+
--- /dev/null
+++ b/arch/mips/lantiq/xway/gpio.c
@@ -0,0 +1,206 @@
+/*
+ *  This program is free software; you can redistribute it and/or modify it
+ *  under the terms of the GNU General Public License version 2 as published
+ *  by the Free Software Foundation.
+ *
+ *  Copyright (C) 2010 John Crispin <blogic@openwrt.org>
+ */
+
+#include <linux/slab.h>
+#include <linux/module.h>
+#include <linux/platform_device.h>
+#include <linux/gpio.h>
+
+#include <lantiq.h>
+
+#define LQ_GPIO0_BASE_ADDR	0x1E100B10
+#define LQ_GPIO1_BASE_ADDR	0x1E100B40
+#define LQ_GPIO_SIZE		0x30
+
+#define LQ_GPIO_OUT			0x00
+#define LQ_GPIO_IN			0x04
+#define LQ_GPIO_DIR			0x08
+#define LQ_GPIO_ALTSEL0		0x0C
+#define LQ_GPIO_ALTSEL1		0x10
+#define LQ_GPIO_OD			0x14
+
+#define PINS_PER_PORT		16
+
+#define lq_gpio_getbit(m, r, p)		!!(lq_r32(m + r) & (1 << p))
+#define lq_gpio_setbit(m, r, p)		lq_w32_mask(0, (1 << p), m + r)
+#define lq_gpio_clearbit(m, r, p)	lq_w32_mask((1 << p), 0, m + r)
+
+struct lq_gpio
+{
+	void __iomem *membase;
+	struct gpio_chip chip;
+};
+
+int
+gpio_to_irq(unsigned int gpio)
+{
+	return -EINVAL;
+}
+EXPORT_SYMBOL(gpio_to_irq);
+
+int
+lq_gpio_setconfig(unsigned int pin, unsigned int reg, unsigned int val)
+{
+	void __iomem *membase = (void*)KSEG1ADDR(LQ_GPIO0_BASE_ADDR);
+	if(pin >= (2 * PINS_PER_PORT))
+		return -EINVAL;
+	if(pin >= PINS_PER_PORT)
+	{
+		pin -= PINS_PER_PORT;
+		membase += LQ_GPIO_SIZE;
+	}
+	if(val)
+		lq_w32_mask(0, (1 << pin), membase + reg);
+	else
+		lq_w32_mask((1 << pin), 0, membase + reg);
+	return 0;
+}
+EXPORT_SYMBOL(lq_gpio_setconfig);
+
+int
+lq_gpio_request(unsigned int pin, unsigned int alt0,
+	unsigned int alt1, unsigned int dir, const char *name)
+{
+	void __iomem *membase = (void*)KSEG1ADDR(LQ_GPIO0_BASE_ADDR);
+	if(pin >= (2 * PINS_PER_PORT))
+		return -EINVAL;
+	if(gpio_request(pin, name))
+	{
+		printk("failed to register %s gpio\n", name);
+		return -EBUSY;
+	}
+	if(dir)
+		gpio_direction_output(pin, 1);
+	else
+		gpio_direction_input(pin);
+	if(pin >= PINS_PER_PORT)
+	{
+		pin -= PINS_PER_PORT;
+		membase += LQ_GPIO_SIZE;
+	}
+	if(alt0)
+		lq_gpio_setbit(membase, LQ_GPIO_ALTSEL0, pin);
+	else
+		lq_gpio_clearbit(membase, LQ_GPIO_ALTSEL0, pin);
+	if(alt1)
+		lq_gpio_setbit(membase, LQ_GPIO_ALTSEL1, pin);
+	else
+		lq_gpio_clearbit(membase, LQ_GPIO_ALTSEL1, pin);
+	return 0;
+}
+EXPORT_SYMBOL(lq_gpio_request);
+
+static void
+lq_gpio_set(struct gpio_chip *chip, unsigned int offset, int value)
+{
+	struct lq_gpio *lq_gpio = container_of(chip, struct lq_gpio, chip);
+	if(value)
+		lq_gpio_setbit(lq_gpio->membase, LQ_GPIO_OUT, offset);
+	else
+		lq_gpio_clearbit(lq_gpio->membase, LQ_GPIO_OUT, offset);
+}
+
+static int
+lq_gpio_get(struct gpio_chip *chip, unsigned int offset)
+{
+	struct lq_gpio *lq_gpio = container_of(chip, struct lq_gpio, chip);
+	return lq_gpio_getbit(lq_gpio->membase, LQ_GPIO_IN, offset);
+}
+
+static int
+lq_gpio_direction_input(struct gpio_chip *chip, unsigned int offset)
+{
+	struct lq_gpio *lq_gpio = container_of(chip, struct lq_gpio, chip);
+	lq_gpio_clearbit(lq_gpio->membase, LQ_GPIO_OD, offset);
+	lq_gpio_clearbit(lq_gpio->membase, LQ_GPIO_DIR, offset);
+	return 0;
+}
+
+static int
+lq_gpio_direction_output(struct gpio_chip *chip, unsigned int offset, int value)
+{
+	struct lq_gpio *lq_gpio = container_of(chip, struct lq_gpio, chip);
+	lq_gpio_setbit(lq_gpio->membase, LQ_GPIO_OD, offset);
+	lq_gpio_setbit(lq_gpio->membase, LQ_GPIO_DIR, offset);
+	lq_gpio_set(chip, offset, value);
+	return 0;
+}
+
+static int
+lq_gpio_req(struct gpio_chip *chip, unsigned offset)
+{
+	struct lq_gpio *lq_gpio = container_of(chip, struct lq_gpio, chip);
+	lq_gpio_clearbit(lq_gpio->membase, LQ_GPIO_ALTSEL0, offset);
+	lq_gpio_clearbit(lq_gpio->membase, LQ_GPIO_ALTSEL1, offset);
+	return 0;
+}
+
+static int
+lq_gpio_probe(struct platform_device *pdev)
+{
+	struct lq_gpio *lq_gpio = kzalloc(sizeof(struct lq_gpio), GFP_KERNEL);
+	struct resource *res = platform_get_resource(pdev, IORESOURCE_MEM, 0);
+	int ret = 0;
+	if(!res)
+	{
+		ret = -ENOENT;
+		goto err_free;
+	}
+	res = request_mem_region(res->start, resource_size(res),
+		dev_name(&pdev->dev));
+	if(!res)
+	{
+		ret = -EBUSY;
+		goto err_free;
+	}
+	lq_gpio->membase = ioremap_nocache(res->start, resource_size(res));
+	if(!lq_gpio->membase)
+	{
+		ret = -ENOMEM;
+		goto err_release_mem_region;
+	}
+	lq_gpio->chip.label = "lq_gpio";
+	lq_gpio->chip.direction_input = lq_gpio_direction_input;
+	lq_gpio->chip.direction_output = lq_gpio_direction_output;
+	lq_gpio->chip.get = lq_gpio_get;
+	lq_gpio->chip.set = lq_gpio_set;
+	lq_gpio->chip.request = lq_gpio_req;
+	lq_gpio->chip.base = PINS_PER_PORT * pdev->id;
+	lq_gpio->chip.ngpio = PINS_PER_PORT;
+	platform_set_drvdata(pdev, lq_gpio);
+	ret = gpiochip_add(&lq_gpio->chip);
+	if(!ret)
+		return 0;
+
+	iounmap(lq_gpio->membase);
+err_release_mem_region:
+	release_mem_region(res->start, resource_size(res));
+err_free:
+    kfree(lq_gpio);
+	return ret;
+}
+
+static struct platform_driver
+lq_gpio_driver = {
+	.probe = lq_gpio_probe,
+	.driver = {
+		.name = "lq_gpio",
+		.owner = THIS_MODULE,
+	},
+};
+
+int __init
+lq_gpio_init(void)
+{
+	int ret = platform_driver_register(&lq_gpio_driver);
+	if(ret)
+		printk(KERN_INFO "lq_gpio : Error registering platfom driver!");
+	return ret;
+}
+
+postcore_initcall(lq_gpio_init);
--- /dev/null
+++ b/arch/mips/lantiq/xway/reset.c
@@ -0,0 +1,53 @@
+/*
+ *  This program is free software; you can redistribute it and/or modify it
+ *  under the terms of the GNU General Public License version 2 as published
+ *  by the Free Software Foundation.
+ *
+ *  Copyright (C) 2010 John Crispin <blogic@openwrt.org>
+ */
+
+#include <linux/init.h>
+#include <linux/io.h>
+#include <linux/pm.h>
+#include <asm/reboot.h>
+
+#include <xway.h>
+
+#define LQ_RCU_RST			((u32 *)(LQ_RCU_BASE_ADDR + 0x0010))
+#define LQ_RCU_RST_ALL		0x40000000
+
+static void
+lq_machine_restart(char *command)
+{
+	printk(KERN_NOTICE "System restart\n");
+	local_irq_disable();
+	lq_w32(lq_r32(LQ_RCU_RST) | LQ_RCU_RST_ALL,	LQ_RCU_RST);
+	for(;;);
+}
+
+static void
+lq_machine_halt(void)
+{
+	printk(KERN_NOTICE "System halted.\n");
+	local_irq_disable();
+	for(;;);
+}
+
+static void
+lq_machine_power_off(void)
+{
+	printk(KERN_NOTICE "Please turn off the power now.\n");
+	local_irq_disable();
+	for(;;);
+}
+
+static int __init
+mips_reboot_setup(void)
+{
+	_machine_restart = lq_machine_restart;
+	_machine_halt = lq_machine_halt;
+	pm_power_off = lq_machine_power_off;
+	return 0;
+}
+
+arch_initcall(mips_reboot_setup);
