--- a/drivers/gpio/Kconfig
+++ b/drivers/gpio/Kconfig
@@ -401,4 +401,12 @@ config GPIO_JANZ_TTL
 	  This driver provides support for driving the pins in output
 	  mode only. Input mode is not supported.
 
+comment "Other GPIO expanders"
+
+config GPIO_NXP_74HC153
+	tristate "NXP 74HC153 Dual 4-input multiplexer"
+	help
+	  Platform driver for NXP 74HC153 Dual 4-input Multiplexer. This
+	  provides a GPIO interface supporting inputs.
+
 endif
--- a/drivers/gpio/Makefile
+++ b/drivers/gpio/Makefile
@@ -18,6 +18,7 @@ obj-$(CONFIG_GPIO_MAX7301)	+= max7301.o
 obj-$(CONFIG_GPIO_MAX732X)	+= max732x.o
 obj-$(CONFIG_GPIO_MC33880)	+= mc33880.o
 obj-$(CONFIG_GPIO_MCP23S08)	+= mcp23s08.o
+obj-$(CONFIG_GPIO_NXP_74HC153)	+= nxp_74hc153.o
 obj-$(CONFIG_GPIO_74X164)	+= 74x164.o
 obj-$(CONFIG_GPIO_PCA953X)	+= pca953x.o
 obj-$(CONFIG_GPIO_PCF857X)	+= pcf857x.o
