--- /dev/null
+++ b/arch/mips/lantiq/falcon/mach-95C3AM1.c
@@ -0,0 +1,103 @@
+#include <linux/init.h>
+#include <linux/platform_device.h>
+#include <linux/i2c-gpio.h>
+#include <machine.h>
+
+#include "devices.h"
+#include "dev-leds-gpio.h"
+
+#define BOARD_95C3AM1_GPIO_LED_0 10
+#define BOARD_95C3AM1_GPIO_LED_1 11
+#define BOARD_95C3AM1_GPIO_LED_2 12
+#define BOARD_95C3AM1_GPIO_LED_3 13
+
+extern unsigned char lq_ethaddr[6];
+
+#ifdef CONFIG_MTD_PARTITIONS
+static struct mtd_partition board_95C3AM1_partitions[] =
+{
+	{
+		.name	= "uboot",
+		.offset	= 0x0,
+		.size	= 0x40000,
+	},
+	{
+		.name	= "uboot_env",
+		.offset	= 0x40000,
+		.size	= 0x40000,	/* 2 sectors for redundant env. */
+	},
+	{
+		.name	= "linux",
+		.offset	= 0x80000,
+		.size	= 0xF80000,	/* map only 16 MiB */
+	},
+};
+
+static struct flash_platform_data board_95C3AM1_flash_platform_data = {
+	.name = "sflash",
+	.parts = board_95C3AM1_partitions,
+	.nr_parts = ARRAY_SIZE(board_95C3AM1_partitions)
+};
+#endif
+
+static struct spi_board_info board_95C3AM1_flash_data __initdata = {
+	.modalias		= "m25p80",
+	.bus_num		= 0,
+	.chip_select		= 0,
+	.max_speed_hz		= 10 * 1000 * 1000,
+	.mode			= SPI_MODE_3,
+#ifdef CONFIG_MTD_PARTITIONS
+	.platform_data		= &board_95C3AM1_flash_platform_data
+#endif
+};
+
+static struct gpio_led board_95C3AM1_leds_gpio[] __initdata = {
+	{
+		.name		= "power",
+		.gpio		= BOARD_95C3AM1_GPIO_LED_0,
+		.active_low	= 0,
+	}, {
+		.name		= "optical",
+		.gpio		= BOARD_95C3AM1_GPIO_LED_1,
+		.active_low	= 0,
+	}, {
+		.name		= "lan",
+		.gpio		= BOARD_95C3AM1_GPIO_LED_2,
+		.active_low	= 0,
+	}, {
+		.name		= "update",
+		.gpio		= BOARD_95C3AM1_GPIO_LED_3,
+		.active_low	= 0,
+	}
+};
+
+static struct i2c_gpio_platform_data board_95C3AM1_i2c_gpio_data = {
+	.sda_pin	= 107,
+	.scl_pin	= 108,
+};
+
+static struct platform_device board_95C3AM1_i2c_gpio_device = {
+	.name		= "i2c-gpio",
+	.id		= 0,
+	.dev = {
+		.platform_data	= &board_95C3AM1_i2c_gpio_data,
+	}
+};
+
+static void __init board_95C3AM1_init(void)
+{
+	falcon_register_asc(0);
+	falcon_register_gpio();
+	falcon_register_wdt();
+	falcon_register_i2c();
+	falcon_register_spi_flash(&board_95C3AM1_flash_data);
+	platform_device_register(&board_95C3AM1_i2c_gpio_device);
+	lq_add_device_leds_gpio(-1, ARRAY_SIZE(board_95C3AM1_leds_gpio),
+						board_95C3AM1_leds_gpio);
+	falcon_register_crypto();
+}
+
+MIPS_MACHINE(LANTIQ_MACH_95C3AM1,
+			"95C3AM1",
+			"95C3AM1 Board",
+			board_95C3AM1_init);
--- a/arch/mips/include/asm/mach-lantiq/machine.h
+++ b/arch/mips/include/asm/mach-lantiq/machine.h
@@ -7,6 +7,7 @@ enum lantiq_mach_type {
 	LANTIQ_MACH_EASY98000,		/* Falcon Eval Board, NOR Flash */
 	LANTIQ_MACH_EASY98000SF,	/* Falcon Eval Board, Serial Flash */
 	LANTIQ_MACH_EASY98020,		/* Falcon Reference Board */
+	LANTIQ_MACH_95C3AM1,		/* Board 95C3AM1 */
 
 	/* XWAY */
 	LANTIQ_MACH_EASY4010,		/* Twinpass evalkit */
--- a/arch/mips/lantiq/falcon/Kconfig
+++ b/arch/mips/lantiq/falcon/Kconfig
@@ -10,6 +10,10 @@ config LANTIQ_MACH_EASY98020
 	bool "Easy98020"
 	default y
 
+config LANTIQ_MACH_95C3AM1
+	bool "95C3AM1"
+	default y
+
 endmenu
 
 endif
--- a/arch/mips/lantiq/falcon/Makefile
+++ b/arch/mips/lantiq/falcon/Makefile
@@ -3,3 +3,4 @@ obj-y += softdog_vpe.o
 obj-$(CONFIG_LANTIQ_MACH_EASY98000) += mach-easy98000.o
 obj-$(CONFIG_LANTIQ_MACH_EASY98000) += dev-leds-easy98000-cpld.o
 obj-$(CONFIG_LANTIQ_MACH_EASY98020) += mach-easy98020.o
+obj-$(CONFIG_LANTIQ_MACH_95C3AM1)   += mach-95C3AM1.o
