--- a/common/Makefile
+++ b/common/Makefile
@@ -127,7 +127,9 @@
 ifdef CONFIG_PCI
 COBJS-$(CONFIG_CMD_PCI) += cmd_pci.o
 endif
+ifdef CONFIG_CMD_PCMCIA
 COBJS-y += cmd_pcmcia.o
+endif
 COBJS-$(CONFIG_CMD_PORTIO) += cmd_portio.o
 COBJS-$(CONFIG_CMD_REGINFO) += cmd_reginfo.o
 COBJS-$(CONFIG_CMD_REISER) += cmd_reiser.o
--- a/drivers/pcmcia/Makefile
+++ b/drivers/pcmcia/Makefile
@@ -28,9 +28,11 @@
 COBJS-$(CONFIG_I82365) += i82365.o
 COBJS-$(CONFIG_8xx) += mpc8xx_pcmcia.o
 COBJS-$(CONFIG_PXA_PCMCIA) += pxa_pcmcia.o
-COBJS-y += rpx_pcmcia.o
+#COBJS-y += rpx_pcmcia.o
+COBJS-$(CONFIG_RPX_PCMCIA) += rpx_pcmcia.o
 COBJS-$(CONFIG_IDE_TI_CARDBUS) += ti_pci1410a.o
-COBJS-y += tqm8xx_pcmcia.o
+#COBJS-y += tqm8xx_pcmcia.o
+COBJS-$(CONFIG_TQM8XX_PCMCIA) += tqm8xx_pcmcia.o
 COBJS-$(CONFIG_MARUBUN_PCCARD) += marubun_pcmcia.o
 
 COBJS	:= $(COBJS-y)
--- a/drivers/usb/phy/Makefile
+++ b/drivers/usb/phy/Makefile
@@ -23,7 +23,7 @@
 LIB	:= $(obj)libusb_phy.a
 
 COBJS-$(CONFIG_TWL4030_USB) += twl4030.o
-COBJS-y := twl4030.o
+#COBJS-y := twl4030.o
 
 COBJS	:= $(COBJS-y)
 SRCS	:= $(COBJS:.o=.c)
--- a/Makefile
+++ b/Makefile
@@ -3414,6 +3414,40 @@
 ## MIPS32 ifxcpe
 #########################################################################
 
+define arcadyan
+$(1)	: unconfig
+	@mkdir -p $(obj)include
+	@mkdir -p $(obj)board/arcadyan/
+	@[ -z "$$(findstring brnboot,$$@)" ] || \
+		{ echo "TEXT_BASE = 0x80002000" >$(obj)board/arcadyan/config.tmp ; \
+			echo "#define CONFIG_SYS_RAMBOOT" >>$(obj)include/config.h ; \
+			echo "#define CONFIG_SYS_BRNBOOT" >>$(obj)include/config.h ; \
+			$(XECHO) "... with brnboot configuration" ; \
+		}
+	@[ -z "$$(findstring ramboot,$$@)" ] || \
+		{ echo "TEXT_BASE = 0xA0400000" >$(obj)board/arcadyan/config.tmp ; \
+			echo "#define CONFIG_SYS_RAMBOOT" >>$(obj)include/config.h ; \
+			$(XECHO) "... with ramboot configuration" ; \
+		}
+	@if [ "$$(findstring flash,$$@)" ] ; then \
+               echo "#TEXT_BASE = 0xB0050000" >$(obj)board/arcadyan/config.tmp ; \
+		echo "#define CONFIG_BOOTSTRAP"  >>$(obj)include/config.h ; \
+		echo "#define CONFIG_USE_DDR_RAM"  >>$(obj)include/config.h ; \
+		echo "#define CONFIG_USE_DDR_RAM_CFG_psc166" >>$(obj)include/config.h ; \
+	fi
+	@$(MKCONFIG) -a $$(word 1,$$(subst _, ,$$@)) mips mips arcadyan "" danube
+endef
+
+$(eval $(call arcadyan, arv3527P%config))
+$(eval $(call arcadyan, arv4520PW%config))
+$(eval $(call arcadyan, arv452CPW%config))
+$(eval $(call arcadyan, arv4525PW%config))
+$(eval $(call arcadyan, arv4510PW%config))
+$(eval $(call arcadyan, arv4518PW%config))
+$(eval $(call arcadyan, arv7518PW%config))
+$(eval $(call arcadyan, arv752DPW%config))
+$(eval $(call arcadyan, arv752DPW22%config))
+
 easy50712%config	: unconfig
 	@mkdir -p $(obj)include
 	@mkdir -p $(obj)board/infineon/easy50712
--- a/net/tftp.c
+++ b/net/tftp.c
@@ -11,9 +11,9 @@
 #include "bootp.h"
 
 #define WELL_KNOWN_PORT	69		/* Well known TFTP port #		*/
-#define TIMEOUT		5000UL		/* Millisecs to timeout for lost pkt */
+#define TIMEOUT		10000UL		/* Millisecs to timeout for lost pkt */
 #ifndef	CONFIG_NET_RETRY_COUNT
-# define TIMEOUT_COUNT	10		/* # of timeouts before giving up  */
+# define TIMEOUT_COUNT	200		/* # of timeouts before giving up  */
 #else
 # define TIMEOUT_COUNT  (CONFIG_NET_RETRY_COUNT * 2)
 #endif
