From e66a022a80d73b1a5d2e02c9db2c42e8b9853b40 Mon Sep 17 00:00:00 2001
From: Ben Hutchings <ben@decadent.org.uk>
Date: Sat, 11 Dec 2010 20:17:54 +0000
Subject: [PATCH] arm/ixp4xx: Rename FREQ macro to avoid collisions
MIME-Version: 1.0
Content-Type: text/plain; charset=UTF-8
Content-Transfer-Encoding: 8bit

FREQ is a ridiculously short name for a platform-specific macro in a
generic header, and it now conflicts with an enumeration in the
gspca/ov519 driver.

Also delete conditional reference to ixp4xx_get_board_tick_rate()
which is not defined anywhere.

Signed-off-by: Ben Hutchings <ben@decadent.org.uk>
Signed-off-by: Krzysztof Hałasa <khc@pm.waw.pl>
---
 arch/arm/mach-ixp4xx/common.c             |    4 ++--
 arch/arm/mach-ixp4xx/include/mach/timex.h |    5 +++--
 drivers/input/misc/ixp4xx-beeper.c        |    6 +-----
 3 files changed, 6 insertions(+), 9 deletions(-)

--- a/arch/arm/mach-ixp4xx/common.c
+++ b/arch/arm/mach-ixp4xx/common.c
@@ -454,7 +454,7 @@ static struct clocksource clocksource_ix
 	.flags		= CLOCK_SOURCE_IS_CONTINUOUS,
 };
 
-unsigned long ixp4xx_timer_freq = FREQ;
+unsigned long ixp4xx_timer_freq = IXP4XX_TIMER_FREQ;
 EXPORT_SYMBOL(ixp4xx_timer_freq);
 static void __init ixp4xx_clocksource_init(void)
 {
@@ -530,7 +530,7 @@ static struct clock_event_device clockev
 
 static void __init ixp4xx_clockevent_init(void)
 {
-	clockevent_ixp4xx.mult = div_sc(FREQ, NSEC_PER_SEC,
+	clockevent_ixp4xx.mult = div_sc(IXP4XX_TIMER_FREQ, NSEC_PER_SEC,
 					clockevent_ixp4xx.shift);
 	clockevent_ixp4xx.max_delta_ns =
 		clockevent_delta2ns(0xfffffffe, &clockevent_ixp4xx);
--- a/arch/arm/mach-ixp4xx/include/mach/timex.h
+++ b/arch/arm/mach-ixp4xx/include/mach/timex.h
@@ -10,6 +10,7 @@
  * 66.66... MHz. We do a convulted calculation of CLOCK_TICK_RATE b/c the
  * timer register ignores the bottom 2 bits of the LATCH value.
  */
-#define FREQ 66666000
-#define CLOCK_TICK_RATE (((FREQ / HZ & ~IXP4XX_OST_RELOAD_MASK) + 1) * HZ)
+#define IXP4XX_TIMER_FREQ 66666000
+#define CLOCK_TICK_RATE \
+	(((IXP4XX_TIMER_FREQ / HZ & ~IXP4XX_OST_RELOAD_MASK) + 1) * HZ)
 
--- a/drivers/input/misc/ixp4xx-beeper.c
+++ b/drivers/input/misc/ixp4xx-beeper.c
@@ -69,11 +69,7 @@ static int ixp4xx_spkr_event(struct inpu
 	}
 
 	if (value > 20 && value < 32767)
-#ifndef FREQ
-		count = (ixp4xx_get_board_tick_rate() / (value * 4)) - 1;
-#else
-		count = (FREQ / (value * 4)) - 1;
-#endif
+		count = (IXP4XX_TIMER_FREQ / (value * 4)) - 1;
 
 	ixp4xx_spkr_control(pin, count);
 
